// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
// Copyright (C) 2016 ARM Ltd.

/dts-v1/;
#include "sun50i-h5.dtsi"
#include "sun50i-h5-cpu-opp.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/pinctrl/sun4i-a10.h>

/ {
	model = "Xunlong Orange Pi PC 2";
	compatible = "xunlong,orangepi-pc2", "allwinner,sun50i-h5";

	reg_vcc3v3: vcc3v3 {
		compatible = "regulator-fixed";
		regulator-name = "vcc3v3";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
	};

	aliases {
		ethernet0 = &emac;
		serial0 = &uart0;
	};

	chosen {
		stdout-path = "serial0:115200n8";
	};

	connector {
		compatible = "hdmi-connector";
		type = "a";

		port {
			hdmi_con_in: endpoint {
				remote-endpoint = <&hdmi_out_con>;
			};
		};
	};

	leds {
		compatible = "gpio-leds";

		led-0 {
			label = "orangepi:green:pwr";
			gpios = <&r_pio 0 10 GPIO_ACTIVE_HIGH>;
			default-state = "on";
		};

		led-1 {
			label = "orangepi:red:status";
			gpios = <&pio 0 20 GPIO_ACTIVE_HIGH>;
		};
	};

	gpio-keys {
		compatible = "gpio-keys";

		key-sw4 {
			label = "sw4";
			linux,code = <BTN_0>;
			gpios = <&r_pio 0 3 GPIO_ACTIVE_LOW>;
			wakeup-source;
		};
	};

	reg_gmac_3v3: gmac-3v3 {
		compatible = "regulator-fixed";
		regulator-name = "gmac-3v3";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		startup-delay-us = <100000>;
		enable-active-high;
		gpio = <&pio 3 6 GPIO_ACTIVE_HIGH>;
	};

	reg_usb0_vbus: usb0-vbus {
		compatible = "regulator-fixed";
		regulator-name = "usb0-vbus";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		enable-active-high;
		gpio = <&r_pio 0 2 GPIO_ACTIVE_HIGH>; /* PL2 */
		status = "okay";
	};
};

&codec {
	allwinner,audio-routing =
		"Line Out", "LINEOUT",
		"MIC1", "Mic",
		"Mic",  "MBIAS";
	status = "okay";
};

&cpu0 {
	cpu-supply = <&reg_vdd_cpux>;
};

&de {
	status = "okay";
};

&ehci0 {
	status = "okay";
};

&ehci1 {
	status = "okay";
};

&ehci2 {
	status = "okay";
};

&ehci3 {
	status = "okay";
};

&emac {
	pinctrl-names = "default";
	pinctrl-0 = <&emac_rgmii_pins>;
	phy-supply = <&reg_gmac_3v3>;
	phy-handle = <&ext_rgmii_phy>;
	phy-mode = "rgmii-id";
	status = "okay";
};

&external_mdio {
	ext_rgmii_phy: ethernet-phy@1 {
		compatible = "ethernet-phy-ieee802.3-c22";
		reg = <1>;
	};
};

&hdmi {
	status = "okay";
};

&hdmi_out {
	hdmi_out_con: endpoint {
		remote-endpoint = <&hdmi_con_in>;
	};
};

&ir {
	pinctrl-names = "default";
	pinctrl-0 = <&r_ir_rx_pin>;
	status = "okay";
};

&mmc0 {
	vmmc-supply = <&reg_vcc3v3>;
	disable-wp;
	bus-width = <4>;
	cd-gpios = <&pio 5 6 GPIO_ACTIVE_LOW>; /* PF6 */
	status = "okay";
};

&ohci0 {
	status = "okay";
};

&ohci1 {
	status = "okay";
};

&ohci2 {
	status = "okay";
};

&ohci3 {
	status = "okay";
};

&r_i2c {
	status = "okay";

	reg_vdd_cpux: regulator@65 {
		compatible = "silergy,sy8106a";
		reg = <0x65>;
		regulator-name = "vdd-cpux";
		silergy,fixed-microvolt = <1100000>;
		regulator-min-microvolt = <1000000>;
		regulator-max-microvolt = <1400000>;
		regulator-ramp-delay = <200>;
		regulator-boot-on;
		regulator-always-on;
	};
};

&spi0  {
	status = "okay";

	flash@0 {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <40000000>;
	};
};

&uart0 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart0_pa_pins>;
	status = "okay";
};

&uart1 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart1_pins>;
	status = "disabled";
};

&uart2 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart2_pins>;
	status = "disabled";
};

&usb_otg {
	dr_mode = "otg";
	status = "okay";
};

&usbphy {
	/* USB Type-A ports' VBUS is always on */
	usb0_id_det-gpios = <&pio 6 12 GPIO_ACTIVE_HIGH>; /* PG12 */
	usb0_vbus-supply = <&reg_usb0_vbus>;
	status = "okay";
};
