// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Device Tree Include file for NXP Layerscape-1028A family SoC.
 *
 * Copyright 2018-2020 NXP
 *
 * Harninder Rai <harninder.rai@nxp.com>
 *
 */

#include <dt-bindings/clock/fsl,qoriq-clockgen.h>
#include <dt-bindings/interrupt-controller/arm-gic.h>
#include <dt-bindings/thermal/thermal.h>

/ {
	compatible = "fsl,ls1028a";
	interrupt-parent = <&gic>;
	#address-cells = <2>;
	#size-cells = <2>;

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu0: cpu@0 {
			device_type = "cpu";
			compatible = "arm,cortex-a72";
			reg = <0x0>;
			enable-method = "psci";
			clocks = <&clockgen QORIQ_CLK_CMUX 0>;
			next-level-cache = <&l2>;
			cpu-idle-states = <&CPU_PW20>;
			#cooling-cells = <2>;
		};

		cpu1: cpu@1 {
			device_type = "cpu";
			compatible = "arm,cortex-a72";
			reg = <0x1>;
			enable-method = "psci";
			clocks = <&clockgen QORIQ_CLK_CMUX 0>;
			next-level-cache = <&l2>;
			cpu-idle-states = <&CPU_PW20>;
			#cooling-cells = <2>;
		};

		l2: l2-cache {
			compatible = "cache";
		};
	};

	idle-states {
		/*
		 * PSCI node is not added default, U-Boot will add missing
		 * parts if it determines to use PSCI.
		 */
		entry-method = "psci";

		CPU_PW20: cpu-pw20 {
			  compatible = "arm,idle-state";
			  idle-state-name = "PW20";
			  arm,psci-suspend-param = <0x0>;
			  entry-latency-us = <2000>;
			  exit-latency-us = <2000>;
			  min-residency-us = <6000>;
		};
	};

	sysclk: sysclk {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <100000000>;
		clock-output-names = "sysclk";
	};

	osc_27m: clock-osc-27m {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <27000000>;
		clock-output-names = "phy_27m";
	};

	dpclk: clock-controller@f1f0000 {
		compatible = "fsl,ls1028a-plldig";
		reg = <0x0 0xf1f0000 0x0 0xffff>;
		#clock-cells = <0>;
		clocks = <&osc_27m>;
	};

	firmware {
		optee: optee  {
			compatible = "linaro,optee-tz";
			method = "smc";
			status = "disabled";
		};
	};

	reboot {
		compatible ="syscon-reboot";
		regmap = <&rst>;
		offset = <0>;
		mask = <0x02>;
	};

	timer {
		compatible = "arm,armv8-timer";
		interrupts = <GIC_PPI 13 (GIC_CPU_MASK_SIMPLE(2) |
					  IRQ_TYPE_LEVEL_LOW)>,
			     <GIC_PPI 14 (GIC_CPU_MASK_SIMPLE(2) |
					  IRQ_TYPE_LEVEL_LOW)>,
			     <GIC_PPI 11 (GIC_CPU_MASK_SIMPLE(2) |
					  IRQ_TYPE_LEVEL_LOW)>,
			     <GIC_PPI 10 (GIC_CPU_MASK_SIMPLE(2) |
					  IRQ_TYPE_LEVEL_LOW)>;
	};

	pmu {
		compatible = "arm,cortex-a72-pmu";
		interrupts = <GIC_PPI 7 IRQ_TYPE_LEVEL_HIGH>;
	};

	gic: interrupt-controller@6000000 {
		compatible= "arm,gic-v3";
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;
		reg= <0x0 0x06000000 0 0x10000>, /* GIC Dist */
			<0x0 0x06040000 0 0x40000>; /* GIC Redistributor */
		#interrupt-cells= <3>;
		interrupt-controller;
		interrupts = <GIC_PPI 9 (GIC_CPU_MASK_RAW(0xf) |
					 IRQ_TYPE_LEVEL_LOW)>;
		its: gic-its@6020000 {
			compatible = "arm,gic-v3-its";
			msi-controller;
			reg = <0x0 0x06020000 0 0x20000>;/* GIC Translater */
		};
	};

	thermal-zones {
		ddr-controller {
			polling-delay-passive = <1000>;
			polling-delay = <5000>;
			thermal-sensors = <&tmu 0>;

			trips {
				ddr-ctrler-alert {
					temperature = <85000>;
					hysteresis = <2000>;
					type = "passive";
				};

				ddr-ctrler-crit {
					temperature = <95000>;
					hysteresis = <2000>;
					type = "critical";
				};
			};
		};

		core-cluster {
			polling-delay-passive = <1000>;
			polling-delay = <5000>;
			thermal-sensors = <&tmu 1>;

			trips {
				core_cluster_alert: core-cluster-alert {
					temperature = <85000>;
					hysteresis = <2000>;
					type = "passive";
				};

				core_cluster_crit: core-cluster-crit {
					temperature = <95000>;
					hysteresis = <2000>;
					type = "critical";
				};
			};

			cooling-maps {
				map0 {
					trip = <&core_cluster_alert>;
					cooling-device =
						<&cpu0 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
						<&cpu1 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
				};
			};
		};
	};

	soc: soc {
		compatible = "simple-bus";
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;

		ddr: memory-controller@1080000 {
			compatible = "fsl,qoriq-memory-controller";
			reg = <0x0 0x1080000 0x0 0x1000>;
			interrupts = <GIC_SPI 17 IRQ_TYPE_LEVEL_HIGH>;
			little-endian;
		};

		dcfg: syscon@1e00000 {
			#address-cells = <1>;
			#size-cells = <1>;
			compatible = "fsl,ls1028a-dcfg", "syscon", "simple-mfd";
			reg = <0x0 0x1e00000 0x0 0x10000>;
			ranges = <0x0 0x0 0x1e00000 0x10000>;
			little-endian;

			fspi_clk: clock-controller@900 {
				compatible = "fsl,ls1028a-flexspi-clk";
				reg = <0x900 0x4>;
				#clock-cells = <0>;
				clocks = <&clockgen QORIQ_CLK_HWACCEL 0>;
				clock-output-names = "fspi_clk";
			};
		};

		rst: syscon@1e60000 {
			compatible = "syscon";
			reg = <0x0 0x1e60000 0x0 0x10000>;
			little-endian;
		};

		scfg: syscon@1fc0000 {
			compatible = "fsl,ls1028a-scfg", "syscon";
			reg = <0x0 0x1fc0000 0x0 0x10000>;
			big-endian;
		};

		clockgen: clock-controller@1300000 {
			compatible = "fsl,ls1028a-clockgen";
			reg = <0x0 0x1300000 0x0 0xa0000>;
			#clock-cells = <2>;
			clocks = <&sysclk>;
		};

		i2c0: i2c@2000000 {
			compatible = "fsl,vf610-i2c";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0 0x2000000 0x0 0x10000>;
			interrupts = <GIC_SPI 34 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(4)>;
			status = "disabled";
		};

		i2c1: i2c@2010000 {
			compatible = "fsl,vf610-i2c";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0 0x2010000 0x0 0x10000>;
			interrupts = <GIC_SPI 34 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(4)>;
			status = "disabled";
		};

		i2c2: i2c@2020000 {
			compatible = "fsl,vf610-i2c";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0 0x2020000 0x0 0x10000>;
			interrupts = <GIC_SPI 35 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(4)>;
			status = "disabled";
		};

		i2c3: i2c@2030000 {
			compatible = "fsl,vf610-i2c";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0 0x2030000 0x0 0x10000>;
			interrupts = <GIC_SPI 35 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(4)>;
			status = "disabled";
		};

		i2c4: i2c@2040000 {
			compatible = "fsl,vf610-i2c";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0 0x2040000 0x0 0x10000>;
			interrupts = <GIC_SPI 74 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(4)>;
			status = "disabled";
		};

		i2c5: i2c@2050000 {
			compatible = "fsl,vf610-i2c";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0 0x2050000 0x0 0x10000>;
			interrupts = <GIC_SPI 74 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(4)>;
			status = "disabled";
		};

		i2c6: i2c@2060000 {
			compatible = "fsl,vf610-i2c";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0 0x2060000 0x0 0x10000>;
			interrupts = <GIC_SPI 75 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(4)>;
			status = "disabled";
		};

		i2c7: i2c@2070000 {
			compatible = "fsl,vf610-i2c";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0 0x2070000 0x0 0x10000>;
			interrupts = <GIC_SPI 75 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(4)>;
			status = "disabled";
		};

		fspi: spi@20c0000 {
			compatible = "nxp,lx2160a-fspi";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0 0x20c0000 0x0 0x10000>,
			      <0x0 0x20000000 0x0 0x10000000>;
			reg-names = "fspi_base", "fspi_mmap";
			interrupts = <GIC_SPI 25 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&fspi_clk>, <&fspi_clk>;
			clock-names = "fspi_en", "fspi";
			status = "disabled";
		};

		dspi0: spi@2100000 {
			compatible = "fsl,ls1028a-dspi", "fsl,ls1021a-v1.0-dspi";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0 0x2100000 0x0 0x10000>;
			interrupts = <GIC_SPI 26 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "dspi";
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>;
			dmas = <&edma0 0 62>, <&edma0 0 60>;
			dma-names = "tx", "rx";
			spi-num-chipselects = <4>;
			little-endian;
			status = "disabled";
		};

		dspi1: spi@2110000 {
			compatible = "fsl,ls1028a-dspi", "fsl,ls1021a-v1.0-dspi";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0 0x2110000 0x0 0x10000>;
			interrupts = <GIC_SPI 26 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "dspi";
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>;
			dmas = <&edma0 0 58>, <&edma0 0 56>;
			dma-names = "tx", "rx";
			spi-num-chipselects = <4>;
			little-endian;
			status = "disabled";
		};

		dspi2: spi@2120000 {
			compatible = "fsl,ls1028a-dspi", "fsl,ls1021a-v1.0-dspi";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0 0x2120000 0x0 0x10000>;
			interrupts = <GIC_SPI 26 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "dspi";
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>;
			dmas = <&edma0 0 54>, <&edma0 0 2>;
			dma-names = "tx", "rx";
			spi-num-chipselects = <3>;
			little-endian;
			status = "disabled";
		};

		esdhc: mmc@2140000 {
			compatible = "fsl,ls1028a-esdhc", "fsl,esdhc";
			reg = <0x0 0x2140000 0x0 0x10000>;
			interrupts = <GIC_SPI 28 IRQ_TYPE_LEVEL_HIGH>;
			clock-frequency = <0>; /* fixed up by bootloader */
			clocks = <&clockgen QORIQ_CLK_HWACCEL 1>;
			voltage-ranges = <1800 1800 3300 3300>;
			sdhci,auto-cmd12;
			little-endian;
			bus-width = <4>;
			status = "disabled";
		};

		esdhc1: mmc@2150000 {
			compatible = "fsl,ls1028a-esdhc", "fsl,esdhc";
			reg = <0x0 0x2150000 0x0 0x10000>;
			interrupts = <GIC_SPI 63 IRQ_TYPE_LEVEL_HIGH>;
			clock-frequency = <0>; /* fixed up by bootloader */
			clocks = <&clockgen QORIQ_CLK_HWACCEL 1>;
			voltage-ranges = <1800 1800>;
			sdhci,auto-cmd12;
			non-removable;
			little-endian;
			bus-width = <4>;
			status = "disabled";
		};

		can0: can@2180000 {
			compatible = "fsl,lx2160ar1-flexcan";
			reg = <0x0 0x2180000 0x0 0x10000>;
			interrupts = <GIC_SPI 21 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>,
				 <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>;
			clock-names = "ipg", "per";
			status = "disabled";
		};

		can1: can@2190000 {
			compatible = "fsl,lx2160ar1-flexcan";
			reg = <0x0 0x2190000 0x0 0x10000>;
			interrupts = <GIC_SPI 22 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>,
				 <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>;
			clock-names = "ipg", "per";
			status = "disabled";
		};

		duart0: serial@21c0500 {
			compatible = "fsl,ns16550", "ns16550a";
			reg = <0x00 0x21c0500 0x0 0x100>;
			interrupts = <GIC_SPI 32 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>;
			status = "disabled";
		};

		duart1: serial@21c0600 {
			compatible = "fsl,ns16550", "ns16550a";
			reg = <0x00 0x21c0600 0x0 0x100>;
			interrupts = <GIC_SPI 32 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>;
			status = "disabled";
		};


		lpuart0: serial@2260000 {
			compatible = "fsl,ls1028a-lpuart";
			reg = <0x0 0x2260000 0x0 0x1000>;
			interrupts = <GIC_SPI 232 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>;
			clock-names = "ipg";
			dma-names = "rx","tx";
			dmas = <&edma0 1 32>,
			       <&edma0 1 33>;
			status = "disabled";
		};

		lpuart1: serial@2270000 {
			compatible = "fsl,ls1028a-lpuart";
			reg = <0x0 0x2270000 0x0 0x1000>;
			interrupts = <GIC_SPI 233 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>;
			clock-names = "ipg";
			dma-names = "rx","tx";
			dmas = <&edma0 1 30>,
			       <&edma0 1 31>;
			status = "disabled";
		};

		lpuart2: serial@2280000 {
			compatible = "fsl,ls1028a-lpuart";
			reg = <0x0 0x2280000 0x0 0x1000>;
			interrupts = <GIC_SPI 234 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>;
			clock-names = "ipg";
			dma-names = "rx","tx";
			dmas = <&edma0 1 28>,
			       <&edma0 1 29>;
			status = "disabled";
		};

		lpuart3: serial@2290000 {
			compatible = "fsl,ls1028a-lpuart";
			reg = <0x0 0x2290000 0x0 0x1000>;
			interrupts = <GIC_SPI 235 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>;
			clock-names = "ipg";
			dma-names = "rx","tx";
			dmas = <&edma0 1 26>,
			       <&edma0 1 27>;
			status = "disabled";
		};

		lpuart4: serial@22a0000 {
			compatible = "fsl,ls1028a-lpuart";
			reg = <0x0 0x22a0000 0x0 0x1000>;
			interrupts = <GIC_SPI 236 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>;
			clock-names = "ipg";
			dma-names = "rx","tx";
			dmas = <&edma0 1 24>,
			       <&edma0 1 25>;
			status = "disabled";
		};

		lpuart5: serial@22b0000 {
			compatible = "fsl,ls1028a-lpuart";
			reg = <0x0 0x22b0000 0x0 0x1000>;
			interrupts = <GIC_SPI 237 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>;
			clock-names = "ipg";
			dma-names = "rx","tx";
			dmas = <&edma0 1 22>,
			       <&edma0 1 23>;
			status = "disabled";
		};

		edma0: dma-controller@22c0000 {
			#dma-cells = <2>;
			compatible = "fsl,ls1028a-edma", "fsl,vf610-edma";
			reg = <0x0 0x22c0000 0x0 0x10000>,
			      <0x0 0x22d0000 0x0 0x10000>,
			      <0x0 0x22e0000 0x0 0x10000>;
			interrupts = <GIC_SPI 56 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 56 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "edma-tx", "edma-err";
			dma-channels = <32>;
			clock-names = "dmamux0", "dmamux1";
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>,
				 <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>;
		};

		gpio1: gpio@2300000 {
			compatible = "fsl,ls1028a-gpio","fsl,qoriq-gpio";
			reg = <0x0 0x2300000 0x0 0x10000>;
			interrupts = <GIC_SPI 36 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			interrupt-controller;
			#interrupt-cells = <2>;
			little-endian;
		};

		gpio2: gpio@2310000 {
			compatible = "fsl,ls1028a-gpio","fsl,qoriq-gpio";
			reg = <0x0 0x2310000 0x0 0x10000>;
			interrupts = <GIC_SPI 36 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			interrupt-controller;
			#interrupt-cells = <2>;
			little-endian;
		};

		gpio3: gpio@2320000 {
			compatible = "fsl,ls1028a-gpio","fsl,qoriq-gpio";
			reg = <0x0 0x2320000 0x0 0x10000>;
			interrupts = <GIC_SPI 37 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			interrupt-controller;
			#interrupt-cells = <2>;
			little-endian;
		};

		usb0: usb@3100000 {
			compatible = "fsl,ls1028a-dwc3", "snps,dwc3";
			reg = <0x0 0x3100000 0x0 0x10000>;
			interrupts = <GIC_SPI 80 IRQ_TYPE_LEVEL_HIGH>;
			dr_mode = "host";
			snps,dis_rxdet_inp3_quirk;
			snps,quirk-frame-length-adjustment = <0x20>;
			snps,incr-burst-type-adjustment = <1>, <4>, <8>, <16>;
		};

		usb1: usb@3110000 {
			compatible = "fsl,ls1028a-dwc3", "snps,dwc3";
			reg = <0x0 0x3110000 0x0 0x10000>;
			interrupts = <GIC_SPI 81 IRQ_TYPE_LEVEL_HIGH>;
			dr_mode = "host";
			snps,dis_rxdet_inp3_quirk;
			snps,quirk-frame-length-adjustment = <0x20>;
			snps,incr-burst-type-adjustment = <1>, <4>, <8>, <16>;
		};

		sata: sata@3200000 {
			compatible = "fsl,ls1028a-ahci";
			reg = <0x0 0x3200000 0x0 0x10000>,
				<0x7 0x100520 0x0 0x4>;
			reg-names = "ahci", "sata-ecc";
			interrupts = <GIC_SPI 133 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>;
			status = "disabled";
		};

		pcie1: pcie@3400000 {
			compatible = "fsl,ls1028a-pcie";
			reg = <0x00 0x03400000 0x0 0x00100000>, /* controller registers */
			      <0x80 0x00000000 0x0 0x00002000>; /* configuration space */
			reg-names = "regs", "config";
			interrupts = <GIC_SPI 108 IRQ_TYPE_LEVEL_HIGH>, /* PME interrupt */
				     <GIC_SPI 109 IRQ_TYPE_LEVEL_HIGH>; /* aer interrupt */
			interrupt-names = "pme", "aer";
			#address-cells = <3>;
			#size-cells = <2>;
			device_type = "pci";
			dma-coherent;
			num-viewport = <8>;
			bus-range = <0x0 0xff>;
			ranges = <0x81000000 0x0 0x00000000 0x80 0x00010000 0x0 0x00010000   /* downstream I/O */
				  0x82000000 0x0 0x40000000 0x80 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
			msi-parent = <&its>;
			#interrupt-cells = <1>;
			interrupt-map-mask = <0 0 0 7>;
			interrupt-map = <0000 0 0 1 &gic 0 0 GIC_SPI 109 IRQ_TYPE_LEVEL_HIGH>,
					<0000 0 0 2 &gic 0 0 GIC_SPI 110 IRQ_TYPE_LEVEL_HIGH>,
					<0000 0 0 3 &gic 0 0 GIC_SPI 111 IRQ_TYPE_LEVEL_HIGH>,
					<0000 0 0 4 &gic 0 0 GIC_SPI 112 IRQ_TYPE_LEVEL_HIGH>;
			iommu-map = <0 &smmu 0 1>; /* Fixed-up by bootloader */
			status = "disabled";
		};

		pcie2: pcie@3500000 {
			compatible = "fsl,ls1028a-pcie";
			reg = <0x00 0x03500000 0x0 0x00100000>, /* controller registers */
			      <0x88 0x00000000 0x0 0x00002000>; /* configuration space */
			reg-names = "regs", "config";
			interrupts = <GIC_SPI 113 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 114 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "pme", "aer";
			#address-cells = <3>;
			#size-cells = <2>;
			device_type = "pci";
			dma-coherent;
			num-viewport = <8>;
			bus-range = <0x0 0xff>;
			ranges = <0x81000000 0x0 0x00000000 0x88 0x00010000 0x0 0x00010000   /* downstream I/O */
				  0x82000000 0x0 0x40000000 0x88 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
			msi-parent = <&its>;
			#interrupt-cells = <1>;
			interrupt-map-mask = <0 0 0 7>;
			interrupt-map = <0000 0 0 1 &gic 0 0 GIC_SPI 114 IRQ_TYPE_LEVEL_HIGH>,
					<0000 0 0 2 &gic 0 0 GIC_SPI 115 IRQ_TYPE_LEVEL_HIGH>,
					<0000 0 0 3 &gic 0 0 GIC_SPI 116 IRQ_TYPE_LEVEL_HIGH>,
					<0000 0 0 4 &gic 0 0 GIC_SPI 117 IRQ_TYPE_LEVEL_HIGH>;
			iommu-map = <0 &smmu 0 1>; /* Fixed-up by bootloader */
			status = "disabled";
		};

		smmu: iommu@5000000 {
			compatible = "arm,mmu-500";
			reg = <0 0x5000000 0 0x800000>;
			#global-interrupts = <8>;
			#iommu-cells = <1>;
			stream-match-mask = <0x7c00>;
			/* global secure fault */
			interrupts = <GIC_SPI 13 IRQ_TYPE_LEVEL_HIGH>,
			/* combined secure interrupt */
				     <GIC_SPI 14 IRQ_TYPE_LEVEL_HIGH>,
			/* global non-secure fault */
				     <GIC_SPI 15 IRQ_TYPE_LEVEL_HIGH>,
			/* combined non-secure interrupt */
				     <GIC_SPI 16 IRQ_TYPE_LEVEL_HIGH>,
			/* performance counter interrupts 0-7 */
				     <GIC_SPI 211 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 212 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 213 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 214 IRQ_TYPE_LEVEL_HIGH>,
			/* per context interrupt, 64 interrupts */
				     <GIC_SPI 146 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 147 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 148 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 150 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 151 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 152 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 153 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 154 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 155 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 156 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 157 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 158 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 159 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 160 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 161 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 162 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 163 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 164 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 165 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 166 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 167 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 168 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 169 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 170 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 171 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 172 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 173 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 174 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 175 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 176 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 177 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 178 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 179 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 180 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 181 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 182 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 183 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 184 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 185 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 186 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 187 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 188 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 189 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 190 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 191 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 192 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 193 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 194 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 195 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 196 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 197 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 198 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 199 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 200 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 201 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 202 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 203 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 204 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 205 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 206 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 207 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 208 IRQ_TYPE_LEVEL_HIGH>, <GIC_SPI 209 IRQ_TYPE_LEVEL_HIGH>;
		};

		crypto: crypto@8000000 {
			compatible = "fsl,sec-v5.0", "fsl,sec-v4.0";
			fsl,sec-era = <10>;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x00 0x8000000 0x100000>;
			reg = <0x00 0x8000000 0x0 0x100000>;
			interrupts = <GIC_SPI 139 IRQ_TYPE_LEVEL_HIGH>;
			dma-coherent;

			sec_jr0: jr@10000 {
				compatible = "fsl,sec-v5.0-job-ring",
					     "fsl,sec-v4.0-job-ring";
				reg	= <0x10000 0x10000>;
				interrupts = <GIC_SPI 140 IRQ_TYPE_LEVEL_HIGH>;
			};

			sec_jr1: jr@20000 {
				compatible = "fsl,sec-v5.0-job-ring",
					     "fsl,sec-v4.0-job-ring";
				reg	= <0x20000 0x10000>;
				interrupts = <GIC_SPI 141 IRQ_TYPE_LEVEL_HIGH>;
			};

			sec_jr2: jr@30000 {
				compatible = "fsl,sec-v5.0-job-ring",
					     "fsl,sec-v4.0-job-ring";
				reg	= <0x30000 0x10000>;
				interrupts = <GIC_SPI 142 IRQ_TYPE_LEVEL_HIGH>;
			};

			sec_jr3: jr@40000 {
				compatible = "fsl,sec-v5.0-job-ring",
					     "fsl,sec-v4.0-job-ring";
				reg	= <0x40000 0x10000>;
				interrupts = <GIC_SPI 143 IRQ_TYPE_LEVEL_HIGH>;
			};
		};

		qdma: dma-controller@8380000 {
			compatible = "fsl,ls1028a-qdma", "fsl,ls1021a-qdma";
			reg = <0x0 0x8380000 0x0 0x1000>, /* Controller regs */
			      <0x0 0x8390000 0x0 0x10000>, /* Status regs */
			      <0x0 0x83a0000 0x0 0x40000>; /* Block regs */
			interrupts = <GIC_SPI 43 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 251 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 252 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 253 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 254 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "qdma-error", "qdma-queue0",
				"qdma-queue1", "qdma-queue2", "qdma-queue3";
			dma-channels = <8>;
			block-number = <1>;
			block-offset = <0x10000>;
			fsl,dma-queues = <2>;
			status-sizes = <64>;
			queue-sizes = <64 64>;
		};

		cluster1_core0_watchdog: watchdog@c000000 {
			compatible = "arm,sp805", "arm,primecell";
			reg = <0x0 0xc000000 0x0 0x1000>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(16)>,
				 <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(16)>;
			clock-names = "wdog_clk", "apb_pclk";
		};

		cluster1_core1_watchdog: watchdog@c010000 {
			compatible = "arm,sp805", "arm,primecell";
			reg = <0x0 0xc010000 0x0 0x1000>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(16)>,
				 <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(16)>;
			clock-names = "wdog_clk", "apb_pclk";
		};

		sai1: audio-controller@f100000 {
			#sound-dai-cells = <0>;
			compatible = "fsl,vf610-sai";
			reg = <0x0 0xf100000 0x0 0x10000>;
			interrupts = <GIC_SPI 82 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>,
				 <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>,
				 <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>,
				 <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>;
			clock-names = "bus", "mclk1", "mclk2", "mclk3";
			dma-names = "tx", "rx";
			dmas = <&edma0 1 4>,
			       <&edma0 1 3>;
			fsl,sai-asynchronous;
			status = "disabled";
		};

		sai2: audio-controller@f110000 {
			#sound-dai-cells = <0>;
			compatible = "fsl,vf610-sai";
			reg = <0x0 0xf110000 0x0 0x10000>;
			interrupts = <GIC_SPI 82 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>,
				 <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>,
				 <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>,
				 <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>;
			clock-names = "bus", "mclk1", "mclk2", "mclk3";
			dma-names = "tx", "rx";
			dmas = <&edma0 1 6>,
			       <&edma0 1 5>;
			fsl,sai-asynchronous;
			status = "disabled";
		};

		sai3: audio-controller@f120000 {
			#sound-dai-cells = <0>;
			compatible = "fsl,vf610-sai";
			reg = <0x0 0xf120000 0x0 0x10000>;
			interrupts = <GIC_SPI 83 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>,
				 <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>,
				 <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>,
				 <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>;
			clock-names = "bus", "mclk1", "mclk2", "mclk3";
			dma-names = "tx", "rx";
			dmas = <&edma0 1 8>,
			       <&edma0 1 7>;
			fsl,sai-asynchronous;
			status = "disabled";
		};

		sai4: audio-controller@f130000 {
			#sound-dai-cells = <0>;
			compatible = "fsl,vf610-sai";
			reg = <0x0 0xf130000 0x0 0x10000>;
			interrupts = <GIC_SPI 83 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>,
				 <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>,
				 <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>,
				 <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>;
			clock-names = "bus", "mclk1", "mclk2", "mclk3";
			dma-names = "tx", "rx";
			dmas = <&edma0 1 10>,
			       <&edma0 1 9>;
			fsl,sai-asynchronous;
			status = "disabled";
		};

		sai5: audio-controller@f140000 {
			#sound-dai-cells = <0>;
			compatible = "fsl,vf610-sai";
			reg = <0x0 0xf140000 0x0 0x10000>;
			interrupts = <GIC_SPI 84 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>,
				 <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>,
				 <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>,
				 <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>;
			clock-names = "bus", "mclk1", "mclk2", "mclk3";
			dma-names = "tx", "rx";
			dmas = <&edma0 1 12>,
			       <&edma0 1 11>;
			fsl,sai-asynchronous;
			status = "disabled";
		};

		sai6: audio-controller@f150000 {
			#sound-dai-cells = <0>;
			compatible = "fsl,vf610-sai";
			reg = <0x0 0xf150000 0x0 0x10000>;
			interrupts = <GIC_SPI 84 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>,
				 <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>,
				 <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>,
				 <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>;
			clock-names = "bus", "mclk1", "mclk2", "mclk3";
			dma-names = "tx", "rx";
			dmas = <&edma0 1 14>,
			       <&edma0 1 13>;
			fsl,sai-asynchronous;
			status = "disabled";
		};

		tmu: tmu@1f80000 {
			compatible = "fsl,qoriq-tmu";
			reg = <0x0 0x1f80000 0x0 0x10000>;
			interrupts = <0 23 0x4>;
			fsl,tmu-range = <0xb0000 0xa0026 0x80048 0x70061>;
			fsl,tmu-calibration = <0x00000000 0x00000024
					       0x00000001 0x0000002b
					       0x00000002 0x00000031
					       0x00000003 0x00000038
					       0x00000004 0x0000003f
					       0x00000005 0x00000045
					       0x00000006 0x0000004c
					       0x00000007 0x00000053
					       0x00000008 0x00000059
					       0x00000009 0x00000060
					       0x0000000a 0x00000066
					       0x0000000b 0x0000006d

					       0x00010000 0x0000001c
					       0x00010001 0x00000024
					       0x00010002 0x0000002c
					       0x00010003 0x00000035
					       0x00010004 0x0000003d
					       0x00010005 0x00000045
					       0x00010006 0x0000004d
					       0x00010007 0x00000055
					       0x00010008 0x0000005e
					       0x00010009 0x00000066
					       0x0001000a 0x0000006e

					       0x00020000 0x00000018
					       0x00020001 0x00000022
					       0x00020002 0x0000002d
					       0x00020003 0x00000038
					       0x00020004 0x00000043
					       0x00020005 0x0000004d
					       0x00020006 0x00000058
					       0x00020007 0x00000063
					       0x00020008 0x0000006e

					       0x00030000 0x00000010
					       0x00030001 0x0000001c
					       0x00030002 0x00000029
					       0x00030003 0x00000036
					       0x00030004 0x00000042
					       0x00030005 0x0000004f
					       0x00030006 0x0000005b
					       0x00030007 0x00000068>;
			little-endian;
			#thermal-sensor-cells = <1>;
		};

		pcie@1f0000000 { /* Integrated Endpoint Root Complex */
			compatible = "pci-host-ecam-generic";
			reg = <0x01 0xf0000000 0x0 0x100000>;
			#address-cells = <3>;
			#size-cells = <2>;
			msi-parent = <&its>;
			device_type = "pci";
			bus-range = <0x0 0x0>;
			dma-coherent;
			msi-map = <0 &its 0x17 0xe>;
			iommu-map = <0 &smmu 0x17 0xe>;
				  /* PF0-6 BAR0 - non-prefetchable memory */
			ranges = <0x82000000 0x1 0xf8000000  0x1 0xf8000000  0x0 0x160000
				  /* PF0-6 BAR2 - prefetchable memory */
				  0xc2000000 0x1 0xf8160000  0x1 0xf8160000  0x0 0x070000
				  /* PF0: VF0-1 BAR0 - non-prefetchable memory */
				  0x82000000 0x1 0xf81d0000  0x1 0xf81d0000  0x0 0x020000
				  /* PF0: VF0-1 BAR2 - prefetchable memory */
				  0xc2000000 0x1 0xf81f0000  0x1 0xf81f0000  0x0 0x020000
				  /* PF1: VF0-1 BAR0 - non-prefetchable memory */
				  0x82000000 0x1 0xf8210000  0x1 0xf8210000  0x0 0x020000
				  /* PF1: VF0-1 BAR2 - prefetchable memory */
				  0xc2000000 0x1 0xf8230000  0x1 0xf8230000  0x0 0x020000
				  /* BAR4 (PF5) - non-prefetchable memory */
				  0x82000000 0x1 0xfc000000  0x1 0xfc000000  0x0 0x400000>;

			enetc_port0: ethernet@0,0 {
				compatible = "fsl,enetc";
				reg = <0x000000 0 0 0 0>;
				status = "disabled";
			};

			enetc_port1: ethernet@0,1 {
				compatible = "fsl,enetc";
				reg = <0x000100 0 0 0 0>;
				status = "disabled";
			};

			enetc_port2: ethernet@0,2 {
				compatible = "fsl,enetc";
				reg = <0x000200 0 0 0 0>;
				phy-mode = "internal";
				status = "disabled";

				fixed-link {
					speed = <2500>;
					full-duplex;
				};
			};

			enetc_mdio_pf3: mdio@0,3 {
				compatible = "fsl,enetc-mdio";
				reg = <0x000300 0 0 0 0>;
				#address-cells = <1>;
				#size-cells = <0>;
			};

			ethernet@0,4 {
				compatible = "fsl,enetc-ptp";
				reg = <0x000400 0 0 0 0>;
				clocks = <&clockgen QORIQ_CLK_HWACCEL 3>;
				little-endian;
				fsl,extts-fifo;
			};

			mscc_felix: ethernet-switch@0,5 {
				reg = <0x000500 0 0 0 0>;
				/* IEP INT_B */
				interrupts = <GIC_SPI 95 IRQ_TYPE_LEVEL_HIGH>;
				status = "disabled";

				ports {
					#address-cells = <1>;
					#size-cells = <0>;

					/* External ports */
					mscc_felix_port0: port@0 {
						reg = <0>;
						status = "disabled";
					};

					mscc_felix_port1: port@1 {
						reg = <1>;
						status = "disabled";
					};

					mscc_felix_port2: port@2 {
						reg = <2>;
						status = "disabled";
					};

					mscc_felix_port3: port@3 {
						reg = <3>;
						status = "disabled";
					};

					/* Internal ports */
					mscc_felix_port4: port@4 {
						reg = <4>;
						phy-mode = "internal";
						status = "disabled";

						fixed-link {
							speed = <2500>;
							full-duplex;
						};
					};

					mscc_felix_port5: port@5 {
						reg = <5>;
						phy-mode = "internal";
						status = "disabled";

						fixed-link {
							speed = <1000>;
							full-duplex;
						};
					};
				};
			};

			enetc_port3: ethernet@0,6 {
				compatible = "fsl,enetc";
				reg = <0x000600 0 0 0 0>;
				phy-mode = "internal";
				status = "disabled";

				fixed-link {
					speed = <1000>;
					full-duplex;
				};
			};

			rcec@1f,0 {
				reg = <0x00f800 0 0 0 0>;
				/* IEP INT_A */
				interrupts = <GIC_SPI 94 IRQ_TYPE_LEVEL_HIGH>;
			};
		};

		/* Integrated Endpoint Register Block */
		ierb@1f0800000 {
			compatible = "fsl,ls1028a-enetc-ierb";
			reg = <0x01 0xf0800000 0x0 0x10000>;
		};

		rcpm: power-controller@1e34040 {
			compatible = "fsl,ls1028a-rcpm", "fsl,qoriq-rcpm-2.1+";
			reg = <0x0 0x1e34040 0x0 0x1c>;
			#fsl,rcpm-wakeup-cells = <7>;
			little-endian;
		};

		ftm_alarm0: timer@2800000 {
			compatible = "fsl,ls1028a-ftm-alarm";
			reg = <0x0 0x2800000 0x0 0x10000>;
			fsl,rcpm-wakeup = <&rcpm 0x0 0x0 0x0 0x0 0x4000 0x0 0x0>;
			interrupts = <GIC_SPI 44 IRQ_TYPE_LEVEL_HIGH>;
		};
	};

	malidp0: display@f080000 {
		compatible = "arm,mali-dp500";
		reg = <0x0 0xf080000 0x0 0x10000>;
		interrupts = <0 222 IRQ_TYPE_LEVEL_HIGH>,
			     <0 223 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-names = "DE", "SE";
		clocks = <&dpclk>,
			 <&clockgen QORIQ_CLK_HWACCEL 2>,
			 <&clockgen QORIQ_CLK_HWACCEL 2>,
			 <&clockgen QORIQ_CLK_HWACCEL 2>;
		clock-names = "pxlclk", "mclk", "aclk", "pclk";
		arm,malidp-output-port-lines = /bits/ 8 <8 8 8>;
		arm,malidp-arqos-value = <0xd000d000>;

		port {
			dp0_out: endpoint {

			};
		};
	};
};
