// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Copyright 2021 Conley Lee
 * Conley Lee <conleylee@foxmail.com>
 */

/dts-v1/;
#include "sun7i-a20.dtsi"
#include "sunxi-common-regulators.dtsi"

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/interrupt-controller/irq.h>

/ {
	model = "HAOYU Electronics Marsboard A20";
	compatible = "haoyu,a20-marsboard", "allwinner,sun7i-a20";

	aliases {
		serial0 = &uart0;
	};

	chosen {
		stdout-path = "serial0:115200n8";
	};

	hdmi-connector {
		compatible = "hdmi-connector";
		type = "a";

		port {
			hdmi_con_in: endpoint {
				remote-endpoint = <&hdmi_out_con>;
			};
		};
	};
};

&ahci {
	target-supply = <&reg_ahci_5v>;
	status = "okay";
};

&codec {
	status = "okay";
};

&cpu0 {
	cpu-supply = <&reg_dcdc2>;
};

&de {
	status = "okay";
};

&ehci0 {
	status = "okay";
};

&ehci1 {
	status = "okay";
};

&gmac {
	pinctrl-names = "default";
	pinctrl-0 = <&gmac_mii_pins>, <&gmac_txerr>;
	phy-handle = <&phy0>;
	phy-mode = "mii";
	status = "okay";
};

&hdmi {
	status = "okay";
};

&hdmi_out {
	hdmi_out_con: endpoint {
		remote-endpoint = <&hdmi_con_in>;
	};
};

&i2c0 {
	status = "okay";

	axp209: pmic@34 {
		reg = <0x34>;
		interrupt-parent = <&nmi_intc>;
		interrupts = <0 IRQ_TYPE_LEVEL_LOW>;
	};
};

&mmc0 {
	vmmc-supply = <&reg_vcc3v3>;
	bus-width = <4>;
	cd-gpios = <&pio 7 10 GPIO_ACTIVE_LOW>; /* PH10 */
	status = "okay";
};

&gmac_mdio {
	phy0: ethernet-phy@0 {
		reg = <0>;
	};
};

&ohci0 {
	status = "okay";
};

&ohci1 {
	status = "okay";
};

&otg_sram {
	status = "okay";
};

&pio {
	gmac_txerr: gmac-txerr-pin {
		pins = "PA17";
		function = "gmac";
	};
};

&reg_ahci_5v {
	status = "okay";
};

#include "axp209.dtsi"

&ac_power_supply {
	status = "okay";
};

&reg_dcdc2 {
	regulator-always-on;
	regulator-min-microvolt = <1000000>;
	regulator-max-microvolt = <1450000>;
	regulator-name = "vdd-cpu";
};

&reg_dcdc3 {
	regulator-always-on;
	regulator-min-microvolt = <1000000>;
	regulator-max-microvolt = <1400000>;
	regulator-name = "vdd-int-dll";
};

&reg_ldo1 {
	regulator-name = "vdd-rtc";
};

&reg_ldo2 {
	regulator-always-on;
	regulator-min-microvolt = <3000000>;
	regulator-max-microvolt = <3000000>;
	regulator-name = "avcc";
};

&reg_usb1_vbus {
	status = "okay";
};

&reg_usb2_vbus {
	status = "okay";
};

&uart0 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart0_pb_pins>;
	status = "okay";
};

&usb_otg {
	dr_mode = "otg";
	status = "okay";
};

&usbphy {
	usb0_id_det-gpios = <&pio 7 4 (GPIO_ACTIVE_HIGH | GPIO_PULL_UP)>; /* PH4 */
	usb1_vbus-supply = <&reg_usb1_vbus>;
	usb2_vbus-supply = <&reg_usb2_vbus>;
	status = "okay";
};
