// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
// Copyright (c) 2019 Jernej Skrabec <jernej.skrabec@siol.net>

/dts-v1/;

#include "sun50i-h6.dtsi"
#include "sun50i-h6-cpu-opp.dtsi"

#include <dt-bindings/gpio/gpio.h>

/ {
	aliases {
		serial0 = &uart0;
	};

	chosen {
		stdout-path = "serial0:115200n8";
	};

	connector {
		compatible = "hdmi-connector";
		ddc-en-gpios = <&pio 7 2 GPIO_ACTIVE_HIGH>; /* PH2 */
		type = "a";

		port {
			hdmi_con_in: endpoint {
				remote-endpoint = <&hdmi_out_con>;
			};
		};
	};

	/* used for FD650 LED display driver */
	i2c {
		compatible = "i2c-gpio";
		sda-gpios = <&pio 7 6 (GPIO_ACTIVE_HIGH|GPIO_OPEN_DRAIN)>; /* PH6 */
		scl-gpios = <&pio 7 5 (GPIO_ACTIVE_HIGH|GPIO_OPEN_DRAIN)>; /* PH5 */
		i2c-gpio,delay-us = <5>;
	};

	reg_vcc1v8: regulator-vcc1v8 {
		compatible = "regulator-fixed";
		regulator-name = "vcc1v8";
		regulator-min-microvolt = <1800000>;
		regulator-max-microvolt = <1800000>;
	};

	reg_vcc3v3: regulator-vcc3v3 {
		compatible = "regulator-fixed";
		regulator-name = "vcc3v3";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
	};

	reg_vdd_cpu_gpu: regulator-vdd-cpu-gpu {
		compatible = "regulator-fixed";
		regulator-name = "vdd-cpu-gpu";
		regulator-min-microvolt = <1135000>;
		regulator-max-microvolt = <1135000>;
	};

	sound-spdif {
		compatible = "simple-audio-card";
		simple-audio-card,name = "sun50i-h6-spdif";

		simple-audio-card,cpu {
			sound-dai = <&spdif>;
		};

		simple-audio-card,codec {
			sound-dai = <&spdif_out>;
		};
	};

	spdif_out: spdif-out {
		#sound-dai-cells = <0>;
		compatible = "linux,spdif-dit";
	};

	wifi_pwrseq: wifi-pwrseq {
		compatible = "mmc-pwrseq-simple";
		clocks = <&rtc CLK_OSC32K_FANOUT>;
		clock-names = "ext_clock";
		reset-gpios = <&r_pio 1 3 GPIO_ACTIVE_LOW>; /* PM3 */
	};
};

&cpu0 {
	cpu-supply = <&reg_vdd_cpu_gpu>;
};

&de {
	status = "okay";
};

&dwc3 {
	status = "okay";
};

&ehci0 {
	status = "okay";
};

&ehci3 {
	status = "okay";
};

&gpu {
	mali-supply = <&reg_vdd_cpu_gpu>;
	status = "okay";
};

&hdmi {
	status = "okay";
};

&hdmi_out {
	hdmi_out_con: endpoint {
		remote-endpoint = <&hdmi_con_in>;
	};
};

&mmc0 {
	pinctrl-names = "default";
	pinctrl-0 = <&mmc0_pins>;
	vmmc-supply = <&reg_vcc3v3>;
	cd-gpios = <&pio 5 6 GPIO_ACTIVE_LOW>;
	disable-wp;
	bus-width = <4>;
	status = "okay";
};

&mmc1 {
	vmmc-supply = <&reg_vcc3v3>;
	vqmmc-supply = <&reg_vcc1v8>;
	mmc-pwrseq = <&wifi_pwrseq>;
	bus-width = <4>;
	non-removable;
	status = "okay";
};

&mmc2 {
	vmmc-supply = <&reg_vcc3v3>;
	vqmmc-supply = <&reg_vcc1v8>;
	bus-width = <8>;
	non-removable;
	cap-mmc-hw-reset;
	mmc-hs200-1_8v;
	status = "okay";
};

&ohci0 {
	status = "okay";
};

&ohci3 {
	status = "okay";
};

&pio {
	vcc-pc-supply = <&reg_vcc1v8>;
	vcc-pd-supply = <&reg_vcc3v3>;
	vcc-pg-supply = <&reg_vcc1v8>;
};

&r_ir {
	status = "okay";
};

&spdif {
	pinctrl-names = "default";
	pinctrl-0 = <&spdif_tx_pin>;
	status = "okay";
};

&uart0 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart0_ph_pins>;
	status = "okay";
};

&usb2otg {
	dr_mode = "host";
	status = "okay";
};

&usb2phy {
	status = "okay";
};

&usb3phy {
	status = "okay";
};
