// SPDX-License-Identifier: GPL-2.0+ OR BSD-3-Clause
/*
 * Copyright (C) 2022 Marek Vasut <marex@denx.de>
 */

#include "stm32mp15xx-dhcor-u-boot.dtsi"

/ {
	aliases {
		mmc0 = &sdmmc1;
		mmc1 = &sdmmc2;
		usb0 = &usbotg_hs;
	};

	config {
		dh,board-coding-gpios = <&gpiog 13 0>, <&gpiod 9 0>;
	};
};

&ethernet0 {
	phy-reset-gpios = <&gpioz 2 GPIO_ACTIVE_LOW>;

	mdio0 {
		ethernet-phy@7 {
			reset-gpios = <&gpioz 2 GPIO_ACTIVE_LOW>;
			reset-assert-us = <11000>;
			reset-deassert-us = <1000>;
		};
	};
};

&sdmmc1 {
	bootph-pre-ram;
	st,use-ckin;
	st,cmd-gpios = <&gpiod 2 0>;
	st,ck-gpios = <&gpioc 12 0>;
	st,ckin-gpios = <&gpioe 4 0>;
};

&sdmmc1_b4_pins_a {
	bootph-pre-ram;
	pins1 {
		bootph-pre-ram;
	};
	pins2 {
		bootph-pre-ram;
	};
};

&sdmmc1_dir_pins_b {
	bootph-pre-ram;
	pins1 {
		bootph-pre-ram;
	};
	pins2 {
		bootph-pre-ram;
	};
};

&sdmmc2 {
	bootph-pre-ram;
};

&sdmmc2_b4_pins_a {
	bootph-pre-ram;
	pins1 {
		bootph-pre-ram;
	};
	pins2 {
		bootph-pre-ram;
	};
};

&sdmmc2_d47_pins_c {
	bootph-pre-ram;
	pins {
		bootph-pre-ram;
	};
};

&uart4 {
	bootph-all;
};

&uart4_pins_b {
	bootph-all;
	pins1 {
		bootph-all;
	};
	pins2 {
		bootph-all;
		/delete-property/ bias-disable;
		bias-pull-up;
	};
};

&usbotg_hs {
	u-boot,force-b-session-valid;
	hnp-srp-disable;
};
