/dts-v1/;

#include <dt-bindings/input/input.h>
#include "tegra20.dtsi"

/ {
	model = "NVIDIA Tegra20 Ventana evaluation board";
	compatible = "nvidia,ventana", "nvidia,tegra20";

	chosen {
		stdout-path = &uartd;
	};

	aliases {
		rtc0 = "/i2c@7000d000/tps6586x@34";
		rtc1 = "/rtc@7000e000";
		serial0 = &uartd;
		usb0 = "/usb@c5000000";
		usb1 = "/usb@c5004000";
		usb2 = "/usb@c5008000";
		mmc0 = "/sdhci@c8000600";
		mmc1 = "/sdhci@c8000400";
	};

	memory {
		reg = <0x00000000 0x40000000>;
	};

	host1x@50000000 {
		status = "okay";
		dc@54200000 {
			status = "okay";
			rgb {
				status = "okay";

				nvidia,panel = <&panel>;

				display-timings {
					timing@0 {
						/* Seaboard has 1366x768 */
						clock-frequency = <70600000>;
						hactive = <1366>;
						vactive = <768>;
						hback-porch = <58>;
						hfront-porch = <58>;
						hsync-len = <58>;
						vback-porch = <4>;
						vfront-porch = <4>;
						vsync-len = <4>;
						hsync-active = <1>;
					};
				};
			};
		};

		hdmi@54280000 {
			status = "okay";

			vdd-supply = <&hdmi_vdd_reg>;
			pll-supply = <&hdmi_pll_reg>;

			nvidia,ddc-i2c-bus = <&hdmi_ddc>;
			nvidia,hpd-gpio = <&gpio TEGRA_GPIO(N, 7)
				GPIO_ACTIVE_HIGH>;
		};
	};

	pinmux@70000014 {
		pinctrl-names = "default";
		pinctrl-0 = <&state_default>;

		state_default: pinmux {
			ata {
				nvidia,pins = "ata";
				nvidia,function = "ide";
			};
			atb {
				nvidia,pins = "atb", "gma", "gme";
				nvidia,function = "sdio4";
			};
			atc {
				nvidia,pins = "atc";
				nvidia,function = "nand";
			};
			atd {
				nvidia,pins = "atd", "ate", "gmb", "spia",
					"spib", "spic";
				nvidia,function = "gmi";
			};
			cdev1 {
				nvidia,pins = "cdev1";
				nvidia,function = "plla_out";
			};
			cdev2 {
				nvidia,pins = "cdev2";
				nvidia,function = "pllp_out4";
			};
			crtp {
				nvidia,pins = "crtp", "lm1";
				nvidia,function = "crt";
			};
			csus {
				nvidia,pins = "csus";
				nvidia,function = "vi_sensor_clk";
			};
			dap1 {
				nvidia,pins = "dap1";
				nvidia,function = "dap1";
			};
			dap2 {
				nvidia,pins = "dap2";
				nvidia,function = "dap2";
			};
			dap3 {
				nvidia,pins = "dap3";
				nvidia,function = "dap3";
			};
			dap4 {
				nvidia,pins = "dap4";
				nvidia,function = "dap4";
			};
			dta {
				nvidia,pins = "dta", "dtb", "dtc", "dtd", "dte";
				nvidia,function = "vi";
			};
			dtf {
				nvidia,pins = "dtf";
				nvidia,function = "i2c3";
			};
			gmc {
				nvidia,pins = "gmc";
				nvidia,function = "uartd";
			};
			gmd {
				nvidia,pins = "gmd";
				nvidia,function = "sflash";
			};
			gpu {
				nvidia,pins = "gpu";
				nvidia,function = "pwm";
			};
			gpu7 {
				nvidia,pins = "gpu7";
				nvidia,function = "rtck";
			};
			gpv {
				nvidia,pins = "gpv", "slxa", "slxk";
				nvidia,function = "pcie";
			};
			hdint {
				nvidia,pins = "hdint";
				nvidia,function = "hdmi";
			};
			i2cp {
				nvidia,pins = "i2cp";
				nvidia,function = "i2cp";
			};
			irrx {
				nvidia,pins = "irrx", "irtx";
				nvidia,function = "uartb";
			};
			kbca {
				nvidia,pins = "kbca", "kbcb", "kbcc", "kbcd",
					"kbce", "kbcf";
				nvidia,function = "kbc";
			};
			lcsn {
				nvidia,pins = "lcsn", "ldc", "lm0", "lpw1",
					"lsdi", "lvp0";
				nvidia,function = "rsvd4";
			};
			ld0 {
				nvidia,pins = "ld0", "ld1", "ld2", "ld3", "ld4",
					"ld5", "ld6", "ld7", "ld8", "ld9",
					"ld10", "ld11", "ld12", "ld13", "ld14",
					"ld15", "ld16", "ld17", "ldi", "lhp0",
					"lhp1", "lhp2", "lhs", "lpp", "lpw0",
					"lpw2", "lsc0", "lsc1", "lsck", "lsda",
					"lspi", "lvp1", "lvs";
				nvidia,function = "displaya";
			};
			owc {
				nvidia,pins = "owc", "spdi", "spdo", "uac";
				nvidia,function = "rsvd2";
			};
			pmc {
				nvidia,pins = "pmc";
				nvidia,function = "pwr_on";
			};
			rm {
				nvidia,pins = "rm";
				nvidia,function = "i2c1";
			};
			sdb {
				nvidia,pins = "sdb", "sdc", "sdd", "slxc";
				nvidia,function = "sdio3";
			};
			sdio1 {
				nvidia,pins = "sdio1";
				nvidia,function = "sdio1";
			};
			slxd {
				nvidia,pins = "slxd";
				nvidia,function = "spdif";
			};
			spid {
				nvidia,pins = "spid", "spie", "spif";
				nvidia,function = "spi1";
			};
			spig {
				nvidia,pins = "spig", "spih";
				nvidia,function = "spi2_alt";
			};
			uaa {
				nvidia,pins = "uaa", "uab", "uda";
				nvidia,function = "ulpi";
			};
			uad {
				nvidia,pins = "uad";
				nvidia,function = "irda";
			};
			uca {
				nvidia,pins = "uca", "ucb";
				nvidia,function = "uartc";
			};
			conf_ata {
				nvidia,pins = "ata", "atb", "atc", "atd",
					"cdev1", "cdev2", "dap1", "dap2",
					"dap4", "ddc", "dtf", "gma", "gmc",
					"gme", "gpu", "gpu7", "i2cp", "irrx",
					"irtx", "pta", "rm", "sdc", "sdd",
					"slxc", "slxd", "slxk", "spdi", "spdo",
					"uac", "uad", "uca", "ucb", "uda";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
			};
			conf_ate {
				nvidia,pins = "ate", "csus", "dap3", "gmd",
					"gpv", "owc", "spia", "spib", "spic",
					"spid", "spie", "spig";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
			};
			conf_ck32 {
				nvidia,pins = "ck32", "ddrc", "pmca", "pmcb",
					"pmcc", "pmcd", "pmce", "xm2c", "xm2d";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
			};
			conf_crtp {
				nvidia,pins = "crtp", "gmb", "slxa", "spih";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
			};
			conf_dta {
				nvidia,pins = "dta", "dtb", "dtc", "dtd";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
			};
			conf_dte {
				nvidia,pins = "dte", "spif";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
			};
			conf_hdint {
				nvidia,pins = "hdint", "lcsn", "ldc", "lm1",
					"lpw1", "lsck", "lsda", "lsdi", "lvp0";
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
			};
			conf_kbca {
				nvidia,pins = "kbca", "kbcb", "kbcc", "kbcd",
					"kbce", "kbcf", "sdio1", "uaa", "uab";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
			};
			conf_lc {
				nvidia,pins = "lc", "ls";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
			};
			conf_ld0 {
				nvidia,pins = "ld0", "ld1", "ld2", "ld3", "ld4",
					"ld5", "ld6", "ld7", "ld8", "ld9",
					"ld10", "ld11", "ld12", "ld13", "ld14",
					"ld15", "ld16", "ld17", "ldi", "lhp0",
					"lhp1", "lhp2", "lhs", "lm0", "lpp",
					"lpw0", "lpw2", "lsc0", "lsc1", "lspi",
					"lvp1", "lvs", "pmc", "sdb";
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
			};
			conf_ld17_0 {
				nvidia,pins = "ld17_0", "ld19_18", "ld21_20",
					"ld23_22";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
			};
			drive_sdio1 {
				nvidia,pins = "drive_sdio1";
				nvidia,high-speed-mode = <TEGRA_PIN_DISABLE>;
				nvidia,schmitt = <TEGRA_PIN_ENABLE>;
				nvidia,low-power-mode = <TEGRA_PIN_LP_DRIVE_DIV_1>;
				nvidia,pull-down-strength = <31>;
				nvidia,pull-up-strength = <31>;
				nvidia,slew-rate-rising = <TEGRA_PIN_SLEW_RATE_SLOWEST>;
				nvidia,slew-rate-falling = <TEGRA_PIN_SLEW_RATE_SLOWEST>;
			};
		};

		state_i2cmux_ddc: pinmux_i2cmux_ddc {
			ddc {
				nvidia,pins = "ddc";
				nvidia,function = "i2c2";
			};
			pta {
				nvidia,pins = "pta";
				nvidia,function = "rsvd4";
			};
		};

		state_i2cmux_pta: pinmux_i2cmux_pta {
			ddc {
				nvidia,pins = "ddc";
				nvidia,function = "rsvd4";
			};
			pta {
				nvidia,pins = "pta";
				nvidia,function = "i2c2";
			};
		};

		state_i2cmux_idle: pinmux_i2cmux_idle {
			ddc {
				nvidia,pins = "ddc";
				nvidia,function = "rsvd4";
			};
			pta {
				nvidia,pins = "pta";
				nvidia,function = "rsvd4";
			};
		};
	};

	i2s@70002800 {
		status = "okay";
	};

	serial@70006300 {
		status = "okay";
		clock-frequency = < 216000000 >;	};

	pwm: pwm@7000a000 {
		status = "okay";
	};

	i2c@7000c000 {
		status = "okay";
		clock-frequency = <400000>;

		wm8903: wm8903@1a {
			compatible = "wlf,wm8903";
			reg = <0x1a>;
			interrupt-parent = <&gpio>;
			interrupts = <TEGRA_GPIO(X, 3) IRQ_TYPE_LEVEL_HIGH>;

			gpio-controller;
			#gpio-cells = <2>;

			micdet-cfg = <0>;
			micdet-delay = <100>;
			gpio-cfg = <0xffffffff 0xffffffff 0 0xffffffff 0xffffffff>;
		};

		/* ALS and proximity sensor */
		isl29018@44 {
			compatible = "isil,isl29018";
			reg = <0x44>;
			interrupt-parent = <&gpio>;
			interrupts = <TEGRA_GPIO(Z, 2) IRQ_TYPE_LEVEL_HIGH>;
		};
	};

	i2c@7000c400 {
		status = "okay";
		clock-frequency = <100000>;
	};

	i2cmux {
		compatible = "i2c-mux-pinctrl";
		#address-cells = <1>;
		#size-cells = <0>;

		i2c-parent = <&{/i2c@7000c400}>;

		pinctrl-names = "ddc", "pta", "idle";
		pinctrl-0 = <&state_i2cmux_ddc>;
		pinctrl-1 = <&state_i2cmux_pta>;
		pinctrl-2 = <&state_i2cmux_idle>;

		hdmi_ddc: i2c@0 {
			reg = <0>;
			#address-cells = <1>;
			#size-cells = <0>;
		};

		lvds_ddc: i2c@1 {
			reg = <1>;
			#address-cells = <1>;
			#size-cells = <0>;
		};
	};

	i2c@7000c500 {
		status = "okay";
		clock-frequency = <400000>;
	};

	i2c@7000d000 {
		status = "okay";
		clock-frequency = <400000>;

		pmic: tps6586x@34 {
			compatible = "ti,tps6586x";
			reg = <0x34>;
			interrupts = <GIC_SPI 86 IRQ_TYPE_LEVEL_HIGH>;

			ti,system-power-controller;

			#gpio-cells = <2>;
			gpio-controller;

			sys-supply = <&vdd_5v0_reg>;
			vin-sm0-supply = <&sys_reg>;
			vin-sm1-supply = <&sys_reg>;
			vin-sm2-supply = <&sys_reg>;
			vinldo01-supply = <&sm2_reg>;
			vinldo23-supply = <&sm2_reg>;
			vinldo4-supply = <&sm2_reg>;
			vinldo678-supply = <&sm2_reg>;
			vinldo9-supply = <&sm2_reg>;

			regulators {
				sys_reg: sys {
					regulator-name = "vdd_sys";
					regulator-always-on;
				};

				sm0 {
					regulator-name = "vdd_sm0,vdd_core";
					regulator-min-microvolt = <1200000>;
					regulator-max-microvolt = <1200000>;
					regulator-always-on;
				};

				sm1 {
					regulator-name = "vdd_sm1,vdd_cpu";
					regulator-min-microvolt = <1000000>;
					regulator-max-microvolt = <1000000>;
					regulator-always-on;
				};

				sm2_reg: sm2 {
					regulator-name = "vdd_sm2,vin_ldo*";
					regulator-min-microvolt = <3700000>;
					regulator-max-microvolt = <3700000>;
					regulator-always-on;
				};

				/* LDO0 is not connected to anything */

				ldo1 {
					regulator-name = "vdd_ldo1,avdd_pll*";
					regulator-min-microvolt = <1100000>;
					regulator-max-microvolt = <1100000>;
					regulator-always-on;
				};

				ldo2 {
					regulator-name = "vdd_ldo2,vdd_rtc";
					regulator-min-microvolt = <1200000>;
					regulator-max-microvolt = <1200000>;
				};

				ldo3 {
					regulator-name = "vdd_ldo3,avdd_usb*";
					regulator-min-microvolt = <3300000>;
					regulator-max-microvolt = <3300000>;
					regulator-always-on;
				};

				ldo4 {
					regulator-name = "vdd_ldo4,avdd_osc,vddio_sys";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
					regulator-always-on;
				};

				ldo5 {
					regulator-name = "vdd_ldo5,vcore_mmc";
					regulator-min-microvolt = <2850000>;
					regulator-max-microvolt = <2850000>;
					regulator-always-on;
				};

				ldo6 {
					regulator-name = "vdd_ldo6,avdd_vdac";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
				};

				hdmi_vdd_reg: ldo7 {
					regulator-name = "vdd_ldo7,avdd_hdmi,vdd_fuse";
					regulator-min-microvolt = <3300000>;
					regulator-max-microvolt = <3300000>;
				};

				hdmi_pll_reg: ldo8 {
					regulator-name = "vdd_ldo8,avdd_hdmi_pll";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
				};

				ldo9 {
					regulator-name = "vdd_ldo9,avdd_2v85,vdd_ddr_rx";
					regulator-min-microvolt = <2850000>;
					regulator-max-microvolt = <2850000>;
					regulator-always-on;
				};

				ldo_rtc {
					regulator-name = "vdd_rtc_out,vdd_cell";
					regulator-min-microvolt = <3300000>;
					regulator-max-microvolt = <3300000>;
					regulator-always-on;
				};
			};
		};

		temperature-sensor@4c {
			compatible = "onnn,nct1008";
			reg = <0x4c>;
		};
	};

	pmc@7000e400 {
		nvidia,invert-interrupt;
		nvidia,suspend-mode = <1>;
		nvidia,cpu-pwr-good-time = <2000>;
		nvidia,cpu-pwr-off-time = <100>;
		nvidia,core-pwr-good-time = <3845 3845>;
		nvidia,core-pwr-off-time = <458>;
		nvidia,sys-clock-req-active-high;
	};

	usb@c5000000 {
		status = "okay";
	};

	usb-phy@c5000000 {
		status = "okay";
	};

	usb@c5004000 {
		status = "okay";
		nvidia,phy-reset-gpio = <&gpio TEGRA_GPIO(V, 1)
			GPIO_ACTIVE_LOW>;
	};

	usb-phy@c5004000 {
		status = "okay";
		nvidia,phy-reset-gpio = <&gpio TEGRA_GPIO(V, 1)
			GPIO_ACTIVE_LOW>;
	};

	usb@c5008000 {
		status = "okay";
	};

	usb-phy@c5008000 {
		status = "okay";
	};

	sdhci@c8000000 {
		status = "okay";
		power-gpios = <&gpio TEGRA_GPIO(K, 6) GPIO_ACTIVE_HIGH>;
		bus-width = <4>;
		keep-power-in-suspend;
	};

	sdhci@c8000400 {
		status = "okay";
		cd-gpios = <&gpio TEGRA_GPIO(I, 5) GPIO_ACTIVE_LOW>;
		wp-gpios = <&gpio TEGRA_GPIO(H, 1) GPIO_ACTIVE_HIGH>;
		power-gpios = <&gpio TEGRA_GPIO(I, 6) GPIO_ACTIVE_HIGH>;
		bus-width = <4>;
	};

	sdhci@c8000600 {
		status = "okay";
		bus-width = <8>;
		non-removable;
	};

	backlight: backlight {
		compatible = "pwm-backlight";

		enable-gpios = <&gpio TEGRA_GPIO(D, 4) GPIO_ACTIVE_HIGH>;
		power-supply = <&vdd_bl_reg>;
		pwms = <&pwm 2 5000000>;

		brightness-levels = <0 4 8 16 32 64 128 255>;
		default-brightness-level = <6>;
	};

	clocks {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <0>;

		clk32k_in: clock@0 {
			compatible = "fixed-clock";
			reg=<0>;
			#clock-cells = <0>;
			clock-frequency = <32768>;
		};
	};

	gpio-keys {
		compatible = "gpio-keys";

		power {
			label = "Power";
			gpios = <&gpio TEGRA_GPIO(V, 2) GPIO_ACTIVE_LOW>;
			linux,code = <KEY_POWER>;
			gpio-key,wakeup;
		};
	};

	panel: panel {
		compatible = "chunghwa,claa101wa01a", "simple-panel";

		power-supply = <&vdd_pnl_reg>;
		enable-gpios = <&gpio TEGRA_GPIO(B, 2) GPIO_ACTIVE_HIGH>;

		backlight = <&backlight>;
		ddc-i2c-bus = <&lvds_ddc>;
	};

	regulators {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <0>;

		vdd_5v0_reg: regulator@0 {
			compatible = "regulator-fixed";
			reg = <0>;
			regulator-name = "vdd_5v0";
			regulator-min-microvolt = <5000000>;
			regulator-max-microvolt = <5000000>;
			regulator-always-on;
		};

		regulator@1 {
			compatible = "regulator-fixed";
			reg = <1>;
			regulator-name = "vdd_1v5";
			regulator-min-microvolt = <1500000>;
			regulator-max-microvolt = <1500000>;
			gpio = <&pmic 0 GPIO_ACTIVE_HIGH>;
		};

		regulator@2 {
			compatible = "regulator-fixed";
			reg = <2>;
			regulator-name = "vdd_1v2";
			regulator-min-microvolt = <1200000>;
			regulator-max-microvolt = <1200000>;
			gpio = <&pmic 1 GPIO_ACTIVE_HIGH>;
			enable-active-high;
		};

		vdd_pnl_reg: regulator@3 {
			compatible = "regulator-fixed";
			reg = <3>;
			regulator-name = "vdd_pnl";
			regulator-min-microvolt = <2800000>;
			regulator-max-microvolt = <2800000>;
			gpio = <&gpio TEGRA_GPIO(C, 6) GPIO_ACTIVE_HIGH>;
			enable-active-high;
		};

		vdd_bl_reg: regulator@4 {
			compatible = "regulator-fixed";
			reg = <4>;
			regulator-name = "vdd_bl";
			regulator-min-microvolt = <2800000>;
			regulator-max-microvolt = <2800000>;
			gpio = <&gpio TEGRA_GPIO(W, 0) GPIO_ACTIVE_HIGH>;
			enable-active-high;
		};
	};

	sound {
		compatible = "nvidia,tegra-audio-wm8903-ventana",
			     "nvidia,tegra-audio-wm8903";
		nvidia,model = "NVIDIA Tegra Ventana";

		nvidia,audio-routing =
			"Headphone Jack", "HPOUTR",
			"Headphone Jack", "HPOUTL",
			"Int Spk", "ROP",
			"Int Spk", "RON",
			"Int Spk", "LOP",
			"Int Spk", "LON",
			"Mic Jack", "MICBIAS",
			"IN1L", "Mic Jack";

		nvidia,i2s-controller = <&tegra_i2s1>;
		nvidia,audio-codec = <&wm8903>;

		nvidia,spkr-en-gpios = <&wm8903 2 GPIO_ACTIVE_HIGH>;
		nvidia,hp-det-gpios = <&gpio TEGRA_GPIO(W, 2) GPIO_ACTIVE_HIGH>;
		nvidia,int-mic-en-gpios = <&gpio TEGRA_GPIO(X, 0)
			GPIO_ACTIVE_HIGH>;
		nvidia,ext-mic-en-gpios = <&gpio TEGRA_GPIO(X, 1)
			GPIO_ACTIVE_HIGH>;

		clocks = <&tegra_car TEGRA20_CLK_PLL_A>,
			 <&tegra_car TEGRA20_CLK_PLL_A_OUT0>,
			 <&tegra_car TEGRA20_CLK_CDEV1>;
		clock-names = "pll_a", "pll_a_out0", "mclk";
	};
};
