// SPDX-License-Identifier: GPL-2.0-or-later OR MIT
/*
 * Copyright 2020-2022 Toradex
 */

#include "imx8mm-u-boot.dtsi"

/ {
	aliases {
		eeprom0 = &eeprom_module;
		eeprom1 = &eeprom_carrier_board;
		eeprom2 = &eeprom_display_adapter;
	};

	sysinfo {
		compatible = "toradex,sysinfo";
	};

	wdt-reboot {
		compatible = "wdt-reboot";
		bootph-pre-ram;
		wdt = <&wdog1>;
	};
};

&{/soc@0/bus@30800000/i2c@30a20000/pmic@25} {
	bootph-pre-ram;
};

&{/soc@0/bus@30800000/i2c@30a20000/pmic@25/regulators} {
	bootph-pre-ram;
};

&aips4 {
	bootph-pre-ram;
};

&binman_imx_fit {
	offset = <0x5fc00>;
};

&gpio1 {
	bootph-pre-ram;
};

&gpio2 {
	bootph-pre-ram;
};

&gpio3 {
	bootph-pre-ram;
};

&gpio4 {
	bootph-pre-ram;
};

&gpio5 {
	bootph-pre-ram;

	ctrl-sleep-moci-hog {
		bootph-pre-ram;
		gpio-hog;
		output-high;
		gpios = <1 GPIO_ACTIVE_HIGH>;
		line-name = "CTRL_SLEEP_MOCI#";

	};
};

&i2c1 {
	bootph-pre-ram;

	eeprom_module: eeprom@50 {
		compatible = "i2c-eeprom";
		pagesize = <16>;
		reg = <0x50>;
	};
};

&i2c2 {
	status = "okay";
};

&i2c4 {
	/* EEPROM on display adapter (MIPI DSI Display Adapter) */
	eeprom_display_adapter: eeprom@50 {
		compatible = "i2c-eeprom";
		pagesize = <16>;
		reg = <0x50>;
	};

	/* EEPROM on carrier board */
	eeprom_carrier_board: eeprom@57 {
		compatible = "i2c-eeprom";
		pagesize = <16>;
		reg = <0x57>;
	};
};

&pinctrl_ctrl_sleep_moci {
	bootph-pre-ram;
};

&pinctrl_i2c1 {
	bootph-pre-ram;
};

&pinctrl_pmic {
	bootph-pre-ram;
};

&pinctrl_uart1 {
	bootph-pre-ram;
};

&pinctrl_usdhc1 {
	bootph-pre-ram;
};

&pinctrl_usdhc2 {
	bootph-pre-ram;
};

&pinctrl_wdog {
	bootph-pre-ram;
};

&uart1 {
	bootph-pre-ram;
};

&usbmisc1 {
	bootph-pre-ram;
};

/* Verdin USB_1 */
&usbotg1 {
	bootph-pre-ram;
};

&usbphynop1 {
	bootph-pre-ram;
};

&usdhc1 {
	bootph-pre-ram;
};

&usdhc2 {
	bootph-pre-ram;
};

&usdhc3 {
	bootph-pre-ram;
};

&wdog1 {
	bootph-pre-ram;
};
