// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Device Tree Include file for NXP Layerscape-1088A family SoC.
 *
 * Copyright 2017-2020 NXP
 *
 * Harninder Rai <harninder.rai@nxp.com>
 *
 */
#include <dt-bindings/clock/fsl,qoriq-clockgen.h>
#include <dt-bindings/interrupt-controller/arm-gic.h>
#include <dt-bindings/thermal/thermal.h>

/ {
	compatible = "fsl,ls1088a";
	interrupt-parent = <&gic>;
	#address-cells = <2>;
	#size-cells = <2>;

	aliases {
		crypto = &crypto;
		rtc1 = &ftm_alarm0;
	};

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		/* We have 2 clusters having 4 Cortex-A53 cores each */
		cpu0: cpu@0 {
			device_type = "cpu";
			compatible = "arm,cortex-a53";
			reg = <0x0>;
			clocks = <&clockgen QORIQ_CLK_CMUX 0>;
			cpu-idle-states = <&CPU_PH20>;
			#cooling-cells = <2>;
		};

		cpu1: cpu@1 {
			device_type = "cpu";
			compatible = "arm,cortex-a53";
			reg = <0x1>;
			clocks = <&clockgen QORIQ_CLK_CMUX 0>;
			cpu-idle-states = <&CPU_PH20>;
			#cooling-cells = <2>;
		};

		cpu2: cpu@2 {
			device_type = "cpu";
			compatible = "arm,cortex-a53";
			reg = <0x2>;
			clocks = <&clockgen QORIQ_CLK_CMUX 0>;
			cpu-idle-states = <&CPU_PH20>;
			#cooling-cells = <2>;
		};

		cpu3: cpu@3 {
			device_type = "cpu";
			compatible = "arm,cortex-a53";
			reg = <0x3>;
			clocks = <&clockgen QORIQ_CLK_CMUX 0>;
			cpu-idle-states = <&CPU_PH20>;
			#cooling-cells = <2>;
		};

		cpu4: cpu@100 {
			device_type = "cpu";
			compatible = "arm,cortex-a53";
			reg = <0x100>;
			clocks = <&clockgen QORIQ_CLK_CMUX 1>;
			cpu-idle-states = <&CPU_PH20>;
			#cooling-cells = <2>;
		};

		cpu5: cpu@101 {
			device_type = "cpu";
			compatible = "arm,cortex-a53";
			reg = <0x101>;
			clocks = <&clockgen QORIQ_CLK_CMUX 1>;
			cpu-idle-states = <&CPU_PH20>;
			#cooling-cells = <2>;
		};

		cpu6: cpu@102 {
			device_type = "cpu";
			compatible = "arm,cortex-a53";
			reg = <0x102>;
			clocks = <&clockgen QORIQ_CLK_CMUX 1>;
			cpu-idle-states = <&CPU_PH20>;
			#cooling-cells = <2>;
		};

		cpu7: cpu@103 {
			device_type = "cpu";
			compatible = "arm,cortex-a53";
			reg = <0x103>;
			clocks = <&clockgen QORIQ_CLK_CMUX 1>;
			cpu-idle-states = <&CPU_PH20>;
			#cooling-cells = <2>;
		};

		CPU_PH20: cpu-ph20 {
			compatible = "arm,idle-state";
			idle-state-name = "PH20";
			arm,psci-suspend-param = <0x0>;
			entry-latency-us = <1000>;
			exit-latency-us = <1000>;
			min-residency-us = <3000>;
		};
	};

	gic: interrupt-controller@6000000 {
		compatible = "arm,gic-v3";
		#interrupt-cells = <3>;
		interrupt-controller;
		reg = <0x0 0x06000000 0 0x10000>, /* GIC Dist */
		      <0x0 0x06100000 0 0x100000>, /* GICR(RD_base+SGI_base)*/
		      <0x0 0x0c0c0000 0 0x2000>, /* GICC */
		      <0x0 0x0c0d0000 0 0x1000>, /* GICH */
		      <0x0 0x0c0e0000 0 0x20000>; /* GICV */
		interrupts = <1 9 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;

		its: gic-its@6020000 {
			compatible = "arm,gic-v3-its";
			msi-controller;
			reg = <0x0 0x6020000 0 0x20000>;
		};
	};

	thermal-zones {
		core-cluster {
			polling-delay-passive = <1000>;
			polling-delay = <5000>;
			thermal-sensors = <&tmu 0>;

			trips {
				core_cluster_alert: core-cluster-alert {
					temperature = <85000>;
					hysteresis = <2000>;
					type = "passive";
				};

				core-cluster-crit {
					temperature = <95000>;
					hysteresis = <2000>;
					type = "critical";
				};
			};

			cooling-maps {
				map0 {
					trip = <&core_cluster_alert>;
					cooling-device =
						<&cpu0 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
						<&cpu1 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
						<&cpu2 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
						<&cpu3 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
						<&cpu4 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
						<&cpu5 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
						<&cpu6 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
						<&cpu7 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
				};
			};
		};

		soc {
			polling-delay-passive = <1000>;
			polling-delay = <5000>;
			thermal-sensors = <&tmu 1>;

			trips {
				soc-crit {
					temperature = <95000>;
					hysteresis = <2000>;
					type = "critical";
				};
			};
		};
	};

	timer {
		compatible = "arm,armv8-timer";
		interrupts = <1 13 IRQ_TYPE_LEVEL_LOW>,/* Physical Secure PPI */
			     <1 14 IRQ_TYPE_LEVEL_LOW>,/* Physical Non-Secure PPI */
			     <1 11 IRQ_TYPE_LEVEL_LOW>,/* Virtual PPI */
			     <1 10 IRQ_TYPE_LEVEL_LOW>;/* Hypervisor PPI */
	};

	pmu {
		compatible = "arm,cortex-a53-pmu";
		interrupts = <GIC_PPI 7 IRQ_TYPE_LEVEL_LOW>;
	};

	psci {
		compatible = "arm,psci-0.2";
		method = "smc";
	};

	sysclk: sysclk {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <100000000>;
		clock-output-names = "sysclk";
	};

	reboot {
		compatible = "syscon-reboot";
		regmap = <&reset>;
		offset = <0x0>;
		mask = <0x02>;
	};

	soc {
		compatible = "simple-bus";
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;
		dma-ranges = <0x0 0x0 0x0 0x0 0x10000 0x00000000>;

		clockgen: clocking@1300000 {
			compatible = "fsl,ls1088a-clockgen";
			reg = <0 0x1300000 0 0xa0000>;
			#clock-cells = <2>;
			clocks = <&sysclk>;
		};

		dcfg: dcfg@1e00000 {
			compatible = "fsl,ls1088a-dcfg", "syscon";
			reg = <0x0 0x1e00000 0x0 0x10000>;
			little-endian;
		};

		reset: syscon@1e60000 {
			compatible = "fsl,ls1088a-reset", "syscon";
			reg = <0x0 0x1e60000 0x0 0x10000>;
		};

		isc: syscon@1f70000 {
			compatible = "fsl,ls1088a-isc", "syscon";
			reg = <0x0 0x1f70000 0x0 0x10000>;
			little-endian;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x0 0x1f70000 0x10000>;

			extirq: interrupt-controller@14 {
				compatible = "fsl,ls1088a-extirq";
				#interrupt-cells = <2>;
				#address-cells = <0>;
				interrupt-controller;
				reg = <0x14 4>;
				interrupt-map =
					<0 0 &gic GIC_SPI 0 IRQ_TYPE_LEVEL_HIGH>,
					<1 0 &gic GIC_SPI 1 IRQ_TYPE_LEVEL_HIGH>,
					<2 0 &gic GIC_SPI 2 IRQ_TYPE_LEVEL_HIGH>,
					<3 0 &gic GIC_SPI 3 IRQ_TYPE_LEVEL_HIGH>,
					<4 0 &gic GIC_SPI 4 IRQ_TYPE_LEVEL_HIGH>,
					<5 0 &gic GIC_SPI 5 IRQ_TYPE_LEVEL_HIGH>,
					<6 0 &gic GIC_SPI 6 IRQ_TYPE_LEVEL_HIGH>,
					<7 0 &gic GIC_SPI 7 IRQ_TYPE_LEVEL_HIGH>,
					<8 0 &gic GIC_SPI 8 IRQ_TYPE_LEVEL_HIGH>,
					<9 0 &gic GIC_SPI 9 IRQ_TYPE_LEVEL_HIGH>,
					<10 0 &gic GIC_SPI 10 IRQ_TYPE_LEVEL_HIGH>,
					<11 0 &gic GIC_SPI 11 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-map-mask = <0xf 0x0>;
			};
		};

		sfp: efuse@1e80000 {
			compatible = "fsl,ls1028a-sfp";
			reg = <0x0 0x1e80000 0x0 0x10000>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(4)>;
			clock-names = "sfp";
		};

		tmu: tmu@1f80000 {
			compatible = "fsl,qoriq-tmu";
			reg = <0x0 0x1f80000 0x0 0x10000>;
			interrupts = <0 23 0x4>;
			fsl,tmu-range = <0xb0000 0x9002a 0x6004c 0x70062>;
			fsl,tmu-calibration =
				/* Calibration data group 1 */
				<0x00000000 0x00000023
				0x00000001 0x0000002a
				0x00000002 0x00000030
				0x00000003 0x00000037
				0x00000004 0x0000003d
				0x00000005 0x00000044
				0x00000006 0x0000004a
				0x00000007 0x00000051
				0x00000008 0x00000057
				0x00000009 0x0000005e
				0x0000000a 0x00000064
				0x0000000b 0x0000006b
				/* Calibration data group 2 */
				0x00010000 0x00000022
				0x00010001 0x0000002a
				0x00010002 0x00000032
				0x00010003 0x0000003a
				0x00010004 0x00000042
				0x00010005 0x0000004a
				0x00010006 0x00000052
				0x00010007 0x0000005a
				0x00010008 0x00000062
				0x00010009 0x0000006a
				/* Calibration data group 3 */
				0x00020000 0x00000021
				0x00020001 0x0000002b
				0x00020002 0x00000035
				0x00020003 0x00000040
				0x00020004 0x0000004a
				0x00020005 0x00000054
				0x00020006 0x0000005e
				/* Calibration data group 4 */
				0x00030000 0x00000010
				0x00030001 0x0000001c
				0x00030002 0x00000027
				0x00030003 0x00000032
				0x00030004 0x0000003e
				0x00030005 0x00000049
				0x00030006 0x00000054
				0x00030007 0x00000060>;
			little-endian;
			#thermal-sensor-cells = <1>;
		};

		dspi: spi@2100000 {
			compatible = "fsl,ls1088a-dspi",
				     "fsl,ls1021a-v1.0-dspi";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0 0x2100000 0x0 0x10000>;
			interrupts = <GIC_SPI 26 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "dspi";
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(2)>;
			spi-num-chipselects = <6>;
			status = "disabled";
		};

		duart0: serial@21c0500 {
			compatible = "fsl,ns16550", "ns16550a";
			reg = <0x0 0x21c0500 0x0 0x100>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(4)>;
			interrupts = <0 32 IRQ_TYPE_LEVEL_HIGH>;
			status = "disabled";
		};

		duart1: serial@21c0600 {
			compatible = "fsl,ns16550", "ns16550a";
			reg = <0x0 0x21c0600 0x0 0x100>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(4)>;
			interrupts = <0 32 IRQ_TYPE_LEVEL_HIGH>;
			status = "disabled";
		};

		gpio0: gpio@2300000 {
			compatible = "fsl,ls1088a-gpio", "fsl,qoriq-gpio";
			reg = <0x0 0x2300000 0x0 0x10000>;
			interrupts = <0 36 IRQ_TYPE_LEVEL_HIGH>;
			little-endian;
			gpio-controller;
			#gpio-cells = <2>;
			interrupt-controller;
			#interrupt-cells = <2>;
		};

		gpio1: gpio@2310000 {
			compatible = "fsl,ls1088a-gpio", "fsl,qoriq-gpio";
			reg = <0x0 0x2310000 0x0 0x10000>;
			interrupts = <0 36 IRQ_TYPE_LEVEL_HIGH>;
			little-endian;
			gpio-controller;
			#gpio-cells = <2>;
			interrupt-controller;
			#interrupt-cells = <2>;
		};

		gpio2: gpio@2320000 {
			compatible = "fsl,ls1088a-gpio", "fsl,qoriq-gpio";
			reg = <0x0 0x2320000 0x0 0x10000>;
			interrupts = <0 37 IRQ_TYPE_LEVEL_HIGH>;
			little-endian;
			gpio-controller;
			#gpio-cells = <2>;
			interrupt-controller;
			#interrupt-cells = <2>;
		};

		gpio3: gpio@2330000 {
			compatible = "fsl,ls1088a-gpio", "fsl,qoriq-gpio";
			reg = <0x0 0x2330000 0x0 0x10000>;
			interrupts = <0 37 IRQ_TYPE_LEVEL_HIGH>;
			little-endian;
			gpio-controller;
			#gpio-cells = <2>;
			interrupt-controller;
			#interrupt-cells = <2>;
		};

		ifc: memory-controller@2240000 {
			compatible = "fsl,ifc";
			reg = <0x0 0x2240000 0x0 0x20000>;
			interrupts = <0 21 IRQ_TYPE_LEVEL_HIGH>;
			little-endian;
			#address-cells = <2>;
			#size-cells = <1>;
			status = "disabled";
		};

		i2c0: i2c@2000000 {
			compatible = "fsl,vf610-i2c";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0 0x2000000 0x0 0x10000>;
			interrupts = <0 34 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(8)>;
			status = "disabled";
		};

		i2c1: i2c@2010000 {
			compatible = "fsl,vf610-i2c";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0 0x2010000 0x0 0x10000>;
			interrupts = <0 34 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(8)>;
			status = "disabled";
		};

		i2c2: i2c@2020000 {
			compatible = "fsl,vf610-i2c";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0 0x2020000 0x0 0x10000>;
			interrupts = <0 35 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(8)>;
			status = "disabled";
		};

		i2c3: i2c@2030000 {
			compatible = "fsl,vf610-i2c";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0 0x2030000 0x0 0x10000>;
			interrupts = <0 35 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(8)>;
			status = "disabled";
		};

		qspi: spi@20c0000 {
			compatible = "fsl,ls2080a-qspi";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0x0 0x20c0000 0x0 0x10000>,
			      <0x0 0x20000000 0x0 0x10000000>;
			reg-names = "QuadSPI", "QuadSPI-memory";
			interrupts = <GIC_SPI 25 IRQ_TYPE_LEVEL_HIGH>;
			clock-names = "qspi_en", "qspi";
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(4)>,
				 <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(4)>;
			status = "disabled";
		};

		esdhc: esdhc@2140000 {
			compatible = "fsl,ls1088a-esdhc", "fsl,esdhc";
			reg = <0x0 0x2140000 0x0 0x10000>;
			interrupts = <0 28 0x4>; /* Level high type */
			clock-frequency = <0>;
			clocks = <&clockgen QORIQ_CLK_HWACCEL 1>;
			voltage-ranges = <1800 1800 3300 3300>;
			sdhci,auto-cmd12;
			little-endian;
			bus-width = <4>;
			status = "disabled";
		};

		usb0: usb@3100000 {
			compatible = "snps,dwc3";
			reg = <0x0 0x3100000 0x0 0x10000>;
			interrupts = <0 80 IRQ_TYPE_LEVEL_HIGH>;
			dr_mode = "host";
			snps,quirk-frame-length-adjustment = <0x20>;
			snps,dis_rxdet_inp3_quirk;
			snps,incr-burst-type-adjustment = <1>, <4>, <8>, <16>;
			status = "disabled";
		};

		usb1: usb@3110000 {
			compatible = "snps,dwc3";
			reg = <0x0 0x3110000 0x0 0x10000>;
			interrupts = <0 81 IRQ_TYPE_LEVEL_HIGH>;
			dr_mode = "host";
			snps,quirk-frame-length-adjustment = <0x20>;
			snps,dis_rxdet_inp3_quirk;
			snps,incr-burst-type-adjustment = <1>, <4>, <8>, <16>;
			status = "disabled";
		};

		sata: sata@3200000 {
			compatible = "fsl,ls1088a-ahci";
			reg = <0x0 0x3200000 0x0 0x10000>,
				<0x7 0x100520 0x0 0x4>;
			reg-names = "ahci", "sata-ecc";
			interrupts = <0 133 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(4)>;
			dma-coherent;
			status = "disabled";
		};

		crypto: crypto@8000000 {
			compatible = "fsl,sec-v5.0", "fsl,sec-v4.0";
			fsl,sec-era = <8>;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0x0 0x00 0x8000000 0x100000>;
			reg = <0x00 0x8000000 0x0 0x100000>;
			interrupts = <GIC_SPI 139 IRQ_TYPE_LEVEL_HIGH>;
			dma-coherent;

			sec_jr0: jr@10000 {
				compatible = "fsl,sec-v5.0-job-ring",
					     "fsl,sec-v4.0-job-ring";
				reg = <0x10000 0x10000>;
				interrupts = <GIC_SPI 140 IRQ_TYPE_LEVEL_HIGH>;
			};

			sec_jr1: jr@20000 {
				compatible = "fsl,sec-v5.0-job-ring",
					     "fsl,sec-v4.0-job-ring";
				reg = <0x20000 0x10000>;
				interrupts = <GIC_SPI 141 IRQ_TYPE_LEVEL_HIGH>;
			};

			sec_jr2: jr@30000 {
				compatible = "fsl,sec-v5.0-job-ring",
					     "fsl,sec-v4.0-job-ring";
				reg = <0x30000 0x10000>;
				interrupts = <GIC_SPI 142 IRQ_TYPE_LEVEL_HIGH>;
			};

			sec_jr3: jr@40000 {
				compatible = "fsl,sec-v5.0-job-ring",
					     "fsl,sec-v4.0-job-ring";
				reg = <0x40000 0x10000>;
				interrupts = <GIC_SPI 143 IRQ_TYPE_LEVEL_HIGH>;
			};
		};

		pcie1: pcie@3400000 {
			compatible = "fsl,ls1088a-pcie";
			reg = <0x00 0x03400000 0x0 0x00100000>, /* controller registers */
			      <0x20 0x00000000 0x0 0x00002000>; /* configuration space */
			reg-names = "regs", "config";
			interrupts = <0 108 IRQ_TYPE_LEVEL_HIGH>; /* aer interrupt */
			interrupt-names = "aer";
			#address-cells = <3>;
			#size-cells = <2>;
			device_type = "pci";
			dma-coherent;
			num-viewport = <256>;
			bus-range = <0x0 0xff>;
			ranges = <0x81000000 0x0 0x00000000 0x20 0x00010000 0x0 0x00010000   /* downstream I/O */
				  0x82000000 0x0 0x40000000 0x20 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
			msi-parent = <&its>;
			#interrupt-cells = <1>;
			interrupt-map-mask = <0 0 0 7>;
			interrupt-map = <0000 0 0 1 &gic 0 0 0 109 IRQ_TYPE_LEVEL_HIGH>,
					<0000 0 0 2 &gic 0 0 0 110 IRQ_TYPE_LEVEL_HIGH>,
					<0000 0 0 3 &gic 0 0 0 111 IRQ_TYPE_LEVEL_HIGH>,
					<0000 0 0 4 &gic 0 0 0 112 IRQ_TYPE_LEVEL_HIGH>;
			iommu-map = <0 &smmu 0 1>; /* Fixed-up by bootloader */
			status = "disabled";
		};

		pcie_ep1: pcie-ep@3400000 {
			compatible = "fsl,ls1088a-pcie-ep", "fsl,ls-pcie-ep";
			reg = <0x00 0x03400000 0x0 0x00100000>,
			      <0x20 0x00000000 0x8 0x00000000>;
			reg-names = "regs", "addr_space";
			num-ib-windows = <24>;
			num-ob-windows = <256>;
			max-functions = /bits/ 8 <2>;
			status = "disabled";
		};

		pcie2: pcie@3500000 {
			compatible = "fsl,ls1088a-pcie";
			reg = <0x00 0x03500000 0x0 0x00100000>, /* controller registers */
			      <0x28 0x00000000 0x0 0x00002000>; /* configuration space */
			reg-names = "regs", "config";
			interrupts = <0 113 IRQ_TYPE_LEVEL_HIGH>; /* aer interrupt */
			interrupt-names = "aer";
			#address-cells = <3>;
			#size-cells = <2>;
			device_type = "pci";
			dma-coherent;
			num-viewport = <6>;
			bus-range = <0x0 0xff>;
			ranges = <0x81000000 0x0 0x00000000 0x28 0x00010000 0x0 0x00010000   /* downstream I/O */
				  0x82000000 0x0 0x40000000 0x28 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
			msi-parent = <&its>;
			#interrupt-cells = <1>;
			interrupt-map-mask = <0 0 0 7>;
			interrupt-map = <0000 0 0 1 &gic 0 0 0 114 IRQ_TYPE_LEVEL_HIGH>,
					<0000 0 0 2 &gic 0 0 0 115 IRQ_TYPE_LEVEL_HIGH>,
					<0000 0 0 3 &gic 0 0 0 116 IRQ_TYPE_LEVEL_HIGH>,
					<0000 0 0 4 &gic 0 0 0 117 IRQ_TYPE_LEVEL_HIGH>;
			iommu-map = <0 &smmu 0 1>; /* Fixed-up by bootloader */
			status = "disabled";
		};

		pcie_ep2: pcie-ep@3500000 {
			compatible = "fsl,ls1088a-pcie-ep", "fsl,ls-pcie-ep";
			reg = <0x00 0x03500000 0x0 0x00100000>,
			      <0x28 0x00000000 0x8 0x00000000>;
			reg-names = "regs", "addr_space";
			num-ib-windows = <6>;
			num-ob-windows = <6>;
			status = "disabled";
		};

		pcie3: pcie@3600000 {
			compatible = "fsl,ls1088a-pcie";
			reg = <0x00 0x03600000 0x0 0x00100000>, /* controller registers */
			      <0x30 0x00000000 0x0 0x00002000>; /* configuration space */
			reg-names = "regs", "config";
			interrupts = <0 118 IRQ_TYPE_LEVEL_HIGH>; /* aer interrupt */
			interrupt-names = "aer";
			#address-cells = <3>;
			#size-cells = <2>;
			device_type = "pci";
			dma-coherent;
			num-viewport = <6>;
			bus-range = <0x0 0xff>;
			ranges = <0x81000000 0x0 0x00000000 0x30 0x00010000 0x0 0x00010000   /* downstream I/O */
				  0x82000000 0x0 0x40000000 0x30 0x40000000 0x0 0x40000000>; /* non-prefetchable memory */
			msi-parent = <&its>;
			#interrupt-cells = <1>;
			interrupt-map-mask = <0 0 0 7>;
			interrupt-map = <0000 0 0 1 &gic 0 0 0 119 IRQ_TYPE_LEVEL_HIGH>,
					<0000 0 0 2 &gic 0 0 0 120 IRQ_TYPE_LEVEL_HIGH>,
					<0000 0 0 3 &gic 0 0 0 121 IRQ_TYPE_LEVEL_HIGH>,
					<0000 0 0 4 &gic 0 0 0 122 IRQ_TYPE_LEVEL_HIGH>;
			iommu-map = <0 &smmu 0 1>; /* Fixed-up by bootloader */
			status = "disabled";
		};

		pcie_ep3: pcie-ep@3600000 {
			compatible = "fsl,ls1088a-pcie-ep", "fsl,ls-pcie-ep";
			reg = <0x00 0x03600000 0x0 0x00100000>,
			      <0x30 0x00000000 0x8 0x00000000>;
			reg-names = "regs", "addr_space";
			num-ib-windows = <6>;
			num-ob-windows = <6>;
			status = "disabled";
		};

		smmu: iommu@5000000 {
			compatible = "arm,mmu-500";
			reg = <0 0x5000000 0 0x800000>;
			#iommu-cells = <1>;
			stream-match-mask = <0x7C00>;
			dma-coherent;
			#global-interrupts = <12>;
				     // global secure fault
			interrupts = <GIC_SPI 13 IRQ_TYPE_LEVEL_HIGH>,
				     // combined secure
				     <GIC_SPI 14 IRQ_TYPE_LEVEL_HIGH>,
				     // global non-secure fault
				     <GIC_SPI 15 IRQ_TYPE_LEVEL_HIGH>,
				     // combined non-secure
				     <GIC_SPI 16 IRQ_TYPE_LEVEL_HIGH>,
				     // performance counter interrupts 0-7
				     <GIC_SPI 211 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 212 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 213 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 214 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 215 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 216 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 217 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 218 IRQ_TYPE_LEVEL_HIGH>,
				     // per context interrupt, 64 interrupts
				     <GIC_SPI 146 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 147 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 148 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 149 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 150 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 151 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 152 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 153 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 154 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 155 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 156 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 157 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 158 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 159 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 160 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 161 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 162 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 163 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 164 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 165 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 166 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 167 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 168 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 169 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 170 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 171 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 172 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 173 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 174 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 175 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 176 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 177 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 178 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 179 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 180 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 181 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 182 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 183 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 184 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 185 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 186 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 187 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 188 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 189 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 190 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 191 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 192 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 193 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 194 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 195 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 196 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 197 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 198 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 199 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 200 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 201 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 202 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 203 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 204 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 205 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 206 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 207 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 208 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 209 IRQ_TYPE_LEVEL_HIGH>;
		};

		console@8340020 {
			compatible = "fsl,dpaa2-console";
			reg = <0x00000000 0x08340020 0 0x2>;
		};

		ptp-timer@8b95000 {
			compatible = "fsl,dpaa2-ptp";
			reg = <0x0 0x8b95000 0x0 0x100>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(1)>;
			little-endian;
			fsl,extts-fifo;
		};

		emdio1: mdio@8b96000 {
			compatible = "fsl,fman-memac-mdio";
			reg = <0x0 0x8b96000 0x0 0x1000>;
			little-endian;
			#address-cells = <1>;
			#size-cells = <0>;
			clock-frequency = <2500000>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(1)>;
			status = "disabled";
		};

		emdio2: mdio@8b97000 {
			compatible = "fsl,fman-memac-mdio";
			reg = <0x0 0x8b97000 0x0 0x1000>;
			little-endian;
			#address-cells = <1>;
			#size-cells = <0>;
			clock-frequency = <2500000>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(1)>;
			status = "disabled";
		};

		pcs_mdio1: mdio@8c07000 {
			compatible = "fsl,fman-memac-mdio";
			reg = <0x0 0x8c07000 0x0 0x1000>;
			little-endian;
			#address-cells = <1>;
			#size-cells = <0>;
			status = "disabled";

			pcs1: ethernet-phy@0 {
				reg = <0>;
			};
		};

		pcs_mdio2: mdio@8c0b000 {
			compatible = "fsl,fman-memac-mdio";
			reg = <0x0 0x8c0b000 0x0 0x1000>;
			little-endian;
			#address-cells = <1>;
			#size-cells = <0>;
			status = "disabled";

			pcs2: ethernet-phy@0 {
				reg = <0>;
			};
		};

		pcs_mdio3: mdio@8c0f000 {
			compatible = "fsl,fman-memac-mdio";
			reg = <0x0 0x8c0f000 0x0 0x1000>;
			little-endian;
			#address-cells = <1>;
			#size-cells = <0>;
			status = "disabled";

			pcs3_0: ethernet-phy@0 {
				reg = <0>;
			};

			pcs3_1: ethernet-phy@1 {
				reg = <1>;
			};

			pcs3_2: ethernet-phy@2 {
				reg = <2>;
			};

			pcs3_3: ethernet-phy@3 {
				reg = <3>;
			};
		};

		pcs_mdio7: mdio@8c1f000 {
			compatible = "fsl,fman-memac-mdio";
			reg = <0x0 0x8c1f000 0x0 0x1000>;
			little-endian;
			#address-cells = <1>;
			#size-cells = <0>;
			status = "disabled";

			pcs7_0: ethernet-phy@0 {
				reg = <0>;
			};

			pcs7_1: ethernet-phy@1 {
				reg = <1>;
			};

			pcs7_2: ethernet-phy@2 {
				reg = <2>;
			};

			pcs7_3: ethernet-phy@3 {
				reg = <3>;
			};
		};

		cluster1_core0_watchdog: wdt@c000000 {
			compatible = "arm,sp805", "arm,primecell";
			reg = <0x0 0xc000000 0x0 0x1000>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(16)>,
				 <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(16)>;
			clock-names = "wdog_clk", "apb_pclk";
		};

		cluster1_core1_watchdog: wdt@c010000 {
			compatible = "arm,sp805", "arm,primecell";
			reg = <0x0 0xc010000 0x0 0x1000>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(16)>,
				 <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(16)>;
			clock-names = "wdog_clk", "apb_pclk";
		};

		cluster1_core2_watchdog: wdt@c020000 {
			compatible = "arm,sp805", "arm,primecell";
			reg = <0x0 0xc020000 0x0 0x1000>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(16)>,
				 <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(16)>;
			clock-names = "wdog_clk", "apb_pclk";
		};

		cluster1_core3_watchdog: wdt@c030000 {
			compatible = "arm,sp805", "arm,primecell";
			reg = <0x0 0xc030000 0x0 0x1000>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(16)>,
				 <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(16)>;
			clock-names = "wdog_clk", "apb_pclk";
		};

		cluster2_core0_watchdog: wdt@c100000 {
			compatible = "arm,sp805", "arm,primecell";
			reg = <0x0 0xc100000 0x0 0x1000>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(16)>,
				 <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(16)>;
			clock-names = "wdog_clk", "apb_pclk";
		};

		cluster2_core1_watchdog: wdt@c110000 {
			compatible = "arm,sp805", "arm,primecell";
			reg = <0x0 0xc110000 0x0 0x1000>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(16)>,
				 <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(16)>;
			clock-names = "wdog_clk", "apb_pclk";
		};

		cluster2_core2_watchdog: wdt@c120000 {
			compatible = "arm,sp805", "arm,primecell";
			reg = <0x0 0xc120000 0x0 0x1000>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(16)>,
				 <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(16)>;
			clock-names = "wdog_clk", "apb_pclk";
		};

		cluster2_core3_watchdog: wdt@c130000 {
			compatible = "arm,sp805", "arm,primecell";
			reg = <0x0 0xc130000 0x0 0x1000>;
			clocks = <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(16)>,
				 <&clockgen QORIQ_CLK_PLATFORM_PLL
					    QORIQ_CLK_PLL_DIV(16)>;
			clock-names = "wdog_clk", "apb_pclk";
		};

		fsl_mc: fsl-mc@80c000000 {
			compatible = "fsl,qoriq-mc";
			reg = <0x00000008 0x0c000000 0 0x40>,	 /* MC portal base */
			      <0x00000000 0x08340000 0 0x40000>; /* MC control reg */
			msi-parent = <&its>;
			iommu-map = <0 &smmu 0 0>;	/* This is fixed-up by u-boot */
			dma-coherent;
			#address-cells = <3>;
			#size-cells = <1>;

			/*
			 * Region type 0x0 - MC portals
			 * Region type 0x1 - QBMAN portals
			 */
			ranges = <0x0 0x0 0x0 0x8 0x0c000000 0x4000000
				  0x1 0x0 0x0 0x8 0x18000000 0x8000000>;

			dpmacs {
				#address-cells = <1>;
				#size-cells = <0>;

				dpmac1: ethernet@1 {
					compatible = "fsl,qoriq-mc-dpmac";
					reg = <1>;
				};

				dpmac2: ethernet@2 {
					compatible = "fsl,qoriq-mc-dpmac";
					reg = <2>;
				};

				dpmac3: ethernet@3 {
					compatible = "fsl,qoriq-mc-dpmac";
					reg = <3>;
				};

				dpmac4: ethernet@4 {
					compatible = "fsl,qoriq-mc-dpmac";
					reg = <4>;
				};

				dpmac5: ethernet@5 {
					compatible = "fsl,qoriq-mc-dpmac";
					reg = <5>;
				};

				dpmac6: ethernet@6 {
					compatible = "fsl,qoriq-mc-dpmac";
					reg = <6>;
				};

				dpmac7: ethernet@7 {
					compatible = "fsl,qoriq-mc-dpmac";
					reg = <7>;
				};

				dpmac8: ethernet@8 {
					compatible = "fsl,qoriq-mc-dpmac";
					reg = <8>;
				};

				dpmac9: ethernet@9 {
					compatible = "fsl,qoriq-mc-dpmac";
					reg = <9>;
				};

				dpmac10: ethernet@a {
					compatible = "fsl,qoriq-mc-dpmac";
					reg = <0xa>;
				};
			};
		};

		rcpm: power-controller@1e34040 {
			compatible = "fsl,ls1088a-rcpm", "fsl,qoriq-rcpm-2.1+";
			reg = <0x0 0x1e34040 0x0 0x18>;
			#fsl,rcpm-wakeup-cells = <6>;
			little-endian;
		};

		ftm_alarm0: timer@2800000 {
			compatible = "fsl,ls1088a-ftm-alarm";
			reg = <0x0 0x2800000 0x0 0x10000>;
			fsl,rcpm-wakeup = <&rcpm 0x0 0x0 0x0 0x0 0x4000 0x0>;
			interrupts = <GIC_SPI 44 IRQ_TYPE_LEVEL_HIGH>;
		};
	};

	firmware {
		optee {
			compatible = "linaro,optee-tz";
			method = "smc";
		};
	};
};
