/*
 * SAMSUNG SMDK5250 board device tree source
 *
 * Copyright (c) 2012 Samsung Electronics Co., Ltd.
 *		http://www.samsung.com
 *
 * This program is free software; you can redistribute it and/or modify
 * it under the terms of the GNU General Public License version 2 as
 * published by the Free Software Foundation.
*/

/dts-v1/;
#include "exynos5250.dtsi"
#include <dt-bindings/interrupt-controller/irq.h>

/ {
	model = "SAMSUNG SMDK5250 board based on EXYNOS5250";
	compatible = "samsung,smdk5250", "samsung,exynos5250";

	aliases {
		i2c0 = "/i2c@12C60000";
		i2c1 = "/i2c@12C70000";
		i2c2 = "/i2c@12C80000";
		i2c3 = "/i2c@12C90000";
		i2c4 = "/i2c@12CA0000";
		i2c5 = "/i2c@12CB0000";
		i2c6 = "/i2c@12CC0000";
		i2c7 = "/i2c@12CD0000";
		spi0 = "/spi@12d20000";
		spi1 = "/spi@12d30000";
		spi2 = "/spi@12d40000";
		spi3 = "/spi@131a0000";
		spi4 = "/spi@131b0000";
		mmc0 = "/mmc@12200000";
		mmc1 = "/mmc@12210000";
		mmc2 = "/mmc@12220000";
		mmc3 = "/mmc@12230000";
		serial0 = "/serial@12C30000";
		console = "/serial@12C30000";
		i2s = "/sound@3830000";
	};

	sromc@12250000 {
		compatible = "samsung,exynos5-sromc";
		bank = <1>;
		srom-timing = <1 9 12 1 6 1 1>;
		width = <2>;
		lan@5000000 {
			compatible = "smsc,lan9215", "smsc,lan";
			reg = <0x5000000 0x100>;
			phy-mode = "mii";
		};
	};

	sound@3830000 {
		samsung,codec-type = "wm8994";
	};

	sound@12d60000 {
		status = "disabled";
	};

	i2c@12C70000 {
		wm8994: soundcodec@1a {
			reg = <0x1a>;
			u-boot,i2c-offset-len = <2>;
			compatible = "wolfson,wm8994";
			#sound-dai-cells = <1>;
		};
	};

	sound {
		compatible = "google,smdk5250-audio-wm8994";

		samsung,model = "SMDK5250-I2S-WM8994";
		samsung,audio-codec = <&wm8994>;

		cpu {
			sound-dai = <&i2s0 0>;
		};

		codec {
			sound-dai = <&wm8994 0>;
		};
	};

	i2c@12C60000 {
		pmic@9 {
			reg = <0x9>;
			compatible = "maxim,max77686";
		};
	};

	tmu@10060000 {
		samsung,min-temp	= <25>;
		samsung,max-temp	= <125>;
		samsung,start-warning	= <95>;
		samsung,start-tripping	= <105>;
		samsung,hw-tripping	= <110>;
		samsung,efuse-min-value	= <40>;
		samsung,efuse-value	= <55>;
		samsung,efuse-max-value	= <100>;
		samsung,slope		= <274761730>;
		samsung,dc-value	= <25>;
	};

	fimd@14400000 {
		samsung,vl-freq = <60>;
		samsung,vl-col = <2560>;
		samsung,vl-row = <1600>;
		samsung,vl-width = <2560>;
		samsung,vl-height = <1600>;

		samsung,vl-clkp;
		samsung,vl-dp;
		samsung,vl-bpix = <4>;

		samsung,vl-hspw = <32>;
		samsung,vl-hbpd = <80>;
		samsung,vl-hfpd = <48>;
		samsung,vl-vspw = <6>;
		samsung,vl-vbpd = <37>;
		samsung,vl-vfpd = <3>;
		samsung,vl-cmd-allow-len = <0xf>;

		samsung,winid = <3>;
		samsung,interface-mode = <1>;
		samsung,dp-enabled = <1>;
		samsung,dual-lcd-enabled = <0>;
	};

	dp@145b0000 {
		samsung,lt-status = <0>;

		samsung,master-mode = <0>;
		samsung,bist-mode = <0>;
		samsung,bist-pattern = <0>;
		samsung,h-sync-polarity = <0>;
		samsung,v-sync-polarity = <0>;
		samsung,interlaced = <0>;
		samsung,color-space = <0>;
		samsung,dynamic-range = <0>;
		samsung,ycbcr-coeff = <0>;
		samsung,color-depth = <1>;
	};

	mmc@12200000 {
		bus-width = <8>;
		samsung,dw-mshc-ciu-div = <3>;
		samsung,dw-mshc-sdr-timing = <1 3>;
		non-removable;
	};

	mmc@12210000 {
		status = "disabled";
	};

	mmc@12220000 {
		bus-width = <4>;
		samsung,dw-mshc-ciu-div = <3>;
		samsung,dw-mshc-sdr-timing = <1 2>;
	};

	mmc@12230000 {
		status = "disabled";
	};

	ehci@12110000 {
		samsung,vbus-gpio = <&gpx2 6 GPIO_ACTIVE_HIGH>;
	};
};

&i2c_0 {
	status = "okay";
	samsung,i2c-sda-delay = <100>;
	samsung,i2c-max-bus-freq = <20000>;

	max77686@09 {
		compatible = "maxim,max77686";
		reg = <0x09>;
		interrupt-parent = <&gpx3>;
		interrupts = <2 IRQ_TYPE_NONE>;

		voltage-regulators {
			ldo1_reg: LDO1 {
				regulator-name = "P1.0V_LDO_OUT1";
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <1000000>;
				regulator-always-on;
			};

			ldo2_reg: LDO2 {
				regulator-name = "P1.2V_LDO_OUT2";
				regulator-min-microvolt = <1200000>;
				regulator-max-microvolt = <1200000>;
				regulator-always-on;
			};

			ldo3_reg: LDO3 {
				regulator-name = "P1.8V_LDO_OUT3";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-always-on;
			};

			ldo4_reg: LDO4 {
				regulator-name = "P2.8V_LDO_OUT4";
				regulator-min-microvolt = <2800000>;
				regulator-max-microvolt = <2800000>;
			};

			ldo5_reg: LDO5 {
				regulator-name = "P1.8V_LDO_OUT5";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
			};

			ldo6_reg: LDO6 {
				regulator-name = "P1.1V_LDO_OUT6";
				regulator-min-microvolt = <1100000>;
				regulator-max-microvolt = <1100000>;
				regulator-always-on;
			};

			ldo7_reg: LDO7 {
				regulator-name = "P1.1V_LDO_OUT7";
				regulator-min-microvolt = <1100000>;
				regulator-max-microvolt = <1100000>;
				regulator-always-on;
			};

			ldo8_reg: LDO8 {
				regulator-name = "P1.0V_LDO_OUT8";
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <1000000>;
			};

			ldo10_reg: LDO10 {
				regulator-name = "P1.8V_LDO_OUT10";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
			};

			ldo11_reg: LDO11 {
				regulator-name = "P1.8V_LDO_OUT11";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
			};

			ldo12_reg: LDO12 {
				regulator-name = "P3.0V_LDO_OUT12";
				regulator-min-microvolt = <3000000>;
				regulator-max-microvolt = <3000000>;
			};

			ldo13_reg: LDO13 {
				regulator-name = "P1.8V_LDO_OUT13";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
			};

			ldo14_reg: LDO14 {
				regulator-name = "P1.8V_LDO_OUT14";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
			};

			ldo15_reg: LDO15 {
				regulator-name = "P1.0V_LDO_OUT15";
				regulator-min-microvolt = <1000000>;
				regulator-max-microvolt = <1000000>;
			};

			ldo16_reg: LDO16 {
				regulator-name = "P1.8V_LDO_OUT16";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
			};

			buck1_reg: BUCK1 {
				regulator-name = "vdd_mif";
				regulator-min-microvolt = <950000>;
				regulator-max-microvolt = <1300000>;
				regulator-always-on;
				regulator-boot-on;
			};

			buck2_reg: BUCK2 {
				regulator-name = "vdd_arm";
				regulator-min-microvolt = <850000>;
				regulator-max-microvolt = <1350000>;
				regulator-always-on;
				regulator-boot-on;
			};

			buck3_reg: BUCK3 {
				regulator-name = "vdd_int";
				regulator-min-microvolt = <900000>;
				regulator-max-microvolt = <1200000>;
				regulator-always-on;
				regulator-boot-on;
			};

			buck4_reg: BUCK4 {
				regulator-name = "vdd_g3d";
				regulator-min-microvolt = <850000>;
				regulator-max-microvolt = <1300000>;
				regulator-always-on;
				regulator-boot-on;
			};

			buck5_reg: BUCK5 {
				regulator-name = "P1.8V_BUCK_OUT5";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <1800000>;
				regulator-always-on;
				regulator-boot-on;
			};
		};
	};
};
