// SPDX-License-Identifier: GPL-2.0+
/*
 *  Copyright (C) 2012 Altera Corporation <www.altera.com>
 */

#include "socfpga_cyclone5.dtsi"
#include "socfpga-common-u-boot.dtsi"

/ {
	model = "SoCFPGA Cyclone V IS1";
	compatible = "anonymous,socfpga-is1", "altr,socfpga-cyclone5", "altr,socfpga";

	chosen {
		bootargs = "console=ttyS0,115200";
		stdout-path = "serial0:115200n8";
	};

	memory {
		name = "memory";
		device_type = "memory";
		reg = <0x0 0x10000000>;
	};

	aliases {
		ethernet0 = &gmac1;
		udc0 = &usb1;
	};

	regulator_3_3v: 3-3-v-regulator {
		compatible = "regulator-fixed";
		regulator-name = "3.3V";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
	};
};

&gmac1 {
	status = "okay";
	phy-mode = "rgmii";

	rxd0-skew-ps = <0>;
	rxd1-skew-ps = <0>;
	rxd2-skew-ps = <0>;
	rxd3-skew-ps = <0>;
	txen-skew-ps = <0>;
	txc-skew-ps = <1560>;
	rxdv-skew-ps = <0>;
	rxc-skew-ps = <1200>;
};

&gpio1 {
	status = "okay";
};

&porta {
	bank-name = "porta";
};

&i2c0 {
	status = "okay";

	eeprom@51 {
		compatible = "atmel,24c32";
		reg = <0x51>;
		pagesize = <32>;
	};

	rtc@68 {
		compatible = "dallas,ds1339";
		reg = <0x68>;
	};
};

&mmc0 {
	status = "okay";
	bootph-all;

	cd-gpios = <&portb 18 0>;
	vmmc-supply = <&regulator_3_3v>;
	vqmmc-supply = <&regulator_3_3v>;
};

&qspi {
	status = "okay";
	bootph-all;

	flash0: n25q00@0 {
		bootph-all;
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "n25q00", "jedec,spi-nor";
		reg = <0>;      /* chip select */
		spi-max-frequency = <100000000>;
		m25p,fast-read;
		page-size = <256>;
		block-size = <16>; /* 2^16, 64KB */
		cdns,tshsl-ns = <50>;
		cdns,tsd2d-ns = <50>;
		cdns,tchsh-ns = <4>;
		cdns,tslch-ns = <4>;
	};
};

&usb1 {
	status = "okay";
};

&uart0 {
	bootph-all;
};

&watchdog0 {
	status = "disabled";
};
