// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
// Copyright (C) 2017 Jagan Teki <jteki@openedev.com>

/dts-v1/;

#include "sun50i-h5.dtsi"

#include <dt-bindings/gpio/gpio.h>

/ {
	model = "OrangePi Zero Plus2";
	compatible = "xunlong,orangepi-zero-plus2", "allwinner,sun50i-h5";

	aliases {
		serial0 = &uart0;
	};

	chosen {
		stdout-path = "serial0:115200n8";
	};

	connector {
		compatible = "hdmi-connector";
		type = "a";

		port {
			hdmi_con_in: endpoint {
				remote-endpoint = <&hdmi_out_con>;
			};
		};
	};

	leds {
		compatible = "gpio-leds";

		led-0 {
			label = "orangepi:green:pwr";
			gpios = <&r_pio 0 10 GPIO_ACTIVE_HIGH>;
			default-state = "on";
		};

		led-1 {
			label = "orangepi:red:status";
			gpios = <&pio 0 17 GPIO_ACTIVE_HIGH>;
		};
	};

	reg_vcc3v3: vcc3v3 {
		compatible = "regulator-fixed";
		regulator-name = "vcc3v3";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
	};

	wifi_pwrseq: pwrseq {
		compatible = "mmc-pwrseq-simple";
		reset-gpios = <&pio 0 9 GPIO_ACTIVE_LOW>; /* PA9 */
		post-power-on-delay-ms = <200>;
	};
};

&de {
	status = "okay";
};

&ehci0 {
	status = "okay";
};

&hdmi {
	status = "okay";
};

&hdmi_out {
	hdmi_out_con: endpoint {
		remote-endpoint = <&hdmi_con_in>;
	};
};

&mmc0 {
	vmmc-supply = <&reg_vcc3v3>;
	disable-wp;
	bus-width = <4>;
	cd-gpios = <&pio 5 6 GPIO_ACTIVE_LOW>;
	status = "okay";
};

&mmc1 {
	vmmc-supply = <&reg_vcc3v3>;
	vqmmc-supply = <&reg_vcc3v3>;
	mmc-pwrseq = <&wifi_pwrseq>;
	bus-width = <4>;
	non-removable;
	status = "okay";

	brcmf: wifi@1 {
		reg = <1>;
		compatible = "brcm,bcm4329-fmac";
		interrupt-parent = <&r_pio>;
		interrupts = <0 7 IRQ_TYPE_LEVEL_LOW>;	/* PL7 */
		interrupt-names = "host-wake";
	};
};

&mmc2 {
	pinctrl-names = "default";
	pinctrl-0 = <&mmc2_8bit_pins>;
	vmmc-supply = <&reg_vcc3v3>;
	bus-width = <8>;
	non-removable;
	cap-mmc-hw-reset;
	status = "okay";
};

&ohci0 {
	status = "okay";
};

&uart0 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart0_pa_pins>;
	status = "okay";
};

&uart1 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart1_pins>, <&uart1_rts_cts_pins>;
	status = "okay";
};

&usb_otg {
	/*
	 * According to schematics CN1 MicroUSB port can be used to take
	 * external 5V to power up the board VBUS. On the contrary CN1 MicroUSB
	 * port cannot provide power externally even if the board is powered
	 * via GPIO pins. It thus makes sense to force peripheral mode.
	 */
	dr_mode = "peripheral";
	status = "okay";
};

&usbphy {
	status = "okay";
};
