// SPDX-License-Identifier: GPL-2.0+
/*
 * Copyright 2013-2015 Freescale Semiconductor, Inc.
 * Copyright 2020 Hitachi Power Grids. All rights reserved.
 */

/dts-v1/;
#include "ls1021a.dtsi"

/ {
	model = "Hitachi-Powergrids SELI8 Service Unit for XMC and FOX";

	chosen {
		stdout-path = &uart0;
	};
};

&enet0 {
	status = "okay";
	tbi-handle = <&tbi0>;
	phy-connection-type = "sgmii";
	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&enet1 {
	status = "okay";
	tbi-handle = <&tbi1>;
	phy-connection-type = "sgmii";
	fixed-link {
		speed = <1000>;
		full-duplex;
	};
};

&enet2 {
	phy-handle = <&debug_phy>;
	phy-connection-type = "rgmii-id";
	max-speed = <100>;
	status = "okay";
};

&i2c0 {
	status = "okay";

	pca9547@70 {
		compatible = "nxp,pca9547";
		reg = <0x70>;
		#address-cells = <1>;
		#size-cells = <0>;
		i2c-mux-idle-disconnect;

		i2c@1 {
			reg = <1>;
			#address-cells = <1>;
			#size-cells = <0>;

			ivm@50 {
				compatible = "atmel,24c02";
				reg = <0x50>;
				label = "MAIN_CTRL";
			};
		};
	};
};

&ifc {
	#address-cells = <2>;
	#size-cells = <1>;
	/* NOR Flash on board */
	ranges = <0x0 0x0 0x60000000 0x04000000>;
	status = "okay";

	nor@0,0 {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "cfi-flash";
		reg = <0x0 0x0 0x4000000>;
		bank-width = <2>;
		device-width = <1>;

		partition@0 {
			label = "rcw";
			reg = <0x0 0x20000>;
			read-only;
		};
		partition@20000 {
			label = "qe";
			reg = <0x20000 0x20000>;
		};
		partition@40000 {
			label = "envred";
			reg = <0x40000 0x20000>;
		};
		partition@60000 {
			label = "env";
			reg = <0x60000 0x20000>;
		};
		partition@100000 {
			label = "u-boot";
			reg = <0x100000 0x100000>;
		};
		partition@200000 {
			label = "redenvred";
			reg = <0x200000 0x20000>;
		};
		partition@220000 {
			label = "redenv";
			reg = <0x220000 0x20000>;
		};
		partition@240000 {
			label = "redu-boot";
			reg = <0x240000 0x100000>;
		};
		partition@340000 {
			label = "ubi0";
			reg = <0x340000 0x03C00000>;
		};
	};
};

&mdio0 {
	debug_phy: ethernet-phy@11 {
		reg = <0x11>;
	};

	tbi0: tbi-phy@0xb {
		reg = <0xb>;
		device_type = "tbi-phy";
	};
};

&mdio1 {
	tbi1: tbi-phy@0xd {
		reg = <0xd>;
		device_type = "tbi-phy";
	};
};

&uart0 {
	status = "okay";
};
