// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Device Tree Include file for Marvell Armada XP family SoC
 *
 * Copyright (C) 2012 Marvell
 *
 * Lior Amsalem <alior@marvell.com>
 * Gregory CLEMENT <gregory.clement@free-electrons.com>
 * Thomas Petazzoni <thomas.petazzoni@free-electrons.com>
 * Ben Dooks <ben.dooks@codethink.co.uk>
 *
 * Contains definitions specific to the Armada XP SoC that are not
 * common to all Armada SoCs.
 */

#include "armada-370-xp.dtsi"

/ {
	#address-cells = <2>;
	#size-cells = <2>;

	model = "Marvell Armada XP family SoC";
	compatible = "marvell,armadaxp", "marvell,armada-370-xp";

	aliases {
		serial2 = &uart2;
		serial3 = &uart3;
	};

	soc {
		compatible = "marvell,armadaxp-mbus", "simple-bus";

		bootrom {
			compatible = "marvell,bootrom";
			reg = <MBUS_ID(0x01, 0x1d) 0 0x100000>;
		};

		internal-regs {
			sdramc: sdramc@1400 {
				compatible = "marvell,armada-xp-sdram-controller";
				reg = <0x1400 0x500>;
			};

			L2: l2-cache@8000 {
				compatible = "marvell,aurora-system-cache";
				reg = <0x08000 0x1000>;
				cache-id-part = <0x100>;
				cache-level = <2>;
				cache-unified;
				wt-override;
			};

			uart2: serial@12200 {
				compatible = "snps,dw-apb-uart";
				pinctrl-0 = <&uart2_pins>;
				pinctrl-names = "default";
				reg = <0x12200 0x100>;
				reg-shift = <2>;
				interrupts = <43>;
				reg-io-width = <1>;
				clocks = <&coreclk 0>;
				status = "disabled";
			};

			uart3: serial@12300 {
				compatible = "snps,dw-apb-uart";
				pinctrl-0 = <&uart3_pins>;
				pinctrl-names = "default";
				reg = <0x12300 0x100>;
				reg-shift = <2>;
				interrupts = <44>;
				reg-io-width = <1>;
				clocks = <&coreclk 0>;
				status = "disabled";
			};

			systemc: system-controller@18200 {
				compatible = "marvell,armada-370-xp-system-controller";
				reg = <0x18200 0x500>;
				#reset-cells = <2>;
			};

			gateclk: clock-gating-control@18220 {
				compatible = "marvell,armada-xp-gating-clock";
				reg = <0x18220 0x4>;
				clocks = <&coreclk 0>;
				#clock-cells = <1>;
			};

			coreclk: mvebu-sar@18230 {
				compatible = "marvell,armada-xp-core-clock";
				reg = <0x18230 0x08>;
				#clock-cells = <1>;
			};

			thermal: thermal@182b0 {
				compatible = "marvell,armadaxp-thermal";
				reg = <0x182b0 0x4
					0x184d0 0x4>;
				status = "okay";
			};

			cpuclk: clock-complex@18700 {
				#clock-cells = <1>;
				compatible = "marvell,armada-xp-cpu-clock";
				reg = <0x18700 0x24>, <0x1c054 0x10>;
				clocks = <&coreclk 1>;
			};

			cpu-config@21000 {
				compatible = "marvell,armada-xp-cpu-config";
				reg = <0x21000 0x8>;
			};

			eth2: ethernet@30000 {
				compatible = "marvell,armada-xp-neta";
				reg = <0x30000 0x4000>;
				interrupts = <12>;
				clocks = <&gateclk 2>;
				status = "disabled";
			};

			usb2: usb@52000 {
				compatible = "marvell,orion-ehci";
				reg = <0x52000 0x500>;
				interrupts = <47>;
				clocks = <&gateclk 20>;
				status = "disabled";
			};

			xor1: xor@60900 {
				compatible = "marvell,orion-xor";
				reg = <0x60900 0x100
				       0x60b00 0x100>;
				clocks = <&gateclk 22>;
				status = "okay";

				xor10 {
					interrupts = <51>;
					dmacap,memcpy;
					dmacap,xor;
				};
				xor11 {
					interrupts = <52>;
					dmacap,memcpy;
					dmacap,xor;
					dmacap,memset;
				};
			};

			ethernet@70000 {
				compatible = "marvell,armada-xp-neta";
			};

			ethernet@74000 {
				compatible = "marvell,armada-xp-neta";
			};

			cesa: crypto@90000 {
				compatible = "marvell,armada-xp-crypto";
				reg = <0x90000 0x10000>;
				reg-names = "regs";
				interrupts = <48>, <49>;
				clocks = <&gateclk 23>, <&gateclk 23>;
				clock-names = "cesa0", "cesa1";
				marvell,crypto-srams = <&crypto_sram0>,
						       <&crypto_sram1>;
				marvell,crypto-sram-size = <0x800>;
			};

			bm: bm@c0000 {
				compatible = "marvell,armada-380-neta-bm";
				reg = <0xc0000 0xac>;
				clocks = <&gateclk 13>;
				internal-mem = <&bm_bppi>;
				status = "disabled";
			};

			xor0: xor@f0900 {
				compatible = "marvell,orion-xor";
				reg = <0xF0900 0x100
				       0xF0B00 0x100>;
				clocks = <&gateclk 28>;
				status = "okay";

				xor00 {
					interrupts = <94>;
					dmacap,memcpy;
					dmacap,xor;
				};
				xor01 {
					interrupts = <95>;
					dmacap,memcpy;
					dmacap,xor;
					dmacap,memset;
				};
			};
		};

		crypto_sram0: sa-sram0 {
			compatible = "mmio-sram";
			reg = <MBUS_ID(0x09, 0x09) 0 0x800>;
			clocks = <&gateclk 23>;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0 MBUS_ID(0x09, 0x09) 0 0x800>;
		};

		crypto_sram1: sa-sram1 {
			compatible = "mmio-sram";
			reg = <MBUS_ID(0x09, 0x05) 0 0x800>;
			clocks = <&gateclk 23>;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0 MBUS_ID(0x09, 0x05) 0 0x800>;
		};

		bm_bppi: bm-bppi {
			compatible = "mmio-sram";
			reg = <MBUS_ID(0x0c, 0x04) 0 0x100000>;
			ranges = <0 MBUS_ID(0x0c, 0x04) 0 0x100000>;
			#address-cells = <1>;
			#size-cells = <1>;
			clocks = <&gateclk 13>;
			no-memory-wc;
			status = "disabled";
		};
	};

	clocks {
		/* 25 MHz reference crystal */
		refclk: oscillator {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <25000000>;
		};
	};
};

&i2c0 {
	compatible = "marvell,mv78230-i2c", "marvell,mv64xxx-i2c";
	reg = <0x11000 0x100>;
};

&i2c1 {
	compatible = "marvell,mv78230-i2c", "marvell,mv64xxx-i2c";
	reg = <0x11100 0x100>;
};

&mpic {
	reg = <0x20a00 0x2d0>, <0x21070 0x58>;
};

&timer {
	compatible = "marvell,armada-xp-timer";
	clocks = <&coreclk 2>, <&refclk>;
	clock-names = "nbclk", "fixed";
};

&watchdog {
	compatible = "marvell,armada-xp-wdt";
	clocks = <&coreclk 2>, <&refclk>;
	clock-names = "nbclk", "fixed";
};

&cpurst {
	reg = <0x20800 0x20>;
};

&usb0 {
	clocks = <&gateclk 18>;
};

&usb1 {
	clocks = <&gateclk 19>;
};

&pinctrl {
	ge0_gmii_pins: ge0-gmii-pins {
		marvell,pins =
		     "mpp0",  "mpp1",  "mpp2",  "mpp3",
		     "mpp4",  "mpp5",  "mpp6",  "mpp7",
		     "mpp8",  "mpp9",  "mpp10", "mpp11",
		     "mpp12", "mpp13", "mpp14", "mpp15",
		     "mpp16", "mpp17", "mpp18", "mpp19",
		     "mpp20", "mpp21", "mpp22", "mpp23";
		marvell,function = "ge0";
	};

	ge0_rgmii_pins: ge0-rgmii-pins {
		marvell,pins =
		     "mpp0", "mpp1", "mpp2", "mpp3",
		     "mpp4", "mpp5", "mpp6", "mpp7",
		     "mpp8", "mpp9", "mpp10", "mpp11";
		marvell,function = "ge0";
	};

	ge1_rgmii_pins: ge1-rgmii-pins {
		marvell,pins =
		     "mpp12", "mpp13", "mpp14", "mpp15",
		     "mpp16", "mpp17", "mpp18", "mpp19",
		     "mpp20", "mpp21", "mpp22", "mpp23";
		marvell,function = "ge1";
	};

	sdio_pins: sdio-pins {
		marvell,pins = "mpp30", "mpp31", "mpp32",
			       "mpp33", "mpp34", "mpp35";
		marvell,function = "sd0";
	};

	spi0_pins: spi0-pins {
		marvell,pins = "mpp36", "mpp37",
			       "mpp38", "mpp39";
		marvell,function = "spi0";
	};

	spi1_pins: spi1-pins {
		marvell,pins = "mpp13", "mpp14",
			       "mpp16", "mpp17";
		marvell,function = "spi1";
	};

	uart2_pins: uart2-pins {
		marvell,pins = "mpp42", "mpp43";
		marvell,function = "uart2";
	};

	uart3_pins: uart3-pins {
		marvell,pins = "mpp44", "mpp45";
		marvell,function = "uart3";
	};
};

&spi0 {
	compatible = "marvell,armada-xp-spi", "marvell,orion-spi";
	pinctrl-0 = <&spi0_pins>;
	pinctrl-names = "default";
};

&spi1 {
	compatible = "marvell,armada-xp-spi", "marvell,orion-spi";
	pinctrl-0 = <&spi1_pins>;
	pinctrl-names = "default";
};
