/dts-v1/;

#include "tegra30.dtsi"

/ {
	model = "NVIDIA Cardhu";
	compatible = "nvidia,cardhu", "nvidia,tegra30";

	chosen {
		stdout-path = &uarta;
	};

	aliases {
		i2c0 = "/i2c@7000d000";
		i2c1 = "/i2c@7000c000";
		i2c2 = "/i2c@7000c400";
		i2c3 = "/i2c@7000c500";
		i2c4 = "/i2c@7000c700";
		mmc0 = "/sdhci@78000600";
		mmc1 = "/sdhci@78000000";
		spi0 = "/spi@7000da00";
		usb0 = "/usb@7d008000";
	};

	memory {
		device_type = "memory";
		reg = <0x80000000 0x40000000>;
	};

	pcie@3000 {
		status = "okay";

		/* AVDD_PEXA and VDD_PEXA inputs are grounded on Cardhu. */
		avdd-pexb-supply = <&ldo1_reg>;
		vdd-pexb-supply = <&ldo1_reg>;
		avdd-pex-pll-supply = <&ldo1_reg>;
		hvdd-pex-supply = <&pex_hvdd_3v3_reg>;
		vddio-pex-ctl-supply = <&sys_3v3_reg>;
		avdd-plle-supply = <&ldo2_reg>;

		pci@1,0 {
			nvidia,num-lanes = <4>;
		};

		pci@2,0 {
			nvidia,num-lanes = <1>;
		};

		pci@3,0 {
			status = "okay";
			nvidia,num-lanes = <1>;
		};
	};

	i2c@7000c000 {
		status = "okay";
		clock-frequency = <100000>;
	};

	i2c@7000c400 {
		status = "okay";
		clock-frequency = <100000>;
	};

	i2c@7000c500 {
		status = "okay";
		clock-frequency = <100000>;
	};

	i2c@7000c700 {
		status = "okay";
		clock-frequency = <100000>;
	};

	i2c@7000d000 {
		status = "okay";
		clock-frequency = <100000>;

		pmic: tps65911@2d {
			compatible = "ti,tps65911";
			reg = <0x2d>;

			interrupts = <GIC_SPI 86 IRQ_TYPE_LEVEL_HIGH>;
			#interrupt-cells = <2>;
			interrupt-controller;

			ti,system-power-controller;

			#gpio-cells = <2>;
			gpio-controller;

			vcc1-supply = <&vdd_ac_bat_reg>;
			vcc2-supply = <&vdd_ac_bat_reg>;
			vcc3-supply = <&vio_reg>;
			vcc4-supply = <&vdd_5v0_reg>;
			vcc5-supply = <&vdd_ac_bat_reg>;
			vcc6-supply = <&vdd2_reg>;
			vcc7-supply = <&vdd_ac_bat_reg>;
			vccio-supply = <&vdd_ac_bat_reg>;

			regulators {
				vdd1_reg: vdd1 {
					regulator-name = "vddio_ddr_1v2";
					regulator-min-microvolt = <1200000>;
					regulator-max-microvolt = <1200000>;
					regulator-always-on;
				};

				vdd2_reg: vdd2 {
					regulator-name = "vdd_1v5_gen";
					regulator-min-microvolt = <1500000>;
					regulator-max-microvolt = <1500000>;
					regulator-always-on;
				};

				vddctrl_reg: vddctrl {
					regulator-name = "vdd_cpu,vdd_sys";
					regulator-min-microvolt = <1000000>;
					regulator-max-microvolt = <1000000>;
					regulator-always-on;
				};

				vio_reg: vio {
					regulator-name = "vdd_1v8_gen";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
					regulator-always-on;
				};

				ldo1_reg: ldo1 {
					regulator-name = "vdd_pexa,vdd_pexb";
					regulator-min-microvolt = <1050000>;
					regulator-max-microvolt = <1050000>;
				};

				ldo2_reg: ldo2 {
					regulator-name = "vdd_sata,avdd_plle";
					regulator-min-microvolt = <1050000>;
					regulator-max-microvolt = <1050000>;
				};

				/* LDO3 is not connected to anything */

				ldo4_reg: ldo4 {
					regulator-name = "vdd_rtc";
					regulator-min-microvolt = <1200000>;
					regulator-max-microvolt = <1200000>;
					regulator-always-on;
				};

				ldo5_reg: ldo5 {
					regulator-name = "vddio_sdmmc,avdd_vdac";
					regulator-min-microvolt = <3300000>;
					regulator-max-microvolt = <3300000>;
					regulator-always-on;
				};

				ldo6_reg: ldo6 {
					regulator-name = "avdd_dsi_csi,pwrdet_mipi";
					regulator-min-microvolt = <1200000>;
					regulator-max-microvolt = <1200000>;
				};

				ldo7_reg: ldo7 {
					regulator-name = "vdd_pllm,x,u,a_p_c_s";
					regulator-min-microvolt = <1200000>;
					regulator-max-microvolt = <1200000>;
					regulator-always-on;
				};

				ldo8_reg: ldo8 {
					regulator-name = "vdd_ddr_hs";
					regulator-min-microvolt = <1000000>;
					regulator-max-microvolt = <1000000>;
					regulator-always-on;
				};
			};
		};
	};

	spi@7000da00 {
		status = "okay";
		spi-max-frequency = <25000000>;
	};

	sdhci@78000000 {
		status = "okay";
		cd-gpios = <&gpio TEGRA_GPIO(I, 5) GPIO_ACTIVE_LOW>;
		wp-gpios = <&gpio TEGRA_GPIO(T, 3) GPIO_ACTIVE_HIGH>;
		power-gpios = <&gpio TEGRA_GPIO(D, 7) GPIO_ACTIVE_HIGH>;
		bus-width = <4>;
	};

	sdhci@78000600 {
		status = "okay";
		bus-width = <8>;
		non-removable;
	};

	usb@7d008000 {
		nvidia,vbus-gpio = <&gpio TEGRA_GPIO(DD, 4) GPIO_ACTIVE_HIGH>;
		status = "okay";
	};

	clocks {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <0>;

		clk32k_in: clock@0 {
			compatible = "fixed-clock";
			reg=<0>;
			#clock-cells = <0>;
			clock-frequency = <32768>;
		};
	};

	regulators {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <0>;

		vdd_ac_bat_reg: regulator@0 {
			compatible = "regulator-fixed";
			reg = <0>;
			regulator-name = "vdd_ac_bat";
			regulator-min-microvolt = <5000000>;
			regulator-max-microvolt = <5000000>;
			regulator-always-on;
		};

		cam_1v8_reg: regulator@1 {
			compatible = "regulator-fixed";
			reg = <1>;
			regulator-name = "cam_1v8";
			regulator-min-microvolt = <1800000>;
			regulator-max-microvolt = <1800000>;
			enable-active-high;
			gpio = <&gpio TEGRA_GPIO(BB, 4) GPIO_ACTIVE_HIGH>;
			vin-supply = <&vio_reg>;
		};

		cp_5v_reg: regulator@2 {
			compatible = "regulator-fixed";
			reg = <2>;
			regulator-name = "cp_5v";
			regulator-min-microvolt = <5000000>;
			regulator-max-microvolt = <5000000>;
			regulator-boot-on;
			regulator-always-on;
			enable-active-high;
			gpio = <&pmic 0 GPIO_ACTIVE_HIGH>;
		};

		emmc_3v3_reg: regulator@3 {
			compatible = "regulator-fixed";
			reg = <3>;
			regulator-name = "emmc_3v3";
			regulator-min-microvolt = <3300000>;
			regulator-max-microvolt = <3300000>;
			regulator-always-on;
			regulator-boot-on;
			enable-active-high;
			gpio = <&gpio TEGRA_GPIO(D, 1) GPIO_ACTIVE_HIGH>;
			vin-supply = <&sys_3v3_reg>;
		};

		modem_3v3_reg: regulator@4 {
			compatible = "regulator-fixed";
			reg = <4>;
			regulator-name = "modem_3v3";
			regulator-min-microvolt = <3300000>;
			regulator-max-microvolt = <3300000>;
			enable-active-high;
			gpio = <&gpio TEGRA_GPIO(D, 6) GPIO_ACTIVE_HIGH>;
		};

		pex_hvdd_3v3_reg: regulator@5 {
			compatible = "regulator-fixed";
			reg = <5>;
			regulator-name = "pex_hvdd_3v3";
			regulator-min-microvolt = <3300000>;
			regulator-max-microvolt = <3300000>;
			enable-active-high;
			gpio = <&gpio TEGRA_GPIO(L, 7) GPIO_ACTIVE_HIGH>;
			vin-supply = <&sys_3v3_reg>;
		};

		vdd_cam1_ldo_reg: regulator@6 {
			compatible = "regulator-fixed";
			reg = <6>;
			regulator-name = "vdd_cam1_ldo";
			regulator-min-microvolt = <2800000>;
			regulator-max-microvolt = <2800000>;
			enable-active-high;
			gpio = <&gpio TEGRA_GPIO(R, 6) GPIO_ACTIVE_HIGH>;
			vin-supply = <&sys_3v3_reg>;
		};

		vdd_cam2_ldo_reg: regulator@7 {
			compatible = "regulator-fixed";
			reg = <7>;
			regulator-name = "vdd_cam2_ldo";
			regulator-min-microvolt = <2800000>;
			regulator-max-microvolt = <2800000>;
			enable-active-high;
			gpio = <&gpio TEGRA_GPIO(R, 7) GPIO_ACTIVE_HIGH>;
			vin-supply = <&sys_3v3_reg>;
		};

		vdd_cam3_ldo_reg: regulator@8 {
			compatible = "regulator-fixed";
			reg = <8>;
			regulator-name = "vdd_cam3_ldo";
			regulator-min-microvolt = <3300000>;
			regulator-max-microvolt = <3300000>;
			enable-active-high;
			gpio = <&gpio TEGRA_GPIO(S, 0) GPIO_ACTIVE_HIGH>;
			vin-supply = <&sys_3v3_reg>;
		};

		vdd_com_reg: regulator@9 {
			compatible = "regulator-fixed";
			reg = <9>;
			regulator-name = "vdd_com";
			regulator-min-microvolt = <3300000>;
			regulator-max-microvolt = <3300000>;
			regulator-always-on;
			regulator-boot-on;
			enable-active-high;
			gpio = <&gpio TEGRA_GPIO(D, 0) GPIO_ACTIVE_HIGH>;
			vin-supply = <&sys_3v3_reg>;
		};

		vdd_fuse_3v3_reg: regulator@10 {
			compatible = "regulator-fixed";
			reg = <10>;
			regulator-name = "vdd_fuse_3v3";
			regulator-min-microvolt = <3300000>;
			regulator-max-microvolt = <3300000>;
			enable-active-high;
			gpio = <&gpio TEGRA_GPIO(L, 6) GPIO_ACTIVE_HIGH>;
			vin-supply = <&sys_3v3_reg>;
		};

		vdd_pnl1_reg: regulator@11 {
			compatible = "regulator-fixed";
			reg = <11>;
			regulator-name = "vdd_pnl1";
			regulator-min-microvolt = <3300000>;
			regulator-max-microvolt = <3300000>;
			regulator-always-on;
			regulator-boot-on;
			enable-active-high;
			gpio = <&gpio TEGRA_GPIO(L, 4) GPIO_ACTIVE_HIGH>;
			vin-supply = <&sys_3v3_reg>;
		};

		vdd_vid_reg: regulator@12 {
			compatible = "regulator-fixed";
			reg = <12>;
			regulator-name = "vddio_vid";
			regulator-min-microvolt = <5000000>;
			regulator-max-microvolt = <5000000>;
			enable-active-high;
			gpio = <&gpio TEGRA_GPIO(T, 0) GPIO_ACTIVE_HIGH>;
			gpio-open-drain;
			vin-supply = <&vdd_5v0_reg>;
		};

		ddr_reg: regulator@100 {
			compatible = "regulator-fixed";
			regulator-name = "ddr";
			reg = <100>;
			regulator-min-microvolt = <1500000>;
			regulator-max-microvolt = <1500000>;
			regulator-always-on;
			regulator-boot-on;
			enable-active-high;
			gpio = <&pmic 7 GPIO_ACTIVE_HIGH>;
		};

		sys_3v3_reg: regulator@101 {
			compatible = "regulator-fixed";
			reg = <101>;
			regulator-name = "sys_3v3";
			regulator-min-microvolt = <3300000>;
			regulator-max-microvolt = <3300000>;
			regulator-always-on;
			regulator-boot-on;
			enable-active-high;
			gpio = <&pmic 6 GPIO_ACTIVE_HIGH>;
		};

		usb1_vbus_reg: regulator@102 {
			compatible = "regulator-fixed";
			reg = <102>;
			regulator-name = "usb1_vbus";
			regulator-min-microvolt = <5000000>;
			regulator-max-microvolt = <5000000>;
			enable-active-high;
			gpio = <&gpio TEGRA_GPIO(DD, 6) GPIO_ACTIVE_HIGH>;
			gpio-open-drain;
			vin-supply = <&vdd_5v0_reg>;
		};

		usb3_vbus_reg: regulator@103 {
			compatible = "regulator-fixed";
			reg = <103>;
			regulator-name = "usb3_vbus";
			regulator-min-microvolt = <5000000>;
			regulator-max-microvolt = <5000000>;
			enable-active-high;
			gpio = <&gpio TEGRA_GPIO(DD, 4) GPIO_ACTIVE_HIGH>;
			gpio-open-drain;
			vin-supply = <&vdd_5v0_reg>;
		};

		vdd_5v0_reg: regulator@104 {
			compatible = "regulator-fixed";
			reg = <104>;
			regulator-name = "5v0";
			regulator-min-microvolt = <5000000>;
			regulator-max-microvolt = <5000000>;
			enable-active-high;
			gpio = <&pmic 8 GPIO_ACTIVE_HIGH>;
		};

		vdd_bl_reg: regulator@105 {
			compatible = "regulator-fixed";
			reg = <105>;
			regulator-name = "vdd_bl";
			regulator-min-microvolt = <5000000>;
			regulator-max-microvolt = <5000000>;
			regulator-always-on;
			regulator-boot-on;
			enable-active-high;
			gpio = <&gpio TEGRA_GPIO(DD, 2) GPIO_ACTIVE_HIGH>;
		};

		vdd_bl2_reg: regulator@106 {
			compatible = "regulator-fixed";
			reg = <106>;
			regulator-name = "vdd_bl2";
			regulator-min-microvolt = <5000000>;
			regulator-max-microvolt = <5000000>;
			regulator-always-on;
			regulator-boot-on;
			enable-active-high;
			gpio = <&gpio TEGRA_GPIO(DD, 0) GPIO_ACTIVE_HIGH>;
		};
	};
};

&uarta {
	status = "okay";
};
