// SPDX-License-Identifier: GPL-2.0
/*
 * support for the bosch am335x based shc c3 board
 *
 * Copyright, (C) 2015 Heiko Schocher <hs@denx.de>
 *
 */
/dts-v1/;

#include "am33xx.dtsi"
#include <dt-bindings/input/input.h>

/ {
	model = "Bosch SHC";
	compatible = "ti,am335x-shc", "ti,am335x-bone", "ti,am33xx";

	aliases {
		mmcblk0 = &mmc1;
		mmcblk1 = &mmc2;
	};

	cpus {
		cpu@0 {
			/*
			 * To consider voltage drop between PMIC and SoC,
			 * tolerance value is reduced to 2% from 4% and
			 * voltage value is increased as a precaution.
			 */
			operating-points = <
				/* kHz    uV */
				594000  1225000
				294000  1125000
			>;
			voltage-tolerance = <2>; /* 2 percentage */
			cpu0-supply = <&dcdc2_reg>;
		};
	};

	gpio-keys {
		compatible = "gpio-keys";

		back-button {
			label = "Back Button";
			gpios = <&gpio1 29 GPIO_ACTIVE_HIGH>;
			linux,code = <KEY_BACK>;
			debounce-interval = <1000>;
			wakeup-source;
		};

		front-button {
			label = "Front Button";
			gpios = <&gpio1 25 GPIO_ACTIVE_HIGH>;
			linux,code = <KEY_FRONT>;
			debounce-interval = <1000>;
			wakeup-source;
		};
	};

	leds {
		pinctrl-names = "default";
		pinctrl-0 = <&user_leds_s0>;

		compatible = "gpio-leds";

		led1 {
			label = "shc:power:red";
			gpios = <&gpio0 23 GPIO_ACTIVE_HIGH>;
			default-state = "off";
		};

		led2 {
			label = "shc:power:bl";
			gpios = <&gpio0 22 GPIO_ACTIVE_HIGH>;
			linux,default-trigger = "timer";
			default-state = "on";
		};

		led3 {
			label = "shc:lan:red";
			gpios = <&gpio0 26 GPIO_ACTIVE_HIGH>;
			default-state = "off";
		};

		led4 {
			label = "shc:lan:bl";
			gpios = <&gpio1 17 GPIO_ACTIVE_HIGH>;
			default-state = "off";
		};

		led5 {
			label = "shc:cloud:red";
			gpios = <&gpio2 2 GPIO_ACTIVE_HIGH>;
			default-state = "off";
		};

		led6 {
			label = "shc:cloud:bl";
			gpios = <&gpio1 18 GPIO_ACTIVE_HIGH>;
			default-state = "off";
		};
	};

	memory@80000000 {
		device_type = "memory";
		reg = <0x80000000 0x20000000>; /* 512 MB */
	};

	vmmcsd_fixed: fixedregulator0 {
		compatible = "regulator-fixed";
		regulator-name = "vmmcsd_fixed";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
	};
};

&aes {
	status = "okay";
};

&cppi41dma  {
	status = "okay";
};

&davinci_mdio {
	pinctrl-names = "default", "sleep";
	pinctrl-0 = <&davinci_mdio_default>;
	pinctrl-1 = <&davinci_mdio_sleep>;
	status = "okay";

	ethernetphy0: ethernet-phy@0 {
		reg = <0>;
		smsc,disable-energy-detect;
	};
};

&epwmss1 {
	status = "okay";

	ehrpwm1: pwm@200 {
		pinctrl-names = "default";
		pinctrl-0 = <&ehrpwm1_pins>;
		status = "okay";
	};
};

&gpio1 {
	hmtc-rst-hog {
		gpio-hog;
		gpios = <24 GPIO_ACTIVE_LOW>;
		output-high;
		line-name = "homematic_reset";
	};

	hmtc-prog-hog {
		gpio-hog;
		gpios = <27 GPIO_ACTIVE_LOW>;
		output-high;
		line-name = "homematic_program";
	};
};

&gpio3 {
	zgb-rst-hog {
		gpio-hog;
		gpios = <18 GPIO_ACTIVE_LOW>;
		output-low;
		line-name = "zigbee_reset";
	};

	zgb-boot-hog {
		gpio-hog;
		gpios = <19 GPIO_ACTIVE_HIGH>;
		output-high;
		line-name = "zigbee_boot";
	};
};

&i2c0 {
	pinctrl-names = "default";
	pinctrl-0 = <&i2c0_pins>;
	status = "okay";
	clock-frequency = <400000>;

	tps: tps@24 {
		reg = <0x24>;
	};

	at24@50 {
		compatible = "atmel,24c32";
		pagesize = <32>;
		reg = <0x50>;
	};

	pcf8563@51 {
		compatible = "nxp,pcf8563";
		reg = <0x51>;
	};
};

&cpsw_emac0 {
	phy-mode = "mii";
	phy-handle = <&ethernetphy0>;
};

&mac {
	pinctrl-names = "default", "sleep";
	pinctrl-0 = <&cpsw_default>;
	pinctrl-1 = <&cpsw_sleep>;
	status = "okay";
	slaves = <1>;
};

&mmc1 {
	pinctrl-names = "default";
	pinctrl-0 = <&mmc1_pins>;
	bus-width = <0x4>;
	cd-gpios = <&gpio0 6 GPIO_ACTIVE_HIGH>;
	cd-inverted;
	max-frequency = <26000000>;
	vmmc-supply = <&vmmcsd_fixed>;
	status = "okay";
};

&mmc2 {
	pinctrl-names = "default";
	pinctrl-0 = <&emmc_pins>;
	bus-width = <8>;
	max-frequency = <26000000>;
	sd-uhs-sdr25;
	vmmc-supply = <&vmmcsd_fixed>;
	status = "okay";
};

&mmc3 {
	pinctrl-names = "default";
	pinctrl-0 = <&mmc3_pins>;
	bus-width = <4>;
	cap-power-off-card;
	max-frequency = <26000000>;
	sd-uhs-sdr25;
	vmmc-supply = <&vmmcsd_fixed>;
	status = "okay";
};

&rtc {
	ti,no-init;
};

&sham {
	status = "okay";
};

&tps {
	compatible = "ti,tps65217";
	ti,pmic-shutdown-controller;

	regulators {
		#address-cells = <1>;
		#size-cells = <0>;

		dcdc1_reg: regulator@0 {
			reg = <0>;
			regulator-name = "vdds_dpr";
			regulator-compatible = "dcdc1";
			regulator-min-microvolt = <1300000>;
			regulator-max-microvolt = <1450000>;
			regulator-boot-on;
			regulator-always-on;
		};

		dcdc2_reg: regulator@1 {
			reg = <1>;
			/*
			 * VDD_MPU voltage limits 0.95V - 1.26V with
			 * +/-4% tolerance
			 */
			regulator-compatible = "dcdc2";
			regulator-name = "vdd_mpu";
			regulator-min-microvolt = <925000>;
			regulator-max-microvolt = <1375000>;
			regulator-boot-on;
			regulator-always-on;
			regulator-ramp-delay = <70000>;
		};

		dcdc3_reg: regulator@2 {
			reg = <2>;
			/*
			 * VDD_CORE voltage limits 0.95V - 1.1V with
			 * +/-4% tolerance
			 */
			regulator-name = "vdd_core";
			regulator-compatible = "dcdc3";
			regulator-min-microvolt = <925000>;
			regulator-max-microvolt = <1125000>;
			regulator-boot-on;
			regulator-always-on;
		};

		ldo1_reg: regulator@3 {
			reg = <3>;
			regulator-name = "vio,vrtc,vdds";
			regulator-compatible = "ldo1";
			regulator-min-microvolt = <1000000>;
			regulator-max-microvolt = <1800000>;
			regulator-always-on;
		};

		ldo2_reg: regulator@4 {
			reg = <4>;
			regulator-name = "vdd_3v3aux";
			regulator-compatible = "ldo2";
			regulator-min-microvolt = <900000>;
			regulator-max-microvolt = <3300000>;
			regulator-always-on;
		};

		ldo3_reg: regulator@5 {
			reg = <5>;
			regulator-name = "vdd_1v8";
			regulator-compatible = "ldo3";
			regulator-min-microvolt = <900000>;
			regulator-max-microvolt = <1800000>;
			regulator-always-on;
		};

		ldo4_reg: regulator@6 {
			reg = <6>;
			regulator-name = "vdd_3v3a";
			regulator-compatible = "ldo4";
			regulator-min-microvolt = <1800000>;
			regulator-max-microvolt = <3300000>;
			regulator-always-on;
		};
	};
};

&uart0 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart0_pins>;
	status = "okay";
};

&uart1 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart1_pins>;
	status = "okay";
};

&uart2 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart2_pins>;
	status = "okay";
};

&uart4 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart4_pins>;
	status = "okay";
};

&usb {
	status = "okay";
};

&usb_ctrl_mod {
	status = "okay";
};

&usb1_phy {
	status = "okay";
};

&usb1 {
	status = "okay";
	dr_mode = "host";
};

&am33xx_pinmux {
	pinctrl-names = "default";
	pinctrl-0 = <&clkout2_pin>;

	clkout2_pin: pinmux_clkout2_pin {
		pinctrl-single,pins = <
			/* xdma_event_intr1.clkout2 */
			AM33XX_PADCONF(AM335X_PIN_XDMA_EVENT_INTR1, PIN_INPUT, MUX_MODE6)
		>;
	};

	cpsw_default: cpsw_default {
		pinctrl-single,pins = <
			/* Slave 1 */
			AM33XX_PADCONF(AM335X_PIN_MII1_RX_ER, PIN_INPUT_PULLDOWN, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_MII1_TX_EN, PIN_OUTPUT_PULLDOWN, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_MII1_RX_DV, PIN_INPUT_PULLDOWN, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_MII1_TXD3, PIN_OUTPUT_PULLDOWN, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_MII1_TXD2, PIN_OUTPUT_PULLDOWN, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_MII1_TXD1, PIN_INPUT_PULLDOWN, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_MII1_TXD0, PIN_INPUT_PULLDOWN, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_MII1_TX_CLK, PIN_INPUT_PULLUP, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_MII1_RX_CLK, PIN_INPUT_PULLDOWN, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_MII1_RXD3, PIN_INPUT_PULLDOWN, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_MII1_RXD2, PIN_INPUT_PULLDOWN, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_MII1_RXD1, PIN_INPUT_PULLDOWN, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_MII1_RXD0, PIN_INPUT_PULLDOWN, MUX_MODE0)
		>;
	};

	cpsw_sleep: cpsw_sleep {
		pinctrl-single,pins = <
			/* Slave 1 reset value */
			AM33XX_PADCONF(AM335X_PIN_MII1_RX_ER, PIN_INPUT_PULLDOWN, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_MII1_TX_EN, PIN_INPUT_PULLDOWN, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_MII1_RX_DV, PIN_INPUT_PULLDOWN, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_MII1_TXD3, PIN_INPUT_PULLDOWN, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_MII1_TXD2, PIN_INPUT_PULLDOWN, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_MII1_TXD1, PIN_INPUT_PULLDOWN, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_MII1_TXD0, PIN_INPUT_PULLDOWN, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_MII1_TX_CLK, PIN_INPUT_PULLDOWN, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_MII1_RX_CLK, PIN_INPUT_PULLDOWN, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_MII1_RXD3, PIN_INPUT_PULLDOWN, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_MII1_RXD2, PIN_INPUT_PULLDOWN, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_MII1_RXD1, PIN_INPUT_PULLDOWN, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_MII1_RXD0, PIN_INPUT_PULLDOWN, MUX_MODE7)
		>;
	};

	davinci_mdio_default: davinci_mdio_default {
		pinctrl-single,pins = <
			AM33XX_PADCONF(AM335X_PIN_MDIO, PIN_INPUT_PULLUP | SLEWCTRL_FAST, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_MDC, PIN_OUTPUT_PULLUP, MUX_MODE0)
		>;
	};

	davinci_mdio_sleep: davinci_mdio_sleep {
		pinctrl-single,pins = <
			/* MDIO reset value */
			AM33XX_PADCONF(AM335X_PIN_MDIO, PIN_INPUT_PULLDOWN, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_MDC, PIN_INPUT_PULLDOWN, MUX_MODE7)
		>;
	};

	ehrpwm1_pins: pinmux_ehrpwm1 {
		pinctrl-single,pins = <
			AM33XX_PADCONF(AM335X_PIN_GPMC_A3, PIN_OUTPUT, MUX_MODE6) /* gpmc_a3.gpio1_19 */
		>;
	};

	emmc_pins: pinmux_emmc_pins {
		pinctrl-single,pins = <
			AM33XX_PADCONF(AM335X_PIN_GPMC_CSN1, PIN_INPUT, MUX_MODE2)
			AM33XX_PADCONF(AM335X_PIN_GPMC_CSN2, PIN_INPUT_PULLUP, MUX_MODE2)
			AM33XX_PADCONF(AM335X_PIN_GPMC_AD0, PIN_INPUT_PULLUP, MUX_MODE1)
			AM33XX_PADCONF(AM335X_PIN_GPMC_AD1, PIN_INPUT_PULLUP, MUX_MODE1)
			AM33XX_PADCONF(AM335X_PIN_GPMC_AD2, PIN_INPUT_PULLUP, MUX_MODE1)
			AM33XX_PADCONF(AM335X_PIN_GPMC_AD3, PIN_INPUT_PULLUP, MUX_MODE1)
			AM33XX_PADCONF(AM335X_PIN_GPMC_AD4, PIN_INPUT_PULLUP, MUX_MODE1)
			AM33XX_PADCONF(AM335X_PIN_GPMC_AD5, PIN_INPUT_PULLUP, MUX_MODE1)
			AM33XX_PADCONF(AM335X_PIN_GPMC_AD6, PIN_INPUT_PULLUP, MUX_MODE1)
			AM33XX_PADCONF(AM335X_PIN_GPMC_AD7, PIN_INPUT_PULLUP, MUX_MODE1)
		>;
	};

	i2c0_pins: pinmux_i2c0_pins {
		pinctrl-single,pins = <
			AM33XX_PADCONF(AM335X_PIN_I2C0_SDA, PIN_INPUT, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_I2C0_SCL, PIN_INPUT, MUX_MODE0)
		>;
	};

	mmc1_pins: pinmux_mmc1_pins {
		pinctrl-single,pins = <
			AM33XX_PADCONF(AM335X_PIN_SPI0_CS1, PIN_INPUT, MUX_MODE5)
		>;
	};

	mmc3_pins: pinmux_mmc3_pins {
		pinctrl-single,pins = <
			AM33XX_PADCONF(AM335X_PIN_GPMC_AD12, PIN_INPUT, MUX_MODE3)
			AM33XX_PADCONF(AM335X_PIN_GPMC_AD13, PIN_INPUT, MUX_MODE3)
			AM33XX_PADCONF(AM335X_PIN_GPMC_AD14, PIN_INPUT, MUX_MODE3)
			AM33XX_PADCONF(AM335X_PIN_GPMC_AD15, PIN_INPUT, MUX_MODE3)
			AM33XX_PADCONF(AM335X_PIN_GPMC_CSN3, PIN_INPUT, MUX_MODE3)
			AM33XX_PADCONF(AM335X_PIN_GPMC_CLK, PIN_INPUT, MUX_MODE3)
		>;
	};

	uart0_pins: pinmux_uart0_pins {
		pinctrl-single,pins = <
			AM33XX_PADCONF(AM335X_PIN_UART0_CTSN, PIN_INPUT_PULLDOWN, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_UART0_RTSN, PIN_OUTPUT, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_UART0_RXD, PIN_INPUT_PULLDOWN, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_UART0_TXD, PIN_OUTPUT, MUX_MODE0)
		>;
	};

	uart1_pins: pinmux_uart1 {
		pinctrl-single,pins = <
			AM33XX_PADCONF(AM335X_PIN_UART1_CTSN, PIN_INPUT_PULLDOWN, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_UART1_RTSN, PIN_OUTPUT, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_UART1_RXD, PIN_INPUT, MUX_MODE0)
			AM33XX_PADCONF(AM335X_PIN_UART1_TXD, PIN_OUTPUT, MUX_MODE0)
		>;
	};

	uart2_pins: pinmux_uart2_pins {
		pinctrl-single,pins = <
			AM33XX_PADCONF(AM335X_PIN_SPI0_SCLK, PIN_INPUT, MUX_MODE1)
			AM33XX_PADCONF(AM335X_PIN_SPI0_D0, PIN_OUTPUT, MUX_MODE1)
		>;
	};

	uart4_pins: pinmux_uart4_pins {
		pinctrl-single,pins = <
			AM33XX_PADCONF(AM335X_PIN_GPMC_WAIT0, PIN_INPUT_PULLUP, MUX_MODE6)
			AM33XX_PADCONF(AM335X_PIN_GPMC_WPN, PIN_OUTPUT_PULLUP, MUX_MODE6)
		>;
	};

	user_leds_s0: user_leds_s0 {
		pinctrl-single,pins = <
			AM33XX_PADCONF(AM335X_PIN_GPMC_AD8, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_GPMC_AD9, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_GPMC_AD10, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_GPMC_AD11, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_GPMC_A0, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_GPMC_A1, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_GPMC_A2, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_GPMC_A4, PIN_OUTPUT_PULLDOWN, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_GPMC_A5, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_GPMC_A6, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_GPMC_A7, PIN_OUTPUT_PULLUP, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_GPMC_A8, PIN_INPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_GPMC_A9, PIN_INPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_GPMC_A10, PIN_INPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_GPMC_A11, PIN_INPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_GPMC_BEN1, PIN_OUTPUT_PULLUP, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_GPMC_CSN0, PIN_INPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_GPMC_ADVN_ALE, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_GPMC_OEN_REN, PIN_INPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_GPMC_WEN, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_GPMC_BEN0_CLE, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_LCD_DATA0, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_LCD_DATA1, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_LCD_DATA2, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_LCD_DATA3, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_LCD_DATA4, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_LCD_DATA5, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_LCD_DATA6, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_LCD_DATA7, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_LCD_DATA8, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_LCD_DATA9, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_LCD_DATA10, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_LCD_DATA11, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_LCD_DATA12, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_LCD_DATA13, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_LCD_DATA14, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_LCD_DATA15, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_LCD_VSYNC, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_LCD_HSYNC, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_LCD_PCLK, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_LCD_AC_BIAS_EN, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_RMII1_REF_CLK, PIN_INPUT_PULLDOWN, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_SPI0_D1, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_SPI0_CS0, PIN_OUTPUT, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_ECAP0_IN_PWM0_OUT, PIN_OUTPUT_PULLUP, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_MCASP0_ACLKR, PIN_OUTPUT_PULLDOWN, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_MCASP0_FSR, PIN_OUTPUT_PULLDOWN, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_MCASP0_AXR1, PIN_INPUT_PULLDOWN, MUX_MODE7)
			AM33XX_PADCONF(AM335X_PIN_MCASP0_AHCLKX, PIN_INPUT_PULLUP, MUX_MODE7)
		>;
	};
};
