// SPDX-License-Identifier: GPL-2.0+ OR MIT
//
// Device Tree Source for UniPhier PXs3 SoC
//
// Copyright (C) 2017 Socionext Inc.
//   Author: Masahiro Yamada <yamada.masahiro@socionext.com>

#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/gpio/uniphier-gpio.h>
#include <dt-bindings/interrupt-controller/arm-gic.h>
#include <dt-bindings/thermal/thermal.h>

/ {
	compatible = "socionext,uniphier-pxs3";
	#address-cells = <2>;
	#size-cells = <2>;
	interrupt-parent = <&gic>;

	cpus {
		#address-cells = <2>;
		#size-cells = <0>;

		cpu-map {
			cluster0 {
				core0 {
					cpu = <&cpu0>;
				};
				core1 {
					cpu = <&cpu1>;
				};
				core2 {
					cpu = <&cpu2>;
				};
				core3 {
					cpu = <&cpu3>;
				};
			};
		};

		cpu0: cpu@0 {
			device_type = "cpu";
			compatible = "arm,cortex-a53";
			reg = <0 0x000>;
			clocks = <&sys_clk 33>;
			enable-method = "psci";
			next-level-cache = <&l2>;
			operating-points-v2 = <&cluster0_opp>;
			#cooling-cells = <2>;
		};

		cpu1: cpu@1 {
			device_type = "cpu";
			compatible = "arm,cortex-a53";
			reg = <0 0x001>;
			clocks = <&sys_clk 33>;
			enable-method = "psci";
			next-level-cache = <&l2>;
			operating-points-v2 = <&cluster0_opp>;
			#cooling-cells = <2>;
		};

		cpu2: cpu@2 {
			device_type = "cpu";
			compatible = "arm,cortex-a53";
			reg = <0 0x002>;
			clocks = <&sys_clk 33>;
			enable-method = "psci";
			next-level-cache = <&l2>;
			operating-points-v2 = <&cluster0_opp>;
			#cooling-cells = <2>;
		};

		cpu3: cpu@3 {
			device_type = "cpu";
			compatible = "arm,cortex-a53";
			reg = <0 0x003>;
			clocks = <&sys_clk 33>;
			enable-method = "psci";
			next-level-cache = <&l2>;
			operating-points-v2 = <&cluster0_opp>;
			#cooling-cells = <2>;
		};

		l2: l2-cache {
			compatible = "cache";
		};
	};

	cluster0_opp: opp-table {
		compatible = "operating-points-v2";
		opp-shared;

		opp-250000000 {
			opp-hz = /bits/ 64 <250000000>;
			clock-latency-ns = <300>;
		};
		opp-325000000 {
			opp-hz = /bits/ 64 <325000000>;
			clock-latency-ns = <300>;
		};
		opp-500000000 {
			opp-hz = /bits/ 64 <500000000>;
			clock-latency-ns = <300>;
		};
		opp-650000000 {
			opp-hz = /bits/ 64 <650000000>;
			clock-latency-ns = <300>;
		};
		opp-666667000 {
			opp-hz = /bits/ 64 <666667000>;
			clock-latency-ns = <300>;
		};
		opp-866667000 {
			opp-hz = /bits/ 64 <866667000>;
			clock-latency-ns = <300>;
		};
		opp-1000000000 {
			opp-hz = /bits/ 64 <1000000000>;
			clock-latency-ns = <300>;
		};
		opp-1300000000 {
			opp-hz = /bits/ 64 <1300000000>;
			clock-latency-ns = <300>;
		};
	};

	psci {
		compatible = "arm,psci-1.0";
		method = "smc";
	};

	clocks {
		refclk: ref {
			compatible = "fixed-clock";
			#clock-cells = <0>;
			clock-frequency = <25000000>;
		};
	};

	emmc_pwrseq: emmc-pwrseq {
		compatible = "mmc-pwrseq-emmc";
		reset-gpios = <&gpio UNIPHIER_GPIO_PORT(5, 7) GPIO_ACTIVE_LOW>;
	};

	timer {
		compatible = "arm,armv8-timer";
		interrupts = <GIC_PPI 13 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_PPI 14 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_PPI 11 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_PPI 10 IRQ_TYPE_LEVEL_HIGH>;
	};

	thermal-zones {
		cpu-thermal {
			polling-delay-passive = <250>;	/* 250ms */
			polling-delay = <1000>;		/* 1000ms */
			thermal-sensors = <&pvtctl>;

			trips {
				cpu_crit: cpu-crit {
					temperature = <110000>;	/* 110C */
					hysteresis = <2000>;
					type = "critical";
				};
				cpu_alert: cpu-alert {
					temperature = <100000>;	/* 100C */
					hysteresis = <2000>;
					type = "passive";
				};
			};

			cooling-maps {
				map0 {
					trip = <&cpu_alert>;
					cooling-device = <&cpu0 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
							 <&cpu1 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
							 <&cpu2 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
							 <&cpu3 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
				};
			};
		};
	};

	reserved-memory {
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;

		secure-memory@81000000 {
			reg = <0x0 0x81000000 0x0 0x01000000>;
			no-map;
		};
	};

	soc@0 {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0 0 0 0xffffffff>;

		spi0: spi@54006000 {
			compatible = "socionext,uniphier-scssi";
			status = "disabled";
			reg = <0x54006000 0x100>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 39 IRQ_TYPE_LEVEL_HIGH>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_spi0>;
			clocks = <&peri_clk 11>;
			resets = <&peri_rst 11>;
		};

		spi1: spi@54006100 {
			compatible = "socionext,uniphier-scssi";
			status = "disabled";
			reg = <0x54006100 0x100>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 216 IRQ_TYPE_LEVEL_HIGH>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_spi1>;
			clocks = <&peri_clk 12>;
			resets = <&peri_rst 12>;
		};

		serial0: serial@54006800 {
			compatible = "socionext,uniphier-uart";
			status = "disabled";
			reg = <0x54006800 0x40>;
			interrupts = <GIC_SPI 33 IRQ_TYPE_LEVEL_HIGH>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_uart0>;
			clocks = <&peri_clk 0>;
			resets = <&peri_rst 0>;
		};

		serial1: serial@54006900 {
			compatible = "socionext,uniphier-uart";
			status = "disabled";
			reg = <0x54006900 0x40>;
			interrupts = <GIC_SPI 35 IRQ_TYPE_LEVEL_HIGH>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_uart1>;
			clocks = <&peri_clk 1>;
			resets = <&peri_rst 1>;
		};

		serial2: serial@54006a00 {
			compatible = "socionext,uniphier-uart";
			status = "disabled";
			reg = <0x54006a00 0x40>;
			interrupts = <GIC_SPI 37 IRQ_TYPE_LEVEL_HIGH>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_uart2>;
			clocks = <&peri_clk 2>;
			resets = <&peri_rst 2>;
		};

		serial3: serial@54006b00 {
			compatible = "socionext,uniphier-uart";
			status = "disabled";
			reg = <0x54006b00 0x40>;
			interrupts = <GIC_SPI 177 IRQ_TYPE_LEVEL_HIGH>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_uart3>;
			clocks = <&peri_clk 3>;
			resets = <&peri_rst 3>;
		};

		gpio: gpio@55000000 {
			compatible = "socionext,uniphier-gpio";
			reg = <0x55000000 0x200>;
			interrupt-parent = <&aidet>;
			interrupt-controller;
			#interrupt-cells = <2>;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-ranges = <&pinctrl 0 0 0>,
				      <&pinctrl 104 0 0>,
				      <&pinctrl 168 0 0>;
			gpio-ranges-group-names = "gpio_range0",
						  "gpio_range1",
						  "gpio_range2";
			ngpios = <286>;
			socionext,interrupt-ranges = <0 48 16>, <16 154 5>,
						     <21 217 3>;
		};

		i2c0: i2c@58780000 {
			compatible = "socionext,uniphier-fi2c";
			status = "disabled";
			reg = <0x58780000 0x80>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 41 IRQ_TYPE_LEVEL_HIGH>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_i2c0>;
			clocks = <&peri_clk 4>;
			resets = <&peri_rst 4>;
			clock-frequency = <100000>;
		};

		i2c1: i2c@58781000 {
			compatible = "socionext,uniphier-fi2c";
			status = "disabled";
			reg = <0x58781000 0x80>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 42 IRQ_TYPE_LEVEL_HIGH>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_i2c1>;
			clocks = <&peri_clk 5>;
			resets = <&peri_rst 5>;
			clock-frequency = <100000>;
		};

		i2c2: i2c@58782000 {
			compatible = "socionext,uniphier-fi2c";
			status = "disabled";
			reg = <0x58782000 0x80>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 43 IRQ_TYPE_LEVEL_HIGH>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_i2c2>;
			clocks = <&peri_clk 6>;
			resets = <&peri_rst 6>;
			clock-frequency = <100000>;
		};

		i2c3: i2c@58783000 {
			compatible = "socionext,uniphier-fi2c";
			status = "disabled";
			reg = <0x58783000 0x80>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 44 IRQ_TYPE_LEVEL_HIGH>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_i2c3>;
			clocks = <&peri_clk 7>;
			resets = <&peri_rst 7>;
			clock-frequency = <100000>;
		};

		/* chip-internal connection for HDMI */
		i2c6: i2c@58786000 {
			compatible = "socionext,uniphier-fi2c";
			reg = <0x58786000 0x80>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 26 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&peri_clk 10>;
			resets = <&peri_rst 10>;
			clock-frequency = <400000>;
		};

		system_bus: system-bus@58c00000 {
			compatible = "socionext,uniphier-system-bus";
			status = "disabled";
			reg = <0x58c00000 0x400>;
			#address-cells = <2>;
			#size-cells = <1>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_system_bus>;
		};

		smpctrl@59801000 {
			compatible = "socionext,uniphier-smpctrl";
			reg = <0x59801000 0x400>;
		};

		sdctrl: syscon@59810000 {
			compatible = "socionext,uniphier-pxs3-sdctrl",
				     "simple-mfd", "syscon";
			reg = <0x59810000 0x400>;

			sd_clk: clock-controller {
				compatible = "socionext,uniphier-pxs3-sd-clock";
				#clock-cells = <1>;
			};

			sd_rst: reset-controller {
				compatible = "socionext,uniphier-pxs3-sd-reset";
				#reset-cells = <1>;
			};
		};

		syscon@59820000 {
			compatible = "socionext,uniphier-pxs3-perictrl",
				     "simple-mfd", "syscon";
			reg = <0x59820000 0x200>;

			peri_clk: clock-controller {
				compatible = "socionext,uniphier-pxs3-peri-clock";
				#clock-cells = <1>;
			};

			peri_rst: reset-controller {
				compatible = "socionext,uniphier-pxs3-peri-reset";
				#reset-cells = <1>;
			};
		};

		emmc: mmc@5a000000 {
			compatible = "socionext,uniphier-sd4hc", "cdns,sd4hc";
			reg = <0x5a000000 0x400>;
			interrupts = <GIC_SPI 78 IRQ_TYPE_LEVEL_HIGH>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_emmc>;
			clocks = <&sys_clk 4>;
			resets = <&sys_rst 4>;
			bus-width = <8>;
			mmc-ddr-1_8v;
			mmc-hs200-1_8v;
			mmc-pwrseq = <&emmc_pwrseq>;
			cdns,phy-input-delay-legacy = <9>;
			cdns,phy-input-delay-mmc-highspeed = <2>;
			cdns,phy-input-delay-mmc-ddr = <3>;
			cdns,phy-dll-delay-sdclk = <21>;
			cdns,phy-dll-delay-sdclk-hsmmc = <21>;
		};

		sd: mmc@5a400000 {
			compatible = "socionext,uniphier-sd-v3.1.1";
			status = "disabled";
			reg = <0x5a400000 0x800>;
			interrupts = <GIC_SPI 76 IRQ_TYPE_LEVEL_HIGH>;
			pinctrl-names = "default", "uhs";
			pinctrl-0 = <&pinctrl_sd>;
			pinctrl-1 = <&pinctrl_sd_uhs>;
			clocks = <&sd_clk 0>;
			reset-names = "host";
			resets = <&sd_rst 0>;
			bus-width = <4>;
			cap-sd-highspeed;
			sd-uhs-sdr12;
			sd-uhs-sdr25;
			sd-uhs-sdr50;
			socionext,syscon-uhs-mode = <&sdctrl 0>;
		};

		soc_glue: syscon@5f800000 {
			compatible = "socionext,uniphier-pxs3-soc-glue",
				     "simple-mfd", "syscon";
			reg = <0x5f800000 0x2000>;

			pinctrl: pinctrl {
				compatible = "socionext,uniphier-pxs3-pinctrl";
			};
		};

		syscon@5f900000 {
			compatible = "socionext,uniphier-pxs3-soc-glue-debug",
				     "simple-mfd", "syscon";
			reg = <0x5f900000 0x2000>;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0 0x5f900000 0x2000>;

			efuse@100 {
				compatible = "socionext,uniphier-efuse";
				reg = <0x100 0x28>;
			};

			efuse@200 {
				compatible = "socionext,uniphier-efuse";
				reg = <0x200 0x68>;
				#address-cells = <1>;
				#size-cells = <1>;

				/* USB cells */
				usb_rterm0: trim@54,4 {
					reg = <0x54 1>;
					bits = <4 2>;
				};
				usb_rterm1: trim@55,4 {
					reg = <0x55 1>;
					bits = <4 2>;
				};
				usb_rterm2: trim@58,4 {
					reg = <0x58 1>;
					bits = <4 2>;
				};
				usb_rterm3: trim@59,4 {
					reg = <0x59 1>;
					bits = <4 2>;
				};
				usb_sel_t0: trim@54,0 {
					reg = <0x54 1>;
					bits = <0 4>;
				};
				usb_sel_t1: trim@55,0 {
					reg = <0x55 1>;
					bits = <0 4>;
				};
				usb_sel_t2: trim@58,0 {
					reg = <0x58 1>;
					bits = <0 4>;
				};
				usb_sel_t3: trim@59,0 {
					reg = <0x59 1>;
					bits = <0 4>;
				};
				usb_hs_i0: trim@56,0 {
					reg = <0x56 1>;
					bits = <0 4>;
				};
				usb_hs_i2: trim@5a,0 {
					reg = <0x5a 1>;
					bits = <0 4>;
				};
			};
		};

		xdmac: dma-controller@5fc10000 {
			compatible = "socionext,uniphier-xdmac";
			reg = <0x5fc10000 0x5300>;
			interrupts = <GIC_SPI 188 IRQ_TYPE_LEVEL_HIGH>;
			dma-channels = <16>;
			#dma-cells = <2>;
		};

		aidet: interrupt-controller@5fc20000 {
			compatible = "socionext,uniphier-pxs3-aidet";
			reg = <0x5fc20000 0x200>;
			interrupt-controller;
			#interrupt-cells = <2>;
		};

		gic: interrupt-controller@5fe00000 {
			compatible = "arm,gic-v3";
			reg = <0x5fe00000 0x10000>,	/* GICD */
			      <0x5fe80000 0x80000>;	/* GICR */
			interrupt-controller;
			#interrupt-cells = <3>;
			interrupts = <GIC_PPI 9 IRQ_TYPE_LEVEL_HIGH>;
		};

		syscon@61840000 {
			compatible = "socionext,uniphier-pxs3-sysctrl",
				     "simple-mfd", "syscon";
			reg = <0x61840000 0x10000>;

			sys_clk: clock-controller {
				compatible = "socionext,uniphier-pxs3-clock";
				#clock-cells = <1>;
			};

			sys_rst: reset-controller {
				compatible = "socionext,uniphier-pxs3-reset";
				#reset-cells = <1>;
			};

			watchdog {
				compatible = "socionext,uniphier-wdt";
			};

			pvtctl: thermal-sensor {
				compatible = "socionext,uniphier-pxs3-thermal";
				interrupts = <GIC_SPI 3 IRQ_TYPE_LEVEL_HIGH>;
				#thermal-sensor-cells = <0>;
				socionext,tmod-calibration = <0x0f22 0x68ee>;
			};
		};

		eth0: ethernet@65000000 {
			compatible = "socionext,uniphier-pxs3-ave4";
			status = "disabled";
			reg = <0x65000000 0x8500>;
			interrupts = <GIC_SPI 66 IRQ_TYPE_LEVEL_HIGH>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_ether_rgmii>;
			clock-names = "ether";
			clocks = <&sys_clk 6>;
			reset-names = "ether";
			resets = <&sys_rst 6>;
			phy-mode = "rgmii-id";
			local-mac-address = [00 00 00 00 00 00];
			socionext,syscon-phy-mode = <&soc_glue 0>;

			mdio0: mdio {
				#address-cells = <1>;
				#size-cells = <0>;
			};
		};

		eth1: ethernet@65200000 {
			compatible = "socionext,uniphier-pxs3-ave4";
			status = "disabled";
			reg = <0x65200000 0x8500>;
			interrupts = <GIC_SPI 67 IRQ_TYPE_LEVEL_HIGH>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_ether1_rgmii>;
			clock-names = "ether";
			clocks = <&sys_clk 7>;
			reset-names = "ether";
			resets = <&sys_rst 7>;
			phy-mode = "rgmii-id";
			local-mac-address = [00 00 00 00 00 00];
			socionext,syscon-phy-mode = <&soc_glue 1>;

			mdio1: mdio {
				#address-cells = <1>;
				#size-cells = <0>;
			};
		};

		ahci0: sata@65600000 {
			compatible = "socionext,uniphier-pxs3-ahci",
				     "generic-ahci";
			status = "disabled";
			reg = <0x65600000 0x10000>;
			interrupts = <GIC_SPI 142 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&sys_clk 28>;
			resets = <&sys_rst 28>, <&ahci0_rst 0>;
			ports-implemented = <1>;
			phys = <&ahci0_phy>;
		};

		sata-controller@65700000 {
			compatible = "socionext,uniphier-pxs3-ahci-glue",
				     "simple-mfd";
			reg = <0x65700000 0x100>;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0 0x65700000 0x100>;

			ahci0_rst: reset-controller@0 {
				compatible = "socionext,uniphier-pxs3-ahci-reset";
				reg = <0x0 0x4>;
				clock-names = "link";
				clocks = <&sys_clk 28>;
				reset-names = "link";
				resets = <&sys_rst 28>;
				#reset-cells = <1>;
			};

			ahci0_phy: phy@10 {
				compatible = "socionext,uniphier-pxs3-ahci-phy";
				reg = <0x10 0x10>;
				clock-names = "link", "phy";
				clocks = <&sys_clk 28>, <&sys_clk 30>;
				reset-names = "link", "phy";
				resets = <&sys_rst 28>, <&sys_rst 30>;
				#phy-cells = <0>;
			};
		};

		ahci1: sata@65800000 {
			compatible = "socionext,uniphier-pxs3-ahci",
				     "generic-ahci";
			status = "disabled";
			reg = <0x65800000 0x10000>;
			interrupts = <GIC_SPI 143 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&sys_clk 29>;
			resets = <&sys_rst 29>, <&ahci1_rst 0>;
			ports-implemented = <1>;
			phys = <&ahci1_phy>;
		};

		sata-controller@65900000 {
			compatible = "socionext,uniphier-pxs3-ahci-glue",
				     "simple-mfd";
			reg = <0x65900000 0x100>;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0 0x65900000 0x100>;

			ahci1_rst: reset-controller@0 {
				compatible = "socionext,uniphier-pxs3-ahci-reset";
				reg = <0x0 0x4>;
				clock-names = "link";
				clocks = <&sys_clk 29>;
				reset-names = "link";
				resets = <&sys_rst 29>;
				#reset-cells = <1>;
			};

			ahci1_phy: phy@10 {
				compatible = "socionext,uniphier-pxs3-ahci-phy";
				reg = <0x10 0x10>;
				clock-names = "link", "phy";
				clocks = <&sys_clk 29>, <&sys_clk 30>;
				reset-names = "link", "phy";
				resets = <&sys_rst 29>, <&sys_rst 30>;
				#phy-cells = <0>;
			};
		};

		usb0: usb@65a00000 {
			compatible = "socionext,uniphier-dwc3", "snps,dwc3";
			status = "disabled";
			reg = <0x65a00000 0xcd00>;
			interrupt-names = "dwc_usb3";
			interrupts = <GIC_SPI 134 IRQ_TYPE_LEVEL_HIGH>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_usb0>, <&pinctrl_usb2>;
			clock-names = "ref", "bus_early", "suspend";
			clocks = <&sys_clk 12>, <&sys_clk 12>, <&sys_clk 12>;
			resets = <&usb0_rst 15>;
			phys = <&usb0_hsphy0>, <&usb0_hsphy1>,
			       <&usb0_ssphy0>, <&usb0_ssphy1>;
			dr_mode = "host";
		};

		usb-controller@65b00000 {
			compatible = "socionext,uniphier-pxs3-dwc3-glue",
				     "simple-mfd";
			reg = <0x65b00000 0x400>;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0 0x65b00000 0x400>;

			usb0_rst: reset-controller@0 {
				compatible = "socionext,uniphier-pxs3-usb3-reset";
				reg = <0x0 0x4>;
				#reset-cells = <1>;
				clock-names = "link";
				clocks = <&sys_clk 12>;
				reset-names = "link";
				resets = <&sys_rst 12>;
			};

			usb0_vbus0: regulator@100 {
				compatible = "socionext,uniphier-pxs3-usb3-regulator";
				reg = <0x100 0x10>;
				clock-names = "link";
				clocks = <&sys_clk 12>;
				reset-names = "link";
				resets = <&sys_rst 12>;
			};

			usb0_vbus1: regulator@110 {
				compatible = "socionext,uniphier-pxs3-usb3-regulator";
				reg = <0x110 0x10>;
				clock-names = "link";
				clocks = <&sys_clk 12>;
				reset-names = "link";
				resets = <&sys_rst 12>;
			};

			usb0_hsphy0: phy@200 {
				compatible = "socionext,uniphier-pxs3-usb3-hsphy";
				reg = <0x200 0x10>;
				#phy-cells = <0>;
				clock-names = "link", "phy";
				clocks = <&sys_clk 12>, <&sys_clk 16>;
				reset-names = "link", "phy";
				resets = <&sys_rst 12>, <&sys_rst 16>;
				vbus-supply = <&usb0_vbus0>;
				nvmem-cell-names = "rterm", "sel_t", "hs_i";
				nvmem-cells = <&usb_rterm0>, <&usb_sel_t0>,
					      <&usb_hs_i0>;
			};

			usb0_hsphy1: phy@210 {
				compatible = "socionext,uniphier-pxs3-usb3-hsphy";
				reg = <0x210 0x10>;
				#phy-cells = <0>;
				clock-names = "link", "phy";
				clocks = <&sys_clk 12>, <&sys_clk 16>;
				reset-names = "link", "phy";
				resets = <&sys_rst 12>, <&sys_rst 16>;
				vbus-supply = <&usb0_vbus1>;
				nvmem-cell-names = "rterm", "sel_t", "hs_i";
				nvmem-cells = <&usb_rterm1>, <&usb_sel_t1>,
					      <&usb_hs_i0>;
			};

			usb0_ssphy0: phy@300 {
				compatible = "socionext,uniphier-pxs3-usb3-ssphy";
				reg = <0x300 0x10>;
				#phy-cells = <0>;
				clock-names = "link", "phy";
				clocks = <&sys_clk 12>, <&sys_clk 17>;
				reset-names = "link", "phy";
				resets = <&sys_rst 12>, <&sys_rst 17>;
				vbus-supply = <&usb0_vbus0>;
			};

			usb0_ssphy1: phy@310 {
				compatible = "socionext,uniphier-pxs3-usb3-ssphy";
				reg = <0x310 0x10>;
				#phy-cells = <0>;
				clock-names = "link", "phy";
				clocks = <&sys_clk 12>, <&sys_clk 18>;
				reset-names = "link", "phy";
				resets = <&sys_rst 12>, <&sys_rst 18>;
				vbus-supply = <&usb0_vbus1>;
			};
		};

		usb1: usb@65c00000 {
			compatible = "socionext,uniphier-dwc3", "snps,dwc3";
			status = "disabled";
			reg = <0x65c00000 0xcd00>;
			interrupt-names = "dwc_usb3";
			interrupts = <GIC_SPI 137 IRQ_TYPE_LEVEL_HIGH>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_usb1>, <&pinctrl_usb3>;
			clock-names = "ref", "bus_early", "suspend";
			clocks = <&sys_clk 13>, <&sys_clk 13>, <&sys_clk 13>;
			resets = <&usb1_rst 15>;
			phys = <&usb1_hsphy0>, <&usb1_hsphy1>,
			       <&usb1_ssphy0>;
			dr_mode = "host";
		};

		usb-controller@65d00000 {
			compatible = "socionext,uniphier-pxs3-dwc3-glue",
				     "simple-mfd";
			reg = <0x65d00000 0x400>;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0 0x65d00000 0x400>;

			usb1_rst: reset-controller@0 {
				compatible = "socionext,uniphier-pxs3-usb3-reset";
				reg = <0x0 0x4>;
				#reset-cells = <1>;
				clock-names = "link";
				clocks = <&sys_clk 13>;
				reset-names = "link";
				resets = <&sys_rst 13>;
			};

			usb1_vbus0: regulator@100 {
				compatible = "socionext,uniphier-pxs3-usb3-regulator";
				reg = <0x100 0x10>;
				clock-names = "link";
				clocks = <&sys_clk 13>;
				reset-names = "link";
				resets = <&sys_rst 13>;
			};

			usb1_vbus1: regulator@110 {
				compatible = "socionext,uniphier-pxs3-usb3-regulator";
				reg = <0x110 0x10>;
				clock-names = "link";
				clocks = <&sys_clk 13>;
				reset-names = "link";
				resets = <&sys_rst 13>;
			};

			usb1_hsphy0: phy@200 {
				compatible = "socionext,uniphier-pxs3-usb3-hsphy";
				reg = <0x200 0x10>;
				#phy-cells = <0>;
				clock-names = "link", "phy", "phy-ext";
				clocks = <&sys_clk 13>, <&sys_clk 20>,
					 <&sys_clk 14>;
				reset-names = "link", "phy";
				resets = <&sys_rst 13>, <&sys_rst 20>;
				vbus-supply = <&usb1_vbus0>;
				nvmem-cell-names = "rterm", "sel_t", "hs_i";
				nvmem-cells = <&usb_rterm2>, <&usb_sel_t2>,
					      <&usb_hs_i2>;
			};

			usb1_hsphy1: phy@210 {
				compatible = "socionext,uniphier-pxs3-usb3-hsphy";
				reg = <0x210 0x10>;
				#phy-cells = <0>;
				clock-names = "link", "phy", "phy-ext";
				clocks = <&sys_clk 13>, <&sys_clk 20>,
					 <&sys_clk 14>;
				reset-names = "link", "phy";
				resets = <&sys_rst 13>, <&sys_rst 20>;
				vbus-supply = <&usb1_vbus1>;
				nvmem-cell-names = "rterm", "sel_t", "hs_i";
				nvmem-cells = <&usb_rterm3>, <&usb_sel_t3>,
					      <&usb_hs_i2>;
			};

			usb1_ssphy0: phy@300 {
				compatible = "socionext,uniphier-pxs3-usb3-ssphy";
				reg = <0x300 0x10>;
				#phy-cells = <0>;
				clock-names = "link", "phy", "phy-ext";
				clocks = <&sys_clk 13>, <&sys_clk 21>,
					 <&sys_clk 14>;
				reset-names = "link", "phy";
				resets = <&sys_rst 13>, <&sys_rst 21>;
				vbus-supply = <&usb1_vbus0>;
			};
		};

		pcie: pcie@66000000 {
			compatible = "socionext,uniphier-pcie";
			status = "disabled";
			reg-names = "dbi", "link", "config";
			reg = <0x66000000 0x1000>, <0x66010000 0x10000>,
			      <0x2fff0000 0x10000>;
			#address-cells = <3>;
			#size-cells = <2>;
			clocks = <&sys_clk 24>;
			resets = <&sys_rst 24>;
			num-lanes = <1>;
			num-viewport = <1>;
			bus-range = <0x0 0xff>;
			device_type = "pci";
			ranges =
			/* downstream I/O */
				<0x81000000 0 0x00000000 0x2ffe0000 0 0x00010000>,
			/* non-prefetchable memory */
				<0x82000000 0 0x20000000 0x20000000 0 0x0ffe0000>;
			#interrupt-cells = <1>;
			interrupt-names = "dma", "msi";
			interrupts = <GIC_SPI 224 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 225 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-map-mask = <0 0 0 7>;
			interrupt-map = <0 0 0 1 &pcie_intc 0>,	/* INTA */
					<0 0 0 2 &pcie_intc 1>,	/* INTB */
					<0 0 0 3 &pcie_intc 2>,	/* INTC */
					<0 0 0 4 &pcie_intc 3>;	/* INTD */
			phy-names = "pcie-phy";
			phys = <&pcie_phy>;

			pcie_intc: legacy-interrupt-controller {
				interrupt-controller;
				#interrupt-cells = <1>;
				interrupt-parent = <&gic>;
				interrupts = <GIC_SPI 226 IRQ_TYPE_LEVEL_HIGH>;
			};
		};

		pcie_phy: phy@66038000 {
			compatible = "socionext,uniphier-pxs3-pcie-phy";
			reg = <0x66038000 0x4000>;
			#phy-cells = <0>;
			clock-names = "link";
			clocks = <&sys_clk 24>;
			reset-names = "link";
			resets = <&sys_rst 24>;
			socionext,syscon = <&soc_glue>;
		};

		nand: nand-controller@68000000 {
			compatible = "socionext,uniphier-denali-nand-v5b";
			status = "disabled";
			reg-names = "nand_data", "denali_reg";
			reg = <0x68000000 0x20>, <0x68100000 0x1000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 65 IRQ_TYPE_LEVEL_HIGH>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_nand>;
			clock-names = "nand", "nand_x", "ecc";
			clocks = <&sys_clk 2>, <&sys_clk 3>, <&sys_clk 3>;
			reset-names = "nand", "reg";
			resets = <&sys_rst 2>, <&sys_rst 2>;
		};
	};
};

#include "uniphier-pinctrl.dtsi"
