// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
// Copyright (C) 2017 Jagan Teki <jteki@openedev.com>

/dts-v1/;

#include "sun50i-a64.dtsi"
#include "sun50i-a64-cpu-opp.dtsi"

#include <dt-bindings/gpio/gpio.h>

/ {
	model = "FriendlyARM NanoPi A64";
	compatible = "friendlyarm,nanopi-a64", "allwinner,sun50i-a64";

	aliases {
		ethernet0 = &emac;
		serial0 = &uart0;
	};

	chosen {
		stdout-path = "serial0:115200n8";
	};

	hdmi-connector {
		compatible = "hdmi-connector";
		type = "a";

		port {
			hdmi_con_in: endpoint {
				remote-endpoint = <&hdmi_out_con>;
			};
		};
	};

	leds {
		compatible = "gpio-leds";

		led {
			label = "nanopi-a64:blue:status";
			gpios = <&pio 3 24 GPIO_ACTIVE_LOW>; /* PD24 */
		};
	};

	wifi_pwrseq: pwrseq {
		compatible = "mmc-pwrseq-simple";
		clocks = <&rtc CLK_OSC32K_FANOUT>;
		clock-names = "ext_clock";
		reset-gpios = <&r_pio 0 2 GPIO_ACTIVE_LOW>; /* PL2 */
	};
};

&cpu0 {
	cpu-supply = <&reg_dcdc2>;
};

&cpu1 {
	cpu-supply = <&reg_dcdc2>;
};

&cpu2 {
	cpu-supply = <&reg_dcdc2>;
};

&cpu3 {
	cpu-supply = <&reg_dcdc2>;
};

&de {
	status = "okay";
};

&ehci0 {
	status = "okay";
};

&ehci1 {
	status = "okay";
};

&emac {
	pinctrl-names = "default";
	pinctrl-0 = <&rgmii_pins>;
	phy-mode = "rgmii";
	phy-handle = <&ext_rgmii_phy>;
	phy-supply = <&reg_dcdc1>;
	status = "okay";
};

&hdmi {
	hvcc-supply = <&reg_dldo1>;
	status = "okay";
};

&hdmi_out {
	hdmi_out_con: endpoint {
		remote-endpoint = <&hdmi_con_in>;
	};
};

/* i2c1 connected with gpio headers like pine64, bananapi */
&i2c1_pins {
	bias-pull-up;
};

&mdio {
	ext_rgmii_phy: ethernet-phy@1 {
		compatible = "ethernet-phy-ieee802.3-c22";
		reg = <7>;
	};
};

&mmc0 {
	pinctrl-names = "default";
	pinctrl-0 = <&mmc0_pins>;
	vmmc-supply = <&reg_dcdc1>;
	cd-gpios = <&pio 5 6 GPIO_ACTIVE_LOW>;
	disable-wp;
	bus-width = <4>;
	status = "okay";
};

&mmc1 {
	pinctrl-names = "default";
	pinctrl-0 = <&mmc1_pins>;
	vmmc-supply = <&reg_dcdc1>;
	vqmmc-supply = <&reg_dldo4>;
	mmc-pwrseq = <&wifi_pwrseq>;
	bus-width = <4>;
	non-removable;
	status = "okay";

	rtl8189etv: wifi@1 {
		reg = <1>;
		interrupt-parent = <&r_pio>;
		interrupts = <0 3 IRQ_TYPE_LEVEL_LOW>; /* PL3 */
		interrupt-names = "host-wake";
	};
};

&ohci0 {
	status = "okay";
};

&ohci1 {
	status = "okay";
};

&r_rsb {
	status = "okay";

	axp803: pmic@3a3 {
		compatible = "x-powers,axp803";
		reg = <0x3a3>;
		interrupt-parent = <&r_intc>;
		interrupts = <0 IRQ_TYPE_LEVEL_LOW>;
	};
};

#include "axp803.dtsi"

&ac_power_supply {
	status = "okay";
};

&reg_aldo2 {
	regulator-always-on;
	regulator-min-microvolt = <1800000>;
	regulator-max-microvolt = <3300000>;
	regulator-name = "vcc-pl";
};

&reg_aldo3 {
	regulator-always-on;
	regulator-min-microvolt = <3000000>;
	regulator-max-microvolt = <3000000>;
	regulator-name = "vcc-pll-avcc";
};

&reg_dcdc1 {
	regulator-always-on;
	regulator-min-microvolt = <3300000>;
	regulator-max-microvolt = <3300000>;
	regulator-name = "vcc-3v3";
};

&reg_dcdc2 {
	regulator-always-on;
	regulator-min-microvolt = <1040000>;
	regulator-max-microvolt = <1300000>;
	regulator-name = "vdd-cpux";
};

/* DCDC3 is polyphased with DCDC2 */

&reg_dcdc5 {
	regulator-always-on;
	regulator-min-microvolt = <1500000>;
	regulator-max-microvolt = <1500000>;
	regulator-name = "vcc-dram";
};

&reg_dcdc6 {
	regulator-always-on;
	regulator-min-microvolt = <1100000>;
	regulator-max-microvolt = <1100000>;
	regulator-name = "vdd-sys";
};

&reg_dldo1 {
	regulator-always-on;
	regulator-min-microvolt = <3300000>;
	regulator-max-microvolt = <3300000>;
	regulator-name = "vcc-hdmi-dsi";
};

&reg_dldo4 {
	regulator-always-on;
	regulator-min-microvolt = <3000000>;
	regulator-max-microvolt = <3000000>;
	regulator-name = "vcc-pg-wifi-io";
};

&reg_eldo1 {
	regulator-min-microvolt = <1800000>;
	regulator-max-microvolt = <1800000>;
	regulator-name = "cpvdd";
};

&reg_fldo1 {
	regulator-min-microvolt = <1200000>;
	regulator-max-microvolt = <1200000>;
	regulator-name = "vcc-1v2-hsic";
};

/*
 * The A64 chip cannot work without this regulator off, although
 * it seems to be only driving the AR100 core.
 * Maybe we don't still know well about CPUs domain.
 */
&reg_fldo2 {
	regulator-always-on;
	regulator-min-microvolt = <1100000>;
	regulator-max-microvolt = <1100000>;
	regulator-name = "vdd-cpus";
};

&reg_rtc_ldo {
	regulator-name = "vcc-rtc";
};

&simplefb_hdmi {
	vcc-hdmi-supply = <&reg_dldo1>;
};

&uart0 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart0_pb_pins>;
	status = "okay";
};

&usbphy {
	status = "okay";
};
