// SPDX-License-Identifier: GPL-2.0+
#include <dt-bindings/interrupt-controller/arm-gic.h>
#include "skeleton.dtsi"

/ {
	model = "Aspeed BMC";
	compatible = "aspeed,ast2600";
	#address-cells = <1>;
	#size-cells = <1>;
	interrupt-parent = <&gic>;

	aliases {
		i2c0 = &i2c0;
		i2c1 = &i2c1;
		i2c2 = &i2c2;
		i2c3 = &i2c3;
		i2c4 = &i2c4;
		i2c5 = &i2c5;
		i2c6 = &i2c6;
		i2c7 = &i2c7;
		i2c8 = &i2c8;
		i2c9 = &i2c9;
		i2c10 = &i2c10;
		i2c11 = &i2c11;
		i2c12 = &i2c12;
		i2c13 = &i2c13;
		i2c14 = &i2c14;
		i2c15 = &i2c15;
		serial0 = &uart1;
		serial1 = &uart2;
		serial2 = &uart3;
		serial3 = &uart4;
		serial4 = &uart5;
		serial5 = &uart6;
		serial6 = &uart7;
		serial7 = &uart8;
		serial8 = &uart9;
		serial9 = &uart10;
		serial10 = &uart11;
		serial11 = &uart12;
		serial12 = &uart13;
	};

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;
		enable-method = "aspeed,ast2600-smp";

		cpu@0 {
			compatible = "arm,cortex-a7";
			device_type = "cpu";
			reg = <0xf00>;
		};

		cpu@1 {
			compatible = "arm,cortex-a7";
			device_type = "cpu";
			reg = <0xf01>;
		};

	};

	timer {
		compatible = "arm,armv7-timer";
		interrupt-parent = <&gic>;
		interrupts = <GIC_PPI 13 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_LOW)>,
				<GIC_PPI 14 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_LOW)>,
				<GIC_PPI 11 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_LOW)>,
				<GIC_PPI 10 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_LOW)>;
	};

	reserved-memory {
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;

		gfx_memory: framebuffer {
			size = <0x01000000>;
			alignment = <0x01000000>;
			compatible = "shared-dma-pool";
			reusable;
		};

		video_memory: video {
			size = <0x04000000>;
			alignment = <0x01000000>;
			compatible = "shared-dma-pool";
			no-map;
		};
	};

	ahb {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		device_type = "soc";
		ranges;

		gic: interrupt-controller@40461000 {
				compatible = "arm,cortex-a7-gic";
				interrupts = <GIC_PPI 9 (GIC_CPU_MASK_SIMPLE(2) | IRQ_TYPE_LEVEL_HIGH)>;
				#interrupt-cells = <3>;
				interrupt-controller;
				interrupt-parent = <&gic>;
				reg = <0x40461000 0x1000>,
					  <0x40462000 0x1000>,
					  <0x40464000 0x2000>,
					  <0x40466000 0x2000>;
		};

		ahbc: ahbc@1e600000 {
			compatible = "aspeed,aspeed-ahbc";
			reg = < 0x1e600000 0x100>;
		};

		pwm_tach: pwm_tach@1e610000 {
			compatible = "aspeed,ast2600-pwm-tach", "simple-mfd", "syscon";
			reg = <0x1e610000 0x100>;
			clocks = <&scu ASPEED_CLK_AHB>;
			resets = <&rst ASPEED_RESET_PWM>;

			pwm: pwm {
				compatible = "aspeed,ast2600-pwm";
				#pwm-cells = <3>;
				#address-cells = <1>;
				#size-cells = <0>;
				status = "disabled";
			};
		};

		fmc: flash-controller@1e620000 {
			reg = <0x1e620000 0xc4>, <0x20000000 0x10000000>;
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "aspeed,ast2600-fmc";
			status = "disabled";
			clocks = <&scu ASPEED_CLK_AHB>;
			num-cs = <3>;

			flash@0 {
				reg = <0>;
				compatible = "jedec,spi-nor";
				status = "disabled";
			};

			flash@1 {
				reg = <1>;
				compatible = "jedec,spi-nor";
				status = "disabled";
			};

			flash@2 {
				reg = <2>;
				compatible = "jedec,spi-nor";
				status = "disabled";
			};
		};

		spi1: flash-controller@1e630000 {
			reg = <0x1e630000 0xc4>, <0x30000000 0x10000000>;
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "aspeed,ast2600-spi";
			clocks = <&scu ASPEED_CLK_AHB>;
			num-cs = <2>;
			status = "disabled";

			flash@0 {
				reg = <0>;
				compatible = "jedec,spi-nor";
				status = "disabled";
			};

			flash@1 {
				reg = <1>;
				compatible = "jedec,spi-nor";
				status = "disabled";
			};
		};

		spi2: flash-controller@1e631000 {
			reg = <0x1e631000 0xc4>, <0x50000000 0x10000000>;
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "aspeed,ast2600-spi";
			clocks = <&scu ASPEED_CLK_AHB>;
			num-cs = <3>;
			status = "disabled";

			flash@0 {
				reg = <0>;
				compatible = "jedec,spi-nor";
				status = "disabled";
			};

			flash@1 {
				reg = <1>;
				compatible = "jedec,spi-nor";
				status = "disabled";
			};

			flash@2 {
				reg = <2>;
				compatible = "jedec,spi-nor";
				status = "disabled";
			};
		};

		hace: hace@1e6d0000 {
			compatible = "aspeed,ast2600-hace";
			reg = <0x1e6d0000 0x200>;
			interrupts = <GIC_SPI 4 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&scu ASPEED_CLK_GATE_YCLK>;
			status = "disabled";
		};

		acry: acry@1e6fa000 {
			compatible = "aspeed,ast2600-acry";
			reg = <0x1e6fa000 0x1000>,
			      <0x1e710000 0x10000>;
			interrupts = <GIC_SPI 160 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&scu ASPEED_CLK_GATE_RSACLK>;
			status = "disabled";
		};

		edac: sdram@1e6e0000 {
			compatible = "aspeed,ast2600-sdram-edac";
			reg = <0x1e6e0000 0x174>;
			interrupts = <GIC_SPI 0 IRQ_TYPE_LEVEL_HIGH>;
		};

		mdio: bus@1e650000 {
			compatible = "simple-bus";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0 0x1e650000 0x100>;

			mdio0: mdio@0 {
				compatible = "aspeed,ast2600-mdio";
				reg = <0 0x8>;
				resets = <&rst ASPEED_RESET_MII>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_mdio1_default>;
				status = "disabled";
			};

			mdio1: mdio@8 {
				compatible = "aspeed,ast2600-mdio";
				reg = <0x8 0x8>;
				resets = <&rst ASPEED_RESET_MII>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_mdio2_default>;
				status = "disabled";
			};

			mdio2: mdio@10 {
				compatible = "aspeed,ast2600-mdio";
				reg = <0x10 0x8>;
				resets = <&rst ASPEED_RESET_MII>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_mdio3_default>;
				status = "disabled";
			};

			mdio3: mdio@18 {
				compatible = "aspeed,ast2600-mdio";
				reg = <0x18 0x8>;
				resets = <&rst ASPEED_RESET_MII>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_mdio4_default>;
				status = "disabled";
			};
		};

		mac0: ftgmac@1e660000 {
			compatible = "aspeed,ast2600-mac", "faraday,ftgmac100";
			reg = <0x1e660000 0x180>, <0x1e650000 0x4>;
			interrupts = <GIC_SPI 2 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&scu ASPEED_CLK_GATE_MAC1CLK>;
			status = "disabled";
		};

		mac1: ftgmac@1e680000 {
			compatible = "aspeed,ast2600-mac", "faraday,ftgmac100";
			reg = <0x1e680000 0x180>, <0x1e650008 0x4>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 3 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&scu ASPEED_CLK_GATE_MAC2CLK>;
			status = "disabled";
		};

		mac2: ftgmac@1e670000 {
			compatible = "aspeed,ast2600-mac", "faraday,ftgmac100";
			reg = <0x1e670000 0x180>, <0x1e650010 0x4>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 32 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&scu ASPEED_CLK_GATE_MAC3CLK>;
			status = "disabled";
		};

		mac3: ftgmac@1e690000 {
			compatible = "aspeed,ast2600-mac", "faraday,ftgmac100";
			reg = <0x1e690000 0x180>, <0x1e650018 0x4>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 33 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&scu ASPEED_CLK_GATE_MAC4CLK>;
			status = "disabled";
		};

		ehci0: usb@1e6a1000 {
			compatible = "aspeed,aspeed-ehci", "usb-ehci";
			reg = <0x1e6a1000 0x100>;
			interrupts = <GIC_SPI 5 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&scu ASPEED_CLK_GATE_USBPORT1CLK>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_usb2ah_default>;
			status = "disabled";
		};

		ehci1: usb@1e6a3000 {
			compatible = "aspeed,aspeed-ehci", "usb-ehci";
			reg = <0x1e6a3000 0x100>;
			interrupts = <GIC_SPI 9 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&scu ASPEED_CLK_GATE_USBPORT2CLK>;
			pinctrl-names = "default";
			pinctrl-0 = <&pinctrl_usb2bh_default>;
			status = "disabled";
		};

		apb {
			compatible = "simple-bus";
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;

			syscon: syscon@1e6e2000 {
				compatible = "aspeed,g6-scu", "syscon", "simple-mfd";
				reg = <0x1e6e2000 0x1000>;
				#address-cells = <1>;
				#size-cells = <1>;
				#clock-cells = <1>;
				#reset-cells = <1>;
				ranges = <0 0x1e6e2000 0x1000>;

				pinctrl: pinctrl {
					compatible = "aspeed,g6-pinctrl";
					aspeed,external-nodes = <&gfx &lhc>;

				};

				vga_scratch: scratch {
					compatible = "aspeed,bmc-misc";
				};

				scu_ic0: interrupt-controller@0 {
					#interrupt-cells = <1>;
					compatible = "aspeed,ast2600-scu-ic";
					reg = <0x560 0x10>;
					interrupt-parent = <&gic>;
					interrupts = <GIC_SPI 12 IRQ_TYPE_LEVEL_HIGH>;
					interrupt-controller;
				};

				scu_ic1: interrupt-controller@1 {
					#interrupt-cells = <1>;
					compatible = "aspeed,ast2600-scu-ic";
					reg = <0x570 0x10>;
					interrupt-parent = <&gic>;
					interrupts = <GIC_SPI 41 IRQ_TYPE_LEVEL_HIGH>;
					interrupt-controller;
				};

			};

			smp-memram@0 {
				compatible = "aspeed,ast2600-smpmem", "syscon";
				reg = <0x1e6e2180 0x40>;
			};

			gfx: display@1e6e6000 {
				compatible = "aspeed,ast2500-gfx", "syscon";
				reg = <0x1e6e6000 0x1000>;
				reg-io-width = <4>;
			};

			pcie_bridge0: pcie@1e6ed000 {
				compatible = "aspeed,ast2600-pcie";
				#address-cells = <3>;
				#size-cells = <2>;
				reg = <0x1e6ed000 0x100>;
				ranges = <0x81000000 0x0 0x0 0x0 0x0 0x10000>,
					 <0x82000000 0x0 0x60000000 0x60000000 0x0 0x10000000>;
				device_type = "pci";
				bus-range = <0x00 0xff>;
				resets = <&rst ASPEED_RESET_PCIE_DEV_O>;
				cfg-handle = <&pcie_cfg0>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_pcie0rc_default>;

				status = "disabled";
			};

			pcie_bridge1: pcie@1e6ed200 {
				compatible = "aspeed,ast2600-pcie";
				#address-cells = <3>;
				#size-cells = <2>;
				reg = <0x1e6ed200 0x100>;
				ranges = <0x81000000 0x0 0x0 0x10000 0x00 0x10000>,
					 <0x82000000 0x0 0x70000000 0x70000000 0x0 0x10000000>;
				device_type = "pci";
				bus-range = <0x00 0xff>;
				resets = <&rst ASPEED_RESET_PCIE_RC_O>;
				cfg-handle = <&pcie_cfg1>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_pcie1rc_default>;

				status = "disabled";
			};

			sdc: sdc@1e740000 {
				compatible = "aspeed,ast2600-sd-controller";
				reg = <0x1e740000 0x100>;
				#address-cells = <1>;
				#size-cells = <1>;
				ranges = <0 0x1e740000 0x10000>;
				clocks = <&scu ASPEED_CLK_GATE_SDCLK>;
				status = "disabled";

				sdhci0: sdhci@1e740100 {
					compatible = "aspeed,ast2600-sdhci", "sdhci";
					reg = <0x100 0x100>;
					interrupts = <GIC_SPI 43 IRQ_TYPE_LEVEL_HIGH>;
					sdhci,auto-cmd12;
					clocks = <&scu ASPEED_CLK_SDIO>;
					status = "disabled";
				};

				sdhci1: sdhci@1e740200 {
					compatible = "aspeed,ast2600-sdhci", "sdhci";
					reg = <0x200 0x100>;
					interrupts = <GIC_SPI 43 IRQ_TYPE_LEVEL_HIGH>;
					sdhci,auto-cmd12;
					clocks = <&scu ASPEED_CLK_SDIO>;
					status = "disabled";
				};
			};

			emmc_controller: sdc@1e750000 {
				compatible = "aspeed,ast2600-sd-controller";
				reg = <0x1e750000 0x100>;
				#address-cells = <1>;
				#size-cells = <1>;
				ranges = <0 0x1e750000 0x10000>;
				clocks = <&scu ASPEED_CLK_GATE_EMMCCLK>;
				status = "disabled";

				emmc: sdhci@1e750100 {
					compatible = "aspeed,ast2600-sdhci";
					reg = <0x100 0x100>;
					sdhci,auto-cmd12;
					interrupts = <GIC_SPI 15 IRQ_TYPE_LEVEL_HIGH>;
					clocks = <&scu ASPEED_CLK_EMMC>;
					pinctrl-names = "default";
					pinctrl-0 = <&pinctrl_emmc_default>;
				};
			};

			h2x: h2x@1e770000 {
				compatible = "aspeed,ast2600-h2x";
				reg = <0x1e770000 0x100>;
				interrupts = <GIC_SPI 29 IRQ_TYPE_LEVEL_HIGH>;
				resets = <&rst ASPEED_RESET_H2X>;
				#address-cells = <1>;
				#size-cells = <1>;
				ranges = <0x0 0x1e770000 0x100>;

				status = "disabled";

				pcie_cfg0: cfg0@80 {
					reg = <0x80 0x80>;
					compatible = "aspeed,ast2600-pcie-cfg";
				};

				pcie_cfg1: cfg1@C0 {
					compatible = "aspeed,ast2600-pcie-cfg";
					reg = <0xC0 0x80>;
				};
			};

			gpio0: gpio@1e780000 {
				compatible = "aspeed,ast2600-gpio";
				reg = <0x1e780000 0x1000>;
				interrupts = <GIC_SPI 40 IRQ_TYPE_LEVEL_HIGH>;
				#gpio-cells = <2>;
				gpio-controller;
				interrupt-controller;
				gpio-ranges = <&pinctrl 0 0 220>;
				ngpios = <208>;
			};

			sgpiom0: sgpiom@1e780500 {
				compatible = "aspeed,ast2600-sgpiom";
				reg = <0x1e780500 0x100>;
				interrupts = <GIC_SPI 51 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&scu ASPEED_CLK_APB2>;
				#gpio-cells = <2>;
				gpio-controller;
				#interrupt-cells = <2>;
				interrupt-controller;
				bus-frequency = <1000000>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_sgpm1_default>;
				status = "disabled";
			};

			sgpiom1: sgpiom@1e780600 {
				compatible = "aspeed,ast2600-sgpiom";
				reg = <0x1e780600 0x100>;
				interrupts = <GIC_SPI 70 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&scu ASPEED_CLK_APB2>;
				#gpio-cells = <2>;
				gpio-controller;
				#interrupt-cells = <2>;
				interrupt-controller;
				bus-frequency = <12000000>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_sgpm2_default>;
				status = "disabled";
			};

			gpio1: gpio@1e780800 {
				compatible = "aspeed,ast2600-gpio";
				reg = <0x1e780800 0x800>;
				interrupts = <GIC_SPI 11 IRQ_TYPE_LEVEL_HIGH>;
				#gpio-cells = <2>;
				gpio-controller;
				interrupt-controller;
				gpio-ranges = <&pinctrl 0 0 208>;
				ngpios = <36>;
			};

			uart1: serial@1e783000 {
				compatible = "ns16550a";
				reg = <0x1e783000 0x20>;
				reg-shift = <2>;
				interrupts = <GIC_SPI 47 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&scu ASPEED_CLK_GATE_UART1CLK>;
				clock-frequency = <1846154>;
				no-loopback-test;
				status = "disabled";
			};

			uart5: serial@1e784000 {
				compatible = "ns16550a";
				reg = <0x1e784000 0x1000>;
				reg-shift = <2>;
				interrupts = <GIC_SPI 36 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&scu ASPEED_CLK_GATE_UART5CLK>;
				clock-frequency = <1846154>;
				no-loopback-test;
				status = "disabled";
			};

			wdt1: watchdog@1e785000 {
				compatible = "aspeed,ast2600-wdt";
				reg = <0x1e785000 0x40>;
				status = "disabled";
			};

			wdt2: watchdog@1e785040 {
				compatible = "aspeed,ast2600-wdt";
				reg = <0x1e785040 0x40>;
				status = "disabled";
			};

			wdt3: watchdog@1e785080 {
				compatible = "aspeed,ast2600-wdt";
				reg = <0x1e785080 0x40>;
				status = "disabled";
			};

			wdt4: watchdog@1e7850C0 {
				compatible = "aspeed,ast2600-wdt";
				reg = <0x1e7850C0 0x40>;
				status = "disabled";
			};

			lpc: lpc@1e789000 {
				compatible = "aspeed,ast2600-lpc", "simple-mfd", "syscon";
				reg = <0x1e789000 0x1000>;

				#address-cells = <1>;
				#size-cells = <1>;
				ranges = <0x0 0x1e789000 0x1000>;

				kcs1: kcs1@0 {
					compatible = "aspeed,ast2600-kcs-bmc";
					reg = <0x0 0x80>;
					interrupts = <GIC_SPI 138 IRQ_TYPE_LEVEL_HIGH>;
					kcs_chan = <1>;
					kcs_addr = <0xCA0>;
					status = "disabled";
				};

				kcs2: kcs2@0 {
					compatible = "aspeed,ast2600-kcs-bmc";
					reg = <0x0 0x80>;
					interrupts = <GIC_SPI 139 IRQ_TYPE_LEVEL_HIGH>;
					kcs_chan = <2>;
					kcs_addr = <0xCA8>;
					status = "disabled";
				};

				kcs3: kcs3@0 {
					compatible = "aspeed,ast2600-kcs-bmc";
					reg = <0x0 0x80>;
					interrupts = <GIC_SPI 140 IRQ_TYPE_LEVEL_HIGH>;
					kcs_chan = <3>;
					kcs_addr = <0xCA2>;
				};

				kcs4: kcs4@0 {
					compatible = "aspeed,ast2600-kcs-bmc";
					reg = <0x0 0x120>;
					interrupts = <GIC_SPI 141 IRQ_TYPE_LEVEL_HIGH>;
					kcs_chan = <4>;
					kcs_addr = <0xCA4>;
					status = "disabled";
				};

				lpc_ctrl: lpc-ctrl@80 {
					compatible = "aspeed,ast2600-lpc-ctrl";
					reg = <0x80 0x80>;
					status = "disabled";
				};

				lpc_snoop: lpc-snoop@80 {
					compatible = "aspeed,ast2600-lpc-snoop";
					reg = <0x80 0x80>;
					interrupts = <GIC_SPI 144 IRQ_TYPE_LEVEL_HIGH>;
					status = "disabled";
				};

				lhc: lhc@a0 {
					compatible = "aspeed,ast2600-lhc";
					reg = <0xa0 0x24 0xc8 0x8>;
				};

				lpc_reset: reset-controller@98 {
					compatible = "aspeed,ast2600-lpc-reset";
					reg = <0x98 0x4>;
					#reset-cells = <1>;
					status = "disabled";
				};

				ibt: ibt@140 {
					compatible = "aspeed,ast2600-ibt-bmc";
					reg = <0x140 0x18>;
					interrupts = <GIC_SPI 143 IRQ_TYPE_LEVEL_HIGH>;
					status = "disabled";
				};

				sio_regs: regs {
					compatible = "aspeed,bmc-misc";
				};

				mbox: mbox@200 {
					compatible = "aspeed,ast2600-mbox";
					reg = <0x200 0x5c>;
					interrupts = <GIC_SPI 54 IRQ_TYPE_LEVEL_HIGH>;
					#mbox-cells = <1>;
					status = "disabled";
				};
			};

			uart2: serial@1e78d000 {
				compatible = "ns16550a";
				reg = <0x1e78d000 0x20>;
				reg-shift = <2>;
				interrupts = <GIC_SPI 48 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&scu ASPEED_CLK_GATE_UART2CLK>;
				clock-frequency = <1846154>;
				no-loopback-test;
				status = "disabled";
			};

			uart3: serial@1e78e000 {
				compatible = "ns16550a";
				reg = <0x1e78e000 0x20>;
				reg-shift = <2>;
				interrupts = <GIC_SPI 49 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&scu ASPEED_CLK_GATE_UART3CLK>;
				clock-frequency = <1846154>;
				no-loopback-test;
				status = "disabled";
			};

			uart4: serial@1e78f000 {
				compatible = "ns16550a";
				reg = <0x1e78f000 0x20>;
				reg-shift = <2>;
				interrupts = <GIC_SPI 50 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&scu ASPEED_CLK_GATE_UART4CLK>;
				clock-frequency = <1846154>;
				no-loopback-test;
				status = "disabled";
			};

			i2c: bus@1e78a000 {
				compatible = "simple-bus";
				reg = <0x1e78a000 0x1000>;
				#address-cells = <1>;
				#size-cells = <1>;
				ranges = <0 0x1e78a000 0x1000>;
			};

			fsim0: fsi@1e79b000 {
				compatible = "aspeed,ast2600-fsi-master", "fsi-master";
				reg = <0x1e79b000 0x94>;
				interrupts = <GIC_SPI 100 IRQ_TYPE_LEVEL_HIGH>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_fsi1_default>;
				clocks = <&scu ASPEED_CLK_GATE_FSICLK>;
				status = "disabled";
			};

			fsim1: fsi@1e79b100 {
				compatible = "aspeed,ast2600-fsi-master", "fsi-master";
				reg = <0x1e79b100 0x94>;
				interrupts = <GIC_SPI 101 IRQ_TYPE_LEVEL_HIGH>;
				pinctrl-names = "default";
				pinctrl-0 = <&pinctrl_fsi2_default>;
				clocks = <&scu ASPEED_CLK_GATE_FSICLK>;
				status = "disabled";
			};

			uart6: serial@1e790000 {
				compatible = "ns16550a";
				reg = <0x1e790000 0x20>;
				reg-shift = <2>;
				interrupts = <GIC_SPI 57 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&scu ASPEED_CLK_GATE_UART6CLK>;
				clock-frequency = <1846154>;
				no-loopback-test;
				status = "disabled";
			};

			uart7: serial@1e790100 {
				compatible = "ns16550a";
				reg = <0x1e790100 0x20>;
				reg-shift = <2>;
				interrupts = <GIC_SPI 58 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&scu ASPEED_CLK_GATE_UART7CLK>;
				clock-frequency = <1846154>;
				no-loopback-test;
				status = "disabled";
			};

			uart8: serial@1e790200 {
				compatible = "ns16550a";
				reg = <0x1e790200 0x20>;
				reg-shift = <2>;
				interrupts = <GIC_SPI 59 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&scu ASPEED_CLK_GATE_UART8CLK>;
				clock-frequency = <1846154>;
				no-loopback-test;
				status = "disabled";
			};

			uart9: serial@1e790300 {
				compatible = "ns16550a";
				reg = <0x1e790300 0x20>;
				reg-shift = <2>;
				interrupts = <GIC_SPI 60 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&scu ASPEED_CLK_GATE_UART9CLK>;
				clock-frequency = <1846154>;
				no-loopback-test;
				status = "disabled";
			};

			uart10: serial@1e790400 {
				compatible = "ns16550a";
				reg = <0x1e790400 0x20>;
				reg-shift = <2>;
				interrupts = <GIC_SPI 61 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&scu ASPEED_CLK_GATE_UART10CLK>;
				clock-frequency = <1846154>;
				no-loopback-test;
				status = "disabled";
			};

			uart11: serial@1e790500 {
				compatible = "ns16550a";
				reg = <0x1e790500 0x20>;
				reg-shift = <2>;
				interrupts = <GIC_SPI 62 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&scu ASPEED_CLK_GATE_UART11CLK>;
				clock-frequency = <1846154>;
				no-loopback-test;
				status = "disabled";
			};

			uart12: serial@1e790600 {
				compatible = "ns16550a";
				reg = <0x1e790600 0x20>;
				reg-shift = <2>;
				interrupts = <GIC_SPI 63 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&scu ASPEED_CLK_GATE_UART12CLK>;
				clock-frequency = <1846154>;
				no-loopback-test;
				status = "disabled";
			};

			uart13: serial@1e790700 {
				compatible = "ns16550a";
				reg = <0x1e790700 0x20>;
				reg-shift = <2>;
				interrupts = <GIC_SPI 64 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&scu ASPEED_CLK_GATE_UART13CLK>;
				clock-frequency = <1846154>;
				no-loopback-test;
				status = "disabled";
			};

			display_port: dp@1e6eb000 {
				compatible = "aspeed,ast2600-displayport";
				reg = <0x1e6eb000 0x200>;
				interrupts = <GIC_SPI 30 IRQ_TYPE_LEVEL_HIGH>;
				resets = <&rst ASPEED_RESET_DP> ,<&rst ASPEED_RESET_DP_MCU>;
				status = "disabled";
			};

		};

	};

};

&i2c {
	i2cglobal: i2cg@00 {
		compatible = "aspeed,ast2600-i2c-global";
		reg = <0x0 0x40>;
		resets = <&rst ASPEED_RESET_I2C>;
#if 0
		new-mode;
#endif
	};

	i2c0: i2c@80 {
		#address-cells = <1>;
		#size-cells = <0>;
		#interrupt-cells = <1>;

		reg = <0x80 0x80 0xC00 0x20>;
		compatible = "aspeed,ast2600-i2c-bus";
		bus-frequency = <100000>;
		interrupts = <GIC_SPI 110 IRQ_TYPE_LEVEL_HIGH>;
		resets = <&rst ASPEED_RESET_I2C>;
		clocks = <&scu ASPEED_CLK_APB2>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_i2c1_default>;
		status = "disabled";
	};

	i2c1: i2c@100 {
		#address-cells = <1>;
		#size-cells = <0>;
		#interrupt-cells = <1>;

		reg = <0x100 0x80 0xC20 0x20>;
		compatible = "aspeed,ast2600-i2c-bus";
		bus-frequency = <100000>;
		interrupts = <GIC_SPI 111 IRQ_TYPE_LEVEL_HIGH>;
		resets = <&rst ASPEED_RESET_I2C>;
		clocks = <&scu ASPEED_CLK_APB2>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_i2c2_default>;
		status = "disabled";
	};

	i2c2: i2c@180 {
		#address-cells = <1>;
		#size-cells = <0>;
		#interrupt-cells = <1>;

		reg = <0x180 0x80 0xC40 0x20>;
		compatible = "aspeed,ast2600-i2c-bus";
		bus-frequency = <100000>;
		interrupts = <GIC_SPI 112 IRQ_TYPE_LEVEL_HIGH>;
		resets = <&rst ASPEED_RESET_I2C>;
		clocks = <&scu ASPEED_CLK_APB2>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_i2c3_default>;
		status = "disabled";
	};

	i2c3: i2c@200 {
		#address-cells = <1>;
		#size-cells = <0>;
		#interrupt-cells = <1>;

		reg = <0x200 0x40 0xC60 0x20>;
		compatible = "aspeed,ast2600-i2c-bus";
		bus-frequency = <100000>;
		interrupts = <GIC_SPI 113 IRQ_TYPE_LEVEL_HIGH>;
		resets = <&rst ASPEED_RESET_I2C>;
		clocks = <&scu ASPEED_CLK_APB2>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_i2c4_default>;
		status = "disabled";
	};

	i2c4: i2c@280 {
		#address-cells = <1>;
		#size-cells = <0>;
		#interrupt-cells = <1>;

		reg = <0x280 0x80 0xC80 0x20>;
		compatible = "aspeed,ast2600-i2c-bus";
		bus-frequency = <100000>;
		interrupts = <GIC_SPI 114 IRQ_TYPE_LEVEL_HIGH>;
		resets = <&rst ASPEED_RESET_I2C>;
		clocks = <&scu ASPEED_CLK_APB2>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_i2c5_default>;
		status = "disabled";
	};

	i2c5: i2c@300 {
		#address-cells = <1>;
		#size-cells = <0>;
		#interrupt-cells = <1>;

		reg = <0x300 0x40 0xCA0 0x20>;
		compatible = "aspeed,ast2600-i2c-bus";
		bus-frequency = <100000>;
		interrupts = <GIC_SPI 115 IRQ_TYPE_LEVEL_HIGH>;
		resets = <&rst ASPEED_RESET_I2C>;
		clocks = <&scu ASPEED_CLK_APB2>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_i2c6_default>;
		status = "disabled";
	};

	i2c6: i2c@380 {
		#address-cells = <1>;
		#size-cells = <0>;
		#interrupt-cells = <1>;

		reg = <0x380 0x80 0xCC0 0x20>;
		compatible = "aspeed,ast2600-i2c-bus";
		bus-frequency = <100000>;
		interrupts = <GIC_SPI 116 IRQ_TYPE_LEVEL_HIGH>;
		resets = <&rst ASPEED_RESET_I2C>;
		clocks = <&scu ASPEED_CLK_APB2>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_i2c7_default>;
		status = "disabled";
	};

	i2c7: i2c@400 {
		#address-cells = <1>;
		#size-cells = <0>;
		#interrupt-cells = <1>;

		reg = <0x400 0x80 0xCE0 0x20>;
		compatible = "aspeed,ast2600-i2c-bus";
		bus-frequency = <100000>;
		interrupts = <GIC_SPI 117 IRQ_TYPE_LEVEL_HIGH>;
		resets = <&rst ASPEED_RESET_I2C>;
		clocks = <&scu ASPEED_CLK_APB2>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_i2c8_default>;
		status = "disabled";
	};

	i2c8: i2c@480 {
		#address-cells = <1>;
		#size-cells = <0>;
		#interrupt-cells = <1>;

		reg = <0x480 0x80 0xD00 0x20>;
		compatible = "aspeed,ast2600-i2c-bus";
		bus-frequency = <100000>;
		interrupts = <GIC_SPI 118 IRQ_TYPE_LEVEL_HIGH>;
		resets = <&rst ASPEED_RESET_I2C>;
		clocks = <&scu ASPEED_CLK_APB2>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_i2c9_default>;
		status = "disabled";
	};

	i2c9: i2c@500 {
		#address-cells = <1>;
		#size-cells = <0>;
		#interrupt-cells = <1>;

		reg = <0x500 0x80 0xD20 0x20>;
		compatible = "aspeed,ast2600-i2c-bus";
		bus-frequency = <100000>;
		interrupts = <GIC_SPI 119 IRQ_TYPE_LEVEL_HIGH>;
		resets = <&rst ASPEED_RESET_I2C>;
		clocks = <&scu ASPEED_CLK_APB2>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_i2c10_default>;
		status = "disabled";
	};

	i2c10: i2c@580 {
		#address-cells = <1>;
		#size-cells = <0>;
		#interrupt-cells = <1>;

		reg = <0x580 0x80 0xD40 0x20>;
		compatible = "aspeed,ast2600-i2c-bus";
		bus-frequency = <100000>;
		interrupts = <GIC_SPI 120 IRQ_TYPE_LEVEL_HIGH>;
		resets = <&rst ASPEED_RESET_I2C>;
		clocks = <&scu ASPEED_CLK_APB2>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_i2c11_default>;
		status = "disabled";
	};

	i2c11: i2c@600 {
		#address-cells = <1>;
		#size-cells = <0>;
		#interrupt-cells = <1>;

		reg = <0x600 0x80 0xD60 0x20>;
		compatible = "aspeed,ast2600-i2c-bus";
		bus-frequency = <100000>;
		interrupts = <GIC_SPI 121 IRQ_TYPE_LEVEL_HIGH>;
		resets = <&rst ASPEED_RESET_I2C>;
		clocks = <&scu ASPEED_CLK_APB2>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_i2c12_default>;
		status = "disabled";
	};

	i2c12: i2c@680 {
		#address-cells = <1>;
		#size-cells = <0>;
		#interrupt-cells = <1>;

		reg = <0x680 0x80 0xD80 0x20>;
		compatible = "aspeed,ast2600-i2c-bus";
		bus-frequency = <100000>;
		interrupts = <GIC_SPI 122 IRQ_TYPE_LEVEL_HIGH>;
		resets = <&rst ASPEED_RESET_I2C>;
		clocks = <&scu ASPEED_CLK_APB2>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_i2c13_default>;
		status = "disabled";
	};

	i2c13: i2c@700 {
		#address-cells = <1>;
		#size-cells = <0>;
		#interrupt-cells = <1>;

		reg = <0x700 0x80 0xDA0 0x20>;
		compatible = "aspeed,ast2600-i2c-bus";
		bus-frequency = <100000>;
		interrupts = <GIC_SPI 123 IRQ_TYPE_LEVEL_HIGH>;
		resets = <&rst ASPEED_RESET_I2C>;
		clocks = <&scu ASPEED_CLK_APB2>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_i2c14_default>;
		status = "disabled";
	};

	i2c14: i2c@780 {
		#address-cells = <1>;
		#size-cells = <0>;
		#interrupt-cells = <1>;

		reg = <0x780 0x80 0xDC0 0x20>;
		compatible = "aspeed,ast2600-i2c-bus";
		bus-frequency = <100000>;
		interrupts = <GIC_SPI 124 IRQ_TYPE_LEVEL_HIGH>;
		resets = <&rst ASPEED_RESET_I2C>;
		clocks = <&scu ASPEED_CLK_APB2>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_i2c15_default>;
		status = "disabled";
	};

	i2c15: i2c@800 {
		#address-cells = <1>;
		#size-cells = <0>;
		#interrupt-cells = <1>;

		reg = <0x800 0x80 0xDE0 0x20>;
		compatible = "aspeed,ast2600-i2c-bus";
		bus-frequency = <100000>;
		interrupts = <GIC_SPI 125 IRQ_TYPE_LEVEL_HIGH>;
		resets = <&rst ASPEED_RESET_I2C>;
		clocks = <&scu ASPEED_CLK_APB2>;
		pinctrl-names = "default";
		pinctrl-0 = <&pinctrl_i2c16_default>;
		status = "disabled";
	};

};

&pinctrl {
	pinctrl_fmcquad_default: fmcquad_default {
		function = "FMCQUAD";
		groups = "FMCQUAD";
	};

	pinctrl_spi1_default: spi1_default {
		function = "SPI1";
		groups = "SPI1";
	};

	pinctrl_spi1abr_default: spi1abr_default {
		function = "SPI1ABR";
		groups = "SPI1ABR";
	};

	pinctrl_spi1cs1_default: spi1cs1_default {
		function = "SPI1CS1";
		groups = "SPI1CS1";
	};

	pinctrl_spi1wp_default: spi1wp_default {
		function = "SPI1WP";
		groups = "SPI1WP";
	};

	pinctrl_spi1quad_default: spi1quad_default {
		function = "SPI1QUAD";
		groups = "SPI1QUAD";
	};

	pinctrl_spi2_default: spi2_default {
		function = "SPI2";
		groups = "SPI2";
	};

	pinctrl_spi2cs1_default: spi2cs1_default {
		function = "SPI2CS1";
		groups = "SPI2CS1";
	};

	pinctrl_spi2cs2_default: spi2cs2_default {
		function = "SPI2CS2";
		groups = "SPI2CS2";
	};

	pinctrl_spi2quad_default: spi2quad_default {
		function = "SPI2QUAD";
		groups = "SPI2QUAD";
	};

	pinctrl_acpi_default: acpi_default {
		function = "ACPI";
		groups = "ACPI";
	};

	pinctrl_adc0_default: adc0_default {
		function = "ADC0";
		groups = "ADC0";
	};

	pinctrl_adc1_default: adc1_default {
		function = "ADC1";
		groups = "ADC1";
	};

	pinctrl_adc10_default: adc10_default {
		function = "ADC10";
		groups = "ADC10";
	};

	pinctrl_adc11_default: adc11_default {
		function = "ADC11";
		groups = "ADC11";
	};

	pinctrl_adc12_default: adc12_default {
		function = "ADC12";
		groups = "ADC12";
	};

	pinctrl_adc13_default: adc13_default {
		function = "ADC13";
		groups = "ADC13";
	};

	pinctrl_adc14_default: adc14_default {
		function = "ADC14";
		groups = "ADC14";
	};

	pinctrl_adc15_default: adc15_default {
		function = "ADC15";
		groups = "ADC15";
	};

	pinctrl_adc2_default: adc2_default {
		function = "ADC2";
		groups = "ADC2";
	};

	pinctrl_adc3_default: adc3_default {
		function = "ADC3";
		groups = "ADC3";
	};

	pinctrl_adc4_default: adc4_default {
		function = "ADC4";
		groups = "ADC4";
	};

	pinctrl_adc5_default: adc5_default {
		function = "ADC5";
		groups = "ADC5";
	};

	pinctrl_adc6_default: adc6_default {
		function = "ADC6";
		groups = "ADC6";
	};

	pinctrl_adc7_default: adc7_default {
		function = "ADC7";
		groups = "ADC7";
	};

	pinctrl_adc8_default: adc8_default {
		function = "ADC8";
		groups = "ADC8";
	};

	pinctrl_adc9_default: adc9_default {
		function = "ADC9";
		groups = "ADC9";
	};

	pinctrl_bmcint_default: bmcint_default {
		function = "BMCINT";
		groups = "BMCINT";
	};

	pinctrl_ddcclk_default: ddcclk_default {
		function = "DDCCLK";
		groups = "DDCCLK";
	};

	pinctrl_ddcdat_default: ddcdat_default {
		function = "DDCDAT";
		groups = "DDCDAT";
	};

	pinctrl_espi_default: espi_default {
		function = "ESPI";
		groups = "ESPI";
	};

	pinctrl_fsi1_default: fsi1_default {
		function = "FSI1";
		groups = "FSI1";
	};

	pinctrl_fsi2_default: fsi2_default {
		function = "FSI2";
		groups = "FSI2";
	};

	pinctrl_fwspics1_default: fwspics1_default {
		function = "FWSPICS1";
		groups = "FWSPICS1";
	};

	pinctrl_fwspics2_default: fwspics2_default {
		function = "FWSPICS2";
		groups = "FWSPICS2";
	};

	pinctrl_gpid0_default: gpid0_default {
		function = "GPID0";
		groups = "GPID0";
	};

	pinctrl_gpid2_default: gpid2_default {
		function = "GPID2";
		groups = "GPID2";
	};

	pinctrl_gpid4_default: gpid4_default {
		function = "GPID4";
		groups = "GPID4";
	};

	pinctrl_gpid6_default: gpid6_default {
		function = "GPID6";
		groups = "GPID6";
	};

	pinctrl_gpie0_default: gpie0_default {
		function = "GPIE0";
		groups = "GPIE0";
	};

	pinctrl_gpie2_default: gpie2_default {
		function = "GPIE2";
		groups = "GPIE2";
	};

	pinctrl_gpie4_default: gpie4_default {
		function = "GPIE4";
		groups = "GPIE4";
	};

	pinctrl_gpie6_default: gpie6_default {
		function = "GPIE6";
		groups = "GPIE6";
	};

	pinctrl_i2c1_default: i2c1_default {
		function = "I2C1";
		groups = "I2C1";
	};

	pinctrl_i2c2_default: i2c2_default {
		function = "I2C2";
		groups = "I2C2";
	};

	pinctrl_i2c3_default: i2c3_default {
		function = "I2C3";
		groups = "I2C3";
	};

	pinctrl_i2c4_default: i2c4_default {
		function = "I2C4";
		groups = "I2C4";
	};

	pinctrl_i2c5_default: i2c5_default {
		function = "I2C5";
		groups = "I2C5";
	};

	pinctrl_i2c6_default: i2c6_default {
		function = "I2C6";
		groups = "I2C6";
	};

	pinctrl_i2c7_default: i2c7_default {
		function = "I2C7";
		groups = "I2C7";
	};

	pinctrl_i2c8_default: i2c8_default {
		function = "I2C8";
		groups = "I2C8";
	};

	pinctrl_i2c9_default: i2c9_default {
		function = "I2C9";
		groups = "I2C9";
	};

	pinctrl_i2c10_default: i2c10_default {
		function = "I2C10";
		groups = "I2C10";
	};

	pinctrl_i2c11_default: i2c11_default {
		function = "I2C11";
		groups = "I2C11";
	};

	pinctrl_i2c12_default: i2c12_default {
		function = "I2C12";
		groups = "I2C12";
	};

	pinctrl_i2c13_default: i2c13_default {
		function = "I2C13";
		groups = "I2C13";
	};

	pinctrl_i2c14_default: i2c14_default {
		function = "I2C14";
		groups = "I2C14";
	};

	pinctrl_i2c15_default: i2c15_default {
		function = "I2C15";
		groups = "I2C15";
	};

	pinctrl_i2c16_default: i2c16_default {
		function = "I2C16";
		groups = "I2C16";
	};

	pinctrl_lad0_default: lad0_default {
		function = "LAD0";
		groups = "LAD0";
	};

	pinctrl_lad1_default: lad1_default {
		function = "LAD1";
		groups = "LAD1";
	};

	pinctrl_lad2_default: lad2_default {
		function = "LAD2";
		groups = "LAD2";
	};

	pinctrl_lad3_default: lad3_default {
		function = "LAD3";
		groups = "LAD3";
	};

	pinctrl_lclk_default: lclk_default {
		function = "LCLK";
		groups = "LCLK";
	};

	pinctrl_lframe_default: lframe_default {
		function = "LFRAME";
		groups = "LFRAME";
	};

	pinctrl_lpchc_default: lpchc_default {
		function = "LPCHC";
		groups = "LPCHC";
	};

	pinctrl_lpcpd_default: lpcpd_default {
		function = "LPCPD";
		groups = "LPCPD";
	};

	pinctrl_lpcplus_default: lpcplus_default {
		function = "LPCPLUS";
		groups = "LPCPLUS";
	};

	pinctrl_lpcpme_default: lpcpme_default {
		function = "LPCPME";
		groups = "LPCPME";
	};

	pinctrl_lpcrst_default: lpcrst_default {
		function = "LPCRST";
		groups = "LPCRST";
	};

	pinctrl_lpcsmi_default: lpcsmi_default {
		function = "LPCSMI";
		groups = "LPCSMI";
	};

	pinctrl_lsirq_default: lsirq_default {
		function = "LSIRQ";
		groups = "LSIRQ";
	};

	pinctrl_mac1link_default: mac1link_default {
		function = "MAC1LINK";
		groups = "MAC1LINK";
	};

	pinctrl_mac2link_default: mac2link_default {
		function = "MAC2LINK";
		groups = "MAC2LINK";
	};

	pinctrl_mac3link_default: mac3link_default {
		function = "MAC3LINK";
		groups = "MAC3LINK";
	};

	pinctrl_mac4link_default: mac4link_default {
		function = "MAC4LINK";
		groups = "MAC4LINK";
	};

	pinctrl_mdio1_default: mdio1_default {
		function = "MDIO1";
		groups = "MDIO1";
	};

	pinctrl_mdio2_default: mdio2_default {
		function = "MDIO2";
		groups = "MDIO2";
	};

	pinctrl_mdio3_default: mdio3_default {
		function = "MDIO3";
		groups = "MDIO3";
	};

	pinctrl_mdio4_default: mdio4_default {
		function = "MDIO4";
		groups = "MDIO4";
	};

	pinctrl_rmii1_default: rmii1_default {
		function = "RMII1";
		groups = "RMII1";
	};

	pinctrl_rmii2_default: rmii2_default {
		function = "RMII2";
		groups = "RMII2";
	};

	pinctrl_rmii3_default: rmii3_default {
		function = "RMII3";
		groups = "RMII3";
	};

	pinctrl_rmii4_default: rmii4_default {
		function = "RMII4";
		groups = "RMII4";
	};

	pinctrl_rmii1rclk_default: rmii1rclk_default {
		function = "RMII1RCLK";
		groups = "RMII1RCLK";
	};

	pinctrl_rmii2rclk_default: rmii2rclk_default {
		function = "RMII2RCLK";
		groups = "RMII2RCLK";
	};

	pinctrl_rmii3rclk_default: rmii3rclk_default {
		function = "RMII3RCLK";
		groups = "RMII3RCLK";
	};

	pinctrl_rmii4rclk_default: rmii4rclk_default {
		function = "RMII4RCLK";
		groups = "RMII4RCLK";
	};

	pinctrl_ncts1_default: ncts1_default {
		function = "NCTS1";
		groups = "NCTS1";
	};

	pinctrl_ncts2_default: ncts2_default {
		function = "NCTS2";
		groups = "NCTS2";
	};

	pinctrl_ncts3_default: ncts3_default {
		function = "NCTS3";
		groups = "NCTS3";
	};

	pinctrl_ncts4_default: ncts4_default {
		function = "NCTS4";
		groups = "NCTS4";
	};

	pinctrl_ndcd1_default: ndcd1_default {
		function = "NDCD1";
		groups = "NDCD1";
	};

	pinctrl_ndcd2_default: ndcd2_default {
		function = "NDCD2";
		groups = "NDCD2";
	};

	pinctrl_ndcd3_default: ndcd3_default {
		function = "NDCD3";
		groups = "NDCD3";
	};

	pinctrl_ndcd4_default: ndcd4_default {
		function = "NDCD4";
		groups = "NDCD4";
	};

	pinctrl_ndsr1_default: ndsr1_default {
		function = "NDSR1";
		groups = "NDSR1";
	};

	pinctrl_ndsr2_default: ndsr2_default {
		function = "NDSR2";
		groups = "NDSR2";
	};

	pinctrl_ndsr3_default: ndsr3_default {
		function = "NDSR3";
		groups = "NDSR3";
	};

	pinctrl_ndsr4_default: ndsr4_default {
		function = "NDSR4";
		groups = "NDSR4";
	};

	pinctrl_ndtr1_default: ndtr1_default {
		function = "NDTR1";
		groups = "NDTR1";
	};

	pinctrl_ndtr2_default: ndtr2_default {
		function = "NDTR2";
		groups = "NDTR2";
	};

	pinctrl_ndtr3_default: ndtr3_default {
		function = "NDTR3";
		groups = "NDTR3";
	};

	pinctrl_ndtr4_default: ndtr4_default {
		function = "NDTR4";
		groups = "NDTR4";
	};

	pinctrl_nri1_default: nri1_default {
		function = "NRI1";
		groups = "NRI1";
	};

	pinctrl_nri2_default: nri2_default {
		function = "NRI2";
		groups = "NRI2";
	};

	pinctrl_nri3_default: nri3_default {
		function = "NRI3";
		groups = "NRI3";
	};

	pinctrl_nri4_default: nri4_default {
		function = "NRI4";
		groups = "NRI4";
	};

	pinctrl_nrts1_default: nrts1_default {
		function = "NRTS1";
		groups = "NRTS1";
	};

	pinctrl_nrts2_default: nrts2_default {
		function = "NRTS2";
		groups = "NRTS2";
	};

	pinctrl_nrts3_default: nrts3_default {
		function = "NRTS3";
		groups = "NRTS3";
	};

	pinctrl_nrts4_default: nrts4_default {
		function = "NRTS4";
		groups = "NRTS4";
	};

	pinctrl_oscclk_default: oscclk_default {
		function = "OSCCLK";
		groups = "OSCCLK";
	};

	pinctrl_pewake_default: pewake_default {
		function = "PEWAKE";
		groups = "PEWAKE";
	};

	pinctrl_pnor_default: pnor_default {
		function = "PNOR";
		groups = "PNOR";
	};

	pinctrl_pwm0_default: pwm0_default {
		function = "PWM0";
		groups = "PWM0";
	};

	pinctrl_pwm1_default: pwm1_default {
		function = "PWM1";
		groups = "PWM1";
	};

	pinctrl_pwm2_default: pwm2_default {
		function = "PWM2";
		groups = "PWM2";
	};

	pinctrl_pwm3_default: pwm3_default {
		function = "PWM3";
		groups = "PWM3";
	};

	pinctrl_pwm4_default: pwm4_default {
		function = "PWM4";
		groups = "PWM4";
	};

	pinctrl_pwm5_default: pwm5_default {
		function = "PWM5";
		groups = "PWM5";
	};

	pinctrl_pwm6_default: pwm6_default {
		function = "PWM6";
		groups = "PWM6";
	};

	pinctrl_pwm7_default: pwm7_default {
		function = "PWM7";
		groups = "PWM7";
	};

	pinctrl_pwm8g0_default: pwm8g0_default {
		function = "PWM8G0";
		groups = "PWM8G0";
	};

	pinctrl_pwm8g1_default: pwm8g1_default {
		function = "PWM8G1";
		groups = "PWM8G1";
	};

	pinctrl_pwm9g0_default: pwm9g0_default {
		function = "PWM9G0";
		groups = "PWM9G0";
	};

	pinctrl_pwm9g1_default: pwm9g1_default {
		function = "PWM9G1";
		groups = "PWM9G1";
	};

	pinctrl_pwm10g0_default: pwm10g0_default {
		function = "PWM10G0";
		groups = "PWM10G0";
	};

	pinctrl_pwm10g1_default: pwm10g1_default {
		function = "PWM10G1";
		groups = "PWM10G1";
	};

	pinctrl_pwm11g0_default: pwm11g0_default {
		function = "PWM11G0";
		groups = "PWM11G0";
	};

	pinctrl_pwm11g1_default: pwm11g1_default {
		function = "PWM11G1";
		groups = "PWM11G1";
	};

	pinctrl_pwm12g0_default: pwm12g0_default {
		function = "PWM12G0";
		groups = "PWM12G0";
	};

	pinctrl_pwm12g1_default: pwm12g1_default {
		function = "PWM12G1";
		groups = "PWM12G1";
	};

	pinctrl_pwm13g0_default: pwm13g0_default {
		function = "PWM13G0";
		groups = "PWM13G0";
	};

	pinctrl_pwm13g1_default: pwm13g1_default {
		function = "PWM13G1";
		groups = "PWM13G1";
	};

	pinctrl_pwm14g0_default: pwm14g0_default {
		function = "PWM14G0";
		groups = "PWM14G0";
	};

	pinctrl_pwm14g1_default: pwm14g1_default {
		function = "PWM14G1";
		groups = "PWM14G1";
	};

	pinctrl_pwm15g0_default: pwm15g0_default {
		function = "PWM15G0";
		groups = "PWM15G0";
	};

	pinctrl_pwm15g1_default: pwm15g1_default {
		function = "PWM15G1";
		groups = "PWM15G1";
	};

	pinctrl_rgmii1_default: rgmii1_default {
		function = "RGMII1";
		groups = "RGMII1";
	};

	pinctrl_rgmii2_default: rgmii2_default {
		function = "RGMII2";
		groups = "RGMII2";
	};

	pinctrl_rgmii3_default: rgmii3_default {
		function = "RGMII3";
		groups = "RGMII3";
	};

	pinctrl_rgmii4_default: rgmii4_default {
		function = "RGMII4";
		groups = "RGMII4";
	};

	pinctrl_rmii1_default: rmii1_default {
		function = "RMII1";
		groups = "RMII1";
	};

	pinctrl_rmii2_default: rmii2_default {
		function = "RMII2";
		groups = "RMII2";
	};

	pinctrl_rxd1_default: rxd1_default {
		function = "RXD1";
		groups = "RXD1";
	};

	pinctrl_rxd2_default: rxd2_default {
		function = "RXD2";
		groups = "RXD2";
	};

	pinctrl_rxd3_default: rxd3_default {
		function = "RXD3";
		groups = "RXD3";
	};

	pinctrl_rxd4_default: rxd4_default {
		function = "RXD4";
		groups = "RXD4";
	};

	pinctrl_salt1_default: salt1_default {
		function = "SALT1";
		groups = "SALT1";
	};

	pinctrl_salt10_default: salt10_default {
		function = "SALT10";
		groups = "SALT10";
	};

	pinctrl_salt11_default: salt11_default {
		function = "SALT11";
		groups = "SALT11";
	};

	pinctrl_salt12_default: salt12_default {
		function = "SALT12";
		groups = "SALT12";
	};

	pinctrl_salt13_default: salt13_default {
		function = "SALT13";
		groups = "SALT13";
	};

	pinctrl_salt14_default: salt14_default {
		function = "SALT14";
		groups = "SALT14";
	};

	pinctrl_salt2_default: salt2_default {
		function = "SALT2";
		groups = "SALT2";
	};

	pinctrl_salt3_default: salt3_default {
		function = "SALT3";
		groups = "SALT3";
	};

	pinctrl_salt4_default: salt4_default {
		function = "SALT4";
		groups = "SALT4";
	};

	pinctrl_salt5_default: salt5_default {
		function = "SALT5";
		groups = "SALT5";
	};

	pinctrl_salt6_default: salt6_default {
		function = "SALT6";
		groups = "SALT6";
	};

	pinctrl_salt7_default: salt7_default {
		function = "SALT7";
		groups = "SALT7";
	};

	pinctrl_salt8_default: salt8_default {
		function = "SALT8";
		groups = "SALT8";
	};

	pinctrl_salt9_default: salt9_default {
		function = "SALT9";
		groups = "SALT9";
	};

	pinctrl_scl1_default: scl1_default {
		function = "SCL1";
		groups = "SCL1";
	};

	pinctrl_scl2_default: scl2_default {
		function = "SCL2";
		groups = "SCL2";
	};

	pinctrl_sd1_default: sd1_default {
		function = "SD1";
		groups = "SD1";
	};

	pinctrl_sd2_default: sd2_default {
		function = "SD2";
		groups = "SD2";
	};

	pinctrl_emmc_default: emmc_default {
		function = "EMMC";
		groups = "EMMC";
	};

	pinctrl_emmcg8_default: emmcg8_default {
		function = "EMMCG8";
		groups = "EMMCG8";
	};

	pinctrl_sda1_default: sda1_default {
		function = "SDA1";
		groups = "SDA1";
	};

	pinctrl_sda2_default: sda2_default {
		function = "SDA2";
		groups = "SDA2";
	};

	pinctrl_sgps1_default: sgps1_default {
		function = "SGPS1";
		groups = "SGPS1";
	};

	pinctrl_sgps2_default: sgps2_default {
		function = "SGPS2";
		groups = "SGPS2";
	};

	pinctrl_sioonctrl_default: sioonctrl_default {
		function = "SIOONCTRL";
		groups = "SIOONCTRL";
	};

	pinctrl_siopbi_default: siopbi_default {
		function = "SIOPBI";
		groups = "SIOPBI";
	};

	pinctrl_siopbo_default: siopbo_default {
		function = "SIOPBO";
		groups = "SIOPBO";
	};

	pinctrl_siopwreq_default: siopwreq_default {
		function = "SIOPWREQ";
		groups = "SIOPWREQ";
	};

	pinctrl_siopwrgd_default: siopwrgd_default {
		function = "SIOPWRGD";
		groups = "SIOPWRGD";
	};

	pinctrl_sios3_default: sios3_default {
		function = "SIOS3";
		groups = "SIOS3";
	};

	pinctrl_sios5_default: sios5_default {
		function = "SIOS5";
		groups = "SIOS5";
	};

	pinctrl_siosci_default: siosci_default {
		function = "SIOSCI";
		groups = "SIOSCI";
	};

	pinctrl_spi1_default: spi1_default {
		function = "SPI1";
		groups = "SPI1";
	};

	pinctrl_spi1cs1_default: spi1cs1_default {
		function = "SPI1CS1";
		groups = "SPI1CS1";
	};

	pinctrl_spi1debug_default: spi1debug_default {
		function = "SPI1DEBUG";
		groups = "SPI1DEBUG";
	};

	pinctrl_spi1passthru_default: spi1passthru_default {
		function = "SPI1PASSTHRU";
		groups = "SPI1PASSTHRU";
	};

	pinctrl_spi2ck_default: spi2ck_default {
		function = "SPI2CK";
		groups = "SPI2CK";
	};

	pinctrl_spi2cs0_default: spi2cs0_default {
		function = "SPI2CS0";
		groups = "SPI2CS0";
	};

	pinctrl_spi2cs1_default: spi2cs1_default {
		function = "SPI2CS1";
		groups = "SPI2CS1";
	};

	pinctrl_spi2miso_default: spi2miso_default {
		function = "SPI2MISO";
		groups = "SPI2MISO";
	};

	pinctrl_spi2mosi_default: spi2mosi_default {
		function = "SPI2MOSI";
		groups = "SPI2MOSI";
	};

	pinctrl_thru0_default: thru0_default {
		function = "THRU0";
		groups = "THRU0";
	};

	pinctrl_thru1_default: thru1_default {
		function = "THRU1";
		groups = "THRU1";
	};

	pinctrl_thru2_default: thru2_default {
		function = "THRU2";
		groups = "THRU2";
	};

	pinctrl_thru3_default: thru3_default {
		function = "THRU3";
		groups = "THRU3";
	};

	pinctrl_timer3_default: timer3_default {
		function = "TIMER3";
		groups = "TIMER3";
	};

	pinctrl_timer4_default: timer4_default {
		function = "TIMER4";
		groups = "TIMER4";
	};

	pinctrl_timer5_default: timer5_default {
		function = "TIMER5";
		groups = "TIMER5";
	};

	pinctrl_timer6_default: timer6_default {
		function = "TIMER6";
		groups = "TIMER6";
	};

	pinctrl_timer7_default: timer7_default {
		function = "TIMER7";
		groups = "TIMER7";
	};

	pinctrl_timer8_default: timer8_default {
		function = "TIMER8";
		groups = "TIMER8";
	};

	pinctrl_txd1_default: txd1_default {
		function = "TXD1";
		groups = "TXD1";
	};

	pinctrl_txd2_default: txd2_default {
		function = "TXD2";
		groups = "TXD2";
	};

	pinctrl_txd3_default: txd3_default {
		function = "TXD3";
		groups = "TXD3";
	};

	pinctrl_txd4_default: txd4_default {
		function = "TXD4";
		groups = "TXD4";
	};

	pinctrl_uart6_default: uart6_default {
		function = "UART6";
		groups = "UART6";
	};

	pinctrl_usbcki_default: usbcki_default {
		function = "USBCKI";
		groups = "USBCKI";
	};

	pinctrl_usb2ah_default: usb2ah_default {
		function = "USB2AH";
		groups = "USB2AH";
	};

	pinctrl_usb11bhid_default: usb11bhid_default {
		function = "USB11BHID";
		groups = "USB11BHID";
	};

	pinctrl_usb2bh_default: usb2bh_default {
		function = "USB2BH";
		groups = "USB2BH";
	};

	pinctrl_vgabiosrom_default: vgabiosrom_default {
		function = "VGABIOSROM";
		groups = "VGABIOSROM";
	};

	pinctrl_vgahs_default: vgahs_default {
		function = "VGAHS";
		groups = "VGAHS";
	};

	pinctrl_vgavs_default: vgavs_default {
		function = "VGAVS";
		groups = "VGAVS";
	};

	pinctrl_vpi24_default: vpi24_default {
		function = "VPI24";
		groups = "VPI24";
	};

	pinctrl_vpo_default: vpo_default {
		function = "VPO";
		groups = "VPO";
	};

	pinctrl_wdtrst1_default: wdtrst1_default {
		function = "WDTRST1";
		groups = "WDTRST1";
	};

	pinctrl_wdtrst2_default: wdtrst2_default {
		function = "WDTRST2";
		groups = "WDTRST2";
	};

	pinctrl_pcie0rc_default: pcie0rc_default {
		function = "PCIE0RC";
		groups = "PCIE0RC";
	};

	pinctrl_pcie1rc_default: pcie1rc_default {
		function = "PCIE1RC";
		groups = "PCIE1RC";
	};

	pinctrl_sgpm1_default: sgpm1_default {
		function = "SGPM1";
		groups = "SGPM1";
	};

	pinctrl_sgpm2_default: sgpm2_default {
		function = "SGPM2";
		groups = "SGPM2";
	};
};
