// SPDX-License-Identifier: GPL-2.0+ OR X11
/*
 * Device Tree Include file for Freescale Layerscape-1046A family SoC.
 *
 * Copyright 2016, Freescale Semiconductor
 * Copyright 2020 NXP
 *
 * Mingkai Hu <Mingkai.hu@freescale.com>
 */

/dts-v1/;
#include "fsl-ls1046a.dtsi"

/ {
	model = "LS1046A RDB Board";

	aliases {
		spi0 = &qspi;
		serial0 = &duart0;
		serial1 = &duart1;
		serial2 = &duart2;
		serial3 = &duart3;
	};

};

&duart0 {
	status = "okay";
};

&duart1 {
	status = "okay";
};

&qspi {
	status = "okay";

	s25fs512s0: flash@0 {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "jedec,spi-nor";
		spi-max-frequency = <50000000>;
		reg = <0>;
	};

	s25fs512s1: flash@1 {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "jedec,spi-nor";
		spi-max-frequency = <50000000>;
		reg = <1>;
	 };
};

&sata {
	status = "okay";
};

&i2c0 {
	status = "okay";
};

&i2c3 {
	status = "okay";
};

#include "fsl-ls1046-post.dtsi"

&fman0 {
	ethernet@e4000 {
		phy-handle = <&rgmii_phy1>;
		phy-connection-type = "rgmii-id";
		status = "okay";
	};

	ethernet@e6000 {
		phy-handle = <&rgmii_phy2>;
		phy-connection-type = "rgmii-id";
		status = "okay";
	};

	ethernet@e8000 {
		phy-handle = <&sgmii_phy1>;
		phy-connection-type = "sgmii";
		status = "okay";
	};

	ethernet@ea000 {
		phy-handle = <&sgmii_phy2>;
		phy-connection-type = "sgmii";
		status = "okay";
	};

	ethernet@f0000 { /* 10GEC1 */
		phy-handle = <&aqr106_phy>;
		phy-connection-type = "xgmii";
		status = "okay";
	};

	ethernet@f2000 { /* 10GEC2 */
		fixed-link = <0 1 1000 0 0>;
		phy-connection-type = "xgmii";
		status = "okay";
	};

	mdio@fc000 {
		rgmii_phy1: ethernet-phy@1 {
			reg = <0x1>;
		};

		rgmii_phy2: ethernet-phy@2 {
			reg = <0x2>;
		};

		sgmii_phy1: ethernet-phy@3 {
			reg = <0x3>;
		};

		sgmii_phy2: ethernet-phy@4 {
			reg = <0x4>;
		};
	};

	mdio@fd000 {
		aqr106_phy: ethernet-phy@0 {
			compatible = "ethernet-phy-ieee802.3-c45";
			interrupts = <0 131 4>;
			reg = <0x0>;
		};
	};
};
