// SPDX-License-Identifier: GPL-2.0
/*
 * Copyright (C) 2016 Marvell International Ltd.
 * Copyright (C) 2020 Sartura Ltd.
 */

#include "armada-8040.dtsi" /* include SoC device tree */

/ {
	model = "iEi-Puzzle-M801";
	compatible = "marvell,armada8040-puzzle-m801",
		     "marvell,armada8040";

	chosen {
		stdout-path = "serial0:115200n8";
	};

	aliases {
		i2c0 = &ap_i2c0;
		i2c1 = &cp0_i2c0;
		i2c2 = &cp0_i2c1;
		i2c3 = &i2c_switch;
		spi0 = &ap_spi0;
		gpio0 = &ap_gpio0;
		gpio1 = &cp0_gpio0;
		gpio2 = &cp0_gpio1;
		gpio3 = &sfpplus_gpio;
	};

	memory@00000000 {
		device_type = "memory";
		reg = <0x0 0x0 0x0 0x80000000>;
	};

	simple-bus {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <0>;

		reg_usb3h0_vbus: usb3-vbus0 {
			compatible = "regulator-fixed";
			pinctrl-names = "default";
			pinctrl-0 = <&cp0_xhci_vbus_pins>;
			regulator-name = "reg-usb3h0-vbus";
			regulator-min-microvolt = <5000000>;
			regulator-max-microvolt = <5000000>;
			startup-delay-us = <500000>;
			enable-active-high;
			regulator-always-on;
			regulator-boot-on;
			gpio = <&cp0_gpio1 15 GPIO_ACTIVE_HIGH>; /* GPIO[47] */
		};
	};
};

&ap_i2c0 {
	status = "okay";
	clock-frequency = <100000>;

	rtc@32 {
		compatible = "epson,rx8010";
		reg = <0x32>;
	};
};

&uart0 {
	status = "okay";
};

&ap_pinctl {
	/*
	 * MPP Bus:
	 * AP SPI0 [0-3]
	 * AP I2C [4-5]
	 * AP GPIO [6]
	 * AP UART 1 RX/TX [7-8]
	 * AP GPIO [9-10]
	 * AP GPIO [12]
	 * UART0 [11,19]
	 */
		  /* 0 1 2 3 4 5 6 7 8 9 */
	pin-func = < 3 3 3 3 3 3 3 3 3 0
		     0 3 0 0 0 0 0 0 0 3 >;
};

&cp0_pinctl {
	/*
	 * MPP Bus:
	 * [0-31] = 0xff: Keep default CP0_shared_pins:
	 * [11] CLKOUT_MPP_11 (out)
	 * [23] LINK_RD_IN_CP2CP (in)
	 * [25] CLKOUT_MPP_25 (out)
	 * [29] AVS_FB_IN_CP2CP (in)
	 * [32,34] SMI
	 * [33]    MSS power down
	 * [35-38] CP0 I2C1 and I2C0
	 * [39] MSS CKE Enable
	 * [40,41] CP0 UART1 TX/RX
	 * [42,43] XSMI (controls two 10G phys)
	 * [47] USB VBUS EN
	 * [48] FAN PWM
	 * [49] 10G port 1 interrupt
	 * [50] 10G port 0 interrupt
	 * [51] 2.5G SFP TX fault
	 * [52] PCIe reset out
	 * [53] 2.5G SFP mode
	 * [54] 2.5G SFP LOS
	 * [55] Micro SD card detect
	 * [56-61] Micro SD
	 * [62] CP1 SFI SFP FAULT
	 */
		/*   0    1    2    3    4    5    6    7    8    9 */
	pin-func = < 0xff 0xff 0xff 0xff 0xff 0xff 0xff 0xff 0xff 0xff
		     0xff 0xff 0xff 0xff 0xff 0xff 0xff 0xff 0xff 0xff
		     0xff 0xff 0xff 0xff 0xff 0xff 0xff 0xff 0xff 0xff
		     0xff 0    7    0xa  7    2    2    2    2    0xa
		     7    7    8    8    0    0    0    0    0    0
		     0    0    0    0    0    0    0xe  0xe  0xe  0xe
		     0xe  0xe  0 >;

	cp0_xhci_vbus_pins: cpm-xhci-vbus-pins {
		marvell,pins = < 47 >;
		marvell,function = <0>;
	};

	cp0_pcie_reset_pins: cpm-pcie-reset-pins {
		marvell,pins = < 52 >;
		marvell,function = <0>;
	};
};

&cp0_sdhci0 {
	pinctrl-names = "default";
	pinctrl-0 = <&cp0_sdhci_pins>;
	bus-width= <4>;
	status = "okay";
};

&cp0_pcie0 {
	num-lanes = <1>;
	pinctrl-names = "default";
	pinctrl-0 = <&cp0_pcie_reset_pins>;
	marvell,reset-gpio = <&cp0_gpio1 20 GPIO_ACTIVE_LOW>; /* GPIO[52] */
	status = "okay";
};

&cp0_i2c0 {
	pinctrl-names = "default";
	pinctrl-0 = <&cp0_i2c0_pins>;
	status = "okay";
	clock-frequency = <100000>;

	sfpplus_gpio: gpio@21 {
		compatible = "nxp,pca9555";
		reg = <0x21>;
		gpio-controller;
		#gpio-cells = <2>;
	};
};

&cp0_i2c1 {
	pinctrl-names = "default";
	pinctrl-0 = <&cp0_i2c1_pins>;
	status = "okay";
	clock-frequency = <100000>;

	i2c_switch: i2c-switch@70 {
		compatible = "nxp,pca9544";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x70>;
	};
};

&cp0_sata0 {
	status = "okay";
};

&cp0_ethernet {
	pinctrl-names = "default";
	status = "okay";
};

&cp0_mdio {
	status = "okay";
	cp0_ge_phy0: ethernet-phy@1 {
		reg = <0>;
	};

	cp0_ge_phy1: ethernet-phy@2 {
		reg = <1>;
	};
};

&cp0_eth0 {
	status = "okay";
	phy-mode = "sfi";
};

&cp0_eth1 {
	status = "okay";
	phy-mode = "sgmii";
	phy = <&cp0_ge_phy0>;
};

&cp0_eth2 {
	status = "okay";
	phy-mode = "sgmii";
	phy = <&cp0_ge_phy1>;
};

&cp0_comphy {
	/*
	 * CP0 Serdes Configuration:
	 * Lane 0: PCIe0 (x1)
	 * Lane 1: SGMII2
	 * Lane 2: SATA0
	 * Lane 3: SGMII1
	 * Lane 4: SFI (10G)
	 * Lane 5: SATA1
	 */
	phy0 {
		phy-type = <COMPHY_TYPE_PEX0>;
	};
	phy1 {
		phy-type = <COMPHY_TYPE_SGMII2>;
		phy-speed = <COMPHY_SPEED_1_25G>;
	};
	phy2 {
		phy-type = <COMPHY_TYPE_SATA0>;
	};
	phy3 {
		phy-type = <COMPHY_TYPE_SGMII1>;
		phy-speed = <COMPHY_SPEED_1_25G>;
	};
	phy4 {
		phy-type = <COMPHY_TYPE_SFI0>;
	};
	phy5 {
		phy-type = <COMPHY_TYPE_SATA1>;
	};
};

&cp1_mdio {
	status = "okay";
	pinctrl-names = "default";
	pinctrl-0 = <&cp1_smi_pins>;

	cp1_ge_phy0: ethernet-phy@3 {
		reg = <1>;
	};

	cp1_ge_phy1: ethernet-phy@4 {
		reg = <0>;
	};
};

&cp1_pcie0 {
	num-lanes = <2>;
	pinctrl-names = "default";
	status = "okay";
};

&cp1_usb3_0 {
	vbus-supply = <&reg_usb3h0_vbus>;
	status = "okay";
};

&cp1_utmi0 {
	status = "okay";
};

&cp1_ethernet {
	status = "okay";
};

&cp1_eth0 {
	status = "okay";
	phy-mode = "sfi";
};

&cp1_eth1 {
	status = "okay";
	phy = <&cp1_ge_phy0>;
	phy-mode = "sgmii";
};

&cp1_eth2 {
	status = "okay";
	phy = <&cp1_ge_phy1>;
	phy-mode = "sgmii";
};

&cp1_pinctl {
	/*
	 * MPP Bus:
	 * [0-5] TDM
	 * [27-28] SMI
	 * [29-30] CP1 MSS I2C
	 * [6-26, 31] GPIO
	 * [32-62] = 0xff: Keep default CP1_shared_pins:
	 */
		/*   0    1    2    3    4    5    6    7    8    9 */
	pin-func = < 0x4  0x4  0x4  0x4  0x4  0x4  0x0  0x0  0x0  0x0
		     0x0  0x0  0x0  0x0  0x0  0x0  0x0  0x0  0x0  0x0
		     0x0  0x0  0x0  0x0  0x0  0x0  0x0  0x8  0x8  0x8
		     0x8  0x0  0xff 0xff 0xff 0xff 0xff 0xff 0xff 0xff
		     0xff 0xff 0xff 0xff 0xff 0xff 0xff 0xff 0xff 0xff
		     0xff 0xff 0xff 0xff 0xff 0xff 0xff 0xff 0xff 0xff
		     0xff 0xff 0xff>;

	cp1_smi_pins: cp1-smi-pins {
		marvell,pins = < 27 28 >;
		marvell,function = <8>;
	};
};

&ap_spi0 {
	status = "okay";

	spi-flash@0 {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "jedec,spi-nor";
		reg = <0>;
		spi-max-frequency = <10000000>;

		partitions {
			compatible = "fixed-partitions";
			#address-cells = <1>;
			#size-cells = <1>;

			partition@u-boot {
				reg = <0x00000000 0x001f0000>;
				label = "u-boot";
			};
			partition@u-boot-env {
				reg = <0x001f0000 0x00010000>;
				label = "u-boot-env";
			};
			partition@ubi1 {
				reg = <0x00200000 0x03f00000>;
				label = "ubi1";
			};
			partition@ubi2 {
				reg = <0x04100000 0x03f00000>;
				label = "ubi2";
			};
		};
	};
};

&cp1_comphy {
	/*
	 * CP1 Serdes Configuration:
	 * Lane 0: PCIe0 (x2)
	 * Lane 1: PCIe0 (x2)
	 * Lane 2: USB HOST 0
	 * Lane 3: SGMII1
	 * Lane 4: SFI (10G)
	 * Lane 5: SGMII2
	 */
	phy0 {
		phy-type = <COMPHY_TYPE_PEX0>;
	};
	phy1 {
		phy-type = <COMPHY_TYPE_PEX0>;
	};
	phy2 {
		phy-type = <COMPHY_TYPE_USB3_HOST0>;
	};
	phy3 {
		phy-type = <COMPHY_TYPE_SGMII1>;
		phy-speed = <COMPHY_SPEED_1_25G>;
	};
	phy4 {
		phy-type = <COMPHY_TYPE_SFI0>;
	};
	phy5 {
		phy-type = <COMPHY_TYPE_SGMII2>;
		phy-speed = <COMPHY_SPEED_1_25G>;
	};
};
