// SPDX-License-Identifier: GPL-2.0
/*
 * Copyright (C) 2020-2023 Texas Instruments Incorporated - https://www.ti.com/
 */

/dts-v1/;

#include "k3-j7200-common-proc-board.dts"
#include "k3-j7200-ddr-evm-lp4-2666.dtsi"
#include "k3-j721e-ddr.dtsi"
#include "k3-j7200-common-proc-board-u-boot.dtsi"

/ {
	aliases {
		remoteproc0 = &sysctrler;
		remoteproc1 = &a72_0;
	};

	a72_0: a72@0 {
		compatible = "ti,am654-rproc";
		reg = <0x0 0x00a90000 0x0 0x10>;
		power-domains = <&k3_pds 61 TI_SCI_PD_EXCLUSIVE>,
				<&k3_pds 202 TI_SCI_PD_EXCLUSIVE>,
				<&k3_pds 4 TI_SCI_PD_EXCLUSIVE>;
		resets = <&k3_reset 202 0>;
		clocks = <&k3_clks 61 1>, <&k3_clks 202 2>, <&k3_clks 4 1> ;
		clock-names = "gtc", "core", "msmc";
		assigned-clocks = <&k3_clks 202 2>, <&k3_clks 61 1>, <&k3_clks 4 1>,
						  <&k3_clks 323 0>;
		assigned-clock-parents= <0>, <0>, <0>, <&k3_clks 323 2>;
		assigned-clock-rates = <2000000000>, <200000000>, <1000000000>;
		ti,sci = <&dmsc>;
		ti,sci-proc-id = <32>;
		ti,sci-host-id = <10>;
		bootph-pre-ram;
	};

	dm_tifs: dm-tifs {
		compatible = "ti,j721e-dm-sci";
		ti,host-id = <3>;
		ti,secure-host;
		mbox-names = "rx", "tx";
		mboxes = <&secure_proxy_mcu 21>,
			<&secure_proxy_mcu 23>;
		bootph-pre-ram;
	};
};

&memorycontroller {
	power-domains = <&k3_pds 8 TI_SCI_PD_SHARED>,
			<&k3_pds 90 TI_SCI_PD_SHARED>;
	clocks = <&k3_clks 8 5>, <&k3_clks 30 9>;
	bootph-pre-ram;
};

&mcu_timer0 {
	/delete-property/ clocks;
	/delete-property/ clocks-names;
	/delete-property/ assigned-clocks;
	/delete-property/ assigned-clock-parents;
	clock-frequency = <250000000>;
	bootph-pre-ram;
};

&secure_proxy_mcu {
	bootph-pre-ram;
	status = "okay";
};

&cbass_mcu_wakeup {
	sysctrler: sysctrler {
		compatible = "ti,am654-tisci-rproc-r5";
		mboxes= <&secure_proxy_mcu 4>,
			<&secure_proxy_mcu 5>;
		mbox-names = "tx", "rx";
		bootph-pre-ram;
	};
};

&dmsc {
	mboxes = <&secure_proxy_mcu 8>,
		<&secure_proxy_mcu 6>, <&secure_proxy_mcu 5>;
	mbox-names = "tx", "rx", "notify";
	ti,host-id = <4>;
	ti,secure-host;
	bootph-pre-ram;
};

&wkup_vtm0 {
	bootph-pre-ram;
};

&ospi0 {
    reg = <0x0 0x47040000 0x0 0x100>,
          <0x0 0x50000000 0x0 0x8000000>;
};

&fss {
	/* enable ranges missing from the FSS node */
	ranges = <0x0 0x47000000 0x0 0x47000000 0x0 0x00068400>,
	         <0x0 0x50000000 0x0 0x50000000 0x0 0x08000000>;
};

&hbmc {
	reg = <0x0 0x47040000 0x0 0x100>,
		<0x0 0x50000000 0x0 0x8000000>;
	ranges = <0x0 0x0 0x0 0x50000000 0x4000000>,
		<0x1 0x0 0x0 0x54000000 0x800000>;
};

&mcu_ringacc {
    ti,sci = <&dm_tifs>;
};

&mcu_udmap {
    ti,sci = <&dm_tifs>;
};

&wkup_vtm0 {
	vdd-supply-2 = <&buckb1>;
	bootph-pre-ram;
};

&tps659414 {
	esm: esm {
		compatible = "ti,tps659413-esm";
		bootph-pre-ram;
	};
};
