// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * Copyright (c) 2023 Collabora Ltd.
 */

#include <dt-bindings/usb/pd.h>
#include "rk3588-u-boot.dtsi"

/ {
	leds {
		led_rgb_b {
			default-state = "on";
		};
	};
};

&fspim2_pins {
	bootph-pre-ram;
	bootph-some-ram;
};

&i2c4 {
	pinctrl-names = "default";
	pinctrl-0 = <&i2c4m1_xfer>;
	status = "okay";

	usbc0: usb-typec@22 {
		compatible = "fcs,fusb302";
		reg = <0x22>;
		interrupt-parent = <&gpio3>;
		interrupts = <RK_PB4 IRQ_TYPE_LEVEL_LOW>;
		pinctrl-names = "default";
		status = "okay";

		usb_con: connector {
			compatible = "usb-c-connector";
			label = "USB-C";
			data-role = "dual";
			power-role = "sink";
			try-power-role = "sink";
			op-sink-microwatt = <1000000>;
			sink-pdos =
				<PDO_FIXED(5000, 3000, PDO_FIXED_USB_COMM)>,
				<PDO_VAR(5000, 20000, 5000)>;
		};
	};
};

&saradc {
	bootph-pre-ram;
	vdd-microvolts = <1800000>;
};

&sdhci {
	cap-mmc-highspeed;
	mmc-hs200-1_8v;
};

&sfc {
	flash@0 {
		bootph-pre-ram;
		bootph-some-ram;
	};
};

&u2phy0 {
	status = "okay";
};

&u2phy0_otg {
	status = "okay";
};

&usbdp_phy0 {
	status = "okay";
};

&usb_host0_xhci {
	dr_mode = "peripheral";
	maximum-speed = "high-speed";
	status = "okay";
};
