// SPDX-License-Identifier: GPL-2.0+

/dts-v1/;

#include <dt-bindings/gpio/aspeed-gpio.h>
#include <dt-bindings/leds/common.h>
#include <dt-bindings/i2c/i2c.h>
#include "ast2600-evb.dts"

/ {
	model = "IBM SBP1";
	compatible = "ibm,sbp1-bmc", "aspeed,ast2600";

	memory@80000000 {
		reg = <0x80000000 0x20000000>;
		device_type = "memory";
	};

	chosen {
		stdout-path = &uart1;
		bootargs = "console=tty0 console=ttyS0,115200 earlycon";
	};

	reserved-memory {
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;

		gfx_memory: framebuffer {
			size = <0x01000000>;
			alignment = <0x01000000>;
			compatible = "shared-dma-pool";
			reusable;
		};
	};
	aliases {
		ethernet0 = &mac2;
		ethernet1 = &mac3;
	};

	cpus {
		cpu@0 {
			clock-frequency = <1200000000>;
		};
		cpu@1 {
			clock-frequency = <1200000000>;
		};
	};

	leds {
		compatible = "gpio-leds";

		led-power {
			label = "LED_BMC_READY";
			gpios = <&gpio0 ASPEED_GPIO(H, 1) GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_GREEN>;
			default-state = "off";
			retain-state-suspended;
			panic-indicator;
		};

		led-id-tpm {
			label = "LED_ID_TPM";
			gpios = <&smb_pex_vr_ctrl 12 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-bat {
			label = "LED_ID_BAT";
			gpios = <&smb_pex_vr_ctrl 16 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-mgmt-port2 {
			label = "LED_ID_MGMT_PORT2";
			gpios = <&smb_pex_vr_ctrl 17 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-mgmt-port1 {
			label = "LED_ID_MGMT_PORT1";
			gpios = <&smb_pex_vr_ctrl 18 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-nic1-port1 {
			label = "LED_ID_NIC1_PORT1";
			gpios = <&smb_pex_vr_ctrl 22 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-nic1-port2 {
			label = "LED_ID_NIC1_PORT2";
			gpios = <&smb_pex_vr_ctrl 23 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-nic2-port1 {
			label = "LED_ID_NIC2_PORT1";
			gpios = <&smb_pex_vr_ctrl 24 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-nic2-port2 {
			label = "LED_ID_NIC2_PORT2";
			gpios = <&smb_pex_vr_ctrl 25 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-m2-ssd2 {
			label = "LED_ID_M2_SSD2";
			gpios = <&smb_pex_vr_ctrl 36 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-m2-ssd1 {
			label = "LED_ID_M2_SSD1";
			gpios = <&smb_pex_vr_ctrl 37 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dwr-frnt-p {
			label = "LED_ID_DWR_FRNT_P";
			gpios = <&smb_svc_pex_cpu3_led 37 GPIO_ACTIVE_HIGH>;
			color = <LED_COLOR_ID_BLUE>;

			default-state = "on";
			retain-state-suspended;
			retain-state-shutdown;
		};

		led-pwr-dwr-frnt {
			label = "LED_PWR_DWR_FRNT";
			gpios = <&smb_svc_pex_cpu3_led 36 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_GREEN>;

			retain-state-suspended;
			retain-state-shutdown;
		};

		led-pwr-dwr-back {
			label = "LED_PWR_DWR_BACK";
			gpios = <&smb_pex_vr_ctrl 34 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_GREEN>;

			retain-state-suspended;
			retain-state-shutdown;
		};

		led-id-dwr-back-p {
			label = "LED_ID_DWR_BACK_P";
			gpios = <&smb_pex_vr_ctrl 35 GPIO_ACTIVE_HIGH>;
			color = <LED_COLOR_ID_BLUE>;

			default-state = "on";
			retain-state-suspended;
			retain-state-shutdown;
		};

		led-id-cpu0 {
			label = "LED_ID_CPU0";
			gpios = <&smb_svc_pex_cpu0_led 39 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-cpu1 {
			label = "LED_ID_CPU1";
			gpios = <&smb_svc_pex_cpu1_led 39 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-cpu2 {
			label = "LED_ID_CPU2";
			gpios = <&smb_svc_pex_cpu2_led 39 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-cpu3 {
			label = "LED_ID_CPU3";
			gpios = <&smb_svc_pex_cpu3_led 39 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c0e2 {
			label = "LED_ID_DIMM_C0E2";
			gpios = <&smb_svc_pex_cpu0_led 20 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c0e1 {
			label = "LED_ID_DIMM_C0E1";
			gpios = <&smb_svc_pex_cpu0_led 21 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c0f2 {
			label = "LED_ID_DIMM_C0F2";
			gpios = <&smb_svc_pex_cpu0_led 22 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c0f1 {
			label = "LED_ID_DIMM_C0F1";
			gpios = <&smb_svc_pex_cpu0_led 23 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c0g2 {
			label = "LED_ID_DIMM_C0G2";
			gpios = <&smb_svc_pex_cpu0_led 24 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c0g1 {
			label = "LED_ID_DIMM_C0G1";
			gpios = <&smb_svc_pex_cpu0_led 25 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c0h2 {
			label = "LED_ID_DIMM_C0H2";
			gpios = <&smb_svc_pex_cpu0_led 26 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c0h1 {
			label = "LED_ID_DIMM_C0H1";
			gpios = <&smb_svc_pex_cpu0_led 27 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c0a2 {
			label = "LED_ID_DIMM_C0A2";
			gpios = <&smb_svc_pex_cpu0_led 28 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c0a1 {
			label = "LED_ID_DIMM_C0A1";
			gpios = <&smb_svc_pex_cpu0_led 29 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c0b2 {
			label = "LED_ID_DIMM_C0B2";
			gpios = <&smb_svc_pex_cpu0_led 30 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c0b1 {
			label = "LED_ID_DIMM_C0B1";
			gpios = <&smb_svc_pex_cpu0_led 31 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c0c2 {
			label = "LED_ID_DIMM_C0C2";
			gpios = <&smb_svc_pex_cpu0_led 32 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c0c1 {
			label = "LED_ID_DIMM_C0C1";
			gpios = <&smb_svc_pex_cpu0_led 33 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c0d2 {
			label = "LED_ID_DIMM_C0D2";
			gpios = <&smb_svc_pex_cpu0_led 34 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c0d1 {
			label = "LED_ID_DIMM_C0D1";
			gpios = <&smb_svc_pex_cpu0_led 35 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c1e2 {
			label = "LED_ID_DIMM_C1E2";
			gpios = <&smb_svc_pex_cpu1_led 20 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c1e1 {
			label = "LED_ID_DIMM_C1E1";
			gpios = <&smb_svc_pex_cpu1_led 21 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c1f2 {
			label = "LED_ID_DIMM_C1F2";
			gpios = <&smb_svc_pex_cpu1_led 22 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c1f1 {
			label = "LED_ID_DIMM_C1F1";
			gpios = <&smb_svc_pex_cpu1_led 23 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c1g2 {
			label = "LED_ID_DIMM_C1G2";
			gpios = <&smb_svc_pex_cpu1_led 24 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c1g1 {
			label = "LED_ID_DIMM_C1G1";
			gpios = <&smb_svc_pex_cpu1_led 25 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c1h2 {
			label = "LED_ID_DIMM_C1H2";
			gpios = <&smb_svc_pex_cpu1_led 26 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c1h1 {
			label = "LED_ID_DIMM_C1H1";
			gpios = <&smb_svc_pex_cpu1_led 27 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c1a2 {
			label = "LED_ID_DIMM_C1A2";
			gpios = <&smb_svc_pex_cpu1_led 28 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c1a1 {
			label = "LED_ID_DIMM_C1A1";
			gpios = <&smb_svc_pex_cpu1_led 29 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c1b2 {
			label = "LED_ID_DIMM_C1B2";
			gpios = <&smb_svc_pex_cpu1_led 30 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c1b1 {
			label = "LED_ID_DIMM_C1B1";
			gpios = <&smb_svc_pex_cpu1_led 31 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c1c2 {
			label = "LED_ID_DIMM_C1C2";
			gpios = <&smb_svc_pex_cpu1_led 32 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c1c1 {
			label = "LED_ID_DIMM_C1C1";
			gpios = <&smb_svc_pex_cpu1_led 33 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c1d2 {
			label = "LED_ID_DIMM_C1D2";
			gpios = <&smb_svc_pex_cpu1_led 34 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c1d1 {
			label = "LED_ID_DIMM_C1D1";
			gpios = <&smb_svc_pex_cpu1_led 35 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c2e2 {
			label = "LED_ID_DIMM_C2E2";
			gpios = <&smb_svc_pex_cpu2_led 20 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c2e1 {
			label = "LED_ID_DIMM_C2E1";
			gpios = <&smb_svc_pex_cpu2_led 21 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c2f2 {
			label = "LED_ID_DIMM_C2F2";
			gpios = <&smb_svc_pex_cpu2_led 22 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c2f1 {
			label = "LED_ID_DIMM_C2F1";
			gpios = <&smb_svc_pex_cpu2_led 23 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c2g2 {
			label = "LED_ID_DIMM_C2G2";
			gpios = <&smb_svc_pex_cpu2_led 24 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c2g1 {
			label = "LED_ID_DIMM_C2G1";
			gpios = <&smb_svc_pex_cpu2_led 25 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c2h2 {
			label = "LED_ID_DIMM_C2H2";
			gpios = <&smb_svc_pex_cpu2_led 26 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c2h1 {
			label = "LED_ID_DIMM_C2H1";
			gpios = <&smb_svc_pex_cpu2_led 27 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c2a2 {
			label = "LED_ID_DIMM_C2A2";
			gpios = <&smb_svc_pex_cpu2_led 28 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c2a1 {
			label = "LED_ID_DIMM_C2A1";
			gpios = <&smb_svc_pex_cpu2_led 29 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c2b2 {
			label = "LED_ID_DIMM_C2B2";
			gpios = <&smb_svc_pex_cpu2_led 30 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c2b1 {
			label = "LED_ID_DIMM_C2B1";
			gpios = <&smb_svc_pex_cpu2_led 31 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c2c2 {
			label = "LED_ID_DIMM_C2C2";
			gpios = <&smb_svc_pex_cpu2_led 32 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c2c1 {
			label = "LED_ID_DIMM_C2C1";
			gpios = <&smb_svc_pex_cpu2_led 33 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c2d2 {
			label = "LED_ID_DIMM_C2D2";
			gpios = <&smb_svc_pex_cpu2_led 34 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c2d1 {
			label = "LED_ID_DIMM_C2D1";
			gpios = <&smb_svc_pex_cpu2_led 35 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c3e2 {
			label = "LED_ID_DIMM_C3E2";
			gpios = <&smb_svc_pex_cpu3_led 20 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c3e1 {
			label = "LED_ID_DIMM_C3E1";
			gpios = <&smb_svc_pex_cpu3_led 21 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c3f2 {
			label = "LED_ID_DIMM_C3F2";
			gpios = <&smb_svc_pex_cpu3_led 22 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c3f1 {
			label = "LED_ID_DIMM_C3F1";
			gpios = <&smb_svc_pex_cpu3_led 23 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c3g2 {
			label = "LED_ID_DIMM_C3G2";
			gpios = <&smb_svc_pex_cpu3_led 24 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c3g1 {
			label = "LED_ID_DIMM_C3G1";
			gpios = <&smb_svc_pex_cpu3_led 25 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c3h2 {
			label = "LED_ID_DIMM_C3H2";
			gpios = <&smb_svc_pex_cpu3_led 26 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c3h1 {
			label = "LED_ID_DIMM_C3H1";
			gpios = <&smb_svc_pex_cpu3_led 27 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c3a2 {
			label = "LED_ID_DIMM_C3A2";
			gpios = <&smb_svc_pex_cpu3_led 28 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c3a1 {
			label = "LED_ID_DIMM_C3A1";
			gpios = <&smb_svc_pex_cpu3_led 29 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c3b2 {
			label = "LED_ID_DIMM_C3B2";
			gpios = <&smb_svc_pex_cpu3_led 30 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c3b1 {
			label = "LED_ID_DIMM_C3B1";
			gpios = <&smb_svc_pex_cpu3_led 31 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c3c2 {
			label = "LED_ID_DIMM_C3C2";
			gpios = <&smb_svc_pex_cpu3_led 32 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c3c1 {
			label = "LED_ID_DIMM_C3C1";
			gpios = <&smb_svc_pex_cpu3_led 33 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c3d2 {
			label = "LED_ID_DIMM_C3D2";
			gpios = <&smb_svc_pex_cpu3_led 34 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-c3d1 {
			label = "LED_ID_DIMM_C3D1";
			gpios = <&smb_svc_pex_cpu3_led 35 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-rssd01 {
			label = "LED_ID_RSSD01";
			gpios = <&smb_svc_pex_rssd01_16 0 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-rssd02 {
			label = "LED_ID_RSSD02";
			gpios = <&smb_svc_pex_rssd01_16 1 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-rssd03 {
			label = "LED_ID_RSSD03";
			gpios = <&smb_svc_pex_rssd01_16 2 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-rssd04 {
			label = "LED_ID_RSSD04";
			gpios = <&smb_svc_pex_rssd01_16 3 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-rssd05 {
			label = "LED_ID_RSSD05";
			gpios = <&smb_svc_pex_rssd01_16 4 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-rssd06 {
			label = "LED_ID_RSSD06";
			gpios = <&smb_svc_pex_rssd01_16 5 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-rssd07 {
			label = "LED_ID_RSSD07";
			gpios = <&smb_svc_pex_rssd01_16 6 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-rssd08 {
			label = "LED_ID_RSSD08";
			gpios = <&smb_svc_pex_rssd01_16 7 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-rssd09 {
			label = "LED_ID_RSSD09";
			gpios = <&smb_svc_pex_rssd01_16 8 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-rssd10 {
			label = "LED_ID_RSSD10";
			gpios = <&smb_svc_pex_rssd01_16 9 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-rssd11 {
			label = "LED_ID_RSSD11";
			gpios = <&smb_svc_pex_rssd01_16 10 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-rssd12 {
			label = "LED_ID_RSSD12";
			gpios = <&smb_svc_pex_rssd01_16 11 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-rssd13 {
			label = "LED_ID_RSSD13";
			gpios = <&smb_svc_pex_rssd01_16 12 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-rssd14 {
			label = "LED_ID_RSSD14";
			gpios = <&smb_svc_pex_rssd01_16 13 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-rssd15 {
			label = "LED_ID_RSSD15";
			gpios = <&smb_svc_pex_rssd01_16 14 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-rssd16 {
			label = "LED_ID_RSSD16";
			gpios = <&smb_svc_pex_rssd01_16 15 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-rssd17 {
			label = "LED_ID_RSSD17";
			gpios = <&smb_svc_pex_rssd17_32 0 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-rssd18 {
			label = "LED_ID_RSSD18";
			gpios = <&smb_svc_pex_rssd17_32 1 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-rssd19 {
			label = "LED_ID_RSSD19";
			gpios = <&smb_svc_pex_rssd17_32 2 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-rssd20 {
			label = "LED_ID_RSSD20";
			gpios = <&smb_svc_pex_rssd17_32 3 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-rssd21 {
			label = "LED_ID_RSSD21";
			gpios = <&smb_svc_pex_rssd17_32 4 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-rssd22 {
			label = "LED_ID_RSSD22";
			gpios = <&smb_svc_pex_rssd17_32 5 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-rssd23 {
			label = "LED_ID_RSSD23";
			gpios = <&smb_svc_pex_rssd17_32 6 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-rssd24 {
			label = "LED_ID_RSSD24";
			gpios = <&smb_svc_pex_rssd17_32 7 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-rssd25 {
			label = "LED_ID_RSSD25";
			gpios = <&smb_svc_pex_rssd17_32 8 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-rssd26 {
			label = "LED_ID_RSSD26";
			gpios = <&smb_svc_pex_rssd17_32 9 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-rssd27 {
			label = "LED_ID_RSSD27";
			gpios = <&smb_svc_pex_rssd17_32 10 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-rssd28 {
			label = "LED_ID_RSSD28";
			gpios = <&smb_svc_pex_rssd17_32 11 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-rssd29 {
			label = "LED_ID_RSSD29";
			gpios = <&smb_svc_pex_rssd17_32 12 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-rssd30 {
			label = "LED_ID_RSSD30";
			gpios = <&smb_svc_pex_rssd17_32 13 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-rssd31 {
			label = "LED_ID_RSSD31";
			gpios = <&smb_svc_pex_rssd17_32 14 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-dimm-rssd32 {
			label = "LED_ID_RSSD32";
			gpios = <&smb_svc_pex_rssd17_32 15 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-fan-asm01 {
			label = "LED_ID_FAN_ASM01";
			gpios = <&smb_svc_pex_rssd01_16 32 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-fan-asm02 {
			label = "LED_ID_FAN_ASM02";
			gpios = <&smb_svc_pex_rssd01_16 33 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-fan-asm03 {
			label = "LED_ID_FAN_ASM03";
			gpios = <&smb_svc_pex_rssd01_16 34 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-fan-asm04 {
			label = "LED_ID_FAN_ASM04";
			gpios = <&smb_svc_pex_rssd01_16 35 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-fan-asm05 {
			label = "LED_ID_FAN_ASM05";
			gpios = <&smb_svc_pex_rssd01_16 36 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-fan-asm06 {
			label = "LED_ID_FAN_ASM06";
			gpios = <&smb_svc_pex_rssd01_16 37 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-fan-asm07 {
			label = "LED_ID_FAN_ASM07";
			gpios = <&smb_svc_pex_rssd17_32 32 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-fan-asm08 {
			label = "LED_ID_FAN_ASM08";
			gpios = <&smb_svc_pex_rssd17_32 33 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-fan-asm09 {
			label = "LED_ID_FAN_ASM09";
			gpios = <&smb_svc_pex_rssd17_32 34 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-fan-asm10 {
			label = "LED_ID_FAN_ASM10";
			gpios = <&smb_svc_pex_rssd17_32 35 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-fan-asm11 {
			label = "LED_ID_FAN_ASM11";
			gpios = <&smb_svc_pex_rssd17_32 36 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};

		led-id-fan-asm12 {
			label = "LED_ID_FAN_ASM12";
			gpios = <&smb_svc_pex_rssd17_32 37 GPIO_ACTIVE_LOW>;
			color = <LED_COLOR_ID_YELLOW>;
		};
	};

	p12v: fixedregulator-p12v {
		compatible = "regulator-fixed";
		regulator-name = "p12v";
		regulator-min-microvolt = <12000000>;
		regulator-max-microvolt = <12000000>;
		regulator-always-on;
		regulator-boot-on;
	};

	p3v3_bmc_aux: fixedregulator-p3v3-bmc-aux {
		compatible = "regulator-fixed";
		regulator-name = "p3v3_bmc_aux";
		regulator-min-microvolt = <3300000>;
		regulator-max-microvolt = <3300000>;
		regulator-always-on;
		regulator-boot-on;
	};

	p1v8_bmc_aux: fixedregulator-p1v8-bmc-aux {
		compatible = "regulator-fixed";
		regulator-name = "p1v8_bmc_aux";
		regulator-min-microvolt = <1800000>;
		regulator-max-microvolt = <1800000>;
		regulator-always-on;
	};

	p1v2_bmc_aux: fixedregulator-p1v2-bmc-aux {
		compatible = "regulator-fixed";
		regulator-name = "p1v2_bmc_aux";
		regulator-min-microvolt = <1200000>;
		regulator-max-microvolt = <1200000>;
		regulator-always-on;
		regulator-boot-on;
	};

	p12v-a-consumer {
		compatible = "regulator-output";
		vout-supply = <&p12v_a>;
	};

	p12v-b-consumer {
		compatible = "regulator-output";
		vout-supply = <&p12v_b>;
	};

	p12v-c-consumer {
		compatible = "regulator-output";
		vout-supply = <&p12v_c>;
	};

	p12v-d-consumer {
		compatible = "regulator-output";
		vout-supply = <&p12v_d>;
	};

	pvccinfaon-cpu0-consumer {
		compatible = "regulator-output";
		vout-supply = <&pvccinfaon_cpu0>;
	};

	pvccfa-ehv-cpu0-consumer {
		compatible = "regulator-output";
		vout-supply = <&pvccfa_ehv_cpu0>;
	};

	pvnn-main-cpu0-consumer {
		compatible = "regulator-output";
		vout-supply = <&pvnn_main_cpu0>;
	};

	pvccin-cpu0-consumer {
		compatible = "regulator-output";
		vout-supply = <&pvccin_cpu0>;
	};

	pvccfa-ehv-fivra-cpu0-consumer {
		compatible = "regulator-output";
		vout-supply = <&pvccfa_ehv_fivra_cpu0>;
	};

	pvccd-hv-cpu0-consumer {
		compatible = "regulator-output";
		vout-supply = <&pvccd_hv_cpu0>;
	};

	pvpp-hbm-cpu0-consumer {
		compatible = "regulator-output";
		vout-supply = <&pvpp_hbm_cpu0>;
	};

	pvccinfaon-cpu1-consumer {
		compatible = "regulator-output";
		vout-supply = <&pvccinfaon_cpu1>;
	};

	pvccfa-ehv-cpu1-consumer {
		compatible = "regulator-output";
		vout-supply = <&pvccfa_ehv_cpu1>;
	};

	pvnn-main-cpu1-consumer {
		compatible = "regulator-output";
		vout-supply = <&pvnn_main_cpu1>;
	};

	pvccin-cpu1-consumer {
		compatible = "regulator-output";
		vout-supply = <&pvccin_cpu1>;
	};

	pvccfa-ehv-fivra-cpu1-consumer {
		compatible = "regulator-output";
		vout-supply = <&pvccfa_ehv_fivra_cpu1>;
	};

	pvccd-hv-cpu1-consumer {
		compatible = "regulator-output";
		vout-supply = <&pvccd_hv_cpu1>;
	};

	pvpp-hbm-cpu1-consumer {
		compatible = "regulator-output";
		vout-supply = <&pvpp_hbm_cpu1>;
	};

	pvccinfaon-cpu2-consumer {
		compatible = "regulator-output";
		vout-supply = <&pvccinfaon_cpu2>;
	};

	pvccfa-ehv-cpu2-consumer {
		compatible = "regulator-output";
		vout-supply = <&pvccfa_ehv_cpu2>;
	};

	pvnn-main-cpu2-consumer {
		compatible = "regulator-output";
		vout-supply = <&pvnn_main_cpu2>;
	};

	pvccin-cpu2-consumer {
		compatible = "regulator-output";
		vout-supply = <&pvccin_cpu2>;
	};

	pvccfa-ehv-fivra-cpu2-consumer {
		compatible = "regulator-output";
		vout-supply = <&pvccfa_ehv_fivra_cpu2>;
	};

	pvccd-hv-cpu2-consumer {
		compatible = "regulator-output";
		vout-supply = <&pvccd_hv_cpu2>;
	};

	pvpp-hbm-cpu2-consumer {
		compatible = "regulator-output";
		vout-supply = <&pvpp_hbm_cpu2>;
	};

	pvccinfaon-cpu3-consumer {
		compatible = "regulator-output";
		vout-supply = <&pvccinfaon_cpu3>;
	};

	pvccfa-ehv-cpu3-consumer {
		compatible = "regulator-output";
		vout-supply = <&pvccfa_ehv_cpu3>;
	};

	pvnn-main-cpu3-consumer {
		compatible = "regulator-output";
		vout-supply = <&pvnn_main_cpu3>;
	};

	pvccin-cpu3-consumer {
		compatible = "regulator-output";
		vout-supply = <&pvccin_cpu3>;
	};

	pvccfa-ehv-fivra-cpu3-consumer {
		compatible = "regulator-output";
		vout-supply = <&pvccfa_ehv_fivra_cpu3>;
	};

	pvccd-hv-cpu3-consumer {
		compatible = "regulator-output";
		vout-supply = <&pvccd_hv_cpu3>;
	};

	pvpp-hbm-cpu3-consumer {
		compatible = "regulator-output";
		vout-supply = <&pvpp_hbm_cpu3>;
	};

	p1v05-pch-aux-consumer {
		compatible = "regulator-output";
		vout-supply = <&p1v05_pch_aux>;
	};

	p1v8-pch-aux-consumer {
		compatible = "regulator-output";
		vout-supply = <&p1v8_pch_aux>;
	};

	p3v3-pch-consumer {
		compatible = "regulator-output";
		vout-supply = <&p3v3_pch>;
	};

	p5v-consumer {
		compatible = "regulator-output";
		vout-supply = <&p5v>;
	};

	smb-m2-ssb-ssd2 {
		compatible = "regulator-output";
		vout-supply = <&sw0_smb_m2_ssb_ssd2>;
	};

	smb-m2-ssb-ssd1 {
		compatible = "regulator-output";
		vout-supply = <&sw0_smb_m2_ssb_ssd1>;
	};

	ssb-rssd01-sw0 {
		compatible = "regulator-output";
		vout-supply = <&sw0_ssb_rssd01>;
	};

	ssb-rssd01-sw1 {
		compatible = "regulator-output";
		vout-supply = <&sw1_ssb_rssd01>;
	};

	ssb-rssd02-sw0 {
		compatible = "regulator-output";
		vout-supply = <&sw0_ssb_rssd02>;
	};

	ssb-rssd02-sw1 {
		compatible = "regulator-output";
		vout-supply = <&sw1_ssb_rssd02>;
	};

	ssb-rssd03-sw0 {
		compatible = "regulator-output";
		vout-supply = <&sw0_ssb_rssd03>;
	};

	ssb-rssd03-sw1 {
		compatible = "regulator-output";
		vout-supply = <&sw1_ssb_rssd03>;
	};

	ssb-rssd04-sw0 {
		compatible = "regulator-output";
		vout-supply = <&sw0_ssb_rssd04>;
	};

	ssb-rssd04-sw1 {
		compatible = "regulator-output";
		vout-supply = <&sw1_ssb_rssd04>;
	};

	ssb-rssd05-sw0 {
		compatible = "regulator-output";
		vout-supply = <&sw0_ssb_rssd05>;
	};

	ssb-rssd05-sw1 {
		compatible = "regulator-output";
		vout-supply = <&sw1_ssb_rssd05>;
	};

	ssb-rssd06-sw0 {
		compatible = "regulator-output";
		vout-supply = <&sw0_ssb_rssd06>;
	};

	ssb-rssd06-sw1 {
		compatible = "regulator-output";
		vout-supply = <&sw1_ssb_rssd06>;
	};

	ssb-rssd07-sw0 {
		compatible = "regulator-output";
		vout-supply = <&sw0_ssb_rssd07>;
	};

	ssb-rssd07-sw1 {
		compatible = "regulator-output";
		vout-supply = <&sw1_ssb_rssd07>;
	};

	ssb-rssd08-sw0 {
		compatible = "regulator-output";
		vout-supply = <&sw0_ssb_rssd08>;
	};

	ssb-rssd08-sw1 {
		compatible = "regulator-output";
		vout-supply = <&sw1_ssb_rssd08>;
	};

	ssb-rssd09-sw0 {
		compatible = "regulator-output";
		vout-supply = <&sw0_ssb_rssd09>;
	};

	ssb-rssd09-sw1 {
		compatible = "regulator-output";
		vout-supply = <&sw1_ssb_rssd09>;
	};

	ssb-rssd10-sw0 {
		compatible = "regulator-output";
		vout-supply = <&sw0_ssb_rssd10>;
	};

	ssb-rssd10-sw1 {
		compatible = "regulator-output";
		vout-supply = <&sw1_ssb_rssd10>;
	};

	ssb-rssd11-sw0 {
		compatible = "regulator-output";
		vout-supply = <&sw0_ssb_rssd11>;
	};

	ssb-rssd11-sw1 {
		compatible = "regulator-output";
		vout-supply = <&sw1_ssb_rssd11>;
	};

	ssb-rssd12-sw0 {
		compatible = "regulator-output";
		vout-supply = <&sw0_ssb_rssd12>;
	};

	ssb-rssd12-sw1 {
		compatible = "regulator-output";
		vout-supply = <&sw1_ssb_rssd12>;
	};

	ssb-rssd13-sw0 {
		compatible = "regulator-output";
		vout-supply = <&sw0_ssb_rssd13>;
	};

	ssb-rssd13-sw1 {
		compatible = "regulator-output";
		vout-supply = <&sw1_ssb_rssd13>;
	};

	ssb-rssd14-sw0 {
		compatible = "regulator-output";
		vout-supply = <&sw0_ssb_rssd14>;
	};

	ssb-rssd14-sw1 {
		compatible = "regulator-output";
		vout-supply = <&sw1_ssb_rssd14>;
	};

	ssb-rssd15-sw0 {
		compatible = "regulator-output";
		vout-supply = <&sw0_ssb_rssd15>;
	};

	ssb-rssd15-sw1 {
		compatible = "regulator-output";
		vout-supply = <&sw1_ssb_rssd15>;
	};

	ssb-rssd16-sw0 {
		compatible = "regulator-output";
		vout-supply = <&sw0_ssb_rssd16>;
	};

	ssb-rssd16-sw1 {
		compatible = "regulator-output";
		vout-supply = <&sw1_ssb_rssd16>;
	};

	ssb-rssd17-sw0 {
		compatible = "regulator-output";
		vout-supply = <&sw0_ssb_rssd17>;
	};

	ssb-rssd17-sw1 {
		compatible = "regulator-output";
		vout-supply = <&sw1_ssb_rssd17>;
	};

	ssb-rssd18-sw0 {
		compatible = "regulator-output";
		vout-supply = <&sw0_ssb_rssd18>;
	};

	ssb-rssd18-sw1 {
		compatible = "regulator-output";
		vout-supply = <&sw1_ssb_rssd18>;
	};

	ssb-rssd19-sw0 {
		compatible = "regulator-output";
		vout-supply = <&sw0_ssb_rssd19>;
	};

	ssb-rssd19-sw1 {
		compatible = "regulator-output";
		vout-supply = <&sw1_ssb_rssd19>;
	};

	ssb-rssd20-sw0 {
		compatible = "regulator-output";
		vout-supply = <&sw0_ssb_rssd20>;
	};

	ssb-rssd20-sw1 {
		compatible = "regulator-output";
		vout-supply = <&sw1_ssb_rssd20>;
	};

	ssb-rssd21-sw0 {
		compatible = "regulator-output";
		vout-supply = <&sw0_ssb_rssd21>;
	};

	ssb-rssd21-sw1 {
		compatible = "regulator-output";
		vout-supply = <&sw1_ssb_rssd21>;
	};

	ssb-rssd22-sw0 {
		compatible = "regulator-output";
		vout-supply = <&sw0_ssb_rssd22>;
	};

	ssb-rssd22-sw1 {
		compatible = "regulator-output";
		vout-supply = <&sw1_ssb_rssd22>;
	};

	ssb-rssd23-sw0 {
		compatible = "regulator-output";
		vout-supply = <&sw0_ssb_rssd23>;
	};

	ssb-rssd23-sw1 {
		compatible = "regulator-output";
		vout-supply = <&sw1_ssb_rssd23>;
	};

	ssb-rssd24-sw0 {
		compatible = "regulator-output";
		vout-supply = <&sw0_ssb_rssd24>;
	};

	ssb-rssd24-sw1 {
		compatible = "regulator-output";
		vout-supply = <&sw1_ssb_rssd24>;
	};

	ssb-rssd25-sw0 {
		compatible = "regulator-output";
		vout-supply = <&sw0_ssb_rssd25>;
	};

	ssb-rssd25-sw1 {
		compatible = "regulator-output";
		vout-supply = <&sw1_ssb_rssd25>;
	};

	ssb-rssd26-sw0 {
		compatible = "regulator-output";
		vout-supply = <&sw0_ssb_rssd26>;
	};

	ssb-rssd26-sw1 {
		compatible = "regulator-output";
		vout-supply = <&sw1_ssb_rssd26>;
	};

	ssb-rssd27-sw0 {
		compatible = "regulator-output";
		vout-supply = <&sw0_ssb_rssd27>;
	};

	ssb-rssd27-sw1 {
		compatible = "regulator-output";
		vout-supply = <&sw1_ssb_rssd27>;
	};

	ssb-rssd28-sw0 {
		compatible = "regulator-output";
		vout-supply = <&sw0_ssb_rssd28>;
	};

	ssb-rssd28-sw1 {
		compatible = "regulator-output";
		vout-supply = <&sw1_ssb_rssd28>;
	};

	ssb-rssd29-sw0 {
		compatible = "regulator-output";
		vout-supply = <&sw0_ssb_rssd29>;
	};

	ssb-rssd29-sw1 {
		compatible = "regulator-output";
		vout-supply = <&sw1_ssb_rssd29>;
	};

	ssb-rssd30-sw0 {
		compatible = "regulator-output";
		vout-supply = <&sw0_ssb_rssd30>;
	};

	ssb-rssd30-sw1 {
		compatible = "regulator-output";
		vout-supply = <&sw1_ssb_rssd30>;
	};

	ssb-rssd31-sw0 {
		compatible = "regulator-output";
		vout-supply = <&sw0_ssb_rssd31>;
	};

	ssb-rssd31-sw1 {
		compatible = "regulator-output";
		vout-supply = <&sw1_ssb_rssd31>;
	};

	ssb-rssd32-sw0 {
		compatible = "regulator-output";
		vout-supply = <&sw0_ssb_rssd32>;
	};

	ssb-rssd32-sw1 {
		compatible = "regulator-output";
		vout-supply = <&sw1_ssb_rssd32>;
	};

	p3v3-nic-consumer {
		compatible = "regulator-output";
		vout-supply = <&p3v3_nic>;
	};

	p1v8-nic-consumer {
		compatible = "regulator-output";
		vout-supply = <&p1v8_nic>;
	};

	p1v2-nic-consumer {
		compatible = "regulator-output";
		vout-supply = <&p1v2_nic>;
	};

	pvcore-nic1-consumer {
		compatible = "regulator-output";
		vout-supply = <&pvcore_nic1>;
	};

	pvcore-nic2-consumer {
		compatible = "regulator-output";
		vout-supply = <&pvcore_nic2>;
	};
};

&lpc_snoop {
	status = "okay";
	snoop-ports = <0x80>, <0x81>;
};

&fmc {
	status = "okay";
	flash@0 {
		status = "okay";
		m25p,fast-read;
		label = "bmc";
		spi-tx-bus-width = <1>;
		spi-rx-bus-width = <4>;
	};

	flash@1 {
		status = "okay";
		m25p,fast-read;
		label = "alt-bmc";
		spi-tx-bus-width = <1>;
		spi-rx-bus-width = <4>;
	};
};

&uart1 {
	bootph-all;
	status = "okay";
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_txd1_default
			&pinctrl_rxd1_default
			&pinctrl_nrts1_default
			&pinctrl_ndtr1_default
			&pinctrl_ndsr1_default
			&pinctrl_ncts1_default
			&pinctrl_ndcd1_default
			&pinctrl_nri1_default>;
};

&uart5 {
	status = "disabled";
};

&mdio {
	status = "okay";
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_mdio3_default &pinctrl_mdio4_default>;
};

&gpio1 {
	status = "disabled";
};

&pinctrl {
	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_vgahs_default &pinctrl_vgavs_default>;
};

&mac0 {
	status = "disabled";
};

&mac1 {
	status = "disabled";
};

&mac2 {
	status = "okay";

	phy-mode = "rgmii";

	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_rgmii3_default>;
};

&mac3 {
	status = "okay";

	phy-mode = "rgmii";

	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_rgmii4_default>;
};

&kcs3 {
	status = "okay";
	aspeed,lpc-io-reg = <0xca2>;
};

&gpio0 {
	status = "okay";

	gpio-line-names =
	/* A0 - A7 */
	"", "", "", "", "", "", "", "",
	/* B0 - B7 */
	"", "", "FM_ADR_TRIGGER_R_N", "RST_PLTRST_BUF_N", "BMC_TPM_RESET_N", "BMC_TPM_IRQ_N",
	"PCH_TPM_RESET_N", "PCH_TPM_IRQ_N",
	/* C0 - C7 */
	"", "", "", "", "", "", "", "",
	/* D0 - D7 */
	"", "", "", "", "", "", "", "",
	/* E0 - E7 */
	"", "", "", "", "", "", "", "",
	/* F0 - F7 */
	"", "", "", "BMC_MUX_CPU1_RST_INT_N", "BMC_MUX_CPU2_RST_INT_N", "", "", "",
	/* G0 - G7 */
	"FM_SSD_CLK_DRVR1_EN", "FM_CK440Q_DEV_EN", "BMC_MAC1_RESET_N", "FM_DB2000_DEV_EN",
	"FM_CPU_RMCA_LVT3_N", "FM_CPU_CATERR_LVT3_N", "FM_DBP_PRESENT_N", "",
	/* H0 - H7 */
	"SMB_SVC_PEX_RSSD17_32_INT", "LED_BMC_RDY", "RST_DBP_N", "", "", "", "", "",
	/* I0 - I7 */
	"JTAG_MUX_MODE_SEL", "JTAG_MUX_TRANS_ENBL", "JTAG_MUX_LSP_SEL5", "JTAG_MUX_MSTR_SEL",
	"JTAG_MUX_LSP_SEL3", "", "JTAG_MUX_ENBL_N", "JTAG_MUX_RST_N",
	/* J0 - J7 */
	"", "", "", "", "", "", "", "",
	/* K0 - K7 */
	"", "", "", "", "", "", "", "",
	/* L0 - L7 */
	"", "", "", "", "RST_RTCRST_N", "RST_SRTCRST_N", "", "",
	/* M0 - M7 */
	"BMC_UART1_CTS_N", "BMC_UART1_DCD_N", "BMC_UART1_DSR_N", "BMC_UART1_RI_N",
	"BMC_UART1_DTR_N", "BMC_UART1_RTS_N", "", "",
	/* N0 - N7 */
	"IRQ_BMC_PCH_NMI", "", "FM_PCH_BMC_THERMTRIP_N", "FM_BIOS_POST_CMPLT_N", "RST_PLTRST_N",
	"FM_FLASH_SEC_OVRD", "FM_SMI_ACTIVE_N", "PWRGD_DBP",
	/* O0 - O7 */
	"CATERR_CPU2_EN", "H_LVT1_THERMTRIP_N", "CATERR_CPU3_EN", "SMB_SVC_PEX_CPU0_LED_INT",
	"H_LVT1_MEMTRIP_N", "", "CATERR_CPU1_EN", "FM_PCH_ADR_COMPLETE_N",
	/* P0 - P7 */
	"PWRGD_SYS_PWROK", "PWRGD_PCH_PWROK", "BMC_MUX_CPU3_RST_INT_N", "BMC_MUX_SVC_RSSD_INT",
	"FM_SLPS4_N", "IRQ_SML0_ALERT_N", "FM_SLPS3_N", "LED_BMC_HB",
	/* Q0 - Q7 */
	"", "PEX_BMC_RST", "PEX_VR_CTRL_RST", "PEX_NIC_RST", "PEX_CPU0_LED_RST", "PEX_CPU1_LED_RST",
	"PEX_CPU2_LED_RST", "PEX_CPU3_LED_RST",
	/* R0 - R7 */
	"BMC_MUX_FANSSB_RSSD17_32_RST_INT_N", "BMC_MUX_FANPWM_RSSD01_16_RST_INT_N",
	"BMC_MUX_SVC_VR_RST_INT_N", "BMC_MUX_NIC_RST_INT_N", "BMC_MUX_SVC_EXP_RST_INT_N",
	"FM_CPU_ERR2_LVT3_N", "BMC_MUX_CPU0_RST_INT_N", "BMC_MUX_M2_RST_INT_N",
	/* S0 - S7 */
	"SMB_SVC_PEX_RSSD01_16_INT", "RST_PCH_RSMRST_R_N", "", "", "BMC_ROT_FPGA_RESET_N",
	"FM_SSD_CLK_DRVR0_EN", "", "",
	/* T0 - T7 */
	"", "", "", "", "", "", "", "",
	/* U0 - U7 */
	"", "", "", "", "", "", "", "",
	/* V0 - V7 */
	"BMC_PEX_IRQ_INT", "RTC_BATT_TEST", "SMB_PEX_VR_CTRL_INT", "SMB_SVC_PEX_CPU3_LED_INT",
	"PWRGD_CPUPWRGD", "SMB_SVC_PEX_CPU2_LED_INT", "SMB_SVC_PEX_CPU1_LED_INT",
	"BMC_MAC0_RESET_N",
	/* W0 - W7 */
	"", "", "", "", "", "", "", "",
	/* X0 - X7 */
	"", "", "", "", "", "", "", "",
	/* Y0 - Y7 */
	"FM_THROTTLE_N", "FM_PASSWORD_CLEAR_N", "H_LVT3_CATERR_DLY_N", "FM_CPU_OL_INT_R_N", "", "",
	"", "",
	/* Z0 - Z7 */
	"FM_CPU_ERR0_LVT3_N", "FM_CPU_ERR1_LVT3_N", "BMC_MUX_VR_PCH_CPU_RST_INT_N",
	"JTAG_MUX_LSP_SEL1", "", "JTAG_MUX_LSP_SEL4", "JTAG_MUX_LSP_SEL2", "";

	pinctrl-names = "default";
	pinctrl-0 = <&pinctrl_gpio0_unbiased_default>;

	line_50 {
		gpio-hog;
		gpios = <50 GPIO_ACTIVE_LOW>;
		output-low;
		line-name = "BMC_MAC1_RESET_N";
	};
	line_175 {
		gpio-hog;
		gpios = <175 GPIO_ACTIVE_LOW>;
		output-low;
		line-name = "BMC_MAC0_RESET_N";
	};

};

&pinctrl {
	pinctrl_gpio0_unbiased_default: gpio_default {
		pins = "AB15", "AD14", "R23", "A18", "AD24", "AD15", "AE14", "AC15", "U25", "AA24",
		       "V24", "W26", "AA23", "V26", "U24", "V25", "AE15", "C15", "F15";
		bias-disable;
	};
};

&i2c1 {
	status = "okay";

	bmc_mux_nic: mux@77 {
		compatible = "maxim,max7357";
		reg = <0x77>;
		#address-cells = <1>;
		#size-cells = <0>;
		reset-gpios = <&gpio0 ASPEED_GPIO(R, 3) (GPIO_ACTIVE_LOW | GPIO_OPEN_DRAIN)>;
		vdd-supply = <&p3v3_aux>;

		i2c@0 {
			reg = <0>;
			#address-cells = <1>;
			#size-cells = <0>;

			smb_pex_nic: pinctrl@20 {
				compatible = "cypress,cy8c9540";
				reg = <0x20>;
				gpio-controller;
				#gpio-cells = <2>;

				interrupt-parent = <&smb_pex_vr_ctrl>;
				interrupts = <8 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-controller;
				#interrupt-cells = <2>;

				vdd-supply = <&p3v3_aux>;
				reset-gpios = <&gpio0 ASPEED_GPIO(Q, 3) GPIO_ACTIVE_HIGH>;

				gpio-reserved-ranges = <19 1>, <22 6>, <30 6>, <38 2>;

				gpio-line-names =
				/* GPORT0 */
				"IRQ_NIC2_OVT_WRNG", "FM_NIC2_ALLSTANDBY_N", "IRQ_NIC2_OVT_SHTDN",
				"SMB_VR_PVCORE_NIC2_ALERT_N", "FM_NIC2_PERST1_N",
				"SMB_NIC2_ALERT_N", "FM_NIC2_PERST3_N", "FM_NIC2_PERST2_N",
				/* GPORT1 */
				"FM_NIC1_RST_N", "FM_NIC1_PERST0_N", "FM_NIC1_PERST2_N",
				"FM_NIC1_PERST3_N", "SMB_NIC1_ALERT_N", "FM_NIC1_PERST1_N",
				"SMB_VR_PVCORE_NIC1_ALERT_N", "IRQ_NIC1_OVT_SHTDN",
				/* GPORT2 */
				"SMB_VR_P3V3_NIC_ALERT_N", "FM_NIC2_FLASH_PRSNT",
				"FM_NIC1_FLASH_PRSNT", "",
				/* GPORT3 */
				"FM_NIC2_PERST0_N", "FM_NIC2_RST_N", "", "", "", "", "", "",
				/* GPORT4 */
				"FM_NIC1_ALLSTANDBY_N", "IRQ_NIC1_OVT_WRNG", "", "", "", "", "", "",
				/* GPORT5 */
				"SMB_VR_P1V8_NIC_ALERT_N", "SMB_VR_P1V2_NIC_ALERT_N", "", "";

				pinctrl-0 = <&U62160_pins>;
				pinctrl-names = "default";
				U62160_pins: cfg-pins {
					pins = "gp03", "gp16", "gp20", "gp50", "gp51";
					function = "gpio";
					input-enable;
					bias-pull-up;
				};
			};
		};

		i2c@1 {
			reg = <1>;
			#address-cells = <1>;
			#size-cells = <0>;
		};

		i2c@2 {
			reg = <2>;
			#address-cells = <1>;
			#size-cells = <0>;

			pvcore_nic2: ir38263-pvcore-nic2@40 {
				compatible = "infineon,ir38263";
				reg = <0x40>;

				regulator-name = "pvcore_nic2";
				regulator-enable-ramp-delay = <2000>;
				vin-supply = <&p12v>;
			};
		};

		i2c@3 {
			reg = <3>;
			#address-cells = <1>;
			#size-cells = <0>;

			pvcore_nic1: ir38263-pvcore-nic1@40 {
				compatible = "infineon,ir38263";
				reg = <0x40>;

				regulator-name = "pvcore_nic1";
				regulator-enable-ramp-delay = <2000>;
				vin-supply = <&p12v>;
			};
		};

		i2c@4 {
			reg = <4>;
			#address-cells = <1>;
			#size-cells = <0>;
		};

		i2c@5 {
			reg = <5>;
			#address-cells = <1>;
			#size-cells = <0>;

			p3v3_nic: ir38263-p3v3-nic@40 {
				compatible = "infineon,ir38263";
				reg = <0x40>;

				regulator-name = "p3v3_nic";
				regulator-enable-ramp-delay = <2000>;
				vin-supply = <&p12v>;
			};
		};

		i2c@6 {
			reg = <6>;
			#address-cells = <1>;
			#size-cells = <0>;

			p1v2_nic: ir38263-p1v2-nic@40 {
				compatible = "infineon,ir38263";
				reg = <0x40>;

				regulator-name = "p1v2_nic";
				regulator-enable-ramp-delay = <2000>;
				vin-supply = <&p12v>;
			};
		};

		i2c@7 {
			reg = <7>;
			#address-cells = <1>;
			#size-cells = <0>;

			p1v8_nic: ir38263-p1v8-nic@40 {
				compatible = "infineon,ir38263";
				reg = <0x40>;

				regulator-name = "p1v8_nic";
				regulator-enable-ramp-delay = <2000>;
				vin-supply = <&p12v>;
			};
		};
	};
};

&i2c2 {
	status = "okay";
};

&i2c3 {
	status = "okay";

	i2cmux1: mux@77 {
		compatible = "maxim,max7357";
		reg = <0x77>;
		#address-cells = <1>;
		#size-cells = <0>;

		reset-gpios = <&gpio0 ASPEED_GPIO(R, 7) (GPIO_ACTIVE_LOW | GPIO_OPEN_DRAIN)>;
		vdd-supply = <&p3v3_aux>;

		i2c@0 {
			reg = <0>;
			#address-cells = <1>;
			#size-cells = <0>;
		};

		i2c@1 {
			reg = <1>;
			#address-cells = <1>;
			#size-cells = <0>;
		};

		i2c@2 {
			reg = <2>;
			#address-cells = <1>;
			#size-cells = <0>;
		};

		i2c@3 {
			reg = <3>;
			#address-cells = <1>;
			#size-cells = <0>;

			smb_m2_ssb_ssd1: regulator@3a {
				compatible = "maxim,max5978";
				reg = <0x3a>;
				vss1-supply = <&p3v3_aux>;

				interrupt-parent = <&smb_pex_vr_ctrl>;
				interrupts = <30 IRQ_TYPE_LEVEL_LOW>;
				leds {
					#address-cells = <1>;
					#size-cells = <0>;

					led@0 {
						reg = <0>;
						label = "m2_ssb_ssd1:green:power";
						default-state = "off";
					};
				};

				regulators {
					sw0_smb_m2_ssb_ssd1: sw0 {
						shunt-resistor-micro-ohms = <12000>;
						regulator-over-current-protection;
						regulator-oc-protection-microamp = <2800000>;
						regulator-name = "p3v3_m2_ssd1";
						regulator-enable-ramp-delay = <10000>;
					};
				};
			};
		};

		i2c@4 {
			reg = <4>;
			#address-cells = <1>;
			#size-cells = <0>;
		};

		i2c@5 {
			reg = <5>;
			#address-cells = <1>;
			#size-cells = <0>;

			smb_m2_ssb_ssd2: regulator@3a {
				compatible = "maxim,max5978";
				reg = <0x3a>;

				interrupt-parent = <&smb_pex_vr_ctrl>;
				interrupts = <39 IRQ_TYPE_LEVEL_LOW>;
				vss1-supply = <&p3v3_aux>;
				leds {
					#address-cells = <1>;
					#size-cells = <0>;

					led@0 {
						reg = <0>;
						label = "m2_ssb_ssd2:green:power";
						default-state = "off";
					};
				};

				regulators {
					sw0_smb_m2_ssb_ssd2: sw0 {
						shunt-resistor-micro-ohms = <12000>;
						regulator-over-current-protection;
						regulator-oc-protection-microamp = <2800000>;
						regulator-name = "p3v3_m2_ssd2";
						regulator-enable-ramp-delay = <10000>;
					};
				};
			};
		};

		i2c@6 {
			reg = <1>;
			#address-cells = <1>;
			#size-cells = <0>;
		};

		i2c@7 {
			reg = <1>;
			#address-cells = <1>;
			#size-cells = <0>;
		};
	};
};

&i2c4 {
	status = "okay";
	multi-master;
	bus-frequency = <1000000>;

	bmc-slave@10 {
		compatible = "ipmb-dev";
		reg = <(0x10 | I2C_OWN_SLAVE_ADDRESS)>;

		i2c-protocol;
	};
};

&i2c5 {
	status = "okay";

	i2cmux2: mux@77 {
		compatible = "maxim,max7357";
		reg = <0x77>;
		#address-cells = <1>;
		#size-cells = <0>;

		reset-gpios = <&gpio0 ASPEED_GPIO(Z, 2) (GPIO_ACTIVE_LOW | GPIO_OPEN_DRAIN)>;
		vdd-supply = <&p3v3_aux>;

		i2c@1 {
			reg = <1>;
			#address-cells = <1>;
			#size-cells = <0>;

			p1v05_pch_aux: ir38263-p1v05-pch-aux@40 {
				compatible = "infineon,ir38263";
				reg = <0x40>;

				regulator-name = "p1v05_pch_aux";
				regulator-enable-ramp-delay = <2000>;
				vin-supply = <&p12v>;
			};
		};

		i2c@2 {
			reg = <2>;
			#address-cells = <1>;
			#size-cells = <0>;

			p1v8_pch_aux: ir38060-p1v8-pch-aux@40 {
				compatible = "infineon,ir38060";
				reg = <0x40>;

				regulator-name = "p1v8_pch_aux";
				regulator-enable-ramp-delay = <2000>;
				vin-supply = <&p12v>;
			};
		};

		i2c@4 {
			reg = <4>;
			#address-cells = <1>;
			#size-cells = <0>;
		};

		i2c@5 {
			reg = <5>;
			#address-cells = <1>;
			#size-cells = <0>;
		};

		i2c@6 {
			reg = <6>;
			#address-cells = <1>;
			#size-cells = <0>;
		};

		i2c@7 {
			reg = <7>;
			#address-cells = <1>;
			#size-cells = <0>;
		};
	};
};

&i2c14 {
	status = "okay";

	i2cmux13: mux@77 {
		compatible = "maxim,max7357";
		reg = <0x77>;
		#address-cells = <1>;
		#size-cells = <0>;

		reset-gpios = <&gpio0 ASPEED_GPIO(R, 6) (GPIO_ACTIVE_LOW | GPIO_OPEN_DRAIN)>;
		vdd-supply = <&p3v3_aux>;

		i2c@0 {
			reg = <0>;
			#address-cells = <1>;
			#size-cells = <0>;

			smb_pex_cpu0_event: pinctrl@20 {
				compatible = "cypress,cy8c9540";
				reg = <0x20>;
				gpio-controller;
				#gpio-cells = <2>;

				interrupt-parent = <&smb_pex_vr_ctrl>;
				interrupts = <10 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-controller;
				#interrupt-cells = <2>;

				vdd-supply = <&p3v3_aux>;
				reset-gpios = <&smb_svc_pex_cpu0_led 16 GPIO_ACTIVE_HIGH>;

				gpio-reserved-ranges = <14 2>, <21 1>, <25 3>, <33 1>;

				gpio-line-names =
				/* GPORT0 */
				"PWRGD_CHD_CPU0", "PWRGD_CHC_CPU0",
				"PWRGD_CHB_CPU0", "PWRGD_CHA_CPU0",
				"PWRGD_CHE_CPU0", "PWRGD_CHF_CPU0",
				"PWRGD_CHG_CPU0", "PWRGD_CHH_CPU0",
				/* GPORT1 */
				"SMB_VR_PVPP_HBM_CPU0_ALERT_N", "SMB_VR_PVCCINFAON_CPU0_ALERT_N",
				"SMB_VR_PVNN_MAIN_CPU0_ALERT_N", "SMB_VR_PVCCD_HV_CPU0_ALERT_N",
				"SMB_VR_PVCCIN_CPU0_ALERT_N", "SEL_SMB_DIMM_CPU0",
				"", "",
				/* GPORT2 */
				"PWRGD_LVC3_CPU0_AB_DRAM_G", "PWRGD_LVC3_CPU0_CD_DRAM_G",
				"PWRGD_LVC3_CPU0_EF_DRAM_G", "PWRGD_LVC3_CPU0_GH_DRAM_G",
				/* GPORT3 */
				"FM_CPU0_DISABLE_COD_N", "",
				"RST_LVC3_CPU0_RESET_N", "PWRGD_LVC3_CPU0_PWRGOOD",
				"PWRGD_PLT_AUX_CPU0_LVT3", "",
				"", "",
				/* GPORT4 */
				"H_LVT3_CPU0_PROCHOT_N", "H_LVT3_CPU0_MEMHOT_IN_N",
				"H_LVT3_CPU0_MEMHOT_OUT_N", "H_LVT3_CPU0_MEMTRIP_OUT_N",
				"H_LVT3_CPU0_THERMTRIP_OUT_N", "",
				"H_LVT3_CPU0_NMI", "FM_S3M_CPU0_CD_INIT_ERROR",
				/* GPORT5 */
				"FM_CPU0_PKG_ID0", "FM_CPU0_PKG_ID1",
				"FM_CPU0_PROC_ID0", "FM_CPU0_PROC_ID1";

				pinctrl-0 = <&U62080_pins>;
				pinctrl-names = "default";
				U62080_pins: cfg-pins {
					pins = "gp10", "gp11", "gp12", "gp13", "gp14";
					function = "gpio";
					input-enable;
					bias-pull-up;
				};
			};
		};

		i2c@1 {
			reg = <1>;
			#address-cells = <1>;
			#size-cells = <0>;
		};

		i2c@2 {
			reg = <2>;
			#address-cells = <1>;
			#size-cells = <0>;

			pvccinfaon-pvccfa-cpu0@58 {
				compatible = "mps,mp2971";
				reg = <0x58>;
				interrupt-parent = <&smb_pex_cpu0_event>;
				interrupts = <9 IRQ_TYPE_LEVEL_LOW>;

				regulators {
					pvccinfaon_cpu0: vout0 {
						regulator-name = "pvccinfaon_cpu0";
						regulator-enable-ramp-delay = <200>;
					};
					pvccfa_ehv_cpu0: vout1 {
						regulator-name = "pvccfa_ehv_cpu0";
						regulator-enable-ramp-delay = <200>;
					};
				};
			};
			tda38640-pvnn-main-cpu0@40 {
				compatible = "infineon,tda38640";
				reg = <0x40>;
				interrupt-parent = <&smb_pex_cpu0_event>;
				interrupts = <10 IRQ_TYPE_LEVEL_LOW>;

				regulators {
					pvnn_main_cpu0: vout {
						regulator-name = "pvnn_main_cpu0";
						regulator-enable-ramp-delay = <200>;
					};
				};
			};
		};

		i2c@3 {
			reg = <3>;
			#address-cells = <1>;
			#size-cells = <0>;

			mp2973-pvccin-pvccfa-cpu0@58 {
				compatible = "mps,mp2973";
				reg = <0x58>;
				interrupt-parent = <&smb_pex_cpu0_event>;
				interrupts = <12 IRQ_TYPE_LEVEL_LOW>;

				regulators {
					pvccin_cpu0: vout0 {
						regulator-name = "pvccin_cpu0";
						regulator-enable-ramp-delay = <200>;
					};
					pvccfa_ehv_fivra_cpu0: vout1 {
						regulator-name = "pvccfa_ehv_fivra_cpu0";
						regulator-enable-ramp-delay = <200>;
					};
				};
			};
		};

		i2c@4 {
			reg = <4>;
			#address-cells = <1>;
			#size-cells = <0>;

			tda38640-pvccd-hv-cpu0@40 {
				compatible = "infineon,tda38640";
				reg = <0x40>;
				interrupt-parent = <&smb_pex_cpu0_event>;
				interrupts = <11 IRQ_TYPE_LEVEL_LOW>;
				infineon,en-pin-fixed-level;

				regulators {
					pvccd_hv_cpu0: vout {
						regulator-name = "pvccd_hv_cpu0";
						regulator-enable-ramp-delay = <200>;
					};
				};
			};
		};

		i2c@5 {
			reg = <5>;
			#address-cells = <1>;
			#size-cells = <0>;

			tda38640-pvpp-hbm-cpu0@40 {
				compatible = "infineon,tda38640";
				reg = <0x40>;
				interrupt-parent = <&smb_pex_cpu0_event>;
				interrupts = <8 IRQ_TYPE_LEVEL_LOW>;

				regulators {
					pvpp_hbm_cpu0: vout {
						regulator-name = "pvpp_hbm_cpu0";
						regulator-enable-ramp-delay = <200>;
					};
				};
			};
		};

		i2c@6 {
			reg = <6>;
			#address-cells = <1>;
			#size-cells = <0>;
		};

		i2c@7 {
			reg = <7>;
			#address-cells = <1>;
			#size-cells = <0>;
		};
	};
};

&i2c7 {
	status = "okay";

	i2cmux4: mux@77 {
		compatible = "maxim,max7357";
		reg = <0x77>;
		#address-cells = <1>;
		#size-cells = <0>;

		reset-gpios = <&gpio0 ASPEED_GPIO(F, 3) (GPIO_ACTIVE_LOW | GPIO_OPEN_DRAIN)>;
		vdd-supply = <&p3v3_aux>;

		i2c@0 {
			reg = <0>;
			#address-cells = <1>;
			#size-cells = <0>;

			smb_pex_cpu1_event: pinctrl@20 {
				compatible = "cypress,cy8c9540";
				reg = <0x20>;
				gpio-controller;
				#gpio-cells = <2>;

				interrupt-parent = <&smb_pex_vr_ctrl>;
				interrupts = <2 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-controller;
				#interrupt-cells = <2>;

				vdd-supply = <&p3v3_aux>;
				reset-gpios = <&smb_svc_pex_cpu1_led 16 GPIO_ACTIVE_HIGH>;

				gpio-reserved-ranges = <14 2>, <21 1>, <25 3>, <33 1>;

				gpio-line-names =
				/* GPORT0 */
				"PWRGD_CHD_CPU1", "PWRGD_CHC_CPU1",
				"PWRGD_CHB_CPU1", "PWRGD_CHA_CPU1",
				"PWRGD_CHE_CPU1", "PWRGD_CHF_CPU1",
				"PWRGD_CHG_CPU1", "PWRGD_CHH_CPU1",
				/* GPORT1 */
				"SMB_VR_PVPP_HBM_CPU1_ALERT_N", "SMB_VR_PVCCINFAON_CPU1_ALERT_N",
				"SMB_VR_PVNN_MAIN_CPU1_ALERT_N", "SMB_VR_PVCCD_HV_CPU1_ALERT_N",
				"SMB_VR_PVCCIN_CPU1_ALERT_N", "SEL_SMB_DIMM_CPU1",
				"", "",
				/* GPORT2 */
				"PWRGD_LVC3_CPU1_AB_DRAM_G", "PWRGD_LVC3_CPU1_CD_DRAM_G",
				"PWRGD_LVC3_CPU1_EF_DRAM_G", "PWRGD_LVC3_CPU1_GH_DRAM_G",
				/* GPORT3 */
				"FM_CPU1_DISABLE_COD_N", "",
				"RST_LVC3_CPU1_RESET_N", "PWRGD_LVC3_CPU1_PWRGOOD",
				"PWRGD_PLT_AUX_CPU1_LVT3", "",
				"", "",
				/* GPORT4 */
				"H_LVT3_CPU1_PROCHOT_N", "H_LVT3_CPU1_MEMHOT_IN_N",
				"H_LVT3_CPU1_MEMHOT_OUT_N", "H_LVT3_CPU1_MEMTRIP_OUT_N",
				"H_LVT3_CPU1_THERMTRIP_OUT_N", "",
				"H_LVT3_CPU1_NMI", "FM_S3M_CPU1_CD_INIT_ERROR",
				/* GPORT5 */
				"FM_CPU1_PKG_ID0", "FM_CPU1_PKG_ID1",
				"FM_CPU1_PROC_ID0", "FM_CPU1_PROC_ID1";

				pinctrl-0 = <&U62090_pins>;
				pinctrl-names = "default";
				U62090_pins: cfg-pins {
					pins = "gp10", "gp11", "gp12", "gp13", "gp14";
					function = "gpio";
					input-enable;
					bias-pull-up;
				};
			};
		};

		i2c@1 {
			reg = <1>;
			#address-cells = <1>;
			#size-cells = <0>;
		};

		i2c@2 {
			reg = <2>;
			#address-cells = <1>;
			#size-cells = <0>;

			pvccinfaon-pvccfa-cpu1@58 {
				compatible = "mps,mp2971";
				reg = <0x58>;
				interrupt-parent = <&smb_pex_cpu1_event>;
				interrupts = <9 IRQ_TYPE_LEVEL_LOW>;

				regulators {
					pvccinfaon_cpu1: vout0 {
						regulator-name = "pvccinfaon_cpu1";
						regulator-enable-ramp-delay = <200>;
					};
					pvccfa_ehv_cpu1: vout1 {
						regulator-name = "pvccfa_ehv_cpu1";
						regulator-enable-ramp-delay = <200>;
					};
				};
			};
			tda38640-pvnn-main-cpu1@40 {
				compatible = "infineon,tda38640";
				reg = <0x40>;
				interrupt-parent = <&smb_pex_cpu1_event>;
				interrupts = <10 IRQ_TYPE_LEVEL_LOW>;

				regulators {
					pvnn_main_cpu1: vout {
						regulator-name = "pvnn_main_cpu1";
						regulator-enable-ramp-delay = <200>;
					};
				};
			};
		};

		i2c@3 {
			reg = <3>;
			#address-cells = <1>;
			#size-cells = <0>;

			mp2973-pvccin-pvccfa-cpu1@58 {
				compatible = "mps,mp2973";
				reg = <0x58>;
				interrupt-parent = <&smb_pex_cpu1_event>;
				interrupts = <12 IRQ_TYPE_LEVEL_LOW>;

				regulators {
					pvccin_cpu1: vout0 {
						regulator-name = "pvccin_cpu1";
						regulator-enable-ramp-delay = <200>;
					};
					pvccfa_ehv_fivra_cpu1: vout1 {
						regulator-name = "pvccfa_ehv_fivra_cpu1";
						regulator-enable-ramp-delay = <200>;
					};
				};
			};
		};

		i2c@4 {
			reg = <4>;
			#address-cells = <1>;
			#size-cells = <0>;

			tda38640-pvccd-hv-cpu1@40 {
				compatible = "infineon,tda38640";
				reg = <0x40>;
				interrupt-parent = <&smb_pex_cpu1_event>;
				interrupts = <11 IRQ_TYPE_LEVEL_LOW>;
				infineon,en-pin-fixed-level;

				regulators {
					pvccd_hv_cpu1: vout {
						regulator-name = "pvccd_hv_cpu1";
						regulator-enable-ramp-delay = <200>;
					};
				};
			};
		};

		i2c@5 {
			reg = <5>;
			#address-cells = <1>;
			#size-cells = <0>;

			tda38640-pvpp-hbm-cpu1@40 {
				compatible = "infineon,tda38640";
				reg = <0x40>;
				interrupt-parent = <&smb_pex_cpu1_event>;
				interrupts = <8 IRQ_TYPE_LEVEL_LOW>;

				regulators {
					pvpp_hbm_cpu1: vout {
						regulator-name = "pvpp_hbm_cpu1";
						regulator-enable-ramp-delay = <200>;
					};
				};
			};
		};

		i2c@6 {
			reg = <6>;
			#address-cells = <1>;
			#size-cells = <0>;
		};

		i2c@7 {
			reg = <7>;
			#address-cells = <1>;
			#size-cells = <0>;
		};
	};
};

&i2c6 {
	status = "okay";

	i2cmux3: mux@77 {
		compatible = "maxim,max7357";
		reg = <0x77>;
		#address-cells = <1>;
		#size-cells = <0>;

		vdd-supply = <&p3v3_aux>;

		i2c@0 {
			reg = <0>;
			#address-cells = <1>;
			#size-cells = <0>;

			smb_pex_cpu2_event: pinctrl@20 {
				compatible = "cypress,cy8c9540";
				reg = <0x20>;
				gpio-controller;
				#gpio-cells = <2>;

				interrupt-parent = <&smb_pex_vr_ctrl>;
				interrupts = <3 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-controller;
				#interrupt-cells = <2>;

				vdd-supply = <&p3v3_aux>;
				reset-gpios = <&smb_svc_pex_cpu2_led 16 GPIO_ACTIVE_HIGH>;

				gpio-reserved-ranges = <14 2>, <21 1>, <25 3>, <33 1>;

				gpio-line-names =
				/* GPORT0 */
				"PWRGD_CHD_CPU2", "PWRGD_CHC_CPU2",
				"PWRGD_CHB_CPU2", "PWRGD_CHA_CPU2",
				"PWRGD_CHE_CPU2", "PWRGD_CHF_CPU2",
				"PWRGD_CHG_CPU2", "PWRGD_CHH_CPU2",
				/* GPORT1 */
				"SMB_VR_PVPP_HBM_CPU2_ALERT_N", "SMB_VR_PVCCINFAON_CPU2_ALERT_N",
				"SMB_VR_PVNN_MAIN_CPU2_ALERT_N", "SMB_VR_PVCCD_HV_CPU2_ALERT_N",
				"SMB_VR_PVCCIN_CPU2_ALERT_N", "SEL_SMB_DIMM_CPU2",
				"", "",
				/* GPORT2 */
				"PWRGD_LVC3_CPU2_AB_DRAM_G", "PWRGD_LVC3_CPU2_CD_DRAM_G",
				"PWRGD_LVC3_CPU2_EF_DRAM_G", "PWRGD_LVC3_CPU2_GH_DRAM_G",
				/* GPORT3 */
				"FM_CPU2_DISABLE_COD_N", "",
				"RST_LVC3_CPU2_RESET_N", "PWRGD_LVC3_CPU2_PWRGOOD",
				"PWRGD_PLT_AUX_CPU2_LVT3", "",
				"", "",
				/* GPORT4 */
				"H_LVT3_CPU2_PROCHOT_N", "H_LVT3_CPU2_MEMHOT_IN_N",
				"H_LVT3_CPU2_MEMHOT_OUT_N", "H_LVT3_CPU2_MEMTRIP_OUT_N",
				"H_LVT3_CPU2_THERMTRIP_OUT_N", "",
				"H_LVT3_CPU2_NMI", "FM_S3M_CPU2_CD_INIT_ERROR",
				/* GPORT5 */
				"FM_CPU2_PKG_ID0", "FM_CPU2_PKG_ID1",
				"FM_CPU2_PROC_ID0", "FM_CPU2_PROC_ID1";

				pinctrl-0 = <&U62100_pins>;
				pinctrl-names = "default";
				U62100_pins: cfg-pins {
					pins = "gp10", "gp11", "gp12", "gp13", "gp14";
					function = "gpio";
					input-enable;
					bias-pull-up;
				};
			};
		};

		i2c@1 {
			reg = <1>;
			#address-cells = <1>;
			#size-cells = <0>;
		};

		i2c@2 {
			reg = <2>;
			#address-cells = <1>;
			#size-cells = <0>;

			pvccinfaon-pvccfa-cpu2@58 {
				compatible = "mps,mp2971";
				reg = <0x58>;
				interrupt-parent = <&smb_pex_cpu2_event>;
				interrupts = <9 IRQ_TYPE_LEVEL_LOW>;

				regulators {
					pvccinfaon_cpu2: vout0 {
						regulator-name = "pvccinfaon_cpu2";
						regulator-enable-ramp-delay = <200>;
					};
					pvccfa_ehv_cpu2: vout1 {
						regulator-name = "pvccfa_ehv_cpu2";
						regulator-enable-ramp-delay = <200>;
					};
				};
			};
			tda38640-pvnn-main-cpu2@40 {
				compatible = "infineon,tda38640";
				reg = <0x40>;
				interrupt-parent = <&smb_pex_cpu2_event>;
				interrupts = <10 IRQ_TYPE_LEVEL_LOW>;

				regulators {
					pvnn_main_cpu2: vout {
						regulator-name = "pvnn_main_cpu2";
						regulator-enable-ramp-delay = <200>;
					};
				};
			};
		};

		i2c@3 {
			reg = <3>;
			#address-cells = <1>;
			#size-cells = <0>;

			mp2973-pvccin-pvccfa-cpu2@58 {
				compatible = "mps,mp2973";
				reg = <0x58>;
				interrupt-parent = <&smb_pex_cpu2_event>;
				interrupts = <12 IRQ_TYPE_LEVEL_LOW>;

				regulators {
					pvccin_cpu2: vout0 {
						regulator-name = "pvccin_cpu2";
						regulator-enable-ramp-delay = <200>;
					};
					pvccfa_ehv_fivra_cpu2: vout1 {
						regulator-name = "pvccfa_ehv_fivra_cpu2";
						regulator-enable-ramp-delay = <200>;
					};
				};
			};
		};

		i2c@4 {
			reg = <4>;
			#address-cells = <1>;
			#size-cells = <0>;

			tda38640-pvccd-hv-cpu2@40 {
				compatible = "infineon,tda38640";
				reg = <0x40>;
				interrupt-parent = <&smb_pex_cpu2_event>;
				interrupts = <11 IRQ_TYPE_LEVEL_LOW>;
				infineon,en-pin-fixed-level;

				regulators {
					pvccd_hv_cpu2: vout {
						regulator-name = "pvccd_hv_cpu2";
						regulator-enable-ramp-delay = <200>;
					};
				};
			};
		};

		i2c@5 {
			reg = <5>;
			#address-cells = <1>;
			#size-cells = <0>;

			tda38640-pvpp-hbm-cpu2@40 {
				compatible = "infineon,tda38640";
				reg = <0x40>;
				interrupt-parent = <&smb_pex_cpu2_event>;
				interrupts = <8 IRQ_TYPE_LEVEL_LOW>;

				regulators {
					pvpp_hbm_cpu2: vout {
						regulator-name = "pvpp_hbm_cpu2";
						regulator-enable-ramp-delay = <200>;
					};
				};
			};
		};

		i2c@6 {
			reg = <6>;
			#address-cells = <1>;
			#size-cells = <0>;
		};

		i2c@7 {
			reg = <7>;
			#address-cells = <1>;
			#size-cells = <0>;
		};
	};
};

&i2c12 {
	status = "okay";

	i2cmux22: mux@77 {
		compatible = "maxim,max7357";
		reg = <0x77>;
		#address-cells = <1>;
		#size-cells = <0>;

		reset-gpios = <&gpio0 ASPEED_GPIO(P, 2) (GPIO_ACTIVE_LOW | GPIO_OPEN_DRAIN)>;
		vdd-supply = <&p3v3_aux>;

		i2c@0 {
			reg = <0>;
			#address-cells = <1>;
			#size-cells = <0>;

			smb_pex_cpu3_event: pinctrl@20 {
				compatible = "cypress,cy8c9540";
				reg = <0x20>;
				gpio-controller;
				#gpio-cells = <2>;

				interrupt-parent = <&smb_pex_vr_ctrl>;
				interrupts = <11 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-controller;
				#interrupt-cells = <2>;

				vdd-supply = <&p3v3_aux>;
				reset-gpios = <&smb_svc_pex_cpu3_led 16 GPIO_ACTIVE_HIGH>;

				gpio-reserved-ranges = <14 2>, <21 1>, <25 3>, <33 1>;

				gpio-line-names =
				/* GPORT0 */
				"PWRGD_CHD_CPU3", "PWRGD_CHC_CPU3",
				"PWRGD_CHB_CPU3", "PWRGD_CHA_CPU3",
				"PWRGD_CHE_CPU3", "PWRGD_CHF_CPU3",
				"PWRGD_CHG_CPU3", "PWRGD_CHH_CPU3",
				/* GPORT1 */
				"SMB_VR_PVPP_HBM_CPU3_ALERT_N", "SMB_VR_PVCCINFAON_CPU3_ALERT_N",
				"SMB_VR_PVNN_MAIN_CPU3_ALERT_N", "SMB_VR_PVCCD_HV_CPU3_ALERT_N",
				"SMB_VR_PVCCIN_CPU3_ALERT_N", "SEL_SMB_DIMM_CPU3",
				"", "",
				/* GPORT2 */
				"PWRGD_LVC3_CPU3_AB_DRAM_G", "PWRGD_LVC3_CPU3_CD_DRAM_G",
				"PWRGD_LVC3_CPU3_EF_DRAM_G", "PWRGD_LVC3_CPU3_GH_DRAM_G",
				/* GPORT3 */
				"FM_CPU3_DISABLE_COD_N", "",
				"RST_LVC3_CPU3_RESET_N", "PWRGD_LVC3_CPU3_PWRGOOD",
				"PWRGD_PLT_AUX_CPU3_LVT3", "",
				"", "",
				/* GPORT4 */
				"H_LVT3_CPU3_PROCHOT_N", "H_LVT3_CPU3_MEMHOT_IN_N",
				"H_LVT3_CPU3_MEMHOT_OUT_N", "H_LVT3_CPU3_MEMTRIP_OUT_N",
				"H_LVT3_CPU3_THERMTRIP_OUT_N", "",
				"H_LVT3_CPU3_NMI", "FM_S3M_CPU3_CD_INIT_ERROR",
				/* GPORT5 */
				"FM_CPU3_PKG_ID0", "FM_CPU3_PKG_ID1",
				"FM_CPU3_PROC_ID0", "FM_CPU3_PROC_ID1";

				pinctrl-0 = <&U62110_pins>;
				pinctrl-names = "default";
				U62110_pins: cfg-pins {
					pins = "gp10", "gp11", "gp12", "gp13", "gp14";
					function = "gpio";
					input-enable;
					bias-pull-up;
				};
			};
		};

		i2c@1 {
			reg = <1>;
			#address-cells = <1>;
			#size-cells = <0>;
		};

		i2c@2 {
			reg = <2>;
			#address-cells = <1>;
			#size-cells = <0>;

			pvccinfaon-pvccfa-cpu3@58 {
				compatible = "mps,mp2971";
				reg = <0x58>;
				interrupt-parent = <&smb_pex_cpu3_event>;
				interrupts = <9 IRQ_TYPE_LEVEL_LOW>;

				regulators {
					pvccinfaon_cpu3: vout0 {
						regulator-name = "pvccinfaon_cpu3";
						regulator-enable-ramp-delay = <200>;
					};
					pvccfa_ehv_cpu3: vout1 {
						regulator-name = "pvccfa_ehv_cpu3";
						regulator-enable-ramp-delay = <200>;
					};
				};
			};
			tda38640-pvnn-main-cpu3@40 {
				compatible = "infineon,tda38640";
				reg = <0x40>;
				interrupt-parent = <&smb_pex_cpu3_event>;
				interrupts = <10 IRQ_TYPE_LEVEL_LOW>;

				regulators {
					pvnn_main_cpu3: vout {
						regulator-name = "pvnn_main_cpu3";
						regulator-enable-ramp-delay = <200>;
					};
				};
			};
		};

		i2c@3 {
			reg = <3>;
			#address-cells = <1>;
			#size-cells = <0>;

			mp2973-pvccin-pvccfa-cpu3@58 {
				compatible = "mps,mp2973";
				reg = <0x58>;
				interrupt-parent = <&smb_pex_cpu3_event>;
				interrupts = <12 IRQ_TYPE_LEVEL_LOW>;

				regulators {
					pvccin_cpu3: vout0 {
						regulator-name = "pvccin_cpu3";
						regulator-enable-ramp-delay = <200>;
					};
					pvccfa_ehv_fivra_cpu3: vout1 {
						regulator-name = "pvccfa_ehv_fivra_cpu3";
						regulator-enable-ramp-delay = <200>;
					};
				};
			};
		};

		i2c@4 {
			reg = <4>;
			#address-cells = <1>;
			#size-cells = <0>;

			tda38640-pvccd-hv-cpu3@40 {
				compatible = "infineon,tda38640";
				reg = <0x40>;
				interrupt-parent = <&smb_pex_cpu3_event>;
				interrupts = <11 IRQ_TYPE_LEVEL_LOW>;
				infineon,en-pin-fixed-level;

				regulators {
					pvccd_hv_cpu3: vout {
						regulator-name = "pvccd_hv_cpu3";
						regulator-enable-ramp-delay = <200>;
					};
				};
			};
		};

		i2c@5 {
			reg = <5>;
			#address-cells = <1>;
			#size-cells = <0>;

			tda38640-pvpp-hbm-cpu3@40 {
				compatible = "infineon,tda38640";
				reg = <0x40>;
				interrupt-parent = <&smb_pex_cpu3_event>;
				interrupts = <8 IRQ_TYPE_LEVEL_LOW>;

				regulators {
					pvpp_hbm_cpu3: vout {
						regulator-name = "pvpp_hbm_cpu3";
						regulator-enable-ramp-delay = <200>;
					};
				};
			};
		};

		i2c@6 {
			reg = <6>;
			#address-cells = <1>;
			#size-cells = <0>;
		};

		i2c@7 {
			reg = <7>;
			#address-cells = <1>;
			#size-cells = <0>;
		};
	};
};

&i2c15 {
	status = "okay";

	i2cmux14: mux@77 {
		compatible = "maxim,max7357";
		reg = <0x77>;
		#address-cells = <1>;
		#size-cells = <0>;

		reset-gpios = <&gpio0 ASPEED_GPIO(R, 1) (GPIO_ACTIVE_LOW | GPIO_OPEN_DRAIN)>;
		vdd-supply = <&p3v3_aux>;

		i2c@0 {
			reg = <0>;
			#address-cells = <1>;
			#size-cells = <0>;

			i2cmux15: mux@70 {
				compatible = "maxim,max7357";
				reg = <0x70>;
				#address-cells = <1>;
				#size-cells = <0>;

				reset-gpios = <&bmc_pex_irq 11 (GPIO_ACTIVE_LOW | GPIO_OPEN_DRAIN)>;
				vdd-supply = <&p3v3_aux>;
			};
		};

		i2c@1 {
			reg = <1>;
			#address-cells = <1>;
			#size-cells = <0>;

			i2cmux16: mux@70 {
				compatible = "maxim,max7357";
				reg = <0x70>;
				#address-cells = <1>;
				#size-cells = <0>;

				reset-gpios = <&bmc_pex_irq 2 (GPIO_ACTIVE_LOW | GPIO_OPEN_DRAIN)>;
				vdd-supply = <&p3v3_aux>;
			};
		};

		i2c@2 {
			reg = <2>;
			#address-cells = <1>;
			#size-cells = <0>;

			i2cmux17: mux@70 {
				compatible = "maxim,max7357";
				reg = <0x70>;
				#address-cells = <1>;
				#size-cells = <0>;

				reset-gpios = <&bmc_pex_irq 0 (GPIO_ACTIVE_LOW | GPIO_OPEN_DRAIN)>;
				vdd-supply = <&p3v3_aux>;
			};
		};

		i2c@3 {
			reg = <3>;
			#address-cells = <1>;
			#size-cells = <0>;

			i2cmux18: mux@70 {
				compatible = "maxim,max7357";
				reg = <0x70>;
				#address-cells = <1>;
				#size-cells = <0>;

				reset-gpios = <&bmc_pex_irq 3 (GPIO_ACTIVE_LOW | GPIO_OPEN_DRAIN)>;
				vdd-supply = <&p3v3_aux>;
			};
		};

		i2c@4 {
			reg = <4>;
			#address-cells = <1>;
			#size-cells = <0>;

			i2cmux19: mux@70 {
				compatible = "maxim,max7357";
				reg = <0x70>;
				#address-cells = <1>;
				#size-cells = <0>;

				reset-gpios = <&bmc_pex_irq 9 (GPIO_ACTIVE_LOW | GPIO_OPEN_DRAIN)>;
				vdd-supply = <&p3v3_aux>;
			};
		};

		i2c@5 {
			reg = <5>;
			#address-cells = <1>;
			#size-cells = <0>;

			smb_pex_rssd17_32: pinctrl@20 {
				compatible = "cypress,cy8c9560";
				reg = <0x20>;
				gpio-controller;
				#gpio-cells = <2>;

				interrupt-parent = <&bmc_pex_irq>;
				interrupts = <13 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-controller;
				#interrupt-cells = <2>;

				vdd-supply = <&p3v3_aux>;
				reset-gpios = <&bmc_pex_irq 19 GPIO_ACTIVE_HIGH>;

				gpio-reserved-ranges = <48 12>;

				gpio-line-names =
				/* GPORT0 */
				"RSSD17_SMBRST_N", "RSSD18_SMBRST_N",
				"RSSD19_SMBRST_N", "RSSD20_SMBRST_N",
				"RSSD21_SMBRST_N", "RSSD22_SMBRST_N",
				"RSSD23_SMBRST_N", "RSSD24_SMBRST_N",
				/* GPORT1 */
				"RSSD25_SMBRST_N", "RSSD26_SMBRST_N",
				"RSSD27_SMBRST_N", "RSSD28_SMBRST_N",
				"RSSD29_SMBRST_N", "RSSD30_SMBRST_N",
				"RSSD31_SMBRST_N", "RSSD32_SMBRST_N",
				/* GPORT2 */
				"RSSD17_PWRDIS", "RSSD18_PWRDIS",
				"RSSD19_PWRDIS", "RSSD20_PWRDIS",
				/* GPORT3 */
				"RSSD21_PWRDIS", "RSSD22_PWRDIS",
				"RSSD23_PWRDIS", "RSSD24_PWRDIS",
				"RSSD25_PWRDIS", "RSSD26_PWRDIS",
				"RSSD27_PWRDIS", "RSSD28_PWRDIS",
				/* GPORT4 */
				"RSSD29_PWRDIS", "RSSD30_PWRDIS",
				"RSSD31_PWRDIS", "RSSD32_PWRDIS",
				"RSSD17_RESET_N", "RSSD18_RESET_N",
				"RSSD19_RESET_N", "RSSD20_RESET_N",
				/* GPORT5 */
				"RSSD21_RESET_N", "RSSD22_RESET_N",
				"RSSD23_RESET_N", "RSSD24_RESET_N",
				"RSSD25_RESET_N", "RSSD26_RESET_N",
				"RSSD27_RESET_N", "RSSD28_RESET_N",
				/* GPORT6 */
				"RSSD29_RESET_N", "RSSD30_RESET_N",
				"RSSD31_RESET_N", "RSSD32_RESET_N",
				"", "",
				"", "",
				/* GPORT7 */
				"", "",
				"", "",
				"", "",
				"", "";
			};
		};

		i2c@6 {
			reg = <6>;
			#address-cells = <1>;
			#size-cells = <0>;

			i2cmux20: mux@70 {
				compatible = "maxim,max7357";
				reg = <0x70>;
				#address-cells = <1>;
				#size-cells = <0>;

				reset-gpios = <&bmc_pex_irq 4 (GPIO_ACTIVE_LOW | GPIO_OPEN_DRAIN)>;
				vdd-supply = <&p3v3_aux>;

				i2c@0 {
					reg = <0>;
					#address-cells = <1>;
					#size-cells = <0>;
				};
				i2c@1 {
					reg = <1>;
					#address-cells = <1>;
					#size-cells = <0>;
				};
				i2c@2 {
					reg = <2>;
					#address-cells = <1>;
					#size-cells = <0>;
				};
				i2c@3 {
					reg = <3>;
					#address-cells = <1>;
					#size-cells = <0>;
				};
				i2c@4 {
					reg = <4>;
					#address-cells = <1>;
					#size-cells = <0>;
				};
				i2c@5 {
					reg = <5>;
					#address-cells = <1>;
					#size-cells = <0>;
				};
				i2c@6 {
					reg = <6>;
					#address-cells = <1>;
					#size-cells = <0>;
				};
				i2c@7 {
					reg = <7>;
					#address-cells = <1>;
					#size-cells = <0>;
				};
			};
		};

		i2c@7 {
			reg = <7>;
			#address-cells = <1>;
			#size-cells = <0>;

			i2cmux21: mux@70 {
				compatible = "maxim,max7357";
				reg = <0x70>;
				#address-cells = <1>;
				#size-cells = <0>;

				reset-gpios = <&bmc_pex_irq 5 (GPIO_ACTIVE_LOW | GPIO_OPEN_DRAIN)>;
				vdd-supply = <&p3v3_aux>;

				i2c@0 {
					reg = <0>;
					#address-cells = <1>;
					#size-cells = <0>;
				};
				i2c@1 {
					reg = <1>;
					#address-cells = <1>;
					#size-cells = <0>;
				};
				i2c@2 {
					reg = <2>;
					#address-cells = <1>;
					#size-cells = <0>;
				};
				i2c@3 {
					reg = <3>;
					#address-cells = <1>;
					#size-cells = <0>;
				};
				i2c@4 {
					reg = <4>;
					#address-cells = <1>;
					#size-cells = <0>;
				};
				i2c@5 {
					reg = <5>;
					#address-cells = <1>;
					#size-cells = <0>;
				};
				i2c@6 {
					reg = <6>;
					#address-cells = <1>;
					#size-cells = <0>;
				};
				i2c@7 {
					reg = <7>;
					#address-cells = <1>;
					#size-cells = <0>;
				};
			};
		};
	};
};

&i2c8 {
	status = "okay";

	i2cmux5: mux@77 {
		compatible = "maxim,max7357";
		reg = <0x77>;
		#address-cells = <1>;
		#size-cells = <0>;

		reset-gpios = <&gpio0 ASPEED_GPIO(R, 0) (GPIO_ACTIVE_LOW | GPIO_OPEN_DRAIN)>;
		vdd-supply = <&p3v3_aux>;

		i2c@0 {
			reg = <0>;
			#address-cells = <1>;
			#size-cells = <0>;

			i2cmux6: mux@70 {
				compatible = "maxim,max7357";
				reg = <0x70>;
				#address-cells = <1>;
				#size-cells = <0>;

				reset-gpios = <&bmc_pex_irq 16 (GPIO_ACTIVE_LOW | GPIO_OPEN_DRAIN)>;
				vdd-supply = <&p3v3_aux>;
			};
		};

		i2c@1 {
			reg = <1>;
			#address-cells = <1>;
			#size-cells = <0>;

			i2cmux7: mux@70 {
				compatible = "maxim,max7357";
				reg = <0x70>;
				#address-cells = <1>;
				#size-cells = <0>;

				reset-gpios = <&bmc_pex_irq 7 (GPIO_ACTIVE_LOW | GPIO_OPEN_DRAIN)>;
				vdd-supply = <&p3v3_aux>;
			};
		};

		i2c@2 {
			reg = <2>;
			#address-cells = <1>;
			#size-cells = <0>;

			i2cmux8: mux@70 {
				compatible = "maxim,max7357";
				reg = <0x70>;
				#address-cells = <1>;
				#size-cells = <0>;

				reset-gpios = <&bmc_pex_irq 1 (GPIO_ACTIVE_LOW | GPIO_OPEN_DRAIN)>;
				vdd-supply = <&p3v3_aux>;
			};
		};

		i2c@3 {
			reg = <3>;
			#address-cells = <1>;
			#size-cells = <0>;

			i2cmux9: mux@70 {
				compatible = "maxim,max7357";
				reg = <0x70>;
				#address-cells = <1>;
				#size-cells = <0>;

				reset-gpios = <&bmc_pex_irq 10 (GPIO_ACTIVE_LOW | GPIO_OPEN_DRAIN)>;
				vdd-supply = <&p3v3_aux>;
			};
		};

		i2c@4 {
			reg = <4>;
			#address-cells = <1>;
			#size-cells = <0>;

			i2cmux10: mux@70 {
				compatible = "maxim,max7357";
				reg = <0x70>;
				#address-cells = <1>;
				#size-cells = <0>;

				reset-gpios = <&bmc_pex_irq 15 (GPIO_ACTIVE_LOW | GPIO_OPEN_DRAIN)>;
				vdd-supply = <&p3v3_aux>;
			};
		};

		i2c@5 {
			reg = <5>;
			#address-cells = <1>;
			#size-cells = <0>;

			smb_pex_rssd_01_16: pinctrl@20 {
				compatible = "cypress,cy8c9560";
				reg = <0x20>;
				gpio-controller;
				#gpio-cells = <2>;

				interrupt-parent = <&bmc_pex_irq>;
				interrupts = <6 IRQ_TYPE_LEVEL_HIGH>;
				interrupt-controller;
				#interrupt-cells = <2>;

				vdd-supply = <&p3v3_aux>;
				reset-gpios = <&bmc_pex_irq 18 GPIO_ACTIVE_HIGH>;

				gpio-reserved-ranges = <48 12>;

				gpio-line-names =
				/* GPORT0 */
				"RSSD01_SMBRST_N", "RSSD02_SMBRST_N",
				"RSSD03_SMBRST_N", "RSSD04_SMBRST_N",
				"RSSD05_SMBRST_N", "RSSD06_SMBRST_N",
				"RSSD07_SMBRST_N", "RSSD08_SMBRST_N",
				/* GPORT1 */
				"RSSD09_SMBRST_N", "RSSD10_SMBRST_N",
				"RSSD11_SMBRST_N", "RSSD12_SMBRST_N",
				"RSSD13_SMBRST_N", "RSSD14_SMBRST_N",
				"RSSD15_SMBRST_N", "RSSD16_SMBRST_N",
				/* GPORT2 */
				"RSSD01_PWRDIS", "RSSD02_PWRDIS",
				"RSSD03_PWRDIS", "RSSD04_PWRDIS",
				/* GPORT3 */
				"RSSD05_PWRDIS", "RSSD06_PWRDIS",
				"RSSD07_PWRDIS", "RSSD08_PWRDIS",
				"RSSD09_PWRDIS", "RSSD10_PWRDIS",
				"RSSD11_PWRDIS", "RSSD12_PWRDIS",
				/* GPORT4 */
				"RSSD13_PWRDIS", "RSSD14_PWRDIS",
				"RSSD15_PWRDIS", "RSSD16_PWRDIS",
				"RSSD01_RESET_N", "RSSD02_RESET_N",
				"RSSD03_RESET_N", "RSSD04_RESET_N",
				/* GPORT5 */
				"RSSD05_RESET_N", "RSSD06_RESET_N",
				"RSSD07_RESET_N", "RSSD08_RESET_N",
				"RSSD09_RESET_N", "RSSD10_RESET_N",
				"RSSD11_RESET_N", "RSSD12_RESET_N",
				/* GPORT6 */
				"RSSD13_RESET_N", "RSSD14_RESET_N",
				"RSSD15_RESET_N", "RSSD16_RESET_N",
				"", "",
				"", "",
				/* GPORT7 */
				"", "",
				"", "",
				"", "",
				"", "";
			};
		};

		i2c@6 {
			reg = <6>;
			#address-cells = <1>;
			#size-cells = <0>;

			i2cmux11: mux@70 {
				compatible = "maxim,max7357";
				reg = <0x70>;
				#address-cells = <1>;
				#size-cells = <0>;

				reset-gpios = <&bmc_pex_irq 12 (GPIO_ACTIVE_LOW | GPIO_OPEN_DRAIN)>;
				vdd-supply = <&p3v3_aux>;

				i2c@0 {
					reg = <0>;
					#address-cells = <1>;
					#size-cells = <0>;
				};
				i2c@1 {
					reg = <1>;
					#address-cells = <1>;
					#size-cells = <0>;
				};
				i2c@2 {
					reg = <2>;
					#address-cells = <1>;
					#size-cells = <0>;
				};
				i2c@3 {
					reg = <3>;
					#address-cells = <1>;
					#size-cells = <0>;
				};
				i2c@4 {
					reg = <4>;
					#address-cells = <1>;
					#size-cells = <0>;
				};
				i2c@5 {
					reg = <5>;
					#address-cells = <1>;
					#size-cells = <0>;
				};
				i2c@6 {
					reg = <6>;
					#address-cells = <1>;
					#size-cells = <0>;
				};
				i2c@7 {
					reg = <7>;
					#address-cells = <1>;
					#size-cells = <0>;
				};
			};
		};

		i2c@7 {
			reg = <7>;
			#address-cells = <1>;
			#size-cells = <0>;

			i2cmux12: mux@70 {
				compatible = "maxim,max7357";
				reg = <0x70>;
				#address-cells = <1>;
				#size-cells = <0>;

				reset-gpios = <&bmc_pex_irq 14 (GPIO_ACTIVE_LOW | GPIO_OPEN_DRAIN)>;
				vdd-supply = <&p3v3_aux>;

				i2c@0 {
					reg = <0>;
					#address-cells = <1>;
					#size-cells = <0>;
				};
				i2c@1 {
					reg = <1>;
					#address-cells = <1>;
					#size-cells = <0>;
				};
				i2c@2 {
					reg = <2>;
					#address-cells = <1>;
					#size-cells = <0>;
				};
				i2c@3 {
					reg = <3>;
					#address-cells = <1>;
					#size-cells = <0>;
				};
				i2c@4 {
					reg = <4>;
					#address-cells = <1>;
					#size-cells = <0>;
				};
				i2c@5 {
					reg = <5>;
					#address-cells = <1>;
					#size-cells = <0>;
				};
				i2c@6 {
					reg = <6>;
					#address-cells = <1>;
					#size-cells = <0>;
				};
				i2c@7 {
					reg = <7>;
					#address-cells = <1>;
					#size-cells = <0>;
				};
			};
		};
	};
};

&i2c13 {
	status = "okay";

	i2cmux23: mux@77 {
		compatible = "maxim,max7357";
		reg = <0x77>;
		#address-cells = <1>;
		#size-cells = <0>;

		reset-gpios = <&gpio0 ASPEED_GPIO(R, 4) (GPIO_ACTIVE_LOW | GPIO_OPEN_DRAIN)>;
		vdd-supply = <&p3v3_bmc_aux>;
	};
};

&i2cmux23 {
	i2c@0 {
		reg = <0>;
		#address-cells = <1>;
		#size-cells = <0>;
		smb_pex_vr_ctrl: pinctrl@20 {
			compatible = "cypress,cy8c9540";
			reg = <0x20>;
			gpio-controller;
			#gpio-cells = <2>;
			interrupt-parent = <&gpio0>;
			interrupts = <ASPEED_GPIO(V, 2) IRQ_TYPE_LEVEL_HIGH>;
			interrupt-controller;
			#interrupt-cells = <2>;
			vdd-supply = <&p3v3_bmc_aux>;
			reset-gpios = <&gpio0 ASPEED_GPIO(Q, 2) GPIO_ACTIVE_HIGH>;
			gpio-line-names =
			/* GPORT0 */
			"BCM0_INPUT_DISABLE_N", "SMB_VR_P3V3_AUX_ALERT_N",
			"SMB_PEX_CPU1_EVENT_INT", "SMB_PEX_CPU2_EVENT_INT",
			"DPIC0_VOLTAGE_DETECTB_N", "DPIC0_VOLTAGE_DETECTA_N",
			"DPIC1_VOLTAGE_DETECTA_N", "DPIC1_VOLTAGE_DETECTB_N",
			/* GPORT1 */
			"SMB_PEX_NIC_INT", "SMB_VR_P1V05_PCH_AUX_ALERT_N",
			"SMB_PEX_CPU0_EVENT_INT", "SMB_PEX_CPU3_EVENT_INT",
			"LED_ID_TPM", "PLUG_DETECT_TPM",
			"PLUG_DETECT_M2_SSD_CARRIER1", "RST_M2_SSD1_PERST_N",
			/* GPORT2 */
			"LED_ID_BAT", "LED_ID_MGMT_PORT2",
			"LED_ID_MGMT_PORT1", "SMB_VR_P5V_AUX_ALERT_N",
			/* GPORT3 */
			"SMB_VR_AUX_SSB_ALERT_N", "BCM1_INPUT_DISABLE_N",
			"LED_ID_NIC1_PORT1", "LED_ID_NIC1_PORT2",
			"LED_ID_NIC2_PORT1", "LED_ID_NIC2_PORT2",
			"RST_M2_SSD2_PERST_N", "PLUG_DETECT_M2_SSD2",
			/* GPORT4 */
			"PLUG_DETECT_BAT", "PLUG_DETECT_M2_SSD1",
			"M2_SSD1_SSB_ALERT_N", "BCM2_INPUT_DISABLE_N",
			"SMB_VR_P1V8_PCH_AUX_ALERT_N", "BCM3_INPUT_DISABLE_N",
			"LED_PWR_DWR_BACK", "LED_ID_DWR_BACK_P",
			/* GPORT5 */
			"LED_ID_M2_SSD2", "LED_ID_M2_SSD1",
			"PLUG_DETECT_M2_SSD_CARRIER2", "M2_SSD2_SSB_ALERT_N";

			pinctrl-0 = <&U62120_input &U62120_input_pullup>;
			pinctrl-names = "default";
			U62120_input: input-pins {
				pins = "gp10";
				function = "gpio";
				input-enable;
				bias-disable;
			};
			U62120_input_pullup: input-pullup-pins {
				pins = "gp01", "gp02", "gp03", "gp11", "gp12", "gp13",
				"gp23", "gp30", "gp40", "gp42", "gp44", "gp53";
				function = "gpio";
				input-enable;
				bias-pull-up;
			};
		};
	};
	i2c@1 {
		reg = <1>;
		#address-cells = <1>;
		#size-cells = <0>;
		bmc_pex_irq: pinctrl@20 {
			compatible = "cypress,cy8c9520";
			reg = <0x20>;
			gpio-controller;
			#gpio-cells = <2>;
			interrupt-parent = <&gpio0>;
			interrupts = <ASPEED_GPIO(V, 0) IRQ_TYPE_LEVEL_HIGH>;
			interrupt-controller;
			#interrupt-cells = <2>;
			vdd-supply = <&p3v3_aux>;
			reset-gpios = <&gpio0 ASPEED_GPIO(Q, 1) GPIO_ACTIVE_HIGH>;
			gpio-line-names =
			/* GPORT0 */
			"SMB_MUX_PWM_FANGRP2_RST_INT_N", "SMB_MUX_SSB_FANGRP2_RST_INT_N",
			"SMB_MUX_PWM_FANGRP1_RST_INT_N", "SMB_MUX_SSB_RSSD01_08_RST_INT_N",
			"SMB_MUX_RSSD01_08_RST_INT_N", "SMB_MUX_RSSD09_16_RST_INT_N",
			"SMB_PEX_RSSD01_16_INT", "SMB_MUX_SSB_FANGRP1_RST_INT_N",
			/* GPORT1 */
			"SMB_SVC_PEX_FAN_ALERT_INT", "SMB_MUX_SSB_RSSD09_16_RST_INT_N",
			"SMB_MUX_SSB_RSSD17_24_RST_INT_N", "SMB_MUX_PWM_FANGRP0_RST_INT_N",
			"SMB_MUX_RSSD17_24_RST_INT_N", "SMB_PEX_RSSD17_32_INT",
			"SMB_MUX_RSSD25_32_RST_INT_N", "SMB_MUX_SSB_RSSD25_32_RST_INT_N",
			/* GPORT2 */
			"SMB_MUX_SSB_FANGRP0_RST_INT_N", "PEX_FAN_ALERT_RST",
			"PEX_RSSD01_16_RST", "PEX_RSSD17_32_RST";
			pinctrl-0 = <&U60000_pins>;
			pinctrl-names = "default";
			U60000_pins: cfg-pins {
				pins = "gp06", "gp10", "gp15";
				function = "gpio";
				input-enable;
				bias-disable;
			};
		};
	};
	i2c@2 {
		reg = <2>;
		#address-cells = <1>;
		#size-cells = <0>;
		i2cmux24: mux@70 {
			compatible = "maxim,max7357";
			reg = <0x70>;
			#address-cells = <1>;
			#size-cells = <0>;

			vdd-supply = <&p3v3_bmc_aux>;
		};
	};
	i2c@3 {
		reg = <3>;
		#address-cells = <1>;
		#size-cells = <0>;
		eeprom@51 {
			compatible = "atmel,24c32";
			reg = <0x51>;
			pagesize = <32>;
			vcc-supply = <&p3v3_bmc_aux>;
		};
	};
	i2c@7 {
		reg = <7>;
		#address-cells = <1>;
		#size-cells = <0>;
		i2cmux25: mux@70 {
			compatible = "maxim,max7357";
			reg = <0x70>;
			#address-cells = <1>;
			#size-cells = <0>;
		};
	};
};

&i2cmux25 {
	reset-gpios = <&gpio0 ASPEED_GPIO(R, 2) (GPIO_ACTIVE_LOW | GPIO_OPEN_DRAIN)>;
	vdd-supply = <&p3v3_bmc_aux>;
	i2c@1 {
		reg = <1>;
		#address-cells = <1>;
		#size-cells = <0>;
		p5v_aux: ir38263-p5v-aux@40 {
			compatible = "infineon,ir38263";
			reg = <0x40>;

			regulator-name = "p5v_aux";
			regulator-enable-ramp-delay = <2000>;
			vin-supply = <&p12v>;
			vbus-supply = <&p3v3_bmc_aux>;
			regulator-always-on;
			regulator-boot-on;
		};
	};
	i2c@2 {
		reg = <2>;
		#address-cells = <1>;
		#size-cells = <0>;
		p3v3_aux: ir38263-p3v3-aux@40 {
			compatible = "infineon,ir38263";
			reg = <0x40>;

			vin-supply = <&p12v>;
			regulator-name = "p3v3_aux";
			/*
			 * 2msec for regulator + 18msec for board capacitance
			 * Note: Every IC has a PTC which slowly charges the bypass
			 * cap.
			 */
			regulator-enable-ramp-delay = <200000>;
		};
	};
	i2c@3 {
		reg = <3>;
		#address-cells = <1>;
		#size-cells = <0>;
		aux_ssb: regulator@3a {
			compatible = "maxim,max5970";
			reg = <0x3a>;
			interrupt-parent = <&smb_pex_vr_ctrl>;
			interrupts = <20 IRQ_TYPE_LEVEL_LOW>;
			vss1-supply = <&p5v_aux>;
			vss2-supply = <&p3v3_aux>;
			regulators {
				p5v: sw0 {
					regulator-name = "p5v";
					shunt-resistor-micro-ohms = <12000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <3400000>;
					regulator-enable-ramp-delay = <100000>;
				};
				p3v3_pch: sw1 {
					regulator-name = "p3v3_pch";
					shunt-resistor-micro-ohms = <12000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <3400000>;
					regulator-enable-ramp-delay = <100000>;
				};
			};
		};
	};
	i2c@4 {
		reg = <4>;
		#address-cells = <1>;
		#size-cells = <0>;
		pli1209bc_p12v_a: regulator@5f {
			compatible = "vicor,pli1209bc";
			reg = <0x5f>;
			regulators {
				p12v_a: vout2 {
					regulator-name = "bcm0";
					regulator-boot-on;
				};
			};
		};
	};
	i2c@5 {
		reg = <5>;
		#address-cells = <1>;
		#size-cells = <0>;
		pli1209bc_p12v_b: regulator@5f {
			compatible = "vicor,pli1209bc";
			reg = <0x5f>;
			regulators {
				p12v_b: vout2 {
					regulator-name = "bcm1";
					regulator-boot-on;
				};
			};
		};
	};
	i2c@6 {
		reg = <6>;
		#address-cells = <1>;
		#size-cells = <0>;
		pli1209bc_p12v_c: regulator@5f {
			compatible = "vicor,pli1209bc";
			reg = <0x5f>;
			regulators {
				p12v_c: vout2 {
					regulator-name = "bcm2";
					regulator-boot-on;
				};
			};
		};
	};
	i2c@7 {
		reg = <7>;
		#address-cells = <1>;
		#size-cells = <0>;
		pli1209bc_p12v_d: regulator@5f {
			compatible = "vicor,pli1209bc";
			reg = <0x5f>;
			regulators {
				p12v_d: vout2 {
					regulator-name = "bcm3";
					regulator-boot-on;
				};
			};
		};
	};
};

&i2cmux24 {

	reset-gpios = <&gpio0 ASPEED_GPIO(P, 3) (GPIO_ACTIVE_LOW | GPIO_OPEN_DRAIN)>;

	i2c@0 {
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0>;
		smb_svc_pex_rssd01_16: pinctrl@20 {
			compatible = "cypress,cy8c9560";
			reg = <0x20>;
			gpio-controller;
			#gpio-cells = <2>;
			interrupt-parent = <&gpio0>;
			interrupts = <ASPEED_GPIO(S, 0) IRQ_TYPE_LEVEL_HIGH>;
			interrupt-controller;
			#interrupt-cells = <2>;
			vdd-supply = <&p3v3_bmc_aux>;
			reset-gpios = <&smb_svc_pex_cpu0_led 17 GPIO_ACTIVE_HIGH>;
			gpio-line-names =
			/* GPORT0 */
			"LED_ID_RSSD01", "LED_ID_RSSD02",
			"LED_ID_RSSD03", "LED_ID_RSSD04",
			"LED_ID_RSSD05", "LED_ID_RSSD06",
			"LED_ID_RSSD07", "LED_ID_RSSD08",
			/* GPORT1 */
			"LED_ID_RSSD09", "LED_ID_RSSD10",
			"LED_ID_RSSD11", "LED_ID_RSSD12",
			"LED_ID_RSSD13", "LED_ID_RSSD14",
			"LED_ID_RSSD15", "LED_ID_RSSD16",
			/* GPORT2 */
			"RSSD01_PRESENT_N", "RSSD02_PRESENT_N",
			"RSSD03_PRESENT_N", "RSSD04_PRESENT_N",
			/* GPORT3 */
			"RSSD05_PRESENT_N", "RSSD06_PRESENT_N",
			"RSSD07_PRESENT_N", "RSSD08_PRESENT_N",
			"RSSD09_PRESENT_N", "RSSD10_PRESENT_N",
			"RSSD11_PRESENT_N", "RSSD12_PRESENT_N",
			/* GPORT4 */
			"RSSD13_PRESENT_N", "RSSD14_PRESENT_N",
			"RSSD15_PRESENT_N", "RSSD16_PRESENT_N",
			"LED_ID_FAN_ASM01", "LED_ID_FAN_ASM02",
			"LED_ID_FAN_ASM03", "LED_ID_FAN_ASM04",
			/* GPORT5 */
			"LED_ID_FAN_ASM05", "LED_ID_FAN_ASM06",
			"PLUG_DETECT_FAN_ASM01", "PLUG_DETECT_FAN_ASM02",
			"PLUG_DETECT_FAN_ASM03", "PLUG_DETECT_FAN_ASM04",
			"PLUG_DETECT_FAN_ASM05", "PLUG_DETECT_FAN_ASM06",
			/* GPORT6 */
			"SSB_RSSD01_ALERT_N", "SSB_RSSD02_ALERT_N",
			"SSB_RSSD03_ALERT_N", "SSB_RSSD04_ALERT_N",
			"SSB_RSSD05_ALERT_N", "SSB_RSSD06_ALERT_N",
			"SSB_RSSD07_ALERT_N", "SSB_RSSD08_ALERT_N",
			/* GPORT7 */
			"SSB_RSSD09_ALERT_N", "SSB_RSSD10_ALERT_N",
			"SSB_RSSD11_ALERT_N", "SSB_RSSD12_ALERT_N",
			"SSB_RSSD13_ALERT_N", "SSB_RSSD14_ALERT_N",
			"SSB_RSSD15_ALERT_N", "SSB_RSSD16_ALERT_N";
			pinctrl-0 = <&U65200_pins>;
			pinctrl-names = "default";
			U65200_pins: cfg-pins {
				pins =  "gp60", "gp61", "gp62",
				"gp63", "gp64", "gp65", "gp66",
				"gp67", "gp70", "gp71", "gp72",
				"gp73", "gp74", "gp75", "gp76", "gp77";
				function = "gpio";
				input-enable;
				bias-pull-up;
			};
		};
	};
	i2c@1 {
		reg = <1>;
		#address-cells = <1>;
		#size-cells = <0>;
		smb_svc_pex_rssd17_32: pinctrl@20 {
			compatible = "cypress,cy8c9560";
			reg = <0x20>;
			gpio-controller;
			#gpio-cells = <2>;
			interrupt-parent = <&gpio0>;
			interrupts = <ASPEED_GPIO(H, 0) IRQ_TYPE_LEVEL_HIGH>;
			interrupt-controller;
			#interrupt-cells = <2>;
			vdd-supply = <&p3v3_bmc_aux>;
			reset-gpios = <&smb_svc_pex_cpu1_led 17 GPIO_ACTIVE_HIGH>;
			gpio-line-names =
			/* GPORT0 */
			"LED_ID_RSSD17", "LED_ID_RSSD18",
			"LED_ID_RSSD19", "LED_ID_RSSD20",
			"LED_ID_RSSD21", "LED_ID_RSSD22",
			"LED_ID_RSSD23", "LED_ID_RSSD24",
			/* GPORT1 */
			"LED_ID_RSSD25", "LED_ID_RSSD26",
			"LED_ID_RSSD27", "LED_ID_RSSD28",
			"LED_ID_RSSD29", "LED_ID_RSSD30",
			"LED_ID_RSSD31", "LED_ID_RSSD32",
			/* GPORT2 */
			"RSSD17_PRESENT_N", "RSSD18_PRESENT_N",
			"RSSD19_PRESENT_N", "RSSD20_PRESENT_N",
			/* GPORT3 */
			"RSSD21_PRESENT_N", "RSSD22_PRESENT_N",
			"RSSD23_PRESENT_N", "RSSD24_PRESENT_N",
			"RSSD25_PRESENT_N", "RSSD26_PRESENT_N",
			"RSSD27_PRESENT_N", "RSSD28_PRESENT_N",
			/* GPORT4 */
			"RSSD29_PRESENT_N", "RSSD30_PRESENT_N",
			"RSSD31_PRESENT_N", "RSSD32_PRESENT_N",
			"LED_ID_FAN_ASM07", "LED_ID_FAN_ASM08",
			"LED_ID_FAN_ASM09", "LED_ID_FAN_ASM10",
			/* GPORT5 */
			"LED_ID_FAN_ASM11", "LED_ID_FAN_ASM12",
			"PLUG_DETECT_FAN_ASM07", "PLUG_DETECT_FAN_ASM08",
			"PLUG_DETECT_FAN_ASM09", "PLUG_DETECT_FAN_ASM10",
			"PLUG_DETECT_FAN_ASM11", "PLUG_DETECT_FAN_ASM12",
			/* GPORT6 */
			"SSB_RSSD17_ALERT_N", "SSB_RSSD18_ALERT_N",
			"SSB_RSSD19_ALERT_N", "SSB_RSSD20_ALERT_N",
			"SSB_RSSD21_ALERT_N", "SSB_RSSD22_ALERT_N",
			"SSB_RSSD23_ALERT_N", "SSB_RSSD24_ALERT_N",
			/* GPORT7 */
			"SSB_RSSD25_ALERT_N", "SSB_RSSD26_ALERT_N",
			"SSB_RSSD27_ALERT_N", "SSB_RSSD28_ALERT_N",
			"SSB_RSSD29_ALERT_N", "SSB_RSSD30_ALERT_N",
			"SSB_RSSD31_ALERT_N", "SSB_RSSD32_ALERT_N";
			pinctrl-0 = <&U65300_pins>;
			pinctrl-names = "default";
			U65300_pins: cfg-pins {
				pins = "gp60", "gp61", "gp62",
				"gp63", "gp64", "gp65", "gp66",
				"gp67", "gp70", "gp71", "gp72",
				"gp73", "gp74", "gp75", "gp76",
				"gp77";
				function = "gpio";
				input-enable;
				bias-pull-up;
			};
		};
	};
	i2c@2 {
		reg = <2>;
		#address-cells = <1>;
		#size-cells = <0>;
		smb_svc_pex_cpu1_led: pinctrl@20 {
			compatible = "cypress,cy8c9540";
			reg = <0x20>;
			gpio-controller;
			#gpio-cells = <2>;
			interrupt-parent = <&gpio0>;
			interrupts = <ASPEED_GPIO(V, 6) IRQ_TYPE_LEVEL_HIGH>;
			interrupt-controller;
			#interrupt-cells = <2>;
			vdd-supply = <&p3v3_bmc_aux>;
			reset-gpios = <&gpio0 ASPEED_GPIO(Q, 5) GPIO_ACTIVE_HIGH>;
			gpio-reserved-ranges = <18 2>, <36 2>;
			gpio-line-names =
			/* GPORT0 */
			"PLUG_DETECT_DIMM_C1E2", "PLUG_DETECT_DIMM_C1E1",
			"PLUG_DETECT_DIMM_C1F2", "PLUG_DETECT_DIMM_C1F1",
			"PLUG_DETECT_DIMM_C1G2", "PLUG_DETECT_DIMM_C1G1",
			"PLUG_DETECT_DIMM_C1H2", "PLUG_DETECT_DIMM_C1H1",
			/* GPORT1 */
			"PLUG_DETECT_DIMM_C1D1", "PLUG_DETECT_DIMM_C1D2",
			"PLUG_DETECT_DIMM_C1C1", "PLUG_DETECT_DIMM_C1C2",
			"PLUG_DETECT_DIMM_C1B1", "PLUG_DETECT_DIMM_C1B2",
			"PLUG_DETECT_DIMM_C1A1", "PLUG_DETECT_DIMM_C1A2",
			/* GPORT2 */
			"PEX_CPU1_EVENT_RST", "SVC_PEX_RSSD17_32_RST",
			"", "",
			/* GPORT3 */
			"LED_ID_DIMM_C1E2", "LED_ID_DIMM_C1E1",
			"LED_ID_DIMM_C1F2", "LED_ID_DIMM_C1F1",
			"LED_ID_DIMM_C1G2", "LED_ID_DIMM_C1G1",
			"LED_ID_DIMM_C1H2", "LED_ID_DIMM_C1H1",
			/* GPORT4 */
			"LED_ID_DIMM_C1A2", "LED_ID_DIMM_C1A1",
			"LED_ID_DIMM_C1B2", "LED_ID_DIMM_C1B1",
			"LED_ID_DIMM_C1C2", "LED_ID_DIMM_C1C1",
			"LED_ID_DIMM_C1D2", "LED_ID_DIMM_C1D1",
			/* GPORT5 */
			"", "",
			"FM_CPU1_SKTOCC_N", "LED_ID_CPU1";
		};
	};
	i2c@3 {
		reg = <3>;
		#address-cells = <1>;
		#size-cells = <0>;
		smb_svc_pex_fan_alert: pinctrl@20 {
			compatible = "cypress,cy8c9560";
			reg = <0x20>;
			gpio-controller;
			#gpio-cells = <2>;
			interrupt-parent = <&bmc_pex_irq>;
			interrupts = <8 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-controller;
			#interrupt-cells = <2>;
			vdd-supply = <&p3v3_aux>;
			reset-gpios = <&bmc_pex_irq 17 GPIO_ACTIVE_HIGH>;
			gpio-reserved-ranges = <24 3>, <51 9>;
			gpio-line-names =
			/* GPORT0 */
			"FAN01_SSB_ALERT_N", "FAN02_SSB_ALERT_N",
			"FAN03_SSB_ALERT_N", "FAN04_SSB_ALERT_N",
			"FAN05_SSB_ALERT_N", "FAN06_SSB_ALERT_N",
			"FAN07_SSB_ALERT_N", "FAN08_SSB_ALERT_N",
			/* GPORT1 */
			"FAN09_SSB_ALERT_N", "FAN10_SSB_ALERT_N",
			"FAN11_SSB_ALERT_N", "FAN12_SSB_ALERT_N",
			"FAN13_SSB_ALERT_N", "FAN14_SSB_ALERT_N",
			"FAN15_SSB_ALERT_N", "FAN16_SSB_ALERT_N",
			/* GPORT2 */
			"FAN17_SSB_ALERT_N", "FAN18_SSB_ALERT_N",
			"FAN19_SSB_ALERT_N", "FAN20_SSB_ALERT_N",
			/* GPORT3 */
			"FAN21_SSB_ALERT_N", "FAN22_SSB_ALERT_N",
			"FAN23_SSB_ALERT_N", "FAN24_SSB_ALERT_N",
			"", "",
			"", "FAN01_PWM_ALERT_N",
			/* GPORT4 */
			"FAN02_PWM_ALERT_N", "FAN03_PWM_ALERT_N",
			"FAN04_PWM_ALERT_N", "FAN05_PWM_ALERT_N",
			"FAN06_PWM_ALERT_N", "FAN07_PWM_ALERT_N",
			"FAN08_PWM_ALERT_N", "FAN09_PWM_ALERT_N",
			/* GPORT5 */
			"FAN10_PWM_ALERT_N", "FAN11_PWM_ALERT_N",
			"FAN12_PWM_ALERT_N", "FAN13_PWM_ALERT_N",
			"FAN14_PWM_ALERT_N", "FAN15_PWM_ALERT_N",
			"FAN16_PWM_ALERT_N", "FAN17_PWM_ALERT_N",
			/* GPORT6 */
			"FAN18_PWM_ALERT_N", "FAN19_PWM_ALERT_N",
			"FAN20_PWM_ALERT_N", "FAN21_PWM_ALERT_N",
			"FAN22_PWM_ALERT_N", "FAN23_PWM_ALERT_N",
			"FAN24_PWM_ALERT_N", "",
			/* GPORT7 */
			"", "",
			"", "",
			"", "",
			"", "";
			pinctrl-0 = <&U65600_pins>;
			pinctrl-names = "default";
			U65600_pins: cfg-pins {
				pins = "gp00", "gp01", "gp02",
				"gp03", "gp04", "gp05", "gp06",
				"gp07", "gp10", "gp11", "gp12",
				"gp13", "gp14", "gp15", "gp16",
				"gp17", "gp20", "gp21", "gp22",
				"gp23", "gp30", "gp31", "gp32",
				"gp33", "gp37", "gp40", "gp41",
				"gp42", "gp43", "gp44", "gp45",
				"gp46", "gp47", "gp50", "gp51",
				"gp52", "gp53", "gp54", "gp55",
				"gp56", "gp57", "gp60", "gp61",
				"gp62", "gp63", "gp64", "gp65",
				"gp66";
				function = "gpio";
				input-enable;
				bias-pull-up;
			};
		};
	};
	i2c@4 {
		reg = <4>;
		#address-cells = <1>;
		#size-cells = <0>;
		smb_svc_pex_cpu2_led: pinctrl@20 {
			compatible = "cypress,cy8c9540";
			reg = <0x20>;
			gpio-controller;
			#gpio-cells = <2>;
			interrupt-parent = <&gpio0>;
			interrupts = <ASPEED_GPIO(V, 5) IRQ_TYPE_LEVEL_HIGH>;
			interrupt-controller;
			#interrupt-cells = <2>;
			vdd-supply = <&p3v3_bmc_aux>;
			reset-gpios = <&gpio0 ASPEED_GPIO(Q, 6) GPIO_ACTIVE_HIGH>;
			gpio-reserved-ranges = <17 3>, <36 2>;
			gpio-line-names =
			/* GPORT0 */
			"PLUG_DETECT_DIMM_C2E2", "PLUG_DETECT_DIMM_C2E1",
			"PLUG_DETECT_DIMM_C2F2", "PLUG_DETECT_DIMM_C2F1",
			"PLUG_DETECT_DIMM_C2G2", "PLUG_DETECT_DIMM_C2G1",
			"PLUG_DETECT_DIMM_C2H2", "PLUG_DETECT_DIMM_C2H1",
			/* GPORT1 */
			"PLUG_DETECT_DIMM_C2D1", "PLUG_DETECT_DIMM_C2D2",
			"PLUG_DETECT_DIMM_C2C1", "PLUG_DETECT_DIMM_C2C2",
			"PLUG_DETECT_DIMM_C2B1", "PLUG_DETECT_DIMM_C2B2",
			"PLUG_DETECT_DIMM_C2A1", "PLUG_DETECT_DIMM_C2A2",
			/* GPORT2 */
			"PEX_CPU2_EVENT_RST", "",
			"", "",
			/* GPORT3 */
			"LED_ID_DIMM_C2E2", "LED_ID_DIMM_C2E1",
			"LED_ID_DIMM_C2F2", "LED_ID_DIMM_C2F1",
			"LED_ID_DIMM_C2G2", "LED_ID_DIMM_C2G1",
			"LED_ID_DIMM_C2H2", "LED_ID_DIMM_C2H1",
			/* GPORT4 */
			"LED_ID_DIMM_C2A2", "LED_ID_DIMM_C2A1",
			"LED_ID_DIMM_C2B2", "LED_ID_DIMM_C2B1",
			"LED_ID_DIMM_C2C2", "LED_ID_DIMM_C2C1",
			"LED_ID_DIMM_C2D2", "LED_ID_DIMM_C2D1",
			/* GPORT5 */
			"", "",
			"FM_CPU2_SKTOCC_N", "LED_ID_CPU2";
		};
	};
	i2c@5 {
		reg = <5>;
		#address-cells = <1>;
		#size-cells = <0>;

		smb_svc_pex_cpu3_led: pinctrl@20 {
			compatible = "cypress,cy8c9540";
			reg = <0x20>;
			gpio-controller;
			#gpio-cells = <2>;
			interrupt-parent = <&gpio0>;
			interrupts = <ASPEED_GPIO(V, 3) IRQ_TYPE_LEVEL_HIGH>;
			interrupt-controller;
			#interrupt-cells = <2>;
			vdd-supply = <&p3v3_bmc_aux>;
			reset-gpios = <&gpio0 ASPEED_GPIO(Q, 7) GPIO_ACTIVE_HIGH>;
			gpio-reserved-ranges = <17 3>;
			gpio-line-names =
			/* GPORT0 */
			"PLUG_DETECT_DIMM_C3E2", "PLUG_DETECT_DIMM_C3E1",
			"PLUG_DETECT_DIMM_C3F2", "PLUG_DETECT_DIMM_C3F1",
			"PLUG_DETECT_DIMM_C3G2", "PLUG_DETECT_DIMM_C3G1",
			"PLUG_DETECT_DIMM_C3H2", "PLUG_DETECT_DIMM_C3H1",
			/* GPORT1 */
			"PLUG_DETECT_DIMM_C3D1", "PLUG_DETECT_DIMM_C3D2",
			"PLUG_DETECT_DIMM_C3C1", "PLUG_DETECT_DIMM_C3C2",
			"PLUG_DETECT_DIMM_C3B1", "PLUG_DETECT_DIMM_C3B2",
			"PLUG_DETECT_DIMM_C3A1", "PLUG_DETECT_DIMM_C3A2",
			/* GPORT2 */
			"PEX_CPU3_EVENT_RST", "",
			"", "",
			/* GPORT3 */
			"LED_ID_DIMM_C3E2", "LED_ID_DIMM_C3E1",
			"LED_ID_DIMM_C3F2", "LED_ID_DIMM_C3F1",
			"LED_ID_DIMM_C3G2", "LED_ID_DIMM_C3G1",
			"LED_ID_DIMM_C3H2", "LED_ID_DIMM_C3H1",
			/* GPORT4 */
			"LED_ID_DIMM_C3A2", "LED_ID_DIMM_C3A1",
			"LED_ID_DIMM_C3B2", "LED_ID_DIMM_C3B1",
			"LED_ID_DIMM_C3C2", "LED_ID_DIMM_C3C1",
			"LED_ID_DIMM_C3D2", "LED_ID_DIMM_C3D1",
			/* GPORT5 */
			"LED_PWR_DWR_FRNT", "LED_ID_DWR_FRNT_P",
			"FM_CPU3_SKTOCC_N", "LED_ID_CPU3";
		};
	};
	i2c@6 {
		reg = <6>;
		#address-cells = <1>;
		#size-cells = <0>;
		smb_svc_pex_cpu0_led: pinctrl@20 {
			compatible = "cypress,cy8c9540";
			reg = <0x20>;
			gpio-controller;
			#gpio-cells = <2>;
			interrupt-parent = <&gpio0>;
			interrupts = <ASPEED_GPIO(O, 3) IRQ_TYPE_LEVEL_HIGH>;
			interrupt-controller;
			#interrupt-cells = <2>;
			vdd-supply = <&p3v3_bmc_aux>;
			reset-gpios = <&gpio0 ASPEED_GPIO(Q, 4) GPIO_ACTIVE_HIGH>;
			gpio-reserved-ranges = <18 2>, <36 2>;
			gpio-line-names =
			/* GPORT0 */
			"PLUG_DETECT_DIMM_C0E2", "PLUG_DETECT_DIMM_C0E1",
			"PLUG_DETECT_DIMM_C0F2", "PLUG_DETECT_DIMM_C0F1",
			"PLUG_DETECT_DIMM_C0G2", "PLUG_DETECT_DIMM_C0G1",
			"PLUG_DETECT_DIMM_C0H2", "PLUG_DETECT_DIMM_C0H1",
			/* GPORT1 */
			"PLUG_DETECT_DIMM_C0D1", "PLUG_DETECT_DIMM_C0D2",
			"PLUG_DETECT_DIMM_C0C1", "PLUG_DETECT_DIMM_C0C2",
			"PLUG_DETECT_DIMM_C0B1", "PLUG_DETECT_DIMM_C0B2",
			"PLUG_DETECT_DIMM_C0A1", "PLUG_DETECT_DIMM_C0A2",
			/* GPORT2 */
			"PEX_CPU0_EVENT_RST", "SVC_PEX_RSSD01_16_RST",
			"", "",
			/* GPORT3 */
			"LED_ID_DIMM_C0E2", "LED_ID_DIMM_C0E1",
			"LED_ID_DIMM_C0F2", "LED_ID_DIMM_C0F1",
			"LED_ID_DIMM_C0G2", "LED_ID_DIMM_C0G1",
			"LED_ID_DIMM_C0H2", "LED_ID_DIMM_C0H1",
			/* GPORT4 */
			"LED_ID_DIMM_C0A2", "LED_ID_DIMM_C0A1",
			"LED_ID_DIMM_C0B2", "LED_ID_DIMM_C0B1",
			"LED_ID_DIMM_C0C2", "LED_ID_DIMM_C0C1",
			"LED_ID_DIMM_C0D2", "LED_ID_DIMM_C0D1",
			/* GPORT5 */
			"", "",
			"FM_CPU0_SKTOCC_N", "LED_ID_CPU0";
		};
	};
};

&i2c9 {
	status = "okay";

	p1v2_bmc_aux_mon: pmic@60 {
		compatible = "maxim,max8952";
		reg = <0x60>;
		max8952,default-mode = <3>;
		max8952,dvs-mode-microvolt = <1100000>, <1100000>,
					     <1100000>, <1100000>;
		max8952,sync-freq = <0>;
		max8952,ramp-speed = <0>;
		regulator-always-on;
		regulator-boot-on;
	};
};

&i2cmux8 {
	i2c@0 {
		reg = <0>;
		#address-cells = <1>;
		#size-cells = <0>;

		fan10_ssb: regulator@3a {
			compatible = "maxim,max5978";
			reg = <0x3a>;
			vss1-supply = <&p12v>;
			interrupt-parent = <&smb_svc_pex_fan_alert>;
			interrupts = <9 IRQ_TYPE_LEVEL_LOW>;

			regulators {
				sw0_fan10_ssb: sw0 {
					regulator-name = "fan10_supply";
					shunt-resistor-micro-ohms = <10000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <3400000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};

	};
	i2c@1 {
		reg = <1>;
		#address-cells = <1>;
		#size-cells = <0>;

		fan12_ssb: regulator@3a {
			compatible = "maxim,max5978";
			reg = <0x3a>;
			vss1-supply = <&p12v>;
			interrupt-parent = <&smb_svc_pex_fan_alert>;
			interrupts = <11 IRQ_TYPE_LEVEL_LOW>;

			regulators {
				sw0_fan12_ssb: sw0 {
					regulator-name = "fan12_supply";
					shunt-resistor-micro-ohms = <10000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <3400000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};

	};
	i2c@2 {
		reg = <2>;
		#address-cells = <1>;
		#size-cells = <0>;

		fan14_ssb: regulator@3a {
			compatible = "maxim,max5978";
			reg = <0x3a>;
			vss1-supply = <&p12v>;
			interrupt-parent = <&smb_svc_pex_fan_alert>;
			interrupts = <13 IRQ_TYPE_LEVEL_LOW>;

			regulators {
				sw0_fan14_ssb: sw0 {
					regulator-name = "fan14_supply";
					shunt-resistor-micro-ohms = <10000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <3400000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@3 {
		reg = <3>;
		#address-cells = <1>;
		#size-cells = <0>;

		fan16_ssb: regulator@3a {
			compatible = "maxim,max5978";
			reg = <0x3a>;
			vss1-supply = <&p12v>;
			interrupt-parent = <&smb_svc_pex_fan_alert>;
			interrupts = <15 IRQ_TYPE_LEVEL_LOW>;

			regulators {
				sw0_fan16_ssb: sw0 {
					regulator-name = "fan16_supply";
					shunt-resistor-micro-ohms = <10000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <3400000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@4 {
		reg = <4>;
		#address-cells = <1>;
		#size-cells = <0>;

		fan18_ssb: regulator@3a {
			compatible = "maxim,max5978";
			reg = <0x3a>;
			vss1-supply = <&p12v>;
			interrupt-parent = <&smb_svc_pex_fan_alert>;
			interrupts = <17 IRQ_TYPE_LEVEL_LOW>;

			regulators {
				sw0_fan18_ssb: sw0 {
					regulator-name = "fan18_supply";
					shunt-resistor-micro-ohms = <10000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <3400000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@5 {
		reg = <5>;
		#address-cells = <1>;
		#size-cells = <0>;

		fan20_ssb: regulator@3a {
			compatible = "maxim,max5978";
			reg = <0x3a>;
			vss1-supply = <&p12v>;
			interrupt-parent = <&smb_svc_pex_fan_alert>;
			interrupts = <19 IRQ_TYPE_LEVEL_LOW>;

			regulators {
				sw0_fan20_ssb: sw0 {
					regulator-name = "fan20_supply";
					shunt-resistor-micro-ohms = <10000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <3400000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@6 {
		reg = <6>;
		#address-cells = <1>;
		#size-cells = <0>;

		fan22_ssb: regulator@3a {
			compatible = "maxim,max5978";
			reg = <0x3a>;
			vss1-supply = <&p12v>;
			interrupt-parent = <&smb_svc_pex_fan_alert>;
			interrupts = <21 IRQ_TYPE_LEVEL_LOW>;

			regulators {
				sw0_fan22_ssb: sw0 {
					regulator-name = "fan22_supply";
					shunt-resistor-micro-ohms = <10000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <3400000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@7 {
		reg = <7>;
		#address-cells = <1>;
		#size-cells = <0>;

		fan24_ssb: regulator@3a {
			compatible = "maxim,max5978";
			reg = <0x3a>;
			vss1-supply = <&p12v>;
			interrupt-parent = <&smb_svc_pex_fan_alert>;
			interrupts = <23 IRQ_TYPE_LEVEL_LOW>;

			regulators {
				sw0_fan24_ssb: sw0 {
					regulator-name = "fan24_supply";
					shunt-resistor-micro-ohms = <10000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <3400000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
};

&i2cmux7 {
	i2c@0 {
		reg = <0>;
		#address-cells = <1>;
		#size-cells = <0>;

		fan17_ssb: regulator@3a {
			compatible = "maxim,max5978";
			reg = <0x3a>;
			vss1-supply = <&p12v>;
			interrupt-parent = <&smb_svc_pex_fan_alert>;
			interrupts = <16 IRQ_TYPE_LEVEL_LOW>;

			regulators {
				sw0_fan17_ssb: sw0 {
					regulator-name = "fan17_supply";
					shunt-resistor-micro-ohms = <10000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <3400000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@1 {
		reg = <1>;
		#address-cells = <1>;
		#size-cells = <0>;

		fan19_ssb: regulator@3a {
			compatible = "maxim,max5978";
			reg = <0x3a>;
			vss1-supply = <&p12v>;
			interrupt-parent = <&smb_svc_pex_fan_alert>;
			interrupts = <18 IRQ_TYPE_LEVEL_LOW>;

			regulators {
				sw0_fan19_ssb: sw0 {
					regulator-name = "fan19_supply";
					shunt-resistor-micro-ohms = <10000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <3400000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@2 {
		reg = <2>;
		#address-cells = <1>;
		#size-cells = <0>;

		fan21_ssb: regulator@3a {
			compatible = "maxim,max5978";
			reg = <0x3a>;
			vss1-supply = <&p12v>;
			interrupt-parent = <&smb_svc_pex_fan_alert>;
			interrupts = <20 IRQ_TYPE_LEVEL_LOW>;

			regulators {
				sw0_fan21_ssb: sw0 {
					regulator-name = "fan21_supply";
					shunt-resistor-micro-ohms = <10000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <3400000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@3 {
		reg = <3>;
		#address-cells = <1>;
		#size-cells = <0>;

		fan23_ssb: regulator@3a {
			compatible = "maxim,max5978";
			reg = <0x3a>;
			vss1-supply = <&p12v>;
			interrupt-parent = <&smb_svc_pex_fan_alert>;
			interrupts = <22 IRQ_TYPE_LEVEL_LOW>;

			regulators {
				sw0_fan23_ssb: sw0 {
					regulator-name = "fan23_supply";
					shunt-resistor-micro-ohms = <10000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <3400000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@4 {
		reg = <4>;
		#address-cells = <1>;
		#size-cells = <0>;

		fan02_ssb: regulator@3a {
			compatible = "maxim,max5978";
			reg = <0x3a>;
			vss1-supply = <&p12v>;
			interrupt-parent = <&smb_svc_pex_fan_alert>;
			interrupts = <1 IRQ_TYPE_LEVEL_LOW>;

			regulators {
				sw0_fan02_ssb: sw0 {
					regulator-name = "fan02_supply";
					shunt-resistor-micro-ohms = <10000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <3400000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@5 {
		reg = <5>;
		#address-cells = <1>;
		#size-cells = <0>;

		fan04_ssb: regulator@3a {
			compatible = "maxim,max5978";
			reg = <0x3a>;
			vss1-supply = <&p12v>;
			interrupt-parent = <&smb_svc_pex_fan_alert>;
			interrupts = <3 IRQ_TYPE_LEVEL_LOW>;

			regulators {
				sw0_fan04_ssb: sw0 {
					regulator-name = "fan04_supply";
					shunt-resistor-micro-ohms = <10000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <3400000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@6 {
		reg = <6>;
		#address-cells = <1>;
		#size-cells = <0>;

		fan06_ssb: regulator@3a {
			compatible = "maxim,max5978";
			reg = <0x3a>;
			vss1-supply = <&p12v>;
			interrupt-parent = <&smb_svc_pex_fan_alert>;
			interrupts = <5 IRQ_TYPE_LEVEL_LOW>;

			regulators {
				sw0_fan06_ssb: sw0 {
					regulator-name = "fan06_supply";
					shunt-resistor-micro-ohms = <10000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <3400000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@7 {
		reg = <7>;
		#address-cells = <1>;
		#size-cells = <0>;

		fan08_ssb: regulator@3a {
			compatible = "maxim,max5978";
			reg = <0x3a>;
			vss1-supply = <&p12v>;
			interrupt-parent = <&smb_svc_pex_fan_alert>;
			interrupts = <7 IRQ_TYPE_LEVEL_LOW>;

			regulators {
				sw0_fan08_ssb: sw0 {
					regulator-name = "fan08_supply";
					shunt-resistor-micro-ohms = <10000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <3400000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
};

&i2cmux6 {
	i2c@0 {
		reg = <0>;
		#address-cells = <1>;
		#size-cells = <0>;

		fan01_ssb: regulator@3a {
			compatible = "maxim,max5978";
			reg = <0x3a>;
			vss1-supply = <&p12v>;
			interrupt-parent = <&smb_svc_pex_fan_alert>;
			interrupts = <0 IRQ_TYPE_LEVEL_LOW>;

			regulators {
				sw0_fan01_ssb: sw0 {
					regulator-name = "fan01_supply";
					shunt-resistor-micro-ohms = <10000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <3400000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@1 {
		reg = <1>;
		#address-cells = <1>;
		#size-cells = <0>;

		fan03_ssb: regulator@3a {
			compatible = "maxim,max5978";
			reg = <0x3a>;
			vss1-supply = <&p12v>;
			interrupt-parent = <&smb_svc_pex_fan_alert>;
			interrupts = <2 IRQ_TYPE_LEVEL_LOW>;

			regulators {
				sw0_fan03_ssb: sw0 {
					regulator-name = "fan03_supply";

					shunt-resistor-micro-ohms = <10000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <3400000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@2 {
		reg = <2>;
		#address-cells = <1>;
		#size-cells = <0>;

		fan05_ssb: regulator@3a {
			compatible = "maxim,max5978";
			reg = <0x3a>;
			vss1-supply = <&p12v>;
			interrupt-parent = <&smb_svc_pex_fan_alert>;
			interrupts = <4 IRQ_TYPE_LEVEL_LOW>;

			regulators {
				sw0_fan05_ssb: sw0 {
					regulator-name = "fan05_supply";
					shunt-resistor-micro-ohms = <10000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <3400000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@3 {
		reg = <3>;
		#address-cells = <1>;
		#size-cells = <0>;

		fan07_ssb: regulator@3a {
			compatible = "maxim,max5978";
			reg = <0x3a>;
			vss1-supply = <&p12v>;
			interrupt-parent = <&smb_svc_pex_fan_alert>;
			interrupts = <6 IRQ_TYPE_LEVEL_LOW>;

			regulators {
				sw0_fan07_ssb: sw0 {
					regulator-name = "fan07_supply";
					shunt-resistor-micro-ohms = <10000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <3400000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@4 {
		reg = <4>;
		#address-cells = <1>;
		#size-cells = <0>;

		fan09_ssb: regulator@3a {
			compatible = "maxim,max5978";
			reg = <0x3a>;
			vss1-supply = <&p12v>;
			interrupt-parent = <&smb_svc_pex_fan_alert>;
			interrupts = <8 IRQ_TYPE_LEVEL_LOW>;

			regulators {
				sw0_fan09_ssb: sw0 {
					regulator-name = "fan09_supply";
					shunt-resistor-micro-ohms = <10000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <3400000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@5 {
		reg = <5>;
		#address-cells = <1>;
		#size-cells = <0>;

		fan11_ssb: regulator@3a {
			compatible = "maxim,max5978";
			reg = <0x3a>;
			vss1-supply = <&p12v>;
			interrupt-parent = <&smb_svc_pex_fan_alert>;
			interrupts = <10 IRQ_TYPE_LEVEL_LOW>;

			regulators {
				sw0_fan11_ssb: sw0 {
					regulator-name = "fan11_supply";
					shunt-resistor-micro-ohms = <10000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <3400000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@6 {
		reg = <6>;
		#address-cells = <1>;
		#size-cells = <0>;

		fan13_ssb: regulator@3a {
			compatible = "maxim,max5978";
			reg = <0x3a>;
			vss1-supply = <&p12v>;
			interrupt-parent = <&smb_svc_pex_fan_alert>;
			interrupts = <12 IRQ_TYPE_LEVEL_LOW>;

			regulators {
				sw0_fan13_ssb: sw0 {
					regulator-name = "fan13_supply";
					shunt-resistor-micro-ohms = <10000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <3400000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@7 {
		reg = <7>;
		#address-cells = <1>;
		#size-cells = <0>;

		fan15_ssb: regulator@3a {
			compatible = "maxim,max5978";
			reg = <0x3a>;
			vss1-supply = <&p12v>;
			interrupt-parent = <&smb_svc_pex_fan_alert>;
			interrupts = <14 IRQ_TYPE_LEVEL_LOW>;

			regulators {
				sw0_fan15_ssb: sw0 {
					regulator-name = "fan15_supply";
					shunt-resistor-micro-ohms = <10000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <3400000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};

	};
};

&i2cmux9 {
	i2c@0 {
		reg = <0>;
		#address-cells = <1>;
		#size-cells = <0>;

		ssb_rssd19: regulator@3a {
			compatible = "maxim,max5970";
			reg = <0x3a>;
			interrupt-parent = <&smb_svc_pex_rssd17_32>;
			interrupts = <46 IRQ_TYPE_LEVEL_LOW>;

			vss1-supply = <&p3v3_aux>;
			vss2-supply = <&p12v>;

			leds {
				#address-cells = <1>;
				#size-cells = <0>;

				led@0 {
					reg = <0>;
					label = "rssd19:green:power";
					default-state = "off";
				};
			};

			regulators {
				sw0_ssb_rssd19: sw0 {
					regulator-name = "rssd19_12v";
					shunt-resistor-micro-ohms = <9000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <4500000>;
					regulator-enable-ramp-delay = <1000>;
				};
				sw1_ssb_rssd19: sw1 {
					regulator-name = "rssd19_3v3";
					shunt-resistor-micro-ohms = <100000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <410000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@1 {
		reg = <1>;
		#address-cells = <1>;
		#size-cells = <0>;

		ssb_rssd18: regulator@3a {
			compatible = "maxim,max5970";
			reg = <0x3a>;
			interrupt-parent = <&smb_svc_pex_rssd17_32>;
			interrupts = <45 IRQ_TYPE_LEVEL_LOW>;

			vss1-supply = <&p3v3_aux>;
			vss2-supply = <&p12v>;

			leds {
				#address-cells = <1>;
				#size-cells = <0>;

				led@0 {
					reg = <0>;
					label = "rssd18:green:power";
					default-state = "off";
				};
			};

			regulators {
				sw0_ssb_rssd18: sw0 {
					regulator-name = "rssd18_12v";
					shunt-resistor-micro-ohms = <9000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <4500000>;
					regulator-enable-ramp-delay = <1000>;
				};
				sw1_ssb_rssd18: sw1 {
					regulator-name = "rssd18_3v3";
					shunt-resistor-micro-ohms = <100000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <410000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@2 {
		reg = <2>;
		#address-cells = <1>;
		#size-cells = <0>;

		ssb_rssd17: regulator@3a {
			compatible = "maxim,max5970";
			reg = <0x3a>;
			interrupt-parent = <&smb_svc_pex_rssd17_32>;
			interrupts = <44 IRQ_TYPE_LEVEL_LOW>;

			vss1-supply = <&p3v3_aux>;
			vss2-supply = <&p12v>;

			leds {
				#address-cells = <1>;
				#size-cells = <0>;

				led@0 {
					reg = <0>;
					label = "rssd17:green:power";
					default-state = "off";
				};
			};

			regulators {
				sw0_ssb_rssd17: sw0 {
					regulator-name = "rssd17_12v";
					shunt-resistor-micro-ohms = <9000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <4500000>;
					regulator-enable-ramp-delay = <1000>;
				};
				sw1_ssb_rssd17: sw1 {
					regulator-name = "rssd17_3v3";
					shunt-resistor-micro-ohms = <100000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <410000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@3 {
		reg = <3>;
		#address-cells = <1>;
		#size-cells = <0>;

		ssb_rssd20: regulator@3a {
			compatible = "maxim,max5970";
			reg = <0x3a>;
			interrupt-parent = <&smb_svc_pex_rssd17_32>;
			interrupts = <47 IRQ_TYPE_LEVEL_LOW>;

			vss1-supply = <&p3v3_aux>;
			vss2-supply = <&p12v>;

			leds {
				#address-cells = <1>;
				#size-cells = <0>;

				led@0 {
					reg = <0>;
					label = "rssd20:green:power";
					default-state = "off";
				};
			};

			regulators {
				sw0_ssb_rssd20: sw0 {
					regulator-name = "rssd20_12v";
					shunt-resistor-micro-ohms = <9000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <4500000>;
					regulator-enable-ramp-delay = <1000>;
				};
				sw1_ssb_rssd20: sw1 {
					regulator-name = "rssd20_3v3";
					shunt-resistor-micro-ohms = <100000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <410000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@4 {
		reg = <4>;
		#address-cells = <1>;
		#size-cells = <0>;

		ssb_rssd21: regulator@3a {
			compatible = "maxim,max5970";
			reg = <0x3a>;
			interrupt-parent = <&smb_svc_pex_rssd17_32>;
			interrupts = <48 IRQ_TYPE_LEVEL_LOW>;

			vss1-supply = <&p3v3_aux>;
			vss2-supply = <&p12v>;

			leds {
				#address-cells = <1>;
				#size-cells = <0>;

				led@0 {
					reg = <0>;
					label = "rssd21:green:power";
					default-state = "off";
				};
			};

			regulators {
				sw0_ssb_rssd21: sw0 {
					regulator-name = "rssd21_12v";
					shunt-resistor-micro-ohms = <9000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <4500000>;
					regulator-enable-ramp-delay = <1000>;
				};
				sw1_ssb_rssd21: sw1 {
					regulator-name = "rssd21_3v3";
					shunt-resistor-micro-ohms = <100000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <410000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@5 {
		reg = <5>;
		#address-cells = <1>;
		#size-cells = <0>;

		ssb_rssd22: regulator@3a {
			compatible = "maxim,max5970";
			reg = <0x3a>;
			interrupt-parent = <&smb_svc_pex_rssd17_32>;
			interrupts = <49 IRQ_TYPE_LEVEL_LOW>;

			vss1-supply = <&p3v3_aux>;
			vss2-supply = <&p12v>;

			leds {
				#address-cells = <1>;
				#size-cells = <0>;

				led@0 {
					reg = <0>;
					label = "rssd22:green:power";
					default-state = "off";
				};
			};

			regulators {
				sw0_ssb_rssd22: sw0 {
					regulator-name = "rssd22_12v";
					shunt-resistor-micro-ohms = <9000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <4500000>;
					regulator-enable-ramp-delay = <1000>;
				};
				sw1_ssb_rssd22: sw1 {
					regulator-name = "rssd22_3v3";
					shunt-resistor-micro-ohms = <100000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <410000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@6 {
		reg = <6>;
		#address-cells = <1>;
		#size-cells = <0>;

		ssb_rssd24: regulator@3a {
			compatible = "maxim,max5970";
			reg = <0x3a>;
			interrupt-parent = <&smb_svc_pex_rssd17_32>;
			interrupts = <51 IRQ_TYPE_LEVEL_LOW>;

			vss1-supply = <&p3v3_aux>;
			vss2-supply = <&p12v>;

			leds {
				#address-cells = <1>;
				#size-cells = <0>;

				led@0 {
					reg = <0>;
					label = "rssd24:green:power";
					default-state = "off";
				};
			};

			regulators {
				sw0_ssb_rssd24: sw0 {
					regulator-name = "rssd24_12v";
					shunt-resistor-micro-ohms = <9000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <4500000>;
					regulator-enable-ramp-delay = <1000>;
				};
				sw1_ssb_rssd24: sw1 {
					regulator-name = "rssd24_3v3";
					shunt-resistor-micro-ohms = <100000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <410000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@7 {
		reg = <7>;
		#address-cells = <1>;
		#size-cells = <0>;

		ssb_rssd23: regulator@3a {
			compatible = "maxim,max5970";
			reg = <0x3a>;
			interrupt-parent = <&smb_svc_pex_rssd17_32>;
			interrupts = <50 IRQ_TYPE_LEVEL_LOW>;

			vss1-supply = <&p3v3_aux>;
			vss2-supply = <&p12v>;

			leds {
				#address-cells = <1>;
				#size-cells = <0>;

				led@0 {
					reg = <0>;
					label = "rssd23:green:power";
					default-state = "off";
				};
			};

			regulators {
				sw0_ssb_rssd23: sw0 {
					regulator-name = "rssd23_12v";
					shunt-resistor-micro-ohms = <9000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <4500000>;
					regulator-enable-ramp-delay = <1000>;
				};
				sw1_ssb_rssd23: sw1 {
					regulator-name = "rssd23_3v3";
					shunt-resistor-micro-ohms = <100000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <410000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
};

&i2cmux10 {
	i2c@0 {
		reg = <0>;
		#address-cells = <1>;
		#size-cells = <0>;

		ssb_rssd25: regulator@3a {
			compatible = "maxim,max5970";
			reg = <0x3a>;
			interrupt-parent = <&smb_svc_pex_rssd17_32>;
			interrupts = <52 IRQ_TYPE_LEVEL_LOW>;

			vss1-supply = <&p3v3_aux>;
			vss2-supply = <&p12v>;

			leds {
				#address-cells = <1>;
				#size-cells = <0>;

				led@0 {
					reg = <0>;
					label = "rssd25:green:power";
					default-state = "off";
				};
			};

			regulators {
				sw0_ssb_rssd25: sw0 {
					regulator-name = "rssd25_12v";
					shunt-resistor-micro-ohms = <9000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <4500000>;
					regulator-enable-ramp-delay = <1000>;
				};
				sw1_ssb_rssd25: sw1 {
					regulator-name = "rssd25_3v3";
					shunt-resistor-micro-ohms = <100000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <410000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@1 {
		reg = <1>;
		#address-cells = <1>;
		#size-cells = <0>;

		ssb_rssd26: regulator@3a {
			compatible = "maxim,max5970";
			reg = <0x3a>;
			interrupt-parent = <&smb_svc_pex_rssd17_32>;
			interrupts = <53 IRQ_TYPE_LEVEL_LOW>;

			vss1-supply = <&p3v3_aux>;
			vss2-supply = <&p12v>;

			leds {
				#address-cells = <1>;
				#size-cells = <0>;

				led@0 {
					reg = <0>;
					label = "rssd26:green:power";
					default-state = "off";
				};
			};

			regulators {
				sw0_ssb_rssd26: sw0 {
					regulator-name = "rssd26_12v";
					shunt-resistor-micro-ohms = <9000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <4500000>;
					regulator-enable-ramp-delay = <1000>;
				};
				sw1_ssb_rssd26: sw1 {
					regulator-name = "rssd26_3v3";
					shunt-resistor-micro-ohms = <100000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <410000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@2 {
		reg = <2>;
		#address-cells = <1>;
		#size-cells = <0>;

		ssb_rssd27: regulator@3a {
			compatible = "maxim,max5970";
			reg = <0x3a>;
			interrupt-parent = <&smb_svc_pex_rssd17_32>;
			interrupts = <54 IRQ_TYPE_LEVEL_LOW>;

			vss1-supply = <&p3v3_aux>;
			vss2-supply = <&p12v>;

			leds {
				#address-cells = <1>;
				#size-cells = <0>;

				led@0 {
					reg = <0>;
					label = "rssd27:green:power";
					default-state = "off";
				};
			};

			regulators {
				sw0_ssb_rssd27: sw0 {
					regulator-name = "rssd27_12v";
					shunt-resistor-micro-ohms = <9000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <4500000>;
					regulator-enable-ramp-delay = <1000>;
				};
				sw1_ssb_rssd27: sw1 {
					regulator-name = "rssd27_3v3";
					shunt-resistor-micro-ohms = <100000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <410000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@3 {
		reg = <3>;
		#address-cells = <1>;
		#size-cells = <0>;

		ssb_rssd32: regulator@3a {
			compatible = "maxim,max5970";
			reg = <0x3a>;
			interrupt-parent = <&smb_svc_pex_rssd17_32>;
			interrupts = <59 IRQ_TYPE_LEVEL_LOW>;

			vss1-supply = <&p3v3_aux>;
			vss2-supply = <&p12v>;

			leds {
				#address-cells = <1>;
				#size-cells = <0>;

				led@0 {
					reg = <0>;
					label = "rssd32:green:power";
					default-state = "off";
				};
			};

			regulators {
				sw0_ssb_rssd32: sw0 {
					regulator-name = "rssd32_12v";
					shunt-resistor-micro-ohms = <9000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <4500000>;
					regulator-enable-ramp-delay = <1000>;
				};
				sw1_ssb_rssd32: sw1 {
					regulator-name = "rssd32_3v3";
					shunt-resistor-micro-ohms = <100000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <410000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@4 {
		reg = <4>;
		#address-cells = <1>;
		#size-cells = <0>;

		ssb_rssd31: regulator@3a {
			compatible = "maxim,max5970";
			reg = <0x3a>;
			interrupt-parent = <&smb_svc_pex_rssd17_32>;
			interrupts = <58 IRQ_TYPE_LEVEL_LOW>;

			vss1-supply = <&p3v3_aux>;
			vss2-supply = <&p12v>;

			leds {
				#address-cells = <1>;
				#size-cells = <0>;

				led@0 {
					reg = <0>;
					label = "rssd31:green:power";
					default-state = "off";
				};
			};

			regulators {
				sw0_ssb_rssd31: sw0 {
					regulator-name = "rssd31_12v";
					shunt-resistor-micro-ohms = <9000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <4500000>;
					regulator-enable-ramp-delay = <1000>;
				};
				sw1_ssb_rssd31: sw1 {
					regulator-name = "rssd31_3v3";
					shunt-resistor-micro-ohms = <100000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <410000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@5 {
		reg = <5>;
		#address-cells = <1>;
		#size-cells = <0>;

		ssb_rssd30: regulator@3a {
			compatible = "maxim,max5970";
			reg = <0x3a>;
			interrupt-parent = <&smb_svc_pex_rssd17_32>;
			interrupts = <57 IRQ_TYPE_LEVEL_LOW>;

			vss1-supply = <&p3v3_aux>;
			vss2-supply = <&p12v>;

			leds {
				#address-cells = <1>;
				#size-cells = <0>;

				led@0 {
					reg = <0>;
					label = "rssd30:green:power";
					default-state = "off";
				};
			};

			regulators {
				sw0_ssb_rssd30: sw0 {
					regulator-name = "rssd30_12v";
					shunt-resistor-micro-ohms = <9000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <4500000>;
					regulator-enable-ramp-delay = <1000>;
				};
				sw1_ssb_rssd30: sw1 {
					regulator-name = "rssd30_3v3";
					shunt-resistor-micro-ohms = <100000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <410000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@6 {
		reg = <6>;
		#address-cells = <1>;
		#size-cells = <0>;

		ssb_rssd29: regulator@3a {
			compatible = "maxim,max5970";
			reg = <0x3a>;
			interrupt-parent = <&smb_svc_pex_rssd17_32>;
			interrupts = <56 IRQ_TYPE_LEVEL_LOW>;

			vss1-supply = <&p3v3_aux>;
			vss2-supply = <&p12v>;

			leds {
				#address-cells = <1>;
				#size-cells = <0>;

				led@0 {
					reg = <0>;
					label = "rssd29:green:power";
					default-state = "off";
				};
			};

			regulators {
				sw0_ssb_rssd29: sw0 {
					regulator-name = "rssd29_12v";
					shunt-resistor-micro-ohms = <9000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <4500000>;
					regulator-enable-ramp-delay = <1000>;
				};
				sw1_ssb_rssd29: sw1 {
					regulator-name = "rssd29_3v3";
					shunt-resistor-micro-ohms = <100000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <410000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@7 {
		reg = <7>;
		#address-cells = <1>;
		#size-cells = <0>;

		ssb_rssd28: regulator@3a {
			compatible = "maxim,max5970";
			reg = <0x3a>;
			interrupt-parent = <&smb_svc_pex_rssd17_32>;
			interrupts = <55 IRQ_TYPE_LEVEL_LOW>;

			vss1-supply = <&p3v3_aux>;
			vss2-supply = <&p12v>;

			leds {
				#address-cells = <1>;
				#size-cells = <0>;

				led@0 {
					reg = <0>;
					label = "rssd28:green:power";
					default-state = "off";
				};
			};

			regulators {
				sw0_ssb_rssd28: sw0 {
					regulator-name = "rssd28_12v";
					shunt-resistor-micro-ohms = <9000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <4500000>;
					regulator-enable-ramp-delay = <1000>;
				};
				sw1_ssb_rssd28: sw1 {
					regulator-name = "rssd28_3v3";
					shunt-resistor-micro-ohms = <100000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <410000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
};

&i2cmux18 {
	i2c@0 {
		reg = <0>;
		#address-cells = <1>;
		#size-cells = <0>;

		ssb_rssd03: regulator@3a {
			compatible = "maxim,max5970";
			reg = <0x3a>;
			interrupt-parent = <&smb_svc_pex_rssd01_16>;
			interrupts = <46 IRQ_TYPE_LEVEL_LOW>;

			vss1-supply = <&p3v3_aux>;
			vss2-supply = <&p12v>;

			leds {
				#address-cells = <1>;
				#size-cells = <0>;

				led@0 {
					reg = <0>;
					label = "rssd03:green:power";
					default-state = "off";
				};
			};

			regulators {
				sw0_ssb_rssd03: sw0 {
					regulator-name = "rssd03_12v";
					shunt-resistor-micro-ohms = <9000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <4500000>;
					regulator-enable-ramp-delay = <1000>;
				};
				sw1_ssb_rssd03: sw1 {
					regulator-name = "rssd03_3v3";
					shunt-resistor-micro-ohms = <100000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <410000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@1 {
		reg = <1>;
		#address-cells = <1>;
		#size-cells = <0>;

		ssb_rssd02: regulator@3a {
			compatible = "maxim,max5970";
			reg = <0x3a>;
			interrupt-parent = <&smb_svc_pex_rssd01_16>;
			interrupts = <45 IRQ_TYPE_LEVEL_LOW>;

			vss1-supply = <&p3v3_aux>;
			vss2-supply = <&p12v>;

			leds {
				#address-cells = <1>;
				#size-cells = <0>;

				led@0 {
					reg = <0>;
					label = "rssd02:green:power";
					default-state = "off";
				};
			};

			regulators {
				sw0_ssb_rssd02: sw0 {
					regulator-name = "rssd02_12v";
					shunt-resistor-micro-ohms = <9000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <4500000>;
					regulator-enable-ramp-delay = <1000>;
				};
				sw1_ssb_rssd02: sw1 {
					regulator-name = "rssd02_3v3";
					shunt-resistor-micro-ohms = <100000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <410000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@2 {
		reg = <2>;
		#address-cells = <1>;
		#size-cells = <0>;

		ssb_rssd01: regulator@3a {
			compatible = "maxim,max5970";
			reg = <0x3a>;
			interrupt-parent = <&smb_svc_pex_rssd01_16>;
			interrupts = <44 IRQ_TYPE_LEVEL_LOW>;

			vss1-supply = <&p3v3_aux>;
			vss2-supply = <&p12v>;

			leds {
				#address-cells = <1>;
				#size-cells = <0>;

				led@0 {
					reg = <0>;
					label = "rssd01:green:power";
					default-state = "off";
				};
			};

			regulators {
				sw0_ssb_rssd01: sw0 {
					regulator-name = "rssd01_12v";
					shunt-resistor-micro-ohms = <9000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <4500000>;
					regulator-enable-ramp-delay = <1000>;
				};
				sw1_ssb_rssd01: sw1 {
					regulator-name = "rssd01_3v3";
					shunt-resistor-micro-ohms = <100000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <410000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@3 {
		reg = <3>;
		#address-cells = <1>;
		#size-cells = <0>;

		ssb_rssd04: regulator@3a {
			compatible = "maxim,max5970";
			reg = <0x3a>;
			interrupt-parent = <&smb_svc_pex_rssd01_16>;
			interrupts = <47 IRQ_TYPE_LEVEL_LOW>;

			vss1-supply = <&p3v3_aux>;
			vss2-supply = <&p12v>;

			leds {
				#address-cells = <1>;
				#size-cells = <0>;

				led@0 {
					reg = <0>;
					label = "rssd04:green:power";
					default-state = "off";
				};
			};

			regulators {
				sw0_ssb_rssd04: sw0 {
					regulator-name = "rssd04_12v";
					shunt-resistor-micro-ohms = <9000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <4500000>;
					regulator-enable-ramp-delay = <1000>;
				};
				sw1_ssb_rssd04: sw1 {
					regulator-name = "rssd04_3v3";
					shunt-resistor-micro-ohms = <100000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <410000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@4 {
		reg = <4>;
		#address-cells = <1>;
		#size-cells = <0>;

		ssb_rssd05: regulator@3a {
			compatible = "maxim,max5970";
			reg = <0x3a>;
			interrupt-parent = <&smb_svc_pex_rssd01_16>;
			interrupts = <48 IRQ_TYPE_LEVEL_LOW>;

			vss1-supply = <&p3v3_aux>;
			vss2-supply = <&p12v>;

			leds {
				#address-cells = <1>;
				#size-cells = <0>;

				led@0 {
					reg = <0>;
					label = "rssd05:green:power";
					default-state = "off";
				};
			};

			regulators {
				sw0_ssb_rssd05: sw0 {
					regulator-name = "rssd05_12v";
					shunt-resistor-micro-ohms = <9000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <4500000>;
					regulator-enable-ramp-delay = <1000>;
				};
				sw1_ssb_rssd05: sw1 {
					regulator-name = "rssd05_3v3";
					shunt-resistor-micro-ohms = <100000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <410000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@5 {
		reg = <5>;
		#address-cells = <1>;
		#size-cells = <0>;

		ssb_rssd08: regulator@3a {
			compatible = "maxim,max5970";
			reg = <0x3a>;
			interrupt-parent = <&smb_svc_pex_rssd01_16>;
			interrupts = <51 IRQ_TYPE_LEVEL_LOW>;

			vss1-supply = <&p3v3_aux>;
			vss2-supply = <&p12v>;

			leds {
				#address-cells = <1>;
				#size-cells = <0>;

				led@0 {
					reg = <0>;
					label = "rssd08:green:power";
					default-state = "off";
				};
			};

			regulators {
				sw0_ssb_rssd08: sw0 {
					regulator-name = "rssd08_12v";
					shunt-resistor-micro-ohms = <9000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <4500000>;
					regulator-enable-ramp-delay = <1000>;
				};
				sw1_ssb_rssd08: sw1 {
					regulator-name = "rssd08_3v3";
					shunt-resistor-micro-ohms = <100000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <410000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@6 {
		reg = <6>;
		#address-cells = <1>;
		#size-cells = <0>;

		ssb_rssd07: regulator@3a {
			compatible = "maxim,max5970";
			reg = <0x3a>;
			interrupt-parent = <&smb_svc_pex_rssd01_16>;
			interrupts = <50 IRQ_TYPE_LEVEL_LOW>;

			vss1-supply = <&p3v3_aux>;
			vss2-supply = <&p12v>;

			leds {
				#address-cells = <1>;
				#size-cells = <0>;

				led@0 {
					reg = <0>;
					label = "rssd07:green:power";
					default-state = "off";
				};
			};

			regulators {
				sw0_ssb_rssd07: sw0 {
					regulator-name = "rssd07_12v";
					shunt-resistor-micro-ohms = <9000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <4500000>;
					regulator-enable-ramp-delay = <1000>;
				};
				sw1_ssb_rssd07: sw1 {
					regulator-name = "rssd07_3v3";
					shunt-resistor-micro-ohms = <100000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <410000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@7 {
		reg = <7>;
		#address-cells = <1>;
		#size-cells = <0>;

		ssb_rssd06: regulator@3a {
			compatible = "maxim,max5970";
			reg = <0x3a>;
			interrupt-parent = <&smb_svc_pex_rssd01_16>;
			interrupts = <49 IRQ_TYPE_LEVEL_LOW>;

			vss1-supply = <&p3v3_aux>;
			vss2-supply = <&p12v>;

			leds {
				#address-cells = <1>;
				#size-cells = <0>;

				led@0 {
					reg = <0>;
					label = "rssd06:green:power";
					default-state = "off";
				};
			};

			regulators {
				sw0_ssb_rssd06: sw0 {
					regulator-name = "rssd06_12v";
					shunt-resistor-micro-ohms = <9000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <4500000>;
					regulator-enable-ramp-delay = <1000>;
				};
				sw1_ssb_rssd06: sw1 {
					regulator-name = "rssd06_3v3";
					shunt-resistor-micro-ohms = <100000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <410000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
};

&i2cmux19 {
	i2c@0 {
		reg = <0>;
		#address-cells = <1>;
		#size-cells = <0>;

		ssb_rssd14: regulator@3a {
			compatible = "maxim,max5970";
			reg = <0x3a>;
			interrupt-parent = <&smb_svc_pex_rssd01_16>;
			interrupts = <57 IRQ_TYPE_LEVEL_LOW>;

			vss1-supply = <&p3v3_aux>;
			vss2-supply = <&p12v>;

			leds {
				#address-cells = <1>;
				#size-cells = <0>;

				led@0 {
					reg = <0>;
					label = "rssd14:green:power";
					default-state = "off";
				};
			};

			regulators {
				sw0_ssb_rssd14: sw0 {
					regulator-name = "rssd14_12v";
					shunt-resistor-micro-ohms = <9000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <4500000>;
					regulator-enable-ramp-delay = <1000>;
				};
				sw1_ssb_rssd14: sw1 {
					regulator-name = "rssd14_3v3";
					shunt-resistor-micro-ohms = <100000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <410000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@1 {
		reg = <1>;
		#address-cells = <1>;
		#size-cells = <0>;

		ssb_rssd13: regulator@3a {
			compatible = "maxim,max5970";
			reg = <0x3a>;
			interrupt-parent = <&smb_svc_pex_rssd01_16>;
			interrupts = <56 IRQ_TYPE_LEVEL_LOW>;

			vss1-supply = <&p3v3_aux>;
			vss2-supply = <&p12v>;

			leds {
				#address-cells = <1>;
				#size-cells = <0>;

				led@0 {
					reg = <0>;
					label = "rssd13:green:power";
					default-state = "off";
				};
			};

			regulators {
				sw0_ssb_rssd13: sw0 {
					regulator-name = "rssd13_12v";
					shunt-resistor-micro-ohms = <9000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <4500000>;
					regulator-enable-ramp-delay = <1000>;
				};
				sw1_ssb_rssd13: sw1 {
					regulator-name = "rssd13_3v3";
					shunt-resistor-micro-ohms = <100000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <410000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@2 {
		reg = <2>;
		#address-cells = <1>;
		#size-cells = <0>;

		ssb_rssd12: regulator@3a {
			compatible = "maxim,max5970";
			reg = <0x3a>;
			interrupt-parent = <&smb_svc_pex_rssd01_16>;
			interrupts = <55 IRQ_TYPE_LEVEL_LOW>;

			vss1-supply = <&p3v3_aux>;
			vss2-supply = <&p12v>;

			leds {
				#address-cells = <1>;
				#size-cells = <0>;

				led@0 {
					reg = <0>;
					label = "rssd12:green:power";
					default-state = "off";
				};
			};

			regulators {
				sw0_ssb_rssd12: sw0 {
					regulator-name = "rssd12_12v";
					shunt-resistor-micro-ohms = <9000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <4500000>;
					regulator-enable-ramp-delay = <1000>;
				};
				sw1_ssb_rssd12: sw1 {
					regulator-name = "rssd12_3v3";
					shunt-resistor-micro-ohms = <100000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <410000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@3 {
		reg = <3>;
		#address-cells = <1>;
		#size-cells = <0>;

		ssb_rssd11: regulator@3a {
			compatible = "maxim,max5970";
			reg = <0x3a>;
			interrupt-parent = <&smb_svc_pex_rssd01_16>;
			interrupts = <54 IRQ_TYPE_LEVEL_LOW>;

			vss1-supply = <&p3v3_aux>;
			vss2-supply = <&p12v>;

			leds {
				#address-cells = <1>;
				#size-cells = <0>;

				led@0 {
					reg = <0>;
					label = "rssd11:green:power";
					default-state = "off";
				};
			};

			regulators {
				sw0_ssb_rssd11: sw0 {
					regulator-name = "rssd11_12v";
					shunt-resistor-micro-ohms = <9000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <4500000>;
					regulator-enable-ramp-delay = <1000>;
				};
				sw1_ssb_rssd11: sw1 {
					regulator-name = "rssd11_3v3";
					shunt-resistor-micro-ohms = <100000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <410000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@4 {
		reg = <4>;
		#address-cells = <1>;
		#size-cells = <0>;

		ssb_rssd10: regulator@3a {
			compatible = "maxim,max5970";
			reg = <0x3a>;
			interrupt-parent = <&smb_svc_pex_rssd01_16>;
			interrupts = <53 IRQ_TYPE_LEVEL_LOW>;

			vss1-supply = <&p3v3_aux>;
			vss2-supply = <&p12v>;

			leds {
				#address-cells = <1>;
				#size-cells = <0>;

				led@0 {
					reg = <0>;
					label = "rssd10:green:power";
					default-state = "off";
				};
			};

			regulators {
				sw0_ssb_rssd10: sw0 {
					regulator-name = "rssd10_12v";
					shunt-resistor-micro-ohms = <9000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <4500000>;
					regulator-enable-ramp-delay = <1000>;
				};
				sw1_ssb_rssd10: sw1 {
					regulator-name = "rssd10_3v3";
					shunt-resistor-micro-ohms = <100000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <410000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@5 {
		reg = <5>;
		#address-cells = <1>;
		#size-cells = <0>;

		ssb_rssd09: regulator@3a {
			compatible = "maxim,max5970";
			reg = <0x3a>;
			interrupt-parent = <&smb_svc_pex_rssd01_16>;
			interrupts = <52 IRQ_TYPE_LEVEL_LOW>;

			vss1-supply = <&p3v3_aux>;
			vss2-supply = <&p12v>;

			leds {
				#address-cells = <1>;
				#size-cells = <0>;

				led@0 {
					reg = <0>;
					label = "rssd09:green:power";
					default-state = "off";
				};
			};

			regulators {
				sw0_ssb_rssd09: sw0 {
					regulator-name = "rssd09_12v";
					shunt-resistor-micro-ohms = <9000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <4500000>;
					regulator-enable-ramp-delay = <1000>;
				};
				sw1_ssb_rssd09: sw1 {
					regulator-name = "rssd09_3v3";
					shunt-resistor-micro-ohms = <100000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <410000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@6 {
		reg = <6>;
		#address-cells = <1>;
		#size-cells = <0>;

		ssb_rssd15: regulator@3a {
			compatible = "maxim,max5970";
			reg = <0x3a>;
			interrupt-parent = <&smb_svc_pex_rssd01_16>;
			interrupts = <58 IRQ_TYPE_LEVEL_LOW>;

			vss1-supply = <&p3v3_aux>;
			vss2-supply = <&p12v>;

			leds {
				#address-cells = <1>;
				#size-cells = <0>;

				led@0 {
					reg = <0>;
					label = "rssd15:green:power";
					default-state = "off";
				};
			};

			regulators {
				sw0_ssb_rssd15: sw0 {
					regulator-name = "rssd15_12v";
					shunt-resistor-micro-ohms = <9000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <4500000>;
					regulator-enable-ramp-delay = <1000>;
				};
				sw1_ssb_rssd15: sw1 {
					regulator-name = "rssd15_3v3";
					shunt-resistor-micro-ohms = <100000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <410000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
	i2c@7 {
		reg = <7>;
		#address-cells = <1>;
		#size-cells = <0>;

		ssb_rssd16: regulator@3a {
			compatible = "maxim,max5970";
			reg = <0x3a>;
			interrupt-parent = <&smb_svc_pex_rssd01_16>;
			interrupts = <59 IRQ_TYPE_LEVEL_LOW>;

			vss1-supply = <&p3v3_aux>;
			vss2-supply = <&p12v>;

			leds {
				#address-cells = <1>;
				#size-cells = <0>;

				led@0 {
					reg = <0>;
					label = "rssd16:green:power";
					default-state = "off";
				};
			};

			regulators {
				sw0_ssb_rssd16: sw0 {
					regulator-name = "rssd16_12v";
					shunt-resistor-micro-ohms = <9000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <4500000>;
					regulator-enable-ramp-delay = <1000>;
				};
				sw1_ssb_rssd16: sw1 {
					regulator-name = "rssd16_3v3";
					shunt-resistor-micro-ohms = <100000>;
					regulator-over-current-protection;
					regulator-oc-protection-microamp = <410000>;
					regulator-enable-ramp-delay = <1000>;
				};
			};
		};
	};
};
