// SPDX-License-Identifier: GPL-2.0

#include <dt-bindings/input/input.h>
#include "tegra30.dtsi"

/ {
	chosen {
		stdout-path = &uartd;
	};

	aliases {
		i2c0 = &pwr_i2c;
		i2c1 = &gen2_i2c;

		mmc0 = &sdmmc4;	/* eMMC */

		rtc0 = &pmic;
		rtc1 = "/rtc@7000e000";

		spi0 = &dsi_spi;

		usb0 = &micro_usb;
	};

	memory {
		device_type = "memory";
		reg = <0x80000000 0x40000000>;
	};

	host1x@50000000 {
		dc@54200000 {
			rgb {
				status = "okay";

				port {
					dpi_output: endpoint {
						remote-endpoint = <&bridge_input>;
						bus-width = <24>;
					};
				};
			};
		};
	};

	bsev@6001b000 {
		status = "okay";
	};

	pinmux@70000868 {
		pinctrl-names = "default";
		pinctrl-0 = <&state_default>;

		state_default: pinmux {
			/* WLAN SDIO pinmux */
			sdmmc1_clk {
				nvidia,pins = "sdmmc1_clk_pz0";
				nvidia,function = "sdmmc1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc1_cmd {
				nvidia,pins = "sdmmc1_cmd_pz1",
						"sdmmc1_dat3_py4",
						"sdmmc1_dat2_py5",
						"sdmmc1_dat1_py6",
						"sdmmc1_dat0_py7";
				nvidia,function = "sdmmc1";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			wlan_reset {
				nvidia,pins = "pv3";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			wlan_host_wake {
				nvidia,pins = "pu6";
				nvidia,function = "pwm3";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* GNSS UART-B pinmux */
			gps_pwr_en {
				nvidia,pins = "kb_row6_pr6";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			gps_ldo_en {
				nvidia,pins = "ulpi_dir_py1";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			gps_clk_ref {
				nvidia,pins = "gmi_ad8_ph0";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			/* Bluetooth UART-C pinmux */
			uartc_cts_rxd {
				nvidia,pins = "uart3_cts_n_pa1",
						"uart3_rxd_pw7";
				nvidia,function = "uartc";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			uartc_rts_txd {
				nvidia,pins = "uart3_rts_n_pc0",
						"uart3_txd_pw6";
				nvidia,function = "uartc";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			bt_reset {
				nvidia,pins = "clk2_req_pcc5";
				nvidia,function = "dap";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			bt_dev_wake {
				nvidia,pins = "kb_row11_ps3";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			bt_host_wake {
				nvidia,pins = "kb_row12_ps4";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			bt_pcm_dap4 {
				nvidia,pins = "dap4_fs_pp4",
						"dap4_din_pp5",
						"dap4_dout_pp6",
						"dap4_sclk_pp7";
				nvidia,function = "i2s3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* EMMC pinmux */
			sdmmc4_clk {
				nvidia,pins = "sdmmc4_clk_pcc4";
				nvidia,function = "sdmmc4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc4_data {
				nvidia,pins = "sdmmc4_cmd_pt7",
						"sdmmc4_dat0_paa0",
						"sdmmc4_dat1_paa1",
						"sdmmc4_dat2_paa2",
						"sdmmc4_dat3_paa3",
						"sdmmc4_dat4_paa4",
						"sdmmc4_dat5_paa5",
						"sdmmc4_dat6_paa6",
						"sdmmc4_dat7_paa7";
				nvidia,function = "sdmmc4";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			sdmmc4_reset {
				nvidia,pins = "sdmmc4_rst_n_pcc3";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* I2C pinmux */
			gen1_i2c {
				nvidia,pins = "gen1_i2c_scl_pc4",
						"gen1_i2c_sda_pc5";
				nvidia,function = "i2c1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
				nvidia,lock = <TEGRA_PIN_DISABLE>;
			};

			gen2_i2c {
				nvidia,pins = "gen2_i2c_scl_pt5",
						"gen2_i2c_sda_pt6";
				nvidia,function = "i2c2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
				nvidia,lock = <TEGRA_PIN_DISABLE>;
			};

			cam_i2c {
				nvidia,pins = "cam_i2c_scl_pbb1",
						"cam_i2c_sda_pbb2";
				nvidia,function = "i2c3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
				nvidia,lock = <TEGRA_PIN_DISABLE>;
			};

			ddc_i2c {
				nvidia,pins = "ddc_scl_pv4",
						"ddc_sda_pv5";
				nvidia,function = "i2c4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,lock = <TEGRA_PIN_DISABLE>;
			};

			pwr_i2c {
				nvidia,pins = "pwr_i2c_scl_pz6",
						"pwr_i2c_sda_pz7";
				nvidia,function = "i2cpwr";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
				nvidia,open-drain = <TEGRA_PIN_ENABLE>;
				nvidia,lock = <TEGRA_PIN_DISABLE>;
			};

			mhl_i2c {
				nvidia,pins = "kb_col6_pq6",
						"kb_col7_pq7";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* GPIO keys pinmux */
			power_key {
				nvidia,pins = "gmi_wp_n_pc7";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			volume_down {
				nvidia,pins = "ulpi_data3_po4";
				nvidia,function = "spi3";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* Sensors pinmux */
			sen_vdd {
				nvidia,pins = "spi1_miso_px7";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			proxi_vdd {
				nvidia,pins = "spi2_miso_px1";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			sen_vio {
				nvidia,pins = "lcd_dc1_pd2";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			nct_irq {
				nvidia,pins = "gmi_iordy_pi5";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			bat_irq {
				nvidia,pins = "kb_row8_ps0";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			charger_irq {
				nvidia,pins = "gmi_cs1_n_pj2";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			mpu_irq {
				nvidia,pins = "gmi_ad12_ph4";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			compass_irq {
				nvidia,pins = "gmi_ad13_ph5";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			light_irq {
				nvidia,pins = "gmi_cs4_n_pk2";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* LED pinmux */
			backlight_en {
				nvidia,pins = "lcd_dc0_pn6";
				nvidia,function = "rsvd3";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			flash_led_en {
				nvidia,pins = "pbb3";
				nvidia,function = "vgp3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			keypad_led {
				nvidia,pins = "kb_row2_pr2",
						"kb_row3_pr3";
				nvidia,function = "rsvd3";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			/* NFC pinmux */
			nfc_irq {
				nvidia,pins = "spi2_cs1_n_pw2";
				nvidia,function = "spi2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			nfc_ven {
				nvidia,pins = "spi1_sck_px5";
				nvidia,function = "spi1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			nfc_firm {
				nvidia,pins = "kb_row0_pr0";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			/* DC pinmux */
			lcd_pwr {
				nvidia,pins = "lcd_pwr0_pb2",
						"lcd_pwr1_pc1";
				nvidia,function = "displaya";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			lcd_wr_n {
				nvidia,pins = "lcd_wr_n_pz3";
				nvidia,function = "displaya";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			lcd_id {
				nvidia,pins = "lcd_m1_pw1";
				nvidia,function = "displaya";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			lcd_pclk {
				nvidia,pins = "lcd_pclk_pb3",
						"lcd_de_pj1",
						"lcd_hsync_pj3",
						"lcd_vsync_pj4";
				nvidia,function = "displaya";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			lcd_rgb_blue {
				nvidia,pins = "lcd_d0_pe0",
						"lcd_d1_pe1",
						"lcd_d2_pe2",
						"lcd_d3_pe3",
						"lcd_d4_pe4",
						"lcd_d5_pe5",
						"lcd_d18_pm2",
						"lcd_d19_pm3";
				nvidia,function = "displaya";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			lcd_rgb_green {
				nvidia,pins = "lcd_d6_pe6",
						"lcd_d7_pe7",
						"lcd_d8_pf0",
						"lcd_d9_pf1",
						"lcd_d10_pf2",
						"lcd_d11_pf3",
						"lcd_d20_pm4",
						"lcd_d21_pm5";
				nvidia,function = "displaya";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			lcd_rgb_red {
				nvidia,pins = "lcd_d12_pf4",
						"lcd_d13_pf5",
						"lcd_d14_pf6",
						"lcd_d15_pf7",
						"lcd_d16_pm0",
						"lcd_d17_pm1",
						"lcd_d22_pm6",
						"lcd_d23_pm7";
				nvidia,function = "displaya";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* Bridge pinmux */
			bridge_reset {
				nvidia,pins = "ulpi_data1_po2";
				nvidia,function = "spi3";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			rgb_ic_en {
				nvidia,pins = "gmi_a18_pb1";
				nvidia,function = "uartd";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			bridge_clk {
				nvidia,pins = "clk3_out_pee0";
				nvidia,function = "extperiph3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			rgb_bridge {
				nvidia,pins = "lcd_sdin_pz2",
						"lcd_sdout_pn5",
						"lcd_cs0_n_pn4",
						"lcd_sck_pz4";
				nvidia,function = "spi5";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* Panel pinmux */
			panel_reset {
				nvidia,pins = "lcd_cs1_n_pw0";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			panel_vio {
				nvidia,pins = "ulpi_clk_py0";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			/* Touchscreen pinmux */
			touch_vdd {
				nvidia,pins = "kb_col1_pq1";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			touch_vio {
				nvidia,pins = "spi1_mosi_px4";
				nvidia,function = "spi2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			touch_int_n {
				nvidia,pins = "kb_col3_pq3";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			touch_rst_n {
				nvidia,pins = "ulpi_data0_po1";
				nvidia,function = "spi3";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			touch_maker_id {
				nvidia,pins = "kb_col2_pq2";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* MHL pinmux */
			mhl_vio {
				nvidia,pins = "pv2";
				nvidia,function = "owr";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			mhl_rst_n {
				nvidia,pins = "clk3_req_pee1";
				nvidia,function = "dev3";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			mhl_int {
				nvidia,pins = "crt_vsync_pv7";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			mhl_sel {
				nvidia,pins = "kb_row10_ps2";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			hdmi_hpd {
				nvidia,pins = "hdmi_int_pn7";
				nvidia,function = "hdmi";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* AUDIO pinmux */
			hp_detect {
				nvidia,pins = "pbb6";
				nvidia,function = "vgp6";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			hp_hook {
				nvidia,pins = "ulpi_data4_po5";
				nvidia,function = "ulpi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			ear_mic_en {
				nvidia,pins = "spi2_mosi_px0";
				nvidia,function = "spi2";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			audio_irq {
				nvidia,pins = "spi2_cs2_n_pw3";
				nvidia,function = "spi3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			audio_mclk {
				nvidia,pins = "clk1_out_pw4";
				nvidia,function = "extperiph1";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			dap_i2s0 {
				nvidia,pins = "dap1_fs_pn0",
						"dap1_din_pn1",
						"dap1_dout_pn2",
						"dap1_sclk_pn3";
				nvidia,function = "i2s0";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			dap_i2s1 {
				nvidia,pins = "dap2_fs_pa2",
						"dap2_sclk_pa3",
						"dap2_din_pa4",
						"dap2_dout_pa5";
				nvidia,function = "i2s1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* MUIC pinmux */
			muic_irq {
				nvidia,pins = "gmi_cs0_n_pj0";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			muic_dp2t {
				nvidia,pins = "pcc2";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			muic_usif {
				nvidia,pins = "ulpi_stp_py3";
				nvidia,function = "spi1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ifx_usb_vbus_en {
				nvidia,pins = "kb_row4_pr4";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			pcb_rev {
				nvidia,pins = "gmi_wait_pi7",
						"gmi_rst_n_pi4";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			jtag_rtck {
				nvidia,pins = "jtag_rtck_pu7";
				nvidia,function = "rtck";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			/* Camera pinmux */
			cam_mclk {
				nvidia,pins = "cam_mclk_pcc0";
				nvidia,function = "vi_alt3";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			cam_pmic_en {
				nvidia,pins = "pbb4";
				nvidia,function = "vgp4";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			front_cam_rst {
				nvidia,pins = "pbb5";
				nvidia,function = "vgp5";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			front_cam_vio {
				nvidia,pins = "ulpi_nxt_py2";
				nvidia,function = "rsvd2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			rear_cam_rst {
				nvidia,pins = "gmi_cs3_n_pk4";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			rear_cam_eprom_pr {
				nvidia,pins = "gmi_cs2_n_pk3";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			rear_cam_vcm_pwdn {
				nvidia,pins = "kb_row1_pr1";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* Haptic pinmux */
			haptic_en {
				nvidia,pins = "gmi_ad9_ph1";
				nvidia,function = "gmi";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			haptic_osc {
				nvidia,pins = "gmi_ad11_ph3";
				nvidia,function = "pwm3";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			/* Modem pinmux */
			cp2ap_ack1_host_active {
				nvidia,pins = "pu5";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			cp2ap_ack2_host_wakeup {
				nvidia,pins = "pv0";
				nvidia,function = "rsvd4";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			ap2cp_ack2_suspend_req {
				nvidia,pins = "kb_row14_ps6";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			ap2cp_ack1_slave_wakeup {
				nvidia,pins = "kb_row15_ps7";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_DOWN>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			cp_kkp {
				nvidia,pins = "kb_col0_pq0";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			cp_crash_irq {
				nvidia,pins = "kb_row13_ps5";
				nvidia,function = "kbc";
				nvidia,pull = <TEGRA_PIN_PULL_UP>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			ap2cp_uarta_tx_ipc {
				nvidia,pins = "pu0";
				nvidia,function = "uarta";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			ap2cp_uarta_rx_ipc {
				nvidia,pins = "pu1";
				nvidia,function = "uarta";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			fota_ap_cts_cp_rts {
				nvidia,pins = "pu2";
				nvidia,function = "uarta";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};
			fota_ap_rts_cp_cts {
				nvidia,pins = "pu3";
				nvidia,function = "uarta";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_ENABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			modem_enable {
				nvidia,pins = "ulpi_data7_po0";
				nvidia,function = "hsi";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};
			modem_reset {
				nvidia,pins = "pv1";
				nvidia,function = "rsvd1";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_DISABLE>;
			};

			dap_i2s2 {
				nvidia,pins = "dap3_fs_pp0",
						"dap3_din_pp1",
						"dap3_dout_pp2",
						"dap3_sclk_pp3";
				nvidia,function = "i2s2";
				nvidia,pull = <TEGRA_PIN_PULL_NONE>;
				nvidia,tristate = <TEGRA_PIN_DISABLE>;
				nvidia,enable-input = <TEGRA_PIN_ENABLE>;
			};

			/* GPIO power/drive control */
			drive_i2c {
				nvidia,pins = "drive_dbg",
						"drive_at5",
						"drive_gme",
						"drive_ddc",
						"drive_ao1";
				nvidia,high-speed-mode = <TEGRA_PIN_DISABLE>;
				nvidia,schmitt = <TEGRA_PIN_ENABLE>;
				nvidia,low-power-mode = <TEGRA_PIN_LP_DRIVE_DIV_1>;
				nvidia,pull-down-strength = <31>;
				nvidia,pull-up-strength = <31>;
				nvidia,slew-rate-rising = <TEGRA_PIN_SLEW_RATE_FASTEST>;
				nvidia,slew-rate-falling = <TEGRA_PIN_SLEW_RATE_FASTEST>;
			};

			drive_uart3 {
				nvidia,pins = "drive_uart3";
				nvidia,high-speed-mode = <TEGRA_PIN_DISABLE>;
				nvidia,schmitt = <TEGRA_PIN_ENABLE>;
				nvidia,low-power-mode = <TEGRA_PIN_LP_DRIVE_DIV_1>;
				nvidia,pull-down-strength = <31>;
				nvidia,pull-up-strength = <31>;
				nvidia,slew-rate-rising = <TEGRA_PIN_SLEW_RATE_FASTEST>;
				nvidia,slew-rate-falling = <TEGRA_PIN_SLEW_RATE_FASTEST>;
			};

			drive_gmi {
				nvidia,pins = "drive_at3";
				nvidia,high-speed-mode = <TEGRA_PIN_DISABLE>;
				nvidia,schmitt = <TEGRA_PIN_ENABLE>;
				nvidia,low-power-mode = <TEGRA_PIN_LP_DRIVE_DIV_1>;
				nvidia,pull-down-strength = <31>;
				nvidia,pull-up-strength = <31>;
				nvidia,slew-rate-rising = <TEGRA_PIN_SLEW_RATE_FASTEST>;
				nvidia,slew-rate-falling = <TEGRA_PIN_SLEW_RATE_FASTEST>;
			};
		};
	};

	uartd: serial@70006300 {
		status = "okay";
	};

	gen2_i2c: i2c@7000c400 {
		status = "okay";
		clock-frequency = <400000>;

		backlight: led-controller@36 {
			compatible = "ti,lm3533";
			reg = <0x36>;

			enable-gpios = <&gpio TEGRA_GPIO(N, 6) GPIO_ACTIVE_HIGH>;

			ti,boost-ovp-microvolt = <24000000>;
			ti,boost-freq-hz = <500000>;

			backlight-0 {
				compatible = "ti,lm3533-backlight";

				ti,max-current-microamp = <23400>;
				ti,linear-mapping-mode;
				ti,hardware-controlled;
			};
		};

		muic@44 {
			compatible = "maxim,max14526-muic";
			reg = <0x44>;

			maxim,ap-usb;

			usif-gpios = <&gpio TEGRA_GPIO(Y, 3) GPIO_ACTIVE_HIGH>;
			dp2t-gpios = <&gpio TEGRA_GPIO(CC, 2) GPIO_ACTIVE_HIGH>;
		};
	};

	pwr_i2c: i2c@7000d000 {
		status = "okay";
		clock-frequency = <400000>;

		pmic: max77663@1c {
			compatible = "maxim,max77663";
			reg = <0x1c>;

			interrupts = <GIC_SPI 86 IRQ_TYPE_LEVEL_HIGH>;
			#interrupt-cells = <2>;
			interrupt-controller;

			#gpio-cells = <2>;
			gpio-controller;

			system-power-controller;

			regulators {
				vdd_1v8_vio: sd2 {
					regulator-name = "vdd_1v8_gen";
					regulator-min-microvolt = <1800000>;
					regulator-max-microvolt = <1800000>;
					regulator-always-on;
					regulator-boot-on;
				};

				avdd_3v3_periph: ldo2 {
					regulator-name = "avdd_usb";
					regulator-min-microvolt = <3300000>;
					regulator-max-microvolt = <3300000>;
					regulator-always-on;
					regulator-boot-on;
				};

				vdd_usd: ldo3 {
					regulator-name = "vdd_sdmmc3";
					regulator-min-microvolt = <3000000>;
					regulator-max-microvolt = <3000000>;
					regulator-always-on;
					regulator-boot-on;
				};

				vcore_emmc: ldo5 {
					regulator-name = "vdd_ddr_rx";
					regulator-min-microvolt = <2850000>;
					regulator-max-microvolt = <2850000>;
					regulator-boot-on;
				};
			};
		};
	};

	dsi_spi: spi@7000dc00 {
		status = "okay";
		spi-max-frequency = <25000000>;

		bridge: bridge-spi@2 {
			compatible = "solomon,ssd2825";
			reg = <2>;

			#address-cells = <1>;
			#size-cells = <0>;

			spi-cpol;
			spi-cpha;

			spi-max-frequency = <1000000>;

			reset-gpios = <&gpio TEGRA_GPIO(O, 2) GPIO_ACTIVE_LOW>;

			dvdd-supply = <&vdd_1v2_rgb>;
			avdd-supply = <&vdd_1v2_rgb>;
			vddio-supply = <&vdd_1v8_vio>;

			solomon,hs-zero-delay-ns = <300>;
			solomon,hs-prep-delay-ns = <65>;

			clocks = <&ssd2825_refclk>;

			ports {
				#address-cells = <1>;
				#size-cells = <0>;

				port@0 {
					reg = <0>;

					bridge_input: endpoint {
						remote-endpoint = <&dpi_output>;
						bus-width = <24>;
					};
				};

				port@1 {
					reg = <1>;

					bridge_output: endpoint {
						remote-endpoint = <&panel_input>;
					};
				};
			};
		};
	};

	sdmmc4: sdhci@78000600 {
		status = "okay";
		bus-width = <8>;
		non-removable;

		vmmc-supply = <&vcore_emmc>;
		vqmmc-supply = <&vdd_1v8_vio>;
	};

	micro_usb: usb@7d000000 {
		status = "okay";
		dr_mode = "otg";
	};

	usb-phy@7d000000 {
		status = "okay";
		nvidia,hssync-start-delay = <0>;
		nvidia,xcvr-lsfslew = <2>;
		nvidia,xcvr-lsrslew = <2>;
		vbus-supply = <&avdd_3v3_periph>;
	};

	/* PMIC has a built-in 32KHz oscillator which is used by PMC */
	clk32k_in: clock-32k {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <32768>;
		clock-output-names = "pmic-oscillator";
	};

	ssd2825_refclk: clock-ssd2825 {
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <24000000>;
		clock-output-names = "ssd2825-refclk";
	};

	gpio-keys {
		compatible = "gpio-keys";

		key-power {
			label = "Power";
			gpios = <&gpio TEGRA_GPIO(C, 7) GPIO_ACTIVE_LOW>;
			linux,code = <KEY_ENTER>;
		};

		key-volume-down {
			label = "Volume Down";
			gpios = <&gpio TEGRA_GPIO(O, 4) GPIO_ACTIVE_LOW>;
			linux,code = <KEY_DOWN>;
		};
	};

	vdd_1v2_rgb: regulator-rgb1v2 {
		compatible = "regulator-fixed";
		regulator-name = "vdd_1v2_rgb";
		regulator-min-microvolt = <1200000>;
		regulator-max-microvolt = <1200000>;
		gpio = <&gpio TEGRA_GPIO(B, 1) GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};

	vcc_3v0_lcd: regulator-lcd3v {
		compatible = "regulator-fixed";
		regulator-name = "vcc_3v0_lcd";
		regulator-min-microvolt = <3000000>;
		regulator-max-microvolt = <3000000>;
	};

	iovcc_1v8_lcd: regulator-lcd1v8 {
		compatible = "regulator-fixed";
		regulator-name = "iovcc_1v8_lcd";
		regulator-min-microvolt = <1800000>;
		regulator-max-microvolt = <1800000>;
		gpio = <&gpio TEGRA_GPIO(Y, 0) GPIO_ACTIVE_HIGH>;
		enable-active-high;
	};
};
