// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
// Copyright (C) 2016 ARM Ltd.
// based on the Allwinner H3 dtsi:
//    Copyright (C) 2015 Jens Kuske <jenskuske@gmail.com>

#include <dt-bindings/clock/sun50i-a64-ccu.h>
#include <dt-bindings/clock/sun6i-rtc.h>
#include <dt-bindings/clock/sun8i-de2.h>
#include <dt-bindings/clock/sun8i-r-ccu.h>
#include <dt-bindings/interrupt-controller/arm-gic.h>
#include <dt-bindings/reset/sun50i-a64-ccu.h>
#include <dt-bindings/reset/sun8i-de2.h>
#include <dt-bindings/reset/sun8i-r-ccu.h>
#include <dt-bindings/thermal/thermal.h>

/ {
	interrupt-parent = <&gic>;
	#address-cells = <1>;
	#size-cells = <1>;

	chosen {
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;

		simplefb_lcd: framebuffer-lcd {
			compatible = "allwinner,simple-framebuffer",
				     "simple-framebuffer";
			allwinner,pipeline = "mixer0-lcd0";
			clocks = <&ccu CLK_TCON0>,
				 <&display_clocks CLK_MIXER0>;
			status = "disabled";
		};

		simplefb_hdmi: framebuffer-hdmi {
			compatible = "allwinner,simple-framebuffer",
				     "simple-framebuffer";
			allwinner,pipeline = "mixer1-lcd1-hdmi";
			clocks = <&display_clocks CLK_MIXER1>,
				 <&ccu CLK_TCON1>, <&ccu CLK_HDMI>;
			status = "disabled";
		};
	};

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu0: cpu@0 {
			compatible = "arm,cortex-a53";
			device_type = "cpu";
			reg = <0>;
			enable-method = "psci";
			clocks = <&ccu CLK_CPUX>;
			clock-names = "cpu";
			#cooling-cells = <2>;
			i-cache-size = <0x8000>;
			i-cache-line-size = <64>;
			i-cache-sets = <256>;
			d-cache-size = <0x8000>;
			d-cache-line-size = <64>;
			d-cache-sets = <128>;
			next-level-cache = <&l2_cache>;
		};

		cpu1: cpu@1 {
			compatible = "arm,cortex-a53";
			device_type = "cpu";
			reg = <1>;
			enable-method = "psci";
			clocks = <&ccu CLK_CPUX>;
			clock-names = "cpu";
			#cooling-cells = <2>;
			i-cache-size = <0x8000>;
			i-cache-line-size = <64>;
			i-cache-sets = <256>;
			d-cache-size = <0x8000>;
			d-cache-line-size = <64>;
			d-cache-sets = <128>;
			next-level-cache = <&l2_cache>;
		};

		cpu2: cpu@2 {
			compatible = "arm,cortex-a53";
			device_type = "cpu";
			reg = <2>;
			enable-method = "psci";
			clocks = <&ccu CLK_CPUX>;
			clock-names = "cpu";
			#cooling-cells = <2>;
			i-cache-size = <0x8000>;
			i-cache-line-size = <64>;
			i-cache-sets = <256>;
			d-cache-size = <0x8000>;
			d-cache-line-size = <64>;
			d-cache-sets = <128>;
			next-level-cache = <&l2_cache>;
		};

		cpu3: cpu@3 {
			compatible = "arm,cortex-a53";
			device_type = "cpu";
			reg = <3>;
			enable-method = "psci";
			clocks = <&ccu CLK_CPUX>;
			clock-names = "cpu";
			#cooling-cells = <2>;
			i-cache-size = <0x8000>;
			i-cache-line-size = <64>;
			i-cache-sets = <256>;
			d-cache-size = <0x8000>;
			d-cache-line-size = <64>;
			d-cache-sets = <128>;
			next-level-cache = <&l2_cache>;
		};

		l2_cache: l2-cache {
			compatible = "cache";
			cache-level = <2>;
			cache-unified;
			cache-size = <0x80000>;
			cache-line-size = <64>;
			cache-sets = <512>;
		};
	};

	de: display-engine {
		compatible = "allwinner,sun50i-a64-display-engine";
		allwinner,pipelines = <&mixer0>,
				      <&mixer1>;
		status = "disabled";
	};

	gpu_opp_table: opp-table-gpu {
		compatible = "operating-points-v2";

		opp-432000000 {
			opp-hz = /bits/ 64 <432000000>;
		};
	};

	osc24M: osc24M-clk {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <24000000>;
		clock-output-names = "osc24M";
	};

	osc32k: osc32k-clk {
		#clock-cells = <0>;
		compatible = "fixed-clock";
		clock-frequency = <32768>;
		clock-output-names = "ext-osc32k";
	};

	pmu {
		compatible = "arm,cortex-a53-pmu";
		interrupts = <GIC_SPI 116 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 117 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 118 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 119 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-affinity = <&cpu0>, <&cpu1>, <&cpu2>, <&cpu3>;
	};

	psci {
		compatible = "arm,psci-0.2";
		method = "smc";
	};

	sound: sound {
		#address-cells = <1>;
		#size-cells = <0>;
		compatible = "simple-audio-card";
		simple-audio-card,name = "sun50i-a64-audio";
		simple-audio-card,aux-devs = <&codec_analog>;
		simple-audio-card,routing =
				"Left DAC", "DACL",
				"Right DAC", "DACR",
				"ADCL", "Left ADC",
				"ADCR", "Right ADC";
		status = "disabled";

		simple-audio-card,dai-link@0 {
			format = "i2s";
			frame-master = <&link0_cpu>;
			bitclock-master = <&link0_cpu>;
			mclk-fs = <128>;

			link0_cpu: cpu {
				sound-dai = <&dai>;
			};

			link0_codec: codec {
				sound-dai = <&codec 0>;
			};
		};
	};

	timer {
		compatible = "arm,armv8-timer";
		allwinner,erratum-unknown1;
		arm,no-tick-in-suspend;
		interrupts = <GIC_PPI 13
			(GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_HIGH)>,
			     <GIC_PPI 14
			(GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_HIGH)>,
			     <GIC_PPI 11
			(GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_HIGH)>,
			     <GIC_PPI 10
			(GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_HIGH)>;
	};

	thermal-zones {
		cpu_thermal: cpu0-thermal {
			/* milliseconds */
			polling-delay-passive = <0>;
			polling-delay = <0>;
			thermal-sensors = <&ths 0>;

			cooling-maps {
				map0 {
					trip = <&cpu_alert0>;
					cooling-device = <&cpu0 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
							 <&cpu1 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
							 <&cpu2 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
							 <&cpu3 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
				};
				map1 {
					trip = <&cpu_alert1>;
					cooling-device = <&cpu0 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
							 <&cpu1 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
							 <&cpu2 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
							 <&cpu3 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
				};
			};

			trips {
				cpu_alert0: cpu-alert0 {
					/* milliCelsius */
					temperature = <75000>;
					hysteresis = <2000>;
					type = "passive";
				};

				cpu_alert1: cpu-alert1 {
					/* milliCelsius */
					temperature = <90000>;
					hysteresis = <2000>;
					type = "hot";
				};

				cpu_crit: cpu-crit {
					/* milliCelsius */
					temperature = <110000>;
					hysteresis = <2000>;
					type = "critical";
				};
			};
		};

		gpu0_thermal: gpu0-thermal {
			/* milliseconds */
			polling-delay-passive = <0>;
			polling-delay = <0>;
			thermal-sensors = <&ths 1>;

			trips {
				gpu0_crit: gpu0-crit {
					temperature = <110000>;
					hysteresis = <2000>;
					type = "critical";
				};
			};
		};

		gpu1_thermal: gpu1-thermal {
			/* milliseconds */
			polling-delay-passive = <0>;
			polling-delay = <0>;
			thermal-sensors = <&ths 2>;

			trips {
				gpu1_crit: gpu1-crit {
					temperature = <110000>;
					hysteresis = <2000>;
					type = "critical";
				};
			};
		};
	};

	soc {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <1>;
		ranges;

		bus@1000000 {
			compatible = "allwinner,sun50i-a64-de2";
			reg = <0x1000000 0x400000>;
			allwinner,sram = <&de2_sram 1>;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges = <0 0x1000000 0x400000>;

			display_clocks: clock@0 {
				compatible = "allwinner,sun50i-a64-de2-clk";
				reg = <0x0 0x10000>;
				clocks = <&ccu CLK_BUS_DE>,
					 <&ccu CLK_DE>;
				clock-names = "bus",
					      "mod";
				resets = <&ccu RST_BUS_DE>;
				#clock-cells = <1>;
				#reset-cells = <1>;
			};

			rotate: rotate@20000 {
				compatible = "allwinner,sun50i-a64-de2-rotate",
					     "allwinner,sun8i-a83t-de2-rotate";
				reg = <0x20000 0x10000>;
				interrupts = <GIC_SPI 96 IRQ_TYPE_LEVEL_HIGH>;
				clocks = <&display_clocks CLK_BUS_ROT>,
					 <&display_clocks CLK_ROT>;
				clock-names = "bus",
					      "mod";
				resets = <&display_clocks RST_ROT>;
			};

			mixer0: mixer@100000 {
				compatible = "allwinner,sun50i-a64-de2-mixer-0";
				reg = <0x100000 0x100000>;
				clocks = <&display_clocks CLK_BUS_MIXER0>,
					 <&display_clocks CLK_MIXER0>;
				clock-names = "bus",
					      "mod";
				resets = <&display_clocks RST_MIXER0>;

				ports {
					#address-cells = <1>;
					#size-cells = <0>;

					mixer0_out: port@1 {
						#address-cells = <1>;
						#size-cells = <0>;
						reg = <1>;

						mixer0_out_tcon0: endpoint@0 {
							reg = <0>;
							remote-endpoint = <&tcon0_in_mixer0>;
						};

						mixer0_out_tcon1: endpoint@1 {
							reg = <1>;
							remote-endpoint = <&tcon1_in_mixer0>;
						};
					};
				};
			};

			mixer1: mixer@200000 {
				compatible = "allwinner,sun50i-a64-de2-mixer-1";
				reg = <0x200000 0x100000>;
				clocks = <&display_clocks CLK_BUS_MIXER1>,
					 <&display_clocks CLK_MIXER1>;
				clock-names = "bus",
					      "mod";
				resets = <&display_clocks RST_MIXER1>;

				ports {
					#address-cells = <1>;
					#size-cells = <0>;

					mixer1_out: port@1 {
						#address-cells = <1>;
						#size-cells = <0>;
						reg = <1>;

						mixer1_out_tcon0: endpoint@0 {
							reg = <0>;
							remote-endpoint = <&tcon0_in_mixer1>;
						};

						mixer1_out_tcon1: endpoint@1 {
							reg = <1>;
							remote-endpoint = <&tcon1_in_mixer1>;
						};
					};
				};
			};
		};

		syscon: syscon@1c00000 {
			compatible = "allwinner,sun50i-a64-system-control";
			reg = <0x01c00000 0x1000>;
			#address-cells = <1>;
			#size-cells = <1>;
			ranges;

			sram_c: sram@18000 {
				compatible = "mmio-sram";
				reg = <0x00018000 0x28000>;
				#address-cells = <1>;
				#size-cells = <1>;
				ranges = <0 0x00018000 0x28000>;

				de2_sram: sram-section@0 {
					compatible = "allwinner,sun50i-a64-sram-c";
					reg = <0x0000 0x28000>;
				};
			};

			sram_c1: sram@1d00000 {
				compatible = "mmio-sram";
				reg = <0x01d00000 0x40000>;
				#address-cells = <1>;
				#size-cells = <1>;
				ranges = <0 0x01d00000 0x40000>;

				ve_sram: sram-section@0 {
					compatible = "allwinner,sun50i-a64-sram-c1",
						     "allwinner,sun4i-a10-sram-c1";
					reg = <0x000000 0x40000>;
				};
			};
		};

		dma: dma-controller@1c02000 {
			compatible = "allwinner,sun50i-a64-dma";
			reg = <0x01c02000 0x1000>;
			interrupts = <GIC_SPI 50 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&ccu CLK_BUS_DMA>;
			dma-channels = <8>;
			dma-requests = <27>;
			resets = <&ccu RST_BUS_DMA>;
			#dma-cells = <1>;
		};

		tcon0: lcd-controller@1c0c000 {
			compatible = "allwinner,sun50i-a64-tcon-lcd",
				     "allwinner,sun8i-a83t-tcon-lcd";
			reg = <0x01c0c000 0x1000>;
			interrupts = <GIC_SPI 86 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&ccu CLK_BUS_TCON0>, <&ccu CLK_TCON0>;
			clock-names = "ahb", "tcon-ch0";
			clock-output-names = "tcon-data-clock";
			#clock-cells = <0>;
			assigned-clocks = <&ccu CLK_TCON0>;
			assigned-clock-parents = <&ccu CLK_PLL_MIPI>;
			resets = <&ccu RST_BUS_TCON0>, <&ccu RST_BUS_LVDS>;
			reset-names = "lcd", "lvds";

			ports {
				#address-cells = <1>;
				#size-cells = <0>;

				tcon0_in: port@0 {
					#address-cells = <1>;
					#size-cells = <0>;
					reg = <0>;

					tcon0_in_mixer0: endpoint@0 {
						reg = <0>;
						remote-endpoint = <&mixer0_out_tcon0>;
					};

					tcon0_in_mixer1: endpoint@1 {
						reg = <1>;
						remote-endpoint = <&mixer1_out_tcon0>;
					};
				};

				tcon0_out: port@1 {
					#address-cells = <1>;
					#size-cells = <0>;
					reg = <1>;

					tcon0_out_dsi: endpoint@1 {
						reg = <1>;
						remote-endpoint = <&dsi_in_tcon0>;
						allwinner,tcon-channel = <1>;
					};
				};
			};
		};

		tcon1: lcd-controller@1c0d000 {
			compatible = "allwinner,sun50i-a64-tcon-tv",
				     "allwinner,sun8i-a83t-tcon-tv";
			reg = <0x01c0d000 0x1000>;
			interrupts = <GIC_SPI 87 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&ccu CLK_BUS_TCON1>, <&ccu CLK_TCON1>;
			clock-names = "ahb", "tcon-ch1";
			resets = <&ccu RST_BUS_TCON1>;
			reset-names = "lcd";

			ports {
				#address-cells = <1>;
				#size-cells = <0>;

				tcon1_in: port@0 {
					#address-cells = <1>;
					#size-cells = <0>;
					reg = <0>;

					tcon1_in_mixer0: endpoint@0 {
						reg = <0>;
						remote-endpoint = <&mixer0_out_tcon1>;
					};

					tcon1_in_mixer1: endpoint@1 {
						reg = <1>;
						remote-endpoint = <&mixer1_out_tcon1>;
					};
				};

				tcon1_out: port@1 {
					#address-cells = <1>;
					#size-cells = <0>;
					reg = <1>;

					tcon1_out_hdmi: endpoint@1 {
						reg = <1>;
						remote-endpoint = <&hdmi_in_tcon1>;
					};
				};
			};
		};

		video-codec@1c0e000 {
			compatible = "allwinner,sun50i-a64-video-engine";
			reg = <0x01c0e000 0x1000>;
			clocks = <&ccu CLK_BUS_VE>, <&ccu CLK_VE>,
				 <&ccu CLK_DRAM_VE>;
			clock-names = "ahb", "mod", "ram";
			resets = <&ccu RST_BUS_VE>;
			interrupts = <GIC_SPI 58 IRQ_TYPE_LEVEL_HIGH>;
			allwinner,sram = <&ve_sram 1>;
		};

		mmc0: mmc@1c0f000 {
			compatible = "allwinner,sun50i-a64-mmc";
			reg = <0x01c0f000 0x1000>;
			clocks = <&ccu CLK_BUS_MMC0>, <&ccu CLK_MMC0>;
			clock-names = "ahb", "mmc";
			resets = <&ccu RST_BUS_MMC0>;
			reset-names = "ahb";
			interrupts = <GIC_SPI 60 IRQ_TYPE_LEVEL_HIGH>;
			max-frequency = <150000000>;
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <0>;
		};

		mmc1: mmc@1c10000 {
			compatible = "allwinner,sun50i-a64-mmc";
			reg = <0x01c10000 0x1000>;
			clocks = <&ccu CLK_BUS_MMC1>, <&ccu CLK_MMC1>;
			clock-names = "ahb", "mmc";
			resets = <&ccu RST_BUS_MMC1>;
			reset-names = "ahb";
			interrupts = <GIC_SPI 61 IRQ_TYPE_LEVEL_HIGH>;
			max-frequency = <150000000>;
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <0>;
		};

		mmc2: mmc@1c11000 {
			compatible = "allwinner,sun50i-a64-emmc";
			reg = <0x01c11000 0x1000>;
			clocks = <&ccu CLK_BUS_MMC2>, <&ccu CLK_MMC2>;
			clock-names = "ahb", "mmc";
			resets = <&ccu RST_BUS_MMC2>;
			reset-names = "ahb";
			interrupts = <GIC_SPI 62 IRQ_TYPE_LEVEL_HIGH>;
			max-frequency = <150000000>;
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <0>;
		};

		sid: eeprom@1c14000 {
			compatible = "allwinner,sun50i-a64-sid";
			reg = <0x1c14000 0x400>;
			#address-cells = <1>;
			#size-cells = <1>;

			ths_calibration: thermal-sensor-calibration@34 {
				reg = <0x34 0x8>;
			};
		};

		crypto: crypto@1c15000 {
			compatible = "allwinner,sun50i-a64-crypto";
			reg = <0x01c15000 0x1000>;
			interrupts = <GIC_SPI 94 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&ccu CLK_BUS_CE>, <&ccu CLK_CE>;
			clock-names = "bus", "mod";
			resets = <&ccu RST_BUS_CE>;
		};

		msgbox: mailbox@1c17000 {
			compatible = "allwinner,sun50i-a64-msgbox",
				     "allwinner,sun6i-a31-msgbox";
			reg = <0x01c17000 0x1000>;
			clocks = <&ccu CLK_BUS_MSGBOX>;
			resets = <&ccu RST_BUS_MSGBOX>;
			interrupts = <GIC_SPI 49 IRQ_TYPE_LEVEL_HIGH>;
			#mbox-cells = <1>;
		};

		usb_otg: usb@1c19000 {
			compatible = "allwinner,sun8i-a33-musb";
			reg = <0x01c19000 0x0400>;
			clocks = <&ccu CLK_BUS_OTG>;
			resets = <&ccu RST_BUS_OTG>;
			interrupts = <GIC_SPI 71 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "mc";
			phys = <&usbphy 0>;
			phy-names = "usb";
			extcon = <&usbphy 0>;
			dr_mode = "otg";
			status = "disabled";
		};

		usbphy: phy@1c19400 {
			compatible = "allwinner,sun50i-a64-usb-phy";
			reg = <0x01c19400 0x14>,
			      <0x01c1a800 0x4>,
			      <0x01c1b800 0x4>;
			reg-names = "phy_ctrl",
				    "pmu0",
				    "pmu1";
			clocks = <&ccu CLK_USB_PHY0>,
				 <&ccu CLK_USB_PHY1>;
			clock-names = "usb0_phy",
				      "usb1_phy";
			resets = <&ccu RST_USB_PHY0>,
				 <&ccu RST_USB_PHY1>;
			reset-names = "usb0_reset",
				      "usb1_reset";
			status = "disabled";
			#phy-cells = <1>;
		};

		ehci0: usb@1c1a000 {
			compatible = "allwinner,sun50i-a64-ehci", "generic-ehci";
			reg = <0x01c1a000 0x100>;
			interrupts = <GIC_SPI 72 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&ccu CLK_BUS_OHCI0>,
				 <&ccu CLK_BUS_EHCI0>,
				 <&ccu CLK_USB_OHCI0>;
			resets = <&ccu RST_BUS_OHCI0>,
				 <&ccu RST_BUS_EHCI0>;
			phys = <&usbphy 0>;
			phy-names = "usb";
			status = "disabled";
		};

		ohci0: usb@1c1a400 {
			compatible = "allwinner,sun50i-a64-ohci", "generic-ohci";
			reg = <0x01c1a400 0x100>;
			interrupts = <GIC_SPI 73 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&ccu CLK_BUS_OHCI0>,
				 <&ccu CLK_USB_OHCI0>;
			resets = <&ccu RST_BUS_OHCI0>;
			phys = <&usbphy 0>;
			phy-names = "usb";
			status = "disabled";
		};

		ehci1: usb@1c1b000 {
			compatible = "allwinner,sun50i-a64-ehci", "generic-ehci";
			reg = <0x01c1b000 0x100>;
			interrupts = <GIC_SPI 74 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&ccu CLK_BUS_OHCI1>,
				 <&ccu CLK_BUS_EHCI1>,
				 <&ccu CLK_USB_OHCI1>;
			resets = <&ccu RST_BUS_OHCI1>,
				 <&ccu RST_BUS_EHCI1>;
			phys = <&usbphy 1>;
			phy-names = "usb";
			status = "disabled";
		};

		ohci1: usb@1c1b400 {
			compatible = "allwinner,sun50i-a64-ohci", "generic-ohci";
			reg = <0x01c1b400 0x100>;
			interrupts = <GIC_SPI 75 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&ccu CLK_BUS_OHCI1>,
				 <&ccu CLK_USB_OHCI1>;
			resets = <&ccu RST_BUS_OHCI1>;
			phys = <&usbphy 1>;
			phy-names = "usb";
			status = "disabled";
		};

		ccu: clock@1c20000 {
			compatible = "allwinner,sun50i-a64-ccu";
			reg = <0x01c20000 0x400>;
			clocks = <&osc24M>, <&rtc CLK_OSC32K>;
			clock-names = "hosc", "losc";
			#clock-cells = <1>;
			#reset-cells = <1>;
		};

		pio: pinctrl@1c20800 {
			compatible = "allwinner,sun50i-a64-pinctrl";
			reg = <0x01c20800 0x400>;
			interrupts = <GIC_SPI 11 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 17 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 21 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&ccu CLK_BUS_PIO>, <&osc24M>,
				 <&rtc CLK_OSC32K>;
			clock-names = "apb", "hosc", "losc";
			gpio-controller;
			#gpio-cells = <3>;
			interrupt-controller;
			#interrupt-cells = <3>;

			/omit-if-no-ref/
			aif2_pins: aif2-pins {
				pins = "PB4", "PB5", "PB6", "PB7";
				function = "aif2";
			};

			/omit-if-no-ref/
			aif3_pins: aif3-pins {
				pins = "PG10", "PG11", "PG12", "PG13";
				function = "aif3";
			};

			csi_pins: csi-pins {
				pins = "PE0", "PE2", "PE3", "PE4", "PE5", "PE6",
				       "PE7", "PE8", "PE9", "PE10", "PE11";
				function = "csi";
			};

			/omit-if-no-ref/
			csi_mclk_pin: csi-mclk-pin {
				pins = "PE1";
				function = "csi";
			};

			i2c0_pins: i2c0-pins {
				pins = "PH0", "PH1";
				function = "i2c0";
			};

			i2c1_pins: i2c1-pins {
				pins = "PH2", "PH3";
				function = "i2c1";
			};

			i2c2_pins: i2c2-pins {
				pins = "PE14", "PE15";
				function = "i2c2";
			};

			/omit-if-no-ref/
			lcd_rgb666_pins: lcd-rgb666-pins {
				pins = "PD0", "PD1", "PD2", "PD3", "PD4",
				       "PD5", "PD6", "PD7", "PD8", "PD9",
				       "PD10", "PD11", "PD12", "PD13",
				       "PD14", "PD15", "PD16", "PD17",
				       "PD18", "PD19", "PD20", "PD21";
				function = "lcd0";
			};

			mmc0_pins: mmc0-pins {
				pins = "PF0", "PF1", "PF2", "PF3",
				       "PF4", "PF5";
				function = "mmc0";
				drive-strength = <30>;
				bias-pull-up;
			};

			mmc1_pins: mmc1-pins {
				pins = "PG0", "PG1", "PG2", "PG3",
				       "PG4", "PG5";
				function = "mmc1";
				drive-strength = <30>;
				bias-pull-up;
			};

			mmc2_pins: mmc2-pins {
				pins = "PC5", "PC6", "PC8", "PC9",
				       "PC10","PC11", "PC12", "PC13",
				       "PC14", "PC15", "PC16";
				function = "mmc2";
				drive-strength = <30>;
				bias-pull-up;
			};

			mmc2_ds_pin: mmc2-ds-pin {
				pins = "PC1";
				function = "mmc2";
				drive-strength = <30>;
				bias-pull-up;
			};

			pwm_pin: pwm-pin {
				pins = "PD22";
				function = "pwm";
			};

			rmii_pins: rmii-pins {
				pins = "PD10", "PD11", "PD13", "PD14", "PD17",
				       "PD18", "PD19", "PD20", "PD22", "PD23";
				function = "emac";
				drive-strength = <40>;
			};

			rgmii_pins: rgmii-pins {
				pins = "PD8", "PD9", "PD10", "PD11", "PD12",
				       "PD13", "PD15", "PD16", "PD17", "PD18",
				       "PD19", "PD20", "PD21", "PD22", "PD23";
				function = "emac";
				drive-strength = <40>;
			};

			spdif_tx_pin: spdif-tx-pin {
				pins = "PH8";
				function = "spdif";
			};

			spi0_pins: spi0-pins {
				pins = "PC0", "PC1", "PC2", "PC3";
				function = "spi0";
			};

			spi1_pins: spi1-pins {
				pins = "PD0", "PD1", "PD2", "PD3";
				function = "spi1";
			};

			uart0_pb_pins: uart0-pb-pins {
				pins = "PB8", "PB9";
				function = "uart0";
			};

			uart1_pins: uart1-pins {
				pins = "PG6", "PG7";
				function = "uart1";
			};

			uart1_rts_cts_pins: uart1-rts-cts-pins {
				pins = "PG8", "PG9";
				function = "uart1";
			};

			uart2_pins: uart2-pins {
				pins = "PB0", "PB1";
				function = "uart2";
			};

			uart3_pins: uart3-pins {
				pins = "PD0", "PD1";
				function = "uart3";
			};

			uart4_pins: uart4-pins {
				pins = "PD2", "PD3";
				function = "uart4";
			};

			uart4_rts_cts_pins: uart4-rts-cts-pins {
				pins = "PD4", "PD5";
				function = "uart4";
			};
		};

		timer@1c20c00 {
			compatible = "allwinner,sun50i-a64-timer",
				     "allwinner,sun8i-a23-timer";
			reg = <0x01c20c00 0xa0>;
			interrupts = <GIC_SPI 18 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 19 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&osc24M>;
		};

		wdt0: watchdog@1c20ca0 {
			compatible = "allwinner,sun50i-a64-wdt",
				     "allwinner,sun6i-a31-wdt";
			reg = <0x01c20ca0 0x20>;
			interrupts = <GIC_SPI 25 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&osc24M>;
		};

		spdif: spdif@1c21000 {
			#sound-dai-cells = <0>;
			compatible = "allwinner,sun50i-a64-spdif",
				     "allwinner,sun8i-h3-spdif";
			reg = <0x01c21000 0x400>;
			interrupts = <GIC_SPI 12 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&ccu CLK_BUS_SPDIF>, <&ccu CLK_SPDIF>;
			resets = <&ccu RST_BUS_SPDIF>;
			clock-names = "apb", "spdif";
			dmas = <&dma 2>;
			dma-names = "tx";
			pinctrl-names = "default";
			pinctrl-0 = <&spdif_tx_pin>;
			status = "disabled";
		};

		lradc: lradc@1c21800 {
			compatible = "allwinner,sun50i-a64-lradc",
				     "allwinner,sun8i-a83t-r-lradc";
			reg = <0x01c21800 0x400>;
			interrupts = <GIC_SPI 30 IRQ_TYPE_LEVEL_HIGH>;
			status = "disabled";
		};

		i2s0: i2s@1c22000 {
			#sound-dai-cells = <0>;
			compatible = "allwinner,sun50i-a64-i2s",
				     "allwinner,sun8i-h3-i2s";
			reg = <0x01c22000 0x400>;
			interrupts = <GIC_SPI 13 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&ccu CLK_BUS_I2S0>, <&ccu CLK_I2S0>;
			clock-names = "apb", "mod";
			resets = <&ccu RST_BUS_I2S0>;
			dma-names = "rx", "tx";
			dmas = <&dma 3>, <&dma 3>;
			status = "disabled";
		};

		i2s1: i2s@1c22400 {
			#sound-dai-cells = <0>;
			compatible = "allwinner,sun50i-a64-i2s",
				     "allwinner,sun8i-h3-i2s";
			reg = <0x01c22400 0x400>;
			interrupts = <GIC_SPI 14 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&ccu CLK_BUS_I2S1>, <&ccu CLK_I2S1>;
			clock-names = "apb", "mod";
			resets = <&ccu RST_BUS_I2S1>;
			dma-names = "rx", "tx";
			dmas = <&dma 4>, <&dma 4>;
			status = "disabled";
		};

		i2s2: i2s@1c22800 {
			#sound-dai-cells = <0>;
			compatible = "allwinner,sun50i-a64-i2s",
				     "allwinner,sun8i-h3-i2s";
			reg = <0x01c22800 0x400>;
			interrupts = <GIC_SPI 15 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&ccu CLK_BUS_I2S2>, <&ccu CLK_I2S2>;
			clock-names = "apb", "mod";
			resets = <&ccu RST_BUS_I2S2>;
			dma-names = "rx", "tx";
			dmas = <&dma 27>, <&dma 27>;
			status = "disabled";
		};

		dai: dai@1c22c00 {
			#sound-dai-cells = <0>;
			compatible = "allwinner,sun50i-a64-codec-i2s";
			reg = <0x01c22c00 0x200>;
			interrupts = <GIC_SPI 29 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&ccu CLK_BUS_CODEC>, <&ccu CLK_AC_DIG>;
			clock-names = "apb", "mod";
			resets = <&ccu RST_BUS_CODEC>;
			dmas = <&dma 15>, <&dma 15>;
			dma-names = "rx", "tx";
			status = "disabled";
		};

		codec: codec@1c22e00 {
			#sound-dai-cells = <1>;
			compatible = "allwinner,sun50i-a64-codec",
				     "allwinner,sun8i-a33-codec";
			reg = <0x01c22e00 0x600>;
			interrupts = <GIC_SPI 28 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&ccu CLK_BUS_CODEC>, <&ccu CLK_AC_DIG>;
			clock-names = "bus", "mod";
			status = "disabled";
		};

		ths: thermal-sensor@1c25000 {
			compatible = "allwinner,sun50i-a64-ths";
			reg = <0x01c25000 0x100>;
			clocks = <&ccu CLK_BUS_THS>, <&ccu CLK_THS>;
			clock-names = "bus", "mod";
			interrupts = <GIC_SPI 31 IRQ_TYPE_LEVEL_HIGH>;
			resets = <&ccu RST_BUS_THS>;
			nvmem-cells = <&ths_calibration>;
			nvmem-cell-names = "calibration";
			#thermal-sensor-cells = <1>;
		};

		uart0: serial@1c28000 {
			compatible = "snps,dw-apb-uart";
			reg = <0x01c28000 0x400>;
			interrupts = <GIC_SPI 0 IRQ_TYPE_LEVEL_HIGH>;
			reg-shift = <2>;
			reg-io-width = <4>;
			clocks = <&ccu CLK_BUS_UART0>;
			resets = <&ccu RST_BUS_UART0>;
			status = "disabled";
		};

		uart1: serial@1c28400 {
			compatible = "snps,dw-apb-uart";
			reg = <0x01c28400 0x400>;
			interrupts = <GIC_SPI 1 IRQ_TYPE_LEVEL_HIGH>;
			reg-shift = <2>;
			reg-io-width = <4>;
			clocks = <&ccu CLK_BUS_UART1>;
			resets = <&ccu RST_BUS_UART1>;
			status = "disabled";
		};

		uart2: serial@1c28800 {
			compatible = "snps,dw-apb-uart";
			reg = <0x01c28800 0x400>;
			interrupts = <GIC_SPI 2 IRQ_TYPE_LEVEL_HIGH>;
			reg-shift = <2>;
			reg-io-width = <4>;
			clocks = <&ccu CLK_BUS_UART2>;
			resets = <&ccu RST_BUS_UART2>;
			status = "disabled";
		};

		uart3: serial@1c28c00 {
			compatible = "snps,dw-apb-uart";
			reg = <0x01c28c00 0x400>;
			interrupts = <GIC_SPI 3 IRQ_TYPE_LEVEL_HIGH>;
			reg-shift = <2>;
			reg-io-width = <4>;
			clocks = <&ccu CLK_BUS_UART3>;
			resets = <&ccu RST_BUS_UART3>;
			status = "disabled";
		};

		uart4: serial@1c29000 {
			compatible = "snps,dw-apb-uart";
			reg = <0x01c29000 0x400>;
			interrupts = <GIC_SPI 4 IRQ_TYPE_LEVEL_HIGH>;
			reg-shift = <2>;
			reg-io-width = <4>;
			clocks = <&ccu CLK_BUS_UART4>;
			resets = <&ccu RST_BUS_UART4>;
			status = "disabled";
		};

		i2c0: i2c@1c2ac00 {
			compatible = "allwinner,sun6i-a31-i2c";
			reg = <0x01c2ac00 0x400>;
			interrupts = <GIC_SPI 6 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&ccu CLK_BUS_I2C0>;
			resets = <&ccu RST_BUS_I2C0>;
			pinctrl-names = "default";
			pinctrl-0 = <&i2c0_pins>;
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <0>;
		};

		i2c1: i2c@1c2b000 {
			compatible = "allwinner,sun6i-a31-i2c";
			reg = <0x01c2b000 0x400>;
			interrupts = <GIC_SPI 7 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&ccu CLK_BUS_I2C1>;
			resets = <&ccu RST_BUS_I2C1>;
			pinctrl-names = "default";
			pinctrl-0 = <&i2c1_pins>;
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <0>;
		};

		i2c2: i2c@1c2b400 {
			compatible = "allwinner,sun6i-a31-i2c";
			reg = <0x01c2b400 0x400>;
			interrupts = <GIC_SPI 8 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&ccu CLK_BUS_I2C2>;
			resets = <&ccu RST_BUS_I2C2>;
			pinctrl-names = "default";
			pinctrl-0 = <&i2c2_pins>;
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <0>;
		};

		spi0: spi@1c68000 {
			compatible = "allwinner,sun8i-h3-spi";
			reg = <0x01c68000 0x1000>;
			interrupts = <GIC_SPI 65 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&ccu CLK_BUS_SPI0>, <&ccu CLK_SPI0>;
			clock-names = "ahb", "mod";
			dmas = <&dma 23>, <&dma 23>;
			dma-names = "rx", "tx";
			pinctrl-names = "default";
			pinctrl-0 = <&spi0_pins>;
			resets = <&ccu RST_BUS_SPI0>;
			status = "disabled";
			num-cs = <1>;
			#address-cells = <1>;
			#size-cells = <0>;
		};

		spi1: spi@1c69000 {
			compatible = "allwinner,sun8i-h3-spi";
			reg = <0x01c69000 0x1000>;
			interrupts = <GIC_SPI 66 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&ccu CLK_BUS_SPI1>, <&ccu CLK_SPI1>;
			clock-names = "ahb", "mod";
			dmas = <&dma 24>, <&dma 24>;
			dma-names = "rx", "tx";
			pinctrl-names = "default";
			pinctrl-0 = <&spi1_pins>;
			resets = <&ccu RST_BUS_SPI1>;
			status = "disabled";
			num-cs = <1>;
			#address-cells = <1>;
			#size-cells = <0>;
		};

		emac: ethernet@1c30000 {
			compatible = "allwinner,sun50i-a64-emac";
			syscon = <&syscon>;
			reg = <0x01c30000 0x10000>;
			interrupts = <GIC_SPI 82 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "macirq";
			resets = <&ccu RST_BUS_EMAC>;
			reset-names = "stmmaceth";
			clocks = <&ccu CLK_BUS_EMAC>;
			clock-names = "stmmaceth";
			status = "disabled";

			mdio: mdio {
				compatible = "snps,dwmac-mdio";
				#address-cells = <1>;
				#size-cells = <0>;
			};
		};

		mali: gpu@1c40000 {
			compatible = "allwinner,sun50i-a64-mali", "arm,mali-400";
			reg = <0x01c40000 0x10000>;
			interrupts = <GIC_SPI 97 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 98 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 99 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 100 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 102 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 103 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 101 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "gp",
					  "gpmmu",
					  "pp0",
					  "ppmmu0",
					  "pp1",
					  "ppmmu1",
					  "pmu";
			clocks = <&ccu CLK_BUS_GPU>, <&ccu CLK_GPU>;
			clock-names = "bus", "core";
			resets = <&ccu RST_BUS_GPU>;
			operating-points-v2 = <&gpu_opp_table>;
		};

		gic: interrupt-controller@1c81000 {
			compatible = "arm,gic-400";
			reg = <0x01c81000 0x1000>,
			      <0x01c82000 0x2000>,
			      <0x01c84000 0x2000>,
			      <0x01c86000 0x2000>;
			interrupts = <GIC_PPI 9 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_HIGH)>;
			interrupt-controller;
			#interrupt-cells = <3>;
		};

		pwm: pwm@1c21400 {
			compatible = "allwinner,sun50i-a64-pwm",
				     "allwinner,sun5i-a13-pwm";
			reg = <0x01c21400 0x400>;
			clocks = <&osc24M>;
			pinctrl-names = "default";
			pinctrl-0 = <&pwm_pin>;
			#pwm-cells = <3>;
			status = "disabled";
		};

		mbus: dram-controller@1c62000 {
			compatible = "allwinner,sun50i-a64-mbus";
			reg = <0x01c62000 0x1000>,
			      <0x01c63000 0x1000>;
			reg-names = "mbus", "dram";
			clocks = <&ccu CLK_MBUS>,
				 <&ccu CLK_DRAM>,
				 <&ccu CLK_BUS_DRAM>;
			clock-names = "mbus", "dram", "bus";
			interrupts = <GIC_SPI 69 IRQ_TYPE_LEVEL_HIGH>;
			#address-cells = <1>;
			#size-cells = <1>;
			dma-ranges = <0x00000000 0x40000000 0xc0000000>;
			#interconnect-cells = <1>;
		};

		csi: csi@1cb0000 {
			compatible = "allwinner,sun50i-a64-csi";
			reg = <0x01cb0000 0x1000>;
			interrupts = <GIC_SPI 84 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&ccu CLK_BUS_CSI>,
				 <&ccu CLK_CSI_SCLK>,
				 <&ccu CLK_DRAM_CSI>;
			clock-names = "bus", "mod", "ram";
			resets = <&ccu RST_BUS_CSI>;
			pinctrl-names = "default";
			pinctrl-0 = <&csi_pins>;
			status = "disabled";
		};

		dsi: dsi@1ca0000 {
			compatible = "allwinner,sun50i-a64-mipi-dsi";
			reg = <0x01ca0000 0x1000>;
			interrupts = <GIC_SPI 89 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&ccu CLK_BUS_MIPI_DSI>;
			resets = <&ccu RST_BUS_MIPI_DSI>;
			phys = <&dphy>;
			phy-names = "dphy";
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <0>;

			port {
				dsi_in_tcon0: endpoint {
					remote-endpoint = <&tcon0_out_dsi>;
				};
			};
		};

		dphy: d-phy@1ca1000 {
			compatible = "allwinner,sun50i-a64-mipi-dphy",
				     "allwinner,sun6i-a31-mipi-dphy";
			reg = <0x01ca1000 0x1000>;
			interrupts = <GIC_SPI 89 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&ccu CLK_BUS_MIPI_DSI>,
				 <&ccu CLK_DSI_DPHY>;
			clock-names = "bus", "mod";
			resets = <&ccu RST_BUS_MIPI_DSI>;
			status = "disabled";
			#phy-cells = <0>;
		};

		deinterlace: deinterlace@1e00000 {
			compatible = "allwinner,sun50i-a64-deinterlace",
				     "allwinner,sun8i-h3-deinterlace";
			reg = <0x01e00000 0x20000>;
			clocks = <&ccu CLK_BUS_DEINTERLACE>,
				 <&ccu CLK_DEINTERLACE>,
				 <&ccu CLK_DRAM_DEINTERLACE>;
			clock-names = "bus", "mod", "ram";
			resets = <&ccu RST_BUS_DEINTERLACE>;
			interrupts = <GIC_SPI 93 IRQ_TYPE_LEVEL_HIGH>;
			interconnects = <&mbus 9>;
			interconnect-names = "dma-mem";
		};

		hdmi: hdmi@1ee0000 {
			compatible = "allwinner,sun50i-a64-dw-hdmi",
				     "allwinner,sun8i-a83t-dw-hdmi";
			reg = <0x01ee0000 0x10000>;
			reg-io-width = <1>;
			interrupts = <GIC_SPI 88 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&ccu CLK_BUS_HDMI>, <&ccu CLK_HDMI_DDC>,
				 <&ccu CLK_HDMI>, <&rtc CLK_OSC32K>;
			clock-names = "iahb", "isfr", "tmds", "cec";
			resets = <&ccu RST_BUS_HDMI1>;
			reset-names = "ctrl";
			phys = <&hdmi_phy>;
			phy-names = "phy";
			status = "disabled";

			ports {
				#address-cells = <1>;
				#size-cells = <0>;

				hdmi_in: port@0 {
					reg = <0>;

					hdmi_in_tcon1: endpoint {
						remote-endpoint = <&tcon1_out_hdmi>;
					};
				};

				hdmi_out: port@1 {
					reg = <1>;
				};
			};
		};

		hdmi_phy: hdmi-phy@1ef0000 {
			compatible = "allwinner,sun50i-a64-hdmi-phy";
			reg = <0x01ef0000 0x10000>;
			clocks = <&ccu CLK_BUS_HDMI>, <&ccu CLK_HDMI_DDC>,
				 <&ccu CLK_PLL_VIDEO0>;
			clock-names = "bus", "mod", "pll-0";
			resets = <&ccu RST_BUS_HDMI0>;
			reset-names = "phy";
			#phy-cells = <0>;
		};

		rtc: rtc@1f00000 {
			compatible = "allwinner,sun50i-a64-rtc",
				     "allwinner,sun8i-h3-rtc";
			reg = <0x01f00000 0x400>;
			interrupts = <GIC_SPI 40 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 41 IRQ_TYPE_LEVEL_HIGH>;
			clock-output-names = "osc32k", "osc32k-out", "iosc";
			clocks = <&osc32k>;
			#clock-cells = <1>;
		};

		r_intc: interrupt-controller@1f00c00 {
			compatible = "allwinner,sun50i-a64-r-intc",
				     "allwinner,sun6i-a31-r-intc";
			interrupt-controller;
			#interrupt-cells = <2>;
			reg = <0x01f00c00 0x400>;
			interrupts = <GIC_SPI 32 IRQ_TYPE_LEVEL_HIGH>;
		};

		r_ccu: clock@1f01400 {
			compatible = "allwinner,sun50i-a64-r-ccu";
			reg = <0x01f01400 0x100>;
			clocks = <&osc24M>, <&rtc CLK_OSC32K>, <&rtc CLK_IOSC>,
				 <&ccu CLK_PLL_PERIPH0>;
			clock-names = "hosc", "losc", "iosc", "pll-periph";
			#clock-cells = <1>;
			#reset-cells = <1>;
		};

		codec_analog: codec-analog@1f015c0 {
			compatible = "allwinner,sun50i-a64-codec-analog";
			reg = <0x01f015c0 0x4>;
			status = "disabled";
		};

		r_i2c: i2c@1f02400 {
			compatible = "allwinner,sun50i-a64-i2c",
				     "allwinner,sun6i-a31-i2c";
			reg = <0x01f02400 0x400>;
			interrupts = <GIC_SPI 44 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&r_ccu CLK_APB0_I2C>;
			resets = <&r_ccu RST_APB0_I2C>;
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <0>;
		};

		r_ir: ir@1f02000 {
			compatible = "allwinner,sun50i-a64-ir",
				     "allwinner,sun6i-a31-ir";
			reg = <0x01f02000 0x400>;
			clocks = <&r_ccu CLK_APB0_IR>, <&r_ccu CLK_IR>;
			clock-names = "apb", "ir";
			resets = <&r_ccu RST_APB0_IR>;
			interrupts = <GIC_SPI 37 IRQ_TYPE_LEVEL_HIGH>;
			pinctrl-names = "default";
			pinctrl-0 = <&r_ir_rx_pin>;
			status = "disabled";
		};

		r_pwm: pwm@1f03800 {
			compatible = "allwinner,sun50i-a64-pwm",
				     "allwinner,sun5i-a13-pwm";
			reg = <0x01f03800 0x400>;
			clocks = <&osc24M>;
			pinctrl-names = "default";
			pinctrl-0 = <&r_pwm_pin>;
			#pwm-cells = <3>;
			status = "disabled";
		};

		r_pio: pinctrl@1f02c00 {
			compatible = "allwinner,sun50i-a64-r-pinctrl";
			reg = <0x01f02c00 0x400>;
			interrupts = <GIC_SPI 45 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&r_ccu CLK_APB0_PIO>, <&osc24M>, <&osc32k>;
			clock-names = "apb", "hosc", "losc";
			gpio-controller;
			#gpio-cells = <3>;
			interrupt-controller;
			#interrupt-cells = <3>;

			r_i2c_pl89_pins: r-i2c-pl89-pins {
				pins = "PL8", "PL9";
				function = "s_i2c";
			};

			r_ir_rx_pin: r-ir-rx-pin {
				pins = "PL11";
				function = "s_cir_rx";
			};

			r_pwm_pin: r-pwm-pin {
				pins = "PL10";
				function = "s_pwm";
			};

			r_rsb_pins: r-rsb-pins {
				pins = "PL0", "PL1";
				function = "s_rsb";
			};
		};

		r_rsb: rsb@1f03400 {
			compatible = "allwinner,sun8i-a23-rsb";
			reg = <0x01f03400 0x400>;
			interrupts = <GIC_SPI 39 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&r_ccu 6>;
			clock-frequency = <3000000>;
			resets = <&r_ccu 2>;
			pinctrl-names = "default";
			pinctrl-0 = <&r_rsb_pins>;
			status = "disabled";
			#address-cells = <1>;
			#size-cells = <0>;
		};
	};
};
