// SPDX-License-Identifier: GPL-2.0
/*
 * dts file for Hisilicon Hi3660 SoC
 *
 * Copyright (C) 2016, Hisilicon Ltd.
 */

#include <dt-bindings/interrupt-controller/arm-gic.h>
#include <dt-bindings/clock/hi3660-clock.h>
#include <dt-bindings/thermal/thermal.h>

/ {
	compatible = "hisilicon,hi3660";
	interrupt-parent = <&gic>;
	#address-cells = <2>;
	#size-cells = <2>;

	psci {
		compatible = "arm,psci-0.2";
		method = "smc";
	};

	cpus {
		#address-cells = <2>;
		#size-cells = <0>;

		cpu-map {
			cluster0 {
				core0 {
					cpu = <&cpu0>;
				};
				core1 {
					cpu = <&cpu1>;
				};
				core2 {
					cpu = <&cpu2>;
				};
				core3 {
					cpu = <&cpu3>;
				};
			};
			cluster1 {
				core0 {
					cpu = <&cpu4>;
				};
				core1 {
					cpu = <&cpu5>;
				};
				core2 {
					cpu = <&cpu6>;
				};
				core3 {
					cpu = <&cpu7>;
				};
			};
		};

		cpu0: cpu@0 {
			compatible = "arm,cortex-a53";
			device_type = "cpu";
			reg = <0x0 0x0>;
			enable-method = "psci";
			next-level-cache = <&A53_L2>;
			cpu-idle-states = <&CPU_SLEEP_0 &CLUSTER_SLEEP_0>;
			capacity-dmips-mhz = <592>;
			clocks = <&stub_clock HI3660_CLK_STUB_CLUSTER0>;
			operating-points-v2 = <&cluster0_opp>;
			#cooling-cells = <2>;
			dynamic-power-coefficient = <110>;
		};

		cpu1: cpu@1 {
			compatible = "arm,cortex-a53";
			device_type = "cpu";
			reg = <0x0 0x1>;
			enable-method = "psci";
			next-level-cache = <&A53_L2>;
			cpu-idle-states = <&CPU_SLEEP_0 &CLUSTER_SLEEP_0>;
			capacity-dmips-mhz = <592>;
			clocks = <&stub_clock HI3660_CLK_STUB_CLUSTER0>;
			operating-points-v2 = <&cluster0_opp>;
			#cooling-cells = <2>;
		};

		cpu2: cpu@2 {
			compatible = "arm,cortex-a53";
			device_type = "cpu";
			reg = <0x0 0x2>;
			enable-method = "psci";
			next-level-cache = <&A53_L2>;
			cpu-idle-states = <&CPU_SLEEP_0 &CLUSTER_SLEEP_0>;
			capacity-dmips-mhz = <592>;
			clocks = <&stub_clock HI3660_CLK_STUB_CLUSTER0>;
			operating-points-v2 = <&cluster0_opp>;
			#cooling-cells = <2>;
		};

		cpu3: cpu@3 {
			compatible = "arm,cortex-a53";
			device_type = "cpu";
			reg = <0x0 0x3>;
			enable-method = "psci";
			next-level-cache = <&A53_L2>;
			cpu-idle-states = <&CPU_SLEEP_0 &CLUSTER_SLEEP_0>;
			capacity-dmips-mhz = <592>;
			clocks = <&stub_clock HI3660_CLK_STUB_CLUSTER0>;
			operating-points-v2 = <&cluster0_opp>;
			#cooling-cells = <2>;
		};

		cpu4: cpu@100 {
			compatible = "arm,cortex-a73";
			device_type = "cpu";
			reg = <0x0 0x100>;
			enable-method = "psci";
			next-level-cache = <&A73_L2>;
			cpu-idle-states = <&CPU_SLEEP_1 &CLUSTER_SLEEP_1>;
			capacity-dmips-mhz = <1024>;
			clocks = <&stub_clock HI3660_CLK_STUB_CLUSTER1>;
			operating-points-v2 = <&cluster1_opp>;
			#cooling-cells = <2>;
			dynamic-power-coefficient = <550>;
		};

		cpu5: cpu@101 {
			compatible = "arm,cortex-a73";
			device_type = "cpu";
			reg = <0x0 0x101>;
			enable-method = "psci";
			next-level-cache = <&A73_L2>;
			cpu-idle-states = <&CPU_SLEEP_1 &CLUSTER_SLEEP_1>;
			capacity-dmips-mhz = <1024>;
			clocks = <&stub_clock HI3660_CLK_STUB_CLUSTER1>;
			operating-points-v2 = <&cluster1_opp>;
			#cooling-cells = <2>;
		};

		cpu6: cpu@102 {
			compatible = "arm,cortex-a73";
			device_type = "cpu";
			reg = <0x0 0x102>;
			enable-method = "psci";
			next-level-cache = <&A73_L2>;
			cpu-idle-states = <&CPU_SLEEP_1 &CLUSTER_SLEEP_1>;
			capacity-dmips-mhz = <1024>;
			clocks = <&stub_clock HI3660_CLK_STUB_CLUSTER1>;
			operating-points-v2 = <&cluster1_opp>;
			#cooling-cells = <2>;
		};

		cpu7: cpu@103 {
			compatible = "arm,cortex-a73";
			device_type = "cpu";
			reg = <0x0 0x103>;
			enable-method = "psci";
			next-level-cache = <&A73_L2>;
			cpu-idle-states = <&CPU_SLEEP_1 &CLUSTER_SLEEP_1>;
			capacity-dmips-mhz = <1024>;
			clocks = <&stub_clock HI3660_CLK_STUB_CLUSTER1>;
			operating-points-v2 = <&cluster1_opp>;
			#cooling-cells = <2>;
		};

		idle-states {
			entry-method = "psci";

			CPU_SLEEP_0: cpu-sleep-0 {
				compatible = "arm,idle-state";
				local-timer-stop;
				arm,psci-suspend-param = <0x0010000>;
				entry-latency-us = <400>;
				exit-latency-us = <650>;
				min-residency-us = <1500>;
			};
			CLUSTER_SLEEP_0: cluster-sleep-0 {
				compatible = "arm,idle-state";
				local-timer-stop;
				arm,psci-suspend-param = <0x1010000>;
				entry-latency-us = <500>;
				exit-latency-us = <1600>;
				min-residency-us = <3500>;
			};


			CPU_SLEEP_1: cpu-sleep-1 {
				compatible = "arm,idle-state";
				local-timer-stop;
				arm,psci-suspend-param = <0x0010000>;
				entry-latency-us = <400>;
				exit-latency-us = <550>;
				min-residency-us = <1500>;
			};

			CLUSTER_SLEEP_1: cluster-sleep-1 {
				compatible = "arm,idle-state";
				local-timer-stop;
				arm,psci-suspend-param = <0x1010000>;
				entry-latency-us = <800>;
				exit-latency-us = <2900>;
				min-residency-us = <3500>;
			};
		};

		A53_L2: l2-cache0 {
			compatible = "cache";
		};

		A73_L2: l2-cache1 {
			compatible = "cache";
		};
	};

	cluster0_opp: opp_table0 {
		compatible = "operating-points-v2";
		opp-shared;

		opp00 {
			opp-hz = /bits/ 64 <533000000>;
			opp-microvolt = <700000>;
			clock-latency-ns = <300000>;
		};

		opp01 {
			opp-hz = /bits/ 64 <999000000>;
			opp-microvolt = <800000>;
			clock-latency-ns = <300000>;
		};

		opp02 {
			opp-hz = /bits/ 64 <1402000000>;
			opp-microvolt = <900000>;
			clock-latency-ns = <300000>;
		};

		opp03 {
			opp-hz = /bits/ 64 <1709000000>;
			opp-microvolt = <1000000>;
			clock-latency-ns = <300000>;
		};

		opp04 {
			opp-hz = /bits/ 64 <1844000000>;
			opp-microvolt = <1100000>;
			clock-latency-ns = <300000>;
		};
	};

	cluster1_opp: opp_table1 {
		compatible = "operating-points-v2";
		opp-shared;

		opp10 {
			opp-hz = /bits/ 64 <903000000>;
			opp-microvolt = <700000>;
			clock-latency-ns = <300000>;
		};

		opp11 {
			opp-hz = /bits/ 64 <1421000000>;
			opp-microvolt = <800000>;
			clock-latency-ns = <300000>;
		};

		opp12 {
			opp-hz = /bits/ 64 <1805000000>;
			opp-microvolt = <900000>;
			clock-latency-ns = <300000>;
		};

		opp13 {
			opp-hz = /bits/ 64 <2112000000>;
			opp-microvolt = <1000000>;
			clock-latency-ns = <300000>;
		};

		opp14 {
			opp-hz = /bits/ 64 <2362000000>;
			opp-microvolt = <1100000>;
			clock-latency-ns = <300000>;
		};
	};

	gic: interrupt-controller@e82b0000 {
		compatible = "arm,gic-400";
		reg = <0x0 0xe82b1000 0 0x1000>, /* GICD */
		      <0x0 0xe82b2000 0 0x2000>, /* GICC */
		      <0x0 0xe82b4000 0 0x2000>, /* GICH */
		      <0x0 0xe82b6000 0 0x2000>; /* GICV */
		#address-cells = <0>;
		#interrupt-cells = <3>;
		interrupt-controller;
		interrupts = <GIC_PPI 9 (GIC_CPU_MASK_SIMPLE(8) |
					 IRQ_TYPE_LEVEL_HIGH)>;
	};

	a53-pmu {
		compatible = "arm,cortex-a53-pmu";
		interrupts = <GIC_SPI 24 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 25 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 26 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 27 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-affinity = <&cpu0>,
				     <&cpu1>,
				     <&cpu2>,
				     <&cpu3>;
	};

	a73-pmu {
		compatible = "arm,cortex-a73-pmu";
		interrupts = <GIC_SPI 2 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 3 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 4 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 5 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-affinity = <&cpu4>,
				     <&cpu5>,
				     <&cpu6>,
				     <&cpu7>;
	};

	timer {
		compatible = "arm,armv8-timer";
		interrupt-parent = <&gic>;
		interrupts = <GIC_PPI 13 (GIC_CPU_MASK_SIMPLE(8) |
					  IRQ_TYPE_LEVEL_LOW)>,
			     <GIC_PPI 14 (GIC_CPU_MASK_SIMPLE(8) |
					  IRQ_TYPE_LEVEL_LOW)>,
			     <GIC_PPI 11 (GIC_CPU_MASK_SIMPLE(8) |
					  IRQ_TYPE_LEVEL_LOW)>,
			     <GIC_PPI 10 (GIC_CPU_MASK_SIMPLE(8) |
					  IRQ_TYPE_LEVEL_LOW)>;
	};

	soc {
		compatible = "simple-bus";
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;

		crg_ctrl: crg_ctrl@fff35000 {
			compatible = "hisilicon,hi3660-crgctrl", "syscon";
			reg = <0x0 0xfff35000 0x0 0x1000>;
			#clock-cells = <1>;
		};

		crg_rst: crg_rst_controller {
			compatible = "hisilicon,hi3660-reset";
			#reset-cells = <2>;
			hisi,rst-syscon = <&crg_ctrl>;
		};


		pctrl: pctrl@e8a09000 {
			compatible = "hisilicon,hi3660-pctrl", "syscon";
			reg = <0x0 0xe8a09000 0x0 0x2000>;
			#clock-cells = <1>;
		};

		pmuctrl: crg_ctrl@fff34000 {
			compatible = "hisilicon,hi3660-pmuctrl", "syscon";
			reg = <0x0 0xfff34000 0x0 0x1000>;
			#clock-cells = <1>;
		};

		sctrl: sctrl@fff0a000 {
			compatible = "hisilicon,hi3660-sctrl", "syscon";
			reg = <0x0 0xfff0a000 0x0 0x1000>;
			#clock-cells = <1>;
		};

		iomcu: iomcu@ffd7e000 {
			compatible = "hisilicon,hi3660-iomcu", "syscon";
			reg = <0x0 0xffd7e000 0x0 0x1000>;
			#clock-cells = <1>;

		};

		iomcu_rst: reset {
			compatible = "hisilicon,hi3660-reset";
			hisi,rst-syscon = <&iomcu>;
			#reset-cells = <2>;
		};

		mailbox: mailbox@e896b000 {
			compatible = "hisilicon,hi3660-mbox";
			reg = <0x0 0xe896b000 0x0 0x1000>;
			interrupts = <GIC_SPI 192 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 193 IRQ_TYPE_LEVEL_HIGH>;
			#mbox-cells = <3>;
		};

		stub_clock: stub_clock@e896b500 {
			compatible = "hisilicon,hi3660-stub-clk";
			reg = <0x0 0xe896b500 0x0 0x0100>;
			#clock-cells = <1>;
			mboxes = <&mailbox 13 3 0>;
		};

		dual_timer0: timer@fff14000 {
			compatible = "arm,sp804", "arm,primecell";
			reg = <0x0 0xfff14000 0x0 0x1000>;
			interrupts = <GIC_SPI 48 IRQ_TYPE_LEVEL_HIGH>,
				     <GIC_SPI 49 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&crg_ctrl HI3660_OSC32K>,
				 <&crg_ctrl HI3660_OSC32K>,
				 <&crg_ctrl HI3660_OSC32K>;
			clock-names = "timer1", "timer2", "apb_pclk";
		};

		i2c0: i2c@ffd71000 {
			compatible = "snps,designware-i2c";
			reg = <0x0 0xffd71000 0x0 0x1000>;
			interrupts = <GIC_SPI 118 IRQ_TYPE_LEVEL_HIGH>;
			#address-cells = <1>;
			#size-cells = <0>;
			clock-frequency = <400000>;
			clocks = <&crg_ctrl HI3660_CLK_GATE_I2C0>;
			resets = <&iomcu_rst 0x20 3>;
			pinctrl-names = "default";
			pinctrl-0 = <&i2c0_pmx_func &i2c0_cfg_func>;
			status = "disabled";
		};

		i2c1: i2c@ffd72000 {
			compatible = "snps,designware-i2c";
			reg = <0x0 0xffd72000 0x0 0x1000>;
			interrupts = <GIC_SPI 119 IRQ_TYPE_LEVEL_HIGH>;
			#address-cells = <1>;
			#size-cells = <0>;
			clock-frequency = <400000>;
			clocks = <&crg_ctrl HI3660_CLK_GATE_I2C1>;
			resets = <&iomcu_rst 0x20 4>;
			pinctrl-names = "default";
			pinctrl-0 = <&i2c1_pmx_func &i2c1_cfg_func>;
			status = "disabled";
		};

		i2c3: i2c@fdf0c000 {
			compatible = "snps,designware-i2c";
			reg = <0x0 0xfdf0c000 0x0 0x1000>;
			interrupts = <GIC_SPI 81 IRQ_TYPE_LEVEL_HIGH>;
			#address-cells = <1>;
			#size-cells = <0>;
			clock-frequency = <400000>;
			clocks = <&crg_ctrl HI3660_CLK_GATE_I2C3>;
			resets = <&crg_rst 0x78 7>;
			pinctrl-names = "default";
			pinctrl-0 = <&i2c3_pmx_func &i2c3_cfg_func>;
			status = "disabled";
		};

		i2c7: i2c@fdf0b000 {
			compatible = "snps,designware-i2c";
			reg = <0x0 0xfdf0b000 0x0 0x1000>;
			interrupts = <GIC_SPI 314 IRQ_TYPE_LEVEL_HIGH>;
			#address-cells = <1>;
			#size-cells = <0>;
			clock-frequency = <400000>;
			clocks = <&crg_ctrl HI3660_CLK_GATE_I2C7>;
			resets = <&crg_rst 0x60 14>;
			pinctrl-names = "default";
			pinctrl-0 = <&i2c7_pmx_func &i2c7_cfg_func>;
			status = "disabled";
		};

		uart0: serial@fdf02000 {
			compatible = "arm,pl011", "arm,primecell";
			reg = <0x0 0xfdf02000 0x0 0x1000>;
			interrupts = <GIC_SPI 74 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&crg_ctrl HI3660_CLK_MUX_UART0>,
				 <&crg_ctrl HI3660_PCLK>;
			clock-names = "uartclk", "apb_pclk";
			pinctrl-names = "default";
			pinctrl-0 = <&uart0_pmx_func &uart0_cfg_func>;
			status = "disabled";
		};

		uart1: serial@fdf00000 {
			compatible = "arm,pl011", "arm,primecell";
			reg = <0x0 0xfdf00000 0x0 0x1000>;
			interrupts = <GIC_SPI 75 IRQ_TYPE_LEVEL_HIGH>;
			dma-names = "rx", "tx";
			dmas =  <&dma0 2 &dma0 3>;
			clocks = <&crg_ctrl HI3660_CLK_GATE_UART1>,
				 <&crg_ctrl HI3660_CLK_GATE_UART1>;
			clock-names = "uartclk", "apb_pclk";
			pinctrl-names = "default";
			pinctrl-0 = <&uart1_pmx_func &uart1_cfg_func>;
			status = "disabled";
		};

		uart2: serial@fdf03000 {
			compatible = "arm,pl011", "arm,primecell";
			reg = <0x0 0xfdf03000 0x0 0x1000>;
			interrupts = <GIC_SPI 76 IRQ_TYPE_LEVEL_HIGH>;
			dma-names = "rx", "tx";
			dmas =  <&dma0 4 &dma0 5>;
			clocks = <&crg_ctrl HI3660_CLK_GATE_UART2>,
				 <&crg_ctrl HI3660_PCLK>;
			clock-names = "uartclk", "apb_pclk";
			pinctrl-names = "default";
			pinctrl-0 = <&uart2_pmx_func &uart2_cfg_func>;
			status = "disabled";
		};

		uart3: serial@ffd74000 {
			compatible = "arm,pl011", "arm,primecell";
			reg = <0x0 0xffd74000 0x0 0x1000>;
			interrupts = <GIC_SPI 114 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&crg_ctrl HI3660_FACTOR_UART3>,
				 <&crg_ctrl HI3660_PCLK>;
			clock-names = "uartclk", "apb_pclk";
			pinctrl-names = "default";
			pinctrl-0 = <&uart3_pmx_func &uart3_cfg_func>;
			status = "disabled";
		};

		uart4: serial@fdf01000 {
			compatible = "arm,pl011", "arm,primecell";
			reg = <0x0 0xfdf01000 0x0 0x1000>;
			interrupts = <GIC_SPI 77 IRQ_TYPE_LEVEL_HIGH>;
			dma-names = "rx", "tx";
			dmas =  <&dma0 6 &dma0 7>;
			clocks = <&crg_ctrl HI3660_CLK_GATE_UART4>,
				 <&crg_ctrl HI3660_CLK_GATE_UART4>;
			clock-names = "uartclk", "apb_pclk";
			pinctrl-names = "default";
			pinctrl-0 = <&uart4_pmx_func &uart4_cfg_func>;
			status = "disabled";
		};

		uart5: serial@fdf05000 {
			compatible = "arm,pl011", "arm,primecell";
			reg = <0x0 0xfdf05000 0x0 0x1000>;
			interrupts = <GIC_SPI 78 IRQ_TYPE_LEVEL_HIGH>;
			dma-names = "rx", "tx";
			dmas =  <&dma0 8 &dma0 9>;
			clocks = <&crg_ctrl HI3660_CLK_GATE_UART5>,
				 <&crg_ctrl HI3660_CLK_GATE_UART5>;
			clock-names = "uartclk", "apb_pclk";
			pinctrl-names = "default";
			pinctrl-0 = <&uart5_pmx_func &uart5_cfg_func>;
			status = "disabled";
		};

		uart6: serial@fff32000 {
			compatible = "arm,pl011", "arm,primecell";
			reg = <0x0 0xfff32000 0x0 0x1000>;
			interrupts = <GIC_SPI 79 IRQ_TYPE_LEVEL_HIGH>;
			clock = <19200000>;
			clocks = <&crg_ctrl HI3660_CLK_UART6>,
				 <&crg_ctrl HI3660_PCLK>;
			clock-names = "uartclk", "apb_pclk";
			pinctrl-names = "default";
			pinctrl-0 = <&uart6_pmx_func &uart6_cfg_func>;
			status = "disabled";
		};

		dma0: dma@fdf30000 {
			compatible = "hisilicon,k3-dma-1.0";
			reg = <0x0 0xfdf30000 0x0 0x1000>;
			#dma-cells = <1>;
			dma-channels = <16>;
			dma-requests = <32>;
			dma-channel-mask = <0xfffe>;
			interrupts = <GIC_SPI 143 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&crg_ctrl HI3660_CLK_GATE_DMAC>;
			dma-no-cci;
			dma-type = "hi3660_dma";
		};

		asp_dmac: dma-controller@e804b000 {
			compatible = "hisilicon,hisi-pcm-asp-dma-1.0";
			reg = <0x0 0xe804b000 0x0 0x1000>;
			#dma-cells = <1>;
			dma-channels = <16>;
			dma-requests = <32>;
			interrupts = <GIC_SPI 216 IRQ_TYPE_LEVEL_HIGH>;
			interrupt-names = "asp_dma_irq";
		};

		rtc0: rtc@fff04000 {
			compatible = "arm,pl031", "arm,primecell";
			reg = <0x0 0xfff04000 0x0 0x1000>;
			interrupts = <GIC_SPI 46 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&crg_ctrl HI3660_PCLK>;
			clock-names = "apb_pclk";
		};

		gpio0: gpio@e8a0b000 {
			compatible = "arm,pl061", "arm,primecell";
			reg = <0 0xe8a0b000 0 0x1000>;
			interrupts = <GIC_SPI 84 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-ranges = <&pmx0 1 0 7>;
			interrupt-controller;
			#interrupt-cells = <2>;
			clocks = <&crg_ctrl HI3660_PCLK_GPIO0>;
			clock-names = "apb_pclk";
		};

		gpio1: gpio@e8a0c000 {
			compatible = "arm,pl061", "arm,primecell";
			reg = <0 0xe8a0c000 0 0x1000>;
			interrupts = <GIC_SPI 85 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-ranges = <&pmx0 1 7 7>;
			interrupt-controller;
			#interrupt-cells = <2>;
			clocks = <&crg_ctrl HI3660_PCLK_GPIO1>;
			clock-names = "apb_pclk";
		};

		gpio2: gpio@e8a0d000 {
			compatible = "arm,pl061", "arm,primecell";
			reg = <0 0xe8a0d000 0 0x1000>;
			interrupts = <GIC_SPI 86 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-ranges = <&pmx0 0 14 8>;
			interrupt-controller;
			#interrupt-cells = <2>;
			clocks = <&crg_ctrl HI3660_PCLK_GPIO2>;
			clock-names = "apb_pclk";
		};

		gpio3: gpio@e8a0e000 {
			compatible = "arm,pl061", "arm,primecell";
			reg = <0 0xe8a0e000 0 0x1000>;
			interrupts = <GIC_SPI 87 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-ranges = <&pmx0 0 22 8>;
			interrupt-controller;
			#interrupt-cells = <2>;
			clocks = <&crg_ctrl HI3660_PCLK_GPIO3>;
			clock-names = "apb_pclk";
		};

		gpio4: gpio@e8a0f000 {
			compatible = "arm,pl061", "arm,primecell";
			reg = <0 0xe8a0f000 0 0x1000>;
			interrupts = <GIC_SPI 88 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-ranges = <&pmx0 0 30 8>;
			interrupt-controller;
			#interrupt-cells = <2>;
			clocks = <&crg_ctrl HI3660_PCLK_GPIO4>;
			clock-names = "apb_pclk";
		};

		gpio5: gpio@e8a10000 {
			compatible = "arm,pl061", "arm,primecell";
			reg = <0 0xe8a10000 0 0x1000>;
			interrupts = <GIC_SPI 89 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-ranges = <&pmx0 0 38 8>;
			interrupt-controller;
			#interrupt-cells = <2>;
			clocks = <&crg_ctrl HI3660_PCLK_GPIO5>;
			clock-names = "apb_pclk";
		};

		gpio6: gpio@e8a11000 {
			compatible = "arm,pl061", "arm,primecell";
			reg = <0 0xe8a11000 0 0x1000>;
			interrupts = <GIC_SPI 90 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-ranges = <&pmx0 0 46 8>;
			interrupt-controller;
			#interrupt-cells = <2>;
			clocks = <&crg_ctrl HI3660_PCLK_GPIO6>;
			clock-names = "apb_pclk";
		};

		gpio7: gpio@e8a12000 {
			compatible = "arm,pl061", "arm,primecell";
			reg = <0 0xe8a12000 0 0x1000>;
			interrupts = <GIC_SPI 91 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-ranges = <&pmx0 0 54 8>;
			interrupt-controller;
			#interrupt-cells = <2>;
			clocks = <&crg_ctrl HI3660_PCLK_GPIO7>;
			clock-names = "apb_pclk";
		};

		gpio8: gpio@e8a13000 {
			compatible = "arm,pl061", "arm,primecell";
			reg = <0 0xe8a13000 0 0x1000>;
			interrupts = <GIC_SPI 92 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-ranges = <&pmx0 0 62 8>;
			interrupt-controller;
			#interrupt-cells = <2>;
			clocks = <&crg_ctrl HI3660_PCLK_GPIO8>;
			clock-names = "apb_pclk";
		};

		gpio9: gpio@e8a14000 {
			compatible = "arm,pl061", "arm,primecell";
			reg = <0 0xe8a14000 0 0x1000>;
			interrupts = <GIC_SPI 93 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-ranges = <&pmx0 0 70 8>;
			interrupt-controller;
			#interrupt-cells = <2>;
			clocks = <&crg_ctrl HI3660_PCLK_GPIO9>;
			clock-names = "apb_pclk";
		};

		gpio10: gpio@e8a15000 {
			compatible = "arm,pl061", "arm,primecell";
			reg = <0 0xe8a15000 0 0x1000>;
			interrupts = <GIC_SPI 94 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-ranges = <&pmx0 0 78 8>;
			interrupt-controller;
			#interrupt-cells = <2>;
			clocks = <&crg_ctrl HI3660_PCLK_GPIO10>;
			clock-names = "apb_pclk";
		};

		gpio11: gpio@e8a16000 {
			compatible = "arm,pl061", "arm,primecell";
			reg = <0 0xe8a16000 0 0x1000>;
			interrupts = <GIC_SPI 95 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-ranges = <&pmx0 0 86 8>;
			interrupt-controller;
			#interrupt-cells = <2>;
			clocks = <&crg_ctrl HI3660_PCLK_GPIO11>;
			clock-names = "apb_pclk";
		};

		gpio12: gpio@e8a17000 {
			compatible = "arm,pl061", "arm,primecell";
			reg = <0 0xe8a17000 0 0x1000>;
			interrupts = <GIC_SPI 96 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-ranges = <&pmx0 0 94 3 &pmx0 7 101 1>;
			interrupt-controller;
			#interrupt-cells = <2>;
			clocks = <&crg_ctrl HI3660_PCLK_GPIO12>;
			clock-names = "apb_pclk";
		};

		gpio13: gpio@e8a18000 {
			compatible = "arm,pl061", "arm,primecell";
			reg = <0 0xe8a18000 0 0x1000>;
			interrupts = <GIC_SPI 97 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-ranges = <&pmx0 0 102 8>;
			interrupt-controller;
			#interrupt-cells = <2>;
			clocks = <&crg_ctrl HI3660_PCLK_GPIO13>;
			clock-names = "apb_pclk";
		};

		gpio14: gpio@e8a19000 {
			compatible = "arm,pl061", "arm,primecell";
			reg = <0 0xe8a19000 0 0x1000>;
			interrupts = <GIC_SPI 98 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-ranges = <&pmx0 0 110 8>;
			interrupt-controller;
			#interrupt-cells = <2>;
			clocks = <&crg_ctrl HI3660_PCLK_GPIO14>;
			clock-names = "apb_pclk";
		};

		gpio15: gpio@e8a1a000 {
			compatible = "arm,pl061", "arm,primecell";
			reg = <0 0xe8a1a000 0 0x1000>;
			interrupts = <GIC_SPI 99 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-ranges = <&pmx0 0 118 6>;
			interrupt-controller;
			#interrupt-cells = <2>;
			clocks = <&crg_ctrl HI3660_PCLK_GPIO15>;
			clock-names = "apb_pclk";
		};

		gpio16: gpio@e8a1b000 {
			compatible = "arm,pl061", "arm,primecell";
			reg = <0 0xe8a1b000 0 0x1000>;
			interrupts = <GIC_SPI 100 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			interrupt-controller;
			#interrupt-cells = <2>;
			clocks = <&crg_ctrl HI3660_PCLK_GPIO16>;
			clock-names = "apb_pclk";
		};

		gpio17: gpio@e8a1c000 {
			compatible = "arm,pl061", "arm,primecell";
			reg = <0 0xe8a1c000 0 0x1000>;
			interrupts = <GIC_SPI 101 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			interrupt-controller;
			#interrupt-cells = <2>;
			clocks = <&crg_ctrl HI3660_PCLK_GPIO17>;
			clock-names = "apb_pclk";
		};

		gpio18: gpio@ff3b4000 {
			compatible = "arm,pl061", "arm,primecell";
			reg = <0 0xff3b4000 0 0x1000>;
			interrupts = <GIC_SPI 102 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-ranges = <&pmx2 0 0 8>;
			interrupt-controller;
			#interrupt-cells = <2>;
			clocks = <&crg_ctrl HI3660_PCLK_GPIO18>;
			clock-names = "apb_pclk";
		};

		gpio19: gpio@ff3b5000 {
			compatible = "arm,pl061", "arm,primecell";
			reg = <0 0xff3b5000 0 0x1000>;
			interrupts = <GIC_SPI 103 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-ranges = <&pmx2 0 8 4>;
			interrupt-controller;
			#interrupt-cells = <2>;
			clocks = <&crg_ctrl HI3660_PCLK_GPIO19>;
			clock-names = "apb_pclk";
		};

		gpio20: gpio@e8a1f000 {
			compatible = "arm,pl061", "arm,primecell";
			reg = <0 0xe8a1f000 0 0x1000>;
			interrupts = <GIC_SPI 104 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			gpio-ranges = <&pmx1 0 0 6>;
			interrupt-controller;
			#interrupt-cells = <2>;
			clocks = <&crg_ctrl HI3660_PCLK_GPIO20>;
			clock-names = "apb_pclk";
		};

		gpio21: gpio@e8a20000 {
			compatible = "arm,pl061", "arm,primecell";
			reg = <0 0xe8a20000 0 0x1000>;
			interrupts = <GIC_SPI 105 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			interrupt-controller;
			#interrupt-cells = <2>;
			gpio-ranges = <&pmx3 0 0 6>;
			clocks = <&crg_ctrl HI3660_PCLK_GPIO21>;
			clock-names = "apb_pclk";
		};

		gpio22: gpio@fff0b000 {
			compatible = "arm,pl061", "arm,primecell";
			reg = <0 0xfff0b000 0 0x1000>;
			interrupts = <GIC_SPI 106 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			/* GPIO176 */
			gpio-ranges = <&pmx4 2 0 6>;
			interrupt-controller;
			#interrupt-cells = <2>;
			clocks = <&sctrl HI3660_PCLK_AO_GPIO0>;
			clock-names = "apb_pclk";
		};

		gpio23: gpio@fff0c000 {
			compatible = "arm,pl061", "arm,primecell";
			reg = <0 0xfff0c000 0 0x1000>;
			interrupts = <GIC_SPI 107 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			/* GPIO184 */
			gpio-ranges = <&pmx4 0 6 7>;
			interrupt-controller;
			#interrupt-cells = <2>;
			clocks = <&sctrl HI3660_PCLK_AO_GPIO1>;
			clock-names = "apb_pclk";
		};

		gpio24: gpio@fff0d000 {
			compatible = "arm,pl061", "arm,primecell";
			reg = <0 0xfff0d000 0 0x1000>;
			interrupts = <GIC_SPI 108 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			/* GPIO192 */
			gpio-ranges = <&pmx4 0 13 8>;
			interrupt-controller;
			#interrupt-cells = <2>;
			clocks = <&sctrl HI3660_PCLK_AO_GPIO2>;
			clock-names = "apb_pclk";
		};

		gpio25: gpio@fff0e000 {
			compatible = "arm,pl061", "arm,primecell";
			reg = <0 0xfff0e000 0 0x1000>;
			interrupts = <GIC_SPI 109 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			/* GPIO200 */
			gpio-ranges = <&pmx4 0 21 4 &pmx4 5 25 3>;
			interrupt-controller;
			#interrupt-cells = <2>;
			clocks = <&sctrl HI3660_PCLK_AO_GPIO3>;
			clock-names = "apb_pclk";
		};

		gpio26: gpio@fff0f000 {
			compatible = "arm,pl061", "arm,primecell";
			reg = <0 0xfff0f000 0 0x1000>;
			interrupts = <GIC_SPI 110 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			/* GPIO208 */
			gpio-ranges = <&pmx4 0 28 8>;
			interrupt-controller;
			#interrupt-cells = <2>;
			clocks = <&sctrl HI3660_PCLK_AO_GPIO4>;
			clock-names = "apb_pclk";
		};

		gpio27: gpio@fff10000 {
			compatible = "arm,pl061", "arm,primecell";
			reg = <0 0xfff10000 0 0x1000>;
			interrupts = <GIC_SPI 111 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			/* GPIO216 */
			gpio-ranges = <&pmx4 0 36 6>;
			interrupt-controller;
			#interrupt-cells = <2>;
			clocks = <&sctrl HI3660_PCLK_AO_GPIO5>;
			clock-names = "apb_pclk";
		};

		gpio28: gpio@fff1d000 {
			compatible = "arm,pl061", "arm,primecell";
			reg = <0 0xfff1d000 0 0x1000>;
			interrupts = <GIC_SPI 141 IRQ_TYPE_LEVEL_HIGH>;
			gpio-controller;
			#gpio-cells = <2>;
			interrupt-controller;
			#interrupt-cells = <2>;
			clocks = <&sctrl HI3660_PCLK_AO_GPIO6>;
			clock-names = "apb_pclk";
		};

		spi2: spi@ffd68000 {
			compatible = "arm,pl022", "arm,primecell";
			reg = <0x0 0xffd68000 0x0 0x1000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 116 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&crg_ctrl HI3660_CLK_GATE_SPI2>;
			clock-names = "apb_pclk";
			pinctrl-names = "default";
			pinctrl-0 = <&spi2_pmx_func>;
			num-cs = <1>;
			cs-gpios = <&gpio27 2 0>;
			status = "disabled";
		};

		spi3: spi@ff3b3000 {
			compatible = "arm,pl022", "arm,primecell";
			reg = <0x0 0xff3b3000 0x0 0x1000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 312 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&crg_ctrl HI3660_CLK_GATE_SPI3>;
			clock-names = "apb_pclk";
			pinctrl-names = "default";
			pinctrl-0 = <&spi3_pmx_func>;
			num-cs = <1>;
			cs-gpios = <&gpio18 5 0>;
			status = "disabled";
		};

		pcie@f4000000 {
			compatible = "hisilicon,kirin960-pcie";
			reg = <0x0 0xf4000000 0x0 0x1000>,
			      <0x0 0xff3fe000 0x0 0x1000>,
			      <0x0 0xf3f20000 0x0 0x40000>,
			      <0x0 0xf5000000 0x0 0x2000>;
			reg-names = "dbi", "apb", "phy", "config";
			bus-range = <0x0  0x1>;
			#address-cells = <3>;
			#size-cells = <2>;
			device_type = "pci";
			ranges = <0x02000000 0x0 0x00000000
				  0x0 0xf6000000
				  0x0 0x02000000>;
			num-lanes = <1>;
			#interrupt-cells = <1>;
			interrupts = <0 283 4>;
			interrupt-names = "msi";
			interrupt-map-mask = <0xf800 0 0 7>;
			interrupt-map = <0x0 0 0 1
					 &gic GIC_SPI 282 IRQ_TYPE_LEVEL_HIGH>,
					<0x0 0 0 2
					 &gic GIC_SPI 283 IRQ_TYPE_LEVEL_HIGH>,
					<0x0 0 0 3
					 &gic GIC_SPI 284 IRQ_TYPE_LEVEL_HIGH>,
					<0x0 0 0 4
					 &gic GIC_SPI 285 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&crg_ctrl HI3660_PCIEPHY_REF>,
				 <&crg_ctrl HI3660_CLK_GATE_PCIEAUX>,
				 <&crg_ctrl HI3660_PCLK_GATE_PCIE_PHY>,
				 <&crg_ctrl HI3660_PCLK_GATE_PCIE_SYS>,
				 <&crg_ctrl HI3660_ACLK_GATE_PCIE>;
			clock-names = "pcie_phy_ref", "pcie_aux",
				      "pcie_apb_phy", "pcie_apb_sys",
				      "pcie_aclk";
			reset-gpios = <&gpio11 1 0 >;
		};

		/* UFS */
		ufs: ufs@ff3b0000 {
			compatible = "hisilicon,hi3660-ufs", "jedec,ufs-1.1";
			/* 0: HCI standard */
			/* 1: UFS SYS CTRL */
			reg = <0x0 0xff3b0000 0x0 0x1000>,
				<0x0 0xff3b1000 0x0 0x1000>;
			interrupt-parent = <&gic>;
			interrupts = <GIC_SPI 278 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&crg_ctrl HI3660_CLK_GATE_UFSIO_REF>,
				<&crg_ctrl HI3660_CLK_GATE_UFSPHY_CFG>;
			clock-names = "ref_clk", "phy_clk";
			freq-table-hz = <0 0>, <0 0>;
			/* offset: 0x84; bit: 12 */
			resets = <&crg_rst 0x84 12>;
			reset-names = "rst";
		};

		/* SD */
		dwmmc1: dwmmc1@ff37f000 {
			compatible = "hisilicon,hi3660-dw-mshc";
			reg = <0x0 0xff37f000 0x0 0x1000>;
			#address-cells = <1>;
			#size-cells = <0>;
			interrupts = <GIC_SPI 139 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&crg_ctrl HI3660_CLK_GATE_SD>,
				<&crg_ctrl HI3660_HCLK_GATE_SD>;
			clock-names = "ciu", "biu";
			clock-frequency = <3200000>;
			resets = <&crg_rst 0x94 18>;
			reset-names = "reset";
			hisilicon,peripheral-syscon = <&sctrl>;
			card-detect-delay = <200>;
			status = "disabled";
		};

		/* SDIO */
		dwmmc2: dwmmc2@ff3ff000 {
			compatible = "hisilicon,hi3660-dw-mshc";
			reg = <0x0 0xff3ff000 0x0 0x1000>;
			#address-cells = <0x1>;
			#size-cells = <0x0>;
			interrupts = <GIC_SPI 140 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&crg_ctrl HI3660_CLK_GATE_SDIO0>,
				 <&crg_ctrl HI3660_HCLK_GATE_SDIO0>;
			clock-names = "ciu", "biu";
			resets = <&crg_rst 0x94 20>;
			reset-names = "reset";
			card-detect-delay = <200>;
			status = "disabled";
		};

		watchdog0: watchdog@e8a06000 {
			compatible = "arm,sp805", "arm,primecell";
			reg = <0x0 0xe8a06000 0x0 0x1000>;
			interrupts = <GIC_SPI 44 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&crg_ctrl HI3660_OSC32K>;
			clock-names = "apb_pclk";
		};

		watchdog1: watchdog@e8a07000 {
			compatible = "arm,sp805", "arm,primecell";
			reg = <0x0 0xe8a07000 0x0 0x1000>;
			interrupts = <GIC_SPI 45 IRQ_TYPE_LEVEL_HIGH>;
			clocks = <&crg_ctrl HI3660_OSC32K>;
			clock-names = "apb_pclk";
		};

		tsensor: tsensor@fff30000 {
			compatible = "hisilicon,hi3660-tsensor";
			reg = <0x0 0xfff30000 0x0 0x1000>;
			interrupts = <GIC_SPI 145 IRQ_TYPE_LEVEL_HIGH>;
			#thermal-sensor-cells = <1>;
		};

		thermal-zones {

			cls0: cls0 {
				polling-delay = <1000>;
				polling-delay-passive = <100>;
				sustainable-power = <4500>;

				/* sensor ID */
				thermal-sensors = <&tsensor 1>;

				trips {
					threshold: trip-point@0 {
						temperature = <65000>;
						hysteresis = <1000>;
						type = "passive";
					};

					target: trip-point@1 {
						temperature = <75000>;
						hysteresis = <1000>;
						type = "passive";
					};
				};

				cooling-maps {
					map0 {
						trip = <&target>;
						contribution = <1024>;
						cooling-device = <&cpu0 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
								 <&cpu1 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
								 <&cpu2 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
								 <&cpu3 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
					};
					map1 {
						trip = <&target>;
						contribution = <512>;
						cooling-device = <&cpu4 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
								 <&cpu5 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
								 <&cpu6 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>,
								 <&cpu7 THERMAL_NO_LIMIT THERMAL_NO_LIMIT>;
					};
				};
			};
		};
	};
};
