// SPDX-License-Identifier: GPL-2.0

/* This include file covers the common peripherals and configuration between
 * bcm2835, bcm2836 and bcm2837 implementations.
 */

/ {
	interrupt-parent = <&intc>;

	soc {
		dma: dma@7e007000 {
			compatible = "brcm,bcm2835-dma";
			reg = <0x7e007000 0xf00>;
			interrupts = <1 16>,
				     <1 17>,
				     <1 18>,
				     <1 19>,
				     <1 20>,
				     <1 21>,
				     <1 22>,
				     <1 23>,
				     <1 24>,
				     <1 25>,
				     <1 26>,
				     /* dma channel 11-14 share one irq */
				     <1 27>,
				     <1 27>,
				     <1 27>,
				     <1 27>,
				     /* unused shared irq for all channels */
				     <1 28>;
			interrupt-names = "dma0",
					  "dma1",
					  "dma2",
					  "dma3",
					  "dma4",
					  "dma5",
					  "dma6",
					  "dma7",
					  "dma8",
					  "dma9",
					  "dma10",
					  "dma11",
					  "dma12",
					  "dma13",
					  "dma14",
					  "dma-shared-all";
			#dma-cells = <1>;
			brcm,dma-channel-mask = <0x7f35>;
		};

		intc: interrupt-controller@7e00b200 {
			compatible = "brcm,bcm2835-armctrl-ic";
			reg = <0x7e00b200 0x200>;
			interrupt-controller;
			#interrupt-cells = <2>;
		};

		pm: watchdog@7e100000 {
			compatible = "brcm,bcm2835-pm", "brcm,bcm2835-pm-wdt";
			#power-domain-cells = <1>;
			#reset-cells = <1>;
			reg = <0x7e100000 0x114>,
			      <0x7e00a000 0x24>;
			clocks = <&clocks BCM2835_CLOCK_V3D>,
				 <&clocks BCM2835_CLOCK_PERI_IMAGE>,
				 <&clocks BCM2835_CLOCK_H264>,
				 <&clocks BCM2835_CLOCK_ISP>;
			clock-names = "v3d", "peri_image", "h264", "isp";
			system-power-controller;
		};

		rng@7e104000 {
			compatible = "brcm,bcm2835-rng";
			reg = <0x7e104000 0x10>;
			interrupts = <2 29>;
		};

		pixelvalve@7e206000 {
			compatible = "brcm,bcm2835-pixelvalve0";
			reg = <0x7e206000 0x100>;
			interrupts = <2 13>; /* pwa0 */
		};

		pixelvalve@7e207000 {
			compatible = "brcm,bcm2835-pixelvalve1";
			reg = <0x7e207000 0x100>;
			interrupts = <2 14>; /* pwa1 */
		};

		thermal: thermal@7e212000 {
			compatible = "brcm,bcm2835-thermal";
			reg = <0x7e212000 0x8>;
			clocks = <&clocks BCM2835_CLOCK_TSENS>;
			#thermal-sensor-cells = <0>;
			status = "disabled";
		};

		i2c2: i2c@7e805000 {
			compatible = "brcm,bcm2835-i2c";
			reg = <0x7e805000 0x1000>;
			interrupts = <2 21>;
			clocks = <&clocks BCM2835_CLOCK_VPU>;
			#address-cells = <1>;
			#size-cells = <0>;
			status = "okay";
		};

		vec: vec@7e806000 {
			compatible = "brcm,bcm2835-vec";
			reg = <0x7e806000 0x1000>;
			clocks = <&clocks BCM2835_CLOCK_VEC>;
			interrupts = <2 27>;
			status = "disabled";
		};

		pixelvalve@7e807000 {
			compatible = "brcm,bcm2835-pixelvalve2";
			reg = <0x7e807000 0x100>;
			interrupts = <2 10>; /* pixelvalve */
		};

		hdmi: hdmi@7e902000 {
			compatible = "brcm,bcm2835-hdmi";
			reg = <0x7e902000 0x600>,
			      <0x7e808000 0x100>;
			interrupts = <2 8>, <2 9>;
			ddc = <&i2c2>;
			clocks = <&clocks BCM2835_PLLH_PIX>,
				 <&clocks BCM2835_CLOCK_HSM>;
			clock-names = "pixel", "hdmi";
			dmas = <&dma 17>;
			dma-names = "audio-rx";
			status = "disabled";
		};

		v3d: v3d@7ec00000 {
			compatible = "brcm,bcm2835-v3d";
			reg = <0x7ec00000 0x1000>;
			interrupts = <1 10>;
		};

		vc4: gpu {
			compatible = "brcm,bcm2835-vc4";
		};
	};
};

&cpu_thermal {
	thermal-sensors = <&thermal>;
};

&gpio {
	i2c_slave_gpio18: i2c_slave_gpio18 {
		brcm,pins = <18 19 20 21>;
		brcm,function = <BCM2835_FSEL_ALT3>;
	};

	jtag_gpio4: jtag_gpio4 {
		brcm,pins = <4 5 6 12 13>;
		brcm,function = <BCM2835_FSEL_ALT5>;
	};

	pwm0_gpio12: pwm0_gpio12 {
		brcm,pins = <12>;
		brcm,function = <BCM2835_FSEL_ALT0>;
	};
	pwm0_gpio18: pwm0_gpio18 {
		brcm,pins = <18>;
		brcm,function = <BCM2835_FSEL_ALT5>;
	};
	pwm0_gpio40: pwm0_gpio40 {
		brcm,pins = <40>;
		brcm,function = <BCM2835_FSEL_ALT0>;
	};
	pwm1_gpio13: pwm1_gpio13 {
		brcm,pins = <13>;
		brcm,function = <BCM2835_FSEL_ALT0>;
	};
	pwm1_gpio19: pwm1_gpio19 {
		brcm,pins = <19>;
		brcm,function = <BCM2835_FSEL_ALT5>;
	};
	pwm1_gpio41: pwm1_gpio41 {
		brcm,pins = <41>;
		brcm,function = <BCM2835_FSEL_ALT0>;
	};
	pwm1_gpio45: pwm1_gpio45 {
		brcm,pins = <45>;
		brcm,function = <BCM2835_FSEL_ALT0>;
	};
};

&i2s {
	dmas = <&dma 2>, <&dma 3>;
	dma-names = "tx", "rx";
};

&sdhost {
	dmas = <&dma 13>;
	dma-names = "rx-tx";
};

&spi {
	dmas = <&dma 6>, <&dma 7>;
	dma-names = "tx", "rx";
};
