// SPDX-License-Identifier: GPL-2.0+
/*
 * Copyright 2018, 2021 NXP
 */

#include <dt-bindings/interrupt-controller/arm-gic.h>
#include "fsl-imx8-ca53.dtsi"
#include <dt-bindings/clock/imx8qm-clock.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/soc/imx_rsrc.h>
#include <dt-bindings/soc/imx8_pd.h>
#include <dt-bindings/pinctrl/pads-imx8qm.h>
#include <dt-bindings/gpio/gpio.h>

/ {
	compatible = "fsl,imx8qm";
	interrupt-parent = <&gic>;
	#address-cells = <2>;
	#size-cells = <2>;

	aliases {
		ethernet0 = &fec1;
		ethernet1 = &fec2;
		gpio0 = &gpio0;
		gpio1 = &gpio1;
		gpio2 = &gpio2;
		gpio3 = &gpio3;
		gpio4 = &gpio4;
		gpio5 = &gpio5;
		gpio6 = &gpio6;
		gpio7 = &gpio7;
		serial0 = &lpuart0;
		serial1 = &lpuart1;
		serial2 = &lpuart2;
		serial3 = &lpuart3;
		serial4 = &lpuart4;
		mmc0 = &usdhc1;
		mmc1 = &usdhc2;
		mmc2 = &usdhc3;
		i2c0 = &i2c0;
		i2c1 = &i2c1;
		i2c2 = &i2c2;
		i2c3 = &i2c3;
		i2c4 = &i2c4;
	};

	memory@80000000 {
		device_type = "memory";
		reg = <0x00000000 0x80000000 0 0x40000000>;
		      /* DRAM space - 1, size : 1 GB DRAM */
	};

	gic: interrupt-controller@51a00000 {
		compatible = "arm,gic-v3";
		reg = <0x0 0x51a00000 0 0x10000>, /* GIC Dist */
		      <0x0 0x51b00000 0 0xC0000>, /* GICR */
		      <0x0 0x52000000 0 0x2000>,  /* GICC */
		      <0x0 0x52010000 0 0x1000>,  /* GICH */
		      <0x0 0x52020000 0 0x20000>; /* GICV */
		#interrupt-cells = <3>;
		interrupt-controller;
		interrupts = <GIC_PPI 9
			(GIC_CPU_MASK_SIMPLE(6) | IRQ_TYPE_LEVEL_HIGH)>;
		interrupt-parent = <&gic>;
	};

	mu: mu@5d1c0000 {
		compatible = "fsl,imx8-mu";
		reg = <0x0 0x5d1c0000 0x0 0x10000>;
		interrupts = <GIC_SPI 177 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-parent = <&gic>;
		fsl,scu_ap_mu_id = <0>;
		status = "okay";

		clk: clk {
			compatible = "fsl,imx8qm-clk";
			#clock-cells = <1>;
		};

		iomuxc: iomuxc {
			compatible = "fsl,imx8qm-iomuxc";
		};
	};

	imx8qm-pm {
		compatible = "simple-bus";
		#address-cells = <1>;
		#size-cells = <0>;

		pd_lsio: PD_LSIO {
			compatible = "nxp,imx8-pd";
			reg = <SC_R_NONE>;
			#power-domain-cells = <0>;
			#address-cells = <1>;
			#size-cells = <0>;

			pd_lsio_gpio0: PD_LSIO_GPIO_0 {
				reg = <SC_R_GPIO_0>;
				#power-domain-cells = <0>;
				power-domains = <&pd_lsio>;
			};
			pd_lsio_gpio1: PD_LSIO_GPIO_1 {
				reg = <SC_R_GPIO_1>;
				#power-domain-cells = <0>;
				power-domains = <&pd_lsio>;
			};
			pd_lsio_gpio2: PD_LSIO_GPIO_2 {
				reg = <SC_R_GPIO_2>;
				#power-domain-cells = <0>;
				power-domains = <&pd_lsio>;
			};
			pd_lsio_gpio3: PD_LSIO_GPIO_3 {
				reg = <SC_R_GPIO_3>;
				#power-domain-cells = <0>;
				power-domains = <&pd_lsio>;
			};
			pd_lsio_gpio4: PD_LSIO_GPIO_4 {
				reg = <SC_R_GPIO_4>;
				#power-domain-cells = <0>;
				power-domains = <&pd_lsio>;
			};
			pd_lsio_gpio5: PD_LSIO_GPIO_5{
				reg = <SC_R_GPIO_5>;
				#power-domain-cells = <0>;
				power-domains = <&pd_lsio>;
			};
			pd_lsio_gpio6:PD_LSIO_GPIO_6 {
				reg = <SC_R_GPIO_6>;
				#power-domain-cells = <0>;
				power-domains = <&pd_lsio>;
			};
			pd_lsio_gpio7: PD_LSIO_GPIO_7 {
				reg = <SC_R_GPIO_7>;
				#power-domain-cells = <0>;
				power-domains = <&pd_lsio>;
			};
		};

		pd_conn: PD_CONN {
			compatible = "nxp,imx8-pd";
			reg = <SC_R_NONE>;
			#power-domain-cells = <0>;
			#address-cells = <1>;
			#size-cells = <0>;

			pd_conn_sdch0: PD_CONN_SDHC_0 {
				reg = <SC_R_SDHC_0>;
				#power-domain-cells = <0>;
				power-domains = <&pd_conn>;
			};
			pd_conn_sdch1: PD_CONN_SDHC_1 {
				reg = <SC_R_SDHC_1>;
				#power-domain-cells = <0>;
				power-domains = <&pd_conn>;
			};
			pd_conn_sdch2: PD_CONN_SDHC_2 {
				reg = <SC_R_SDHC_2>;
				#power-domain-cells = <0>;
				power-domains = <&pd_conn>;
			};
			pd_conn_enet0: PD_CONN_ENET_0 {
				reg = <SC_R_ENET_0>;
				#power-domain-cells = <0>;
				power-domains = <&pd_conn>;
				wakeup-irq = <258>;
			};
			pd_conn_enet1: PD_CONN_ENET_1 {
				reg = <SC_R_ENET_1>;
				#power-domain-cells = <0>;
				power-domains = <&pd_conn>;
				fsl,wakeup_irq = <262>;
			};
		};

		pd_dma: PD_DMA {
			compatible = "nxp,imx8-pd";
			reg = <SC_R_NONE>;
			#power-domain-cells = <0>;
			#address-cells = <1>;
			#size-cells = <0>;

			pd_dma_lpi2c0: PD_DMA_I2C_0 {
				reg = <SC_R_I2C_0>;
				#power-domain-cells = <0>;
				power-domains = <&pd_dma>;
			};
			pd_dma_lpi2c1: PD_DMA_I2C_1 {
				reg = <SC_R_I2C_1>;
				#power-domain-cells = <0>;
				power-domains = <&pd_dma>;
			};
			pd_dma_lpi2c2:PD_DMA_I2C_2 {
				reg = <SC_R_I2C_2>;
				#power-domain-cells = <0>;
				power-domains = <&pd_dma>;
			};
			pd_dma_lpi2c3: PD_DMA_I2C_3 {
				reg = <SC_R_I2C_3>;
				#power-domain-cells = <0>;
				power-domains = <&pd_dma>;
			};
			pd_dma_lpi2c4: PD_DMA_I2C_4 {
				reg = <SC_R_I2C_4>;
				#power-domain-cells = <0>;
				power-domains = <&pd_dma>;
			};
			pd_dma_lpuart0: PD_DMA_UART0 {
				reg = <SC_R_UART_0>;
				#power-domain-cells = <0>;
				power-domains = <&pd_dma>;
				wakeup-irq = <345>;
			};
			pd_dma_lpuart1: PD_DMA_UART1 {
				reg = <SC_R_UART_1>;
				#power-domain-cells = <0>;
				power-domains = <&pd_dma>;
				wakeup-irq = <346>;
			};
			pd_dma_lpuart2: PD_DMA_UART2 {
				reg = <SC_R_UART_2>;
				#power-domain-cells = <0>;
				power-domains = <&pd_dma>;
				wakeup-irq = <347>;
			};
			pd_dma_lpuart3: PD_DMA_UART3 {
				reg = <SC_R_UART_3>;
				#power-domain-cells = <0>;
				power-domains = <&pd_dma>;
				wakeup-irq = <348>;
			};
			pd_dma_lpuart4: PD_DMA_UART4 {
				reg = <SC_R_UART_4>;
				#power-domain-cells = <0>;
				power-domains = <&pd_dma>;
				wakeup-irq = <349>;
			};
		};

		pd_caam: PD_CAAM {
			compatible = "nxp,imx8-pd";
			reg = <SC_R_NONE>;
			#power-domain-cells = <0>;
			#address-cells = <1>;
			#size-cells = <0>;

			pd_caam_jr1: PD_CAAM_JR1 {
				reg = <SC_R_CAAM_JR1>;
				#power-domain-cells = <0>;
				power-domains = <&pd_caam>;
			};
			pd_caam_jr2: PD_CAAM_JR2 {
				reg = <SC_R_CAAM_JR2>;
				#power-domain-cells = <0>;
				power-domains = <&pd_caam>;
			};
			pd_caam_jr3: PD_CAAM_JR3 {
				reg = <SC_R_CAAM_JR3>;
				#power-domain-cells = <0>;
				power-domains = <&pd_caam>;
			};
		};
	};

	i2c0: i2c@5a800000 {
		compatible = "fsl,imx8qm-lpi2c", "fsl,imx7ulp-lpi2c";
		reg = <0x0 0x5a800000 0x0 0x4000>;
		interrupts = <GIC_SPI 220 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-parent = <&gic>;
		clocks = <&clk IMX8QM_I2C0_CLK>,
			 <&clk IMX8QM_I2C0_IPG_CLK>;
		clock-names = "per", "ipg";
		assigned-clocks = <&clk IMX8QM_I2C0_CLK>;
		assigned-clock-rates = <24000000>;
		power-domains = <&pd_dma_lpi2c0>;
		status = "disabled";
	};

	i2c1: i2c@5a810000 {
		compatible = "fsl,imx8qm-lpi2c", "fsl,imx7ulp-lpi2c";
		reg = <0x0 0x5a810000 0x0 0x4000>;
		interrupts = <GIC_SPI 221 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-parent = <&gic>;
		clocks = <&clk IMX8QM_I2C1_CLK>,
			 <&clk IMX8QM_I2C1_IPG_CLK>;
		clock-names = "per", "ipg";
		assigned-clocks = <&clk IMX8QM_I2C1_CLK>;
		assigned-clock-rates = <24000000>;
		power-domains = <&pd_dma_lpi2c1>;
		status = "disabled";
	};

	i2c2: i2c@5a820000 {
		compatible = "fsl,imx8qm-lpi2c", "fsl,imx7ulp-lpi2c";
		reg = <0x0 0x5a820000 0x0 0x4000>;
		interrupts = <GIC_SPI 222 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-parent = <&gic>;
		clocks = <&clk IMX8QM_I2C2_CLK>,
			 <&clk IMX8QM_I2C2_IPG_CLK>;
		clock-names = "per", "ipg";
		assigned-clocks = <&clk IMX8QM_I2C2_CLK>;
		assigned-clock-rates = <24000000>;
		power-domains = <&pd_dma_lpi2c2>;
		status = "disabled";
	};

	i2c3: i2c@5a830000 {
		compatible = "fsl,imx8qm-lpi2c", "fsl,imx7ulp-lpi2c";
		reg = <0x0 0x5a830000 0x0 0x4000>;
		interrupts = <GIC_SPI 223 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-parent = <&gic>;
		clocks = <&clk IMX8QM_I2C3_CLK>,
			 <&clk IMX8QM_I2C3_IPG_CLK>;
		clock-names = "per", "ipg";
		assigned-clocks = <&clk IMX8QM_I2C3_CLK>;
		assigned-clock-rates = <24000000>;
		power-domains = <&pd_dma_lpi2c3>;
		status = "disabled";
	};

	i2c4: i2c@5a840000 {
		compatible = "fsl,imx8qm-lpi2c", "fsl,imx7ulp-lpi2c";
		reg = <0x0 0x5a840000 0x0 0x4000>;
		interrupts = <GIC_SPI 224 IRQ_TYPE_LEVEL_HIGH>;
		interrupt-parent = <&gic>;
		clocks = <&clk IMX8QM_I2C4_CLK>,
			 <&clk IMX8QM_I2C4_IPG_CLK>;
		clock-names = "per", "ipg";
		assigned-clocks = <&clk IMX8QM_I2C4_CLK>;
		assigned-clock-rates = <24000000>;
		power-domains = <&pd_dma_lpi2c4>;
		status = "disabled";
	};

	gpio0: gpio@5d080000 {
		compatible = "fsl,imx8qm-gpio", "fsl,imx35-gpio";
		reg = <0x0 0x5d080000 0x0 0x10000>;
		interrupts = <GIC_SPI 136 IRQ_TYPE_LEVEL_HIGH>;
		gpio-controller;
		#gpio-cells = <2>;
		power-domains = <&pd_lsio_gpio0>;
		interrupt-controller;
		#interrupt-cells = <2>;
	};

	gpio1: gpio@5d090000 {
		compatible = "fsl,imx8qm-gpio", "fsl,imx35-gpio";
		reg = <0x0 0x5d090000 0x0 0x10000>;
		interrupts = <GIC_SPI 137 IRQ_TYPE_LEVEL_HIGH>;
		gpio-controller;
		#gpio-cells = <2>;
		power-domains = <&pd_lsio_gpio1>;
		interrupt-controller;
		#interrupt-cells = <2>;
	};

	gpio2: gpio@5d0a0000 {
		compatible = "fsl,imx8qm-gpio", "fsl,imx35-gpio";
		reg = <0x0 0x5d0a0000 0x0 0x10000>;
		interrupts = <GIC_SPI 138 IRQ_TYPE_LEVEL_HIGH>;
		gpio-controller;
		#gpio-cells = <2>;
		power-domains = <&pd_lsio_gpio2>;
		interrupt-controller;
		#interrupt-cells = <2>;
	};

	gpio3: gpio@5d0b0000 {
		compatible = "fsl,imx8qm-gpio", "fsl,imx35-gpio";
		reg = <0x0 0x5d0b0000 0x0 0x10000>;
		interrupts = <GIC_SPI 139 IRQ_TYPE_LEVEL_HIGH>;
		gpio-controller;
		#gpio-cells = <2>;
		power-domains = <&pd_lsio_gpio3>;
		interrupt-controller;
		#interrupt-cells = <2>;
	};

	gpio4: gpio@5d0c0000 {
		compatible = "fsl,imx8qm-gpio", "fsl,imx35-gpio";
		reg = <0x0 0x5d0c0000 0x0 0x10000>;
		interrupts = <GIC_SPI 140 IRQ_TYPE_LEVEL_HIGH>;
		gpio-controller;
		#gpio-cells = <2>;
		power-domains = <&pd_lsio_gpio4>;
		interrupt-controller;
		#interrupt-cells = <2>;
	};

	gpio5: gpio@5d0d0000 {
		compatible = "fsl,imx8qm-gpio", "fsl,imx35-gpio";
		reg = <0x0 0x5d0d0000 0x0 0x10000>;
		interrupts = <GIC_SPI 141 IRQ_TYPE_LEVEL_HIGH>;
		gpio-controller;
		#gpio-cells = <2>;
		power-domains = <&pd_lsio_gpio5>;
		interrupt-controller;
		#interrupt-cells = <2>;
	};

	gpio6: gpio@5d0e0000 {
		compatible = "fsl,imx8qm-gpio", "fsl,imx35-gpio";
		reg = <0x0 0x5d0e0000 0x0 0x10000>;
		interrupts = <GIC_SPI 142 IRQ_TYPE_LEVEL_HIGH>;
		gpio-controller;
		#gpio-cells = <2>;
		power-domains = <&pd_lsio_gpio6>;
		interrupt-controller;
		#interrupt-cells = <2>;
	};

	gpio7: gpio@5d0f0000 {
		compatible = "fsl,imx8qm-gpio", "fsl,imx35-gpio";
		reg = <0x0 0x5d0f0000 0x0 0x10000>;
		interrupts = <GIC_SPI 143 IRQ_TYPE_LEVEL_HIGH>;
		gpio-controller;
		#gpio-cells = <2>;
		power-domains = <&pd_lsio_gpio7>;
		interrupt-controller;
		#interrupt-cells = <2>;
	};

	lpuart0: serial@5a060000 {
		compatible = "fsl,imx8qm-lpuart";
		reg = <0x0 0x5a060000 0x0 0x1000>;
		interrupts = <GIC_SPI 345 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&clk IMX8QM_UART0_CLK>,
			 <&clk IMX8QM_UART0_IPG_CLK>;
		clock-names = "per", "ipg";
		assigned-clocks = <&clk IMX8QM_UART0_CLK>;
		assigned-clock-rates = <80000000>;
		power-domains = <&pd_dma_lpuart0>;
		status = "disabled";
	};

	lpuart1: serial@5a070000 {
		compatible = "fsl,imx8qm-lpuart";
		reg = <0x0 0x5a070000 0x0 0x1000>;
		interrupts = <GIC_SPI 346 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&clk IMX8QM_UART1_CLK>,
			 <&clk IMX8QM_UART1_IPG_CLK>;
		clock-names = "per", "ipg";
		assigned-clocks = <&clk IMX8QM_UART1_CLK>;
		assigned-clock-rates = <80000000>;
		power-domains = <&pd_dma_lpuart1>;
		status = "disabled";
	};

	lpuart2: serial@5a080000 {
		compatible = "fsl,imx8qm-lpuart";
		reg = <0x0 0x5a080000 0x0 0x1000>;
		interrupts = <GIC_SPI 347 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&clk IMX8QM_UART2_CLK>,
			 <&clk IMX8QM_UART2_IPG_CLK>;
		clock-names = "per", "ipg";
		assigned-clocks = <&clk IMX8QM_UART2_CLK>;
		assigned-clock-rates = <80000000>;
		power-domains = <&pd_dma_lpuart2>;
		status = "disabled";
	};

	lpuart3: serial@5a090000 {
		compatible = "fsl,imx8qm-lpuart";
		reg = <0x0 0x5a090000 0x0 0x1000>;
		interrupts = <GIC_SPI 348 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&clk IMX8QM_UART3_CLK>,
			 <&clk IMX8QM_UART3_IPG_CLK>;
		clock-names = "per", "ipg";
		assigned-clocks = <&clk IMX8QM_UART3_CLK>;
		assigned-clock-rates = <80000000>;
		power-domains = <&pd_dma_lpuart3>;
		status = "disabled";
	};

	lpuart4: serial@5a0a0000 {
		compatible = "fsl,imx8qm-lpuart";
		reg = <0x0 0x5a0a0000 0x0 0x1000>;
		interrupts = <GIC_SPI 349 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&clk IMX8QM_UART4_CLK>,
			 <&clk IMX8QM_UART4_IPG_CLK>;
		clock-names = "per", "ipg";
		assigned-clocks = <&clk IMX8QM_UART4_CLK>;
		assigned-clock-rates = <80000000>;
		power-domains = <&pd_dma_lpuart4>;
		status = "disabled";
	};

	usdhc1: usdhc@5b010000 {
		compatible = "fsl,imx8qm-usdhc", "fsl,imx6sl-usdhc";
		interrupt-parent = <&gic>;
		interrupts = <GIC_SPI 232 IRQ_TYPE_LEVEL_HIGH>;
		reg = <0x0 0x5b010000 0x0 0x10000>;
		clocks = <&clk IMX8QM_SDHC0_IPG_CLK>,
			 <&clk IMX8QM_SDHC0_CLK>,
			 <&clk IMX8QM_CLK_DUMMY>;
		clock-names = "ipg", "per", "ahb";
		assigned-clocks = <&clk IMX8QM_SDHC0_DIV>;
		assigned-clock-rates = <400000000>;
		power-domains = <&pd_conn_sdch0>;
		fsl,tuning-start-tap = <20>;
		fsl,tuning-step= <2>;
		status = "disabled";
	};

	usdhc2: usdhc@5b020000 {
		compatible = "fsl,imx8qm-usdhc", "fsl,imx6sl-usdhc";
		interrupt-parent = <&gic>;
		interrupts = <GIC_SPI 233 IRQ_TYPE_LEVEL_HIGH>;
		reg = <0x0 0x5b020000 0x0 0x10000>;
		clocks = <&clk IMX8QM_SDHC1_IPG_CLK>,
			 <&clk IMX8QM_SDHC1_CLK>,
			 <&clk IMX8QM_CLK_DUMMY>;
		clock-names = "ipg", "per", "ahb";
		assigned-clocks = <&clk IMX8QM_SDHC1_DIV>;
		assigned-clock-rates = <200000000>;
		power-domains = <&pd_conn_sdch1>;
		fsl,tuning-start-tap = <20>;
		fsl,tuning-step= <2>;
		status = "disabled";
	};

	usdhc3: usdhc@5b030000 {
		compatible = "fsl,imx8qm-usdhc", "fsl,imx6sl-usdhc";
		interrupt-parent = <&gic>;
		interrupts = <GIC_SPI 234 IRQ_TYPE_LEVEL_HIGH>;
		reg = <0x0 0x5b030000 0x0 0x10000>;
		clocks = <&clk IMX8QM_SDHC2_IPG_CLK>,
			 <&clk IMX8QM_SDHC2_CLK>,
			 <&clk IMX8QM_CLK_DUMMY>;
		clock-names = "ipg", "per", "ahb";
		assigned-clocks = <&clk IMX8QM_SDHC2_DIV>;
		assigned-clock-rates = <200000000>;
		power-domains = <&pd_conn_sdch2>;
		status = "disabled";
	};

	fec1: ethernet@5b040000 {
		compatible = "fsl,imx8qm-fec", "fsl,imx7d-fec";
		reg = <0x0 0x5b040000 0x0 0x10000>;
		interrupts = <GIC_SPI 258 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 256 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 257 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 259 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&clk IMX8QM_ENET0_IPG_CLK>,
			 <&clk IMX8QM_ENET0_AHB_CLK>,
			 <&clk IMX8QM_ENET0_RGMII_TX_CLK>,
			 <&clk IMX8QM_ENET0_PTP_CLK>,
			 <&clk IMX8QM_ENET0_TX_CLK>;
		clock-names = "ipg", "ahb", "enet_clk_ref", "ptp",
			      "enet_2x_txclk";
		assigned-clocks = <&clk IMX8QM_ENET0_ROOT_DIV>,
				  <&clk IMX8QM_ENET0_REF_DIV>;
		assigned-clock-rates = <250000000>, <125000000>;
		fsl,num-tx-queues=<3>;
		fsl,num-rx-queues=<3>;
		fsl,wakeup_irq = <0>;
		power-domains = <&pd_conn_enet0>;
		status = "disabled";
	};

	fec2: ethernet@5b050000 {
		compatible = "fsl,imx8qm-fec", "fsl,imx7d-fec";
		reg = <0x0 0x5b050000 0x0 0x10000>;
		interrupts = <GIC_SPI 262 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 260 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 261 IRQ_TYPE_LEVEL_HIGH>,
			     <GIC_SPI 263 IRQ_TYPE_LEVEL_HIGH>;
		clocks = <&clk IMX8QM_ENET1_IPG_CLK>,
			 <&clk IMX8QM_ENET1_AHB_CLK>,
			 <&clk IMX8QM_ENET1_RGMII_TX_CLK>,
			 <&clk IMX8QM_ENET1_PTP_CLK>,
			 <&clk IMX8QM_ENET1_TX_CLK>;
		clock-names = "ipg", "ahb", "enet_clk_ref", "ptp",
			      "enet_2x_txclk";
		assigned-clocks = <&clk IMX8QM_ENET1_ROOT_DIV>,
				  <&clk IMX8QM_ENET1_REF_DIV>;
		assigned-clock-rates = <250000000>, <125000000>;
		fsl,num-tx-queues=<3>;
		fsl,num-rx-queues=<3>;
		fsl,wakeup_irq = <0>;
		power-domains = <&pd_conn_enet1>;
		status = "disabled";
	};

	crypto: caam@0x31400000 {
		compatible = "fsl,sec-v4.0";
		reg = <0 0x31400000 0 0x400000>;
		interrupts = <GIC_SPI 148 IRQ_TYPE_LEVEL_HIGH>;
		#address-cells = <1>;
		#size-cells = <1>;
		ranges = <0 0 0x31400000 0x400000>;
		fsl,first-jr-index = <2>;
		fsl,sec-era = <9>;

		sec_jr1: jr1@0x20000 {
			compatible = "fsl,sec-v4.0-job-ring";
			reg = <0x20000 0x1000>;
			interrupts = <GIC_SPI 452 IRQ_TYPE_LEVEL_HIGH>;
			power-domains = <&pd_caam_jr1>;
			status = "disabled";
		};

		sec_jr2: jr2@30000 {
			compatible = "fsl,sec-v4.0-job-ring";
			reg = <0x30000 0x1000>;
			interrupts = <GIC_SPI 453 IRQ_TYPE_LEVEL_HIGH>;
			power-domains = <&pd_caam_jr2>;
			status = "okay";
		};

		sec_jr3: jr3@40000 {
			compatible = "fsl,sec-v4.0-job-ring";
			reg = <0x40000 0x1000>;
			interrupts = <GIC_SPI 454 IRQ_TYPE_LEVEL_HIGH>;
			power-domains = <&pd_caam_jr3>;
			status = "okay";
		};
	};
};

&A53_0 {
	clocks = <&clk IMX8QM_A53_DIV>;
};
