// SPDX-License-Identifier: GPL-2.0
/*
 * Copyright (C) 2018 Intel Corporation
 */

/dts-v1/;
#include <dt-bindings/reset/altr,rst-mgr-s10.h>
#include <dt-bindings/gpio/gpio.h>

/ {
	compatible = "altr,socfpga-stratix10";
	#address-cells = <2>;
	#size-cells = <2>;

	cpus {
		#address-cells = <1>;
		#size-cells = <0>;

		cpu0: cpu@0 {
			compatible = "arm,cortex-a53", "arm,armv8";
			device_type = "cpu";
			enable-method = "psci";
			reg = <0x0>;
		};

		cpu1: cpu@1 {
			compatible = "arm,cortex-a53", "arm,armv8";
			device_type = "cpu";
			enable-method = "psci";
			reg = <0x1>;
		};

		cpu2: cpu@2 {
			compatible = "arm,cortex-a53", "arm,armv8";
			device_type = "cpu";
			enable-method = "psci";
			reg = <0x2>;
		};

		cpu3: cpu@3 {
			compatible = "arm,cortex-a53", "arm,armv8";
			device_type = "cpu";
			enable-method = "psci";
			reg = <0x3>;
		};
	};

	pmu {
		compatible = "arm,armv8-pmuv3";
		interrupts = <0 120 8>,
			     <0 121 8>,
			     <0 122 8>,
			     <0 123 8>;
		interrupt-affinity = <&cpu0>,
				     <&cpu1>,
				     <&cpu2>,
				     <&cpu3>;
		interrupt-parent = <&intc>;
	};

	psci {
		compatible = "arm,psci-0.2";
		method = "smc";
	};

	intc: intc@fffc1000 {
		compatible = "arm,gic-400", "arm,cortex-a15-gic";
		#interrupt-cells = <3>;
		interrupt-controller;
		reg = <0x0 0xfffc1000 0x0 0x1000>,
		      <0x0 0xfffc2000 0x0 0x2000>,
		      <0x0 0xfffc4000 0x0 0x2000>,
		      <0x0 0xfffc6000 0x0 0x2000>;
	};

	soc {
		#address-cells = <1>;
		#size-cells = <1>;
		compatible = "simple-bus";
		device_type = "soc";
		interrupt-parent = <&intc>;
		ranges = <0 0 0 0xffffffff>;
		bootph-all;

		clkmgr: clkmgr@ffd10000 {
			compatible = "altr,clk-mgr";
			reg = <0xffd10000 0x1000>;
		};

		gmac0: ethernet@ff800000 {
			compatible = "altr,socfpga-stmmac", "snps,dwmac-3.74a", "snps,dwmac";
			reg = <0xff800000 0x2000>;
			interrupts = <0 90 4>;
			interrupt-names = "macirq";
			mac-address = [00 00 00 00 00 00];
			resets = <&rst EMAC0_RESET>, <&rst EMAC0_OCP_RESET>;
			reset-names = "stmmaceth";
			altr,sysmgr-syscon = <&sysmgr 0x44 0>;
			status = "disabled";
		};

		gmac1: ethernet@ff802000 {
			compatible = "altr,socfpga-stmmac", "snps,dwmac-3.74a", "snps,dwmac";
			reg = <0xff802000 0x2000>;
			interrupts = <0 91 4>;
			interrupt-names = "macirq";
			mac-address = [00 00 00 00 00 00];
			resets = <&rst EMAC1_RESET>, <&rst EMAC1_OCP_RESET>;
			reset-names = "stmmaceth";
			altr,sysmgr-syscon = <&sysmgr 0x48 0>;
			status = "disabled";
		};

		gmac2: ethernet@ff804000 {
			compatible = "altr,socfpga-stmmac", "snps,dwmac-3.74a", "snps,dwmac";
			reg = <0xff804000 0x2000>;
			interrupts = <0 92 4>;
			interrupt-names = "macirq";
			mac-address = [00 00 00 00 00 00];
			resets = <&rst EMAC2_RESET>, <&rst EMAC2_OCP_RESET>;
			reset-names = "stmmaceth";
			altr,sysmgr-syscon = <&sysmgr 0x4c 0>;
			status = "disabled";
		};

		gpio0: gpio@ffc03200 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "snps,dw-apb-gpio";
			reg = <0xffc03200 0x100>;
			resets = <&rst GPIO0_RESET>;
			status = "disabled";

			porta: gpio-controller@0 {
				compatible = "snps,dw-apb-gpio-port";
				gpio-controller;
				#gpio-cells = <2>;
				snps,nr-gpios = <24>;
				reg = <0>;
				interrupt-controller;
				#interrupt-cells = <2>;
				interrupts = <0 110 4>;
				bank-name = "porta";
			};
		};

		gpio1: gpio@ffc03300 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "snps,dw-apb-gpio";
			reg = <0xffc03300 0x100>;
			resets = <&rst GPIO1_RESET>;
			status = "disabled";

			portb: gpio-controller@0 {
				compatible = "snps,dw-apb-gpio-port";
				gpio-controller;
				#gpio-cells = <2>;
				snps,nr-gpios = <24>;
				reg = <0>;
				interrupt-controller;
				#interrupt-cells = <2>;
				interrupts = <0 111 4>;
				bank-name = "portb";
			};
		};

		i2c0: i2c@ffc02800 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "snps,designware-i2c";
			reg = <0xffc02800 0x100>;
			interrupts = <0 103 4>;
			resets = <&rst I2C0_RESET>;
			reset-names = "i2c";
			status = "disabled";
		};

		i2c1: i2c@ffc02900 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "snps,designware-i2c";
			reg = <0xffc02900 0x100>;
			interrupts = <0 104 4>;
			resets = <&rst I2C1_RESET>;
			reset-names = "i2c";
			status = "disabled";
		};

		i2c2: i2c@ffc02a00 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "snps,designware-i2c";
			reg = <0xffc02a00 0x100>;
			interrupts = <0 105 4>;
			resets = <&rst I2C2_RESET>;
			reset-names = "i2c";
			status = "disabled";
		};

		i2c3: i2c@ffc02b00 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "snps,designware-i2c";
			reg = <0xffc02b00 0x100>;
			interrupts = <0 106 4>;
			resets = <&rst I2C3_RESET>;
			reset-names = "i2c";
			status = "disabled";
		};

		i2c4: i2c@ffc02c00 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "snps,designware-i2c";
			reg = <0xffc02c00 0x100>;
			interrupts = <0 107 4>;
			resets = <&rst I2C4_RESET>;
			reset-names = "i2c";
			status = "disabled";
		};

		mmc: dwmmc0@ff808000 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "altr,socfpga-dw-mshc";
			reg = <0xff808000 0x1000>;
			interrupts = <0 96 4>;
			fifo-depth = <0x400>;
			resets = <&rst SDMMC_RESET>, <&rst SDMMC_OCP_RESET>;
			bootph-all;
			status = "disabled";
		};

		nand: nand@ffb90000 {
			#address-cells = <1>;
			#size-cells = <0>;
			compatible = "altr,socfpga-denali-nand";
			reg = <0xffb90000 0x10000>,
			      <0xffb80000 0x1000>;
			reg-names = "nand_data", "denali_reg";
			interrupts = <0 97 4>;
			resets = <&rst NAND_RESET>, <&rst NAND_OCP_RESET>;
			status = "disabled";
		};

		ocram: sram@ffe00000 {
			compatible = "mmio-sram";
			reg = <0xffe00000 0x100000>;
		};

		qspi: spi@ff8d2000 {
			compatible = "cdns,qspi-nor";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0xff8d2000 0x100>,
			      <0xff900000 0x100000>;
			interrupts = <0 3 4>;
			cdns,fifo-depth = <128>;
			cdns,fifo-width = <4>;
			cdns,trigger-address = <0x00000000>;
			status = "disabled";
		};

		rst: rstmgr@ffd11000 {
			#reset-cells = <1>;
			compatible = "altr,rst-mgr";
			reg = <0xffd11000 0x1000>;
			altr,modrst-offset = <0x20>;
			bootph-all;
		};

		sdr: sdr@f8000400 {
			 compatible = "altr,sdr-ctl-s10";
			 reg = <0xf8000400 0x80>,
			       <0xf8010000 0x190>,
			       <0xf8011000 0x500>;
			 resets = <&rst DDRSCH_RESET>;
			 bootph-all;
		 };

		spi0: spi@ffda4000 {
			compatible = "intel,stratix10-spi",
				     "snps,dw-apb-ssi-4.00a", "snps,dw-apb-ssi";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0xffda4000 0x1000>;
			interrupts = <0 99 4>;
			resets = <&rst SPIM0_RESET>;
			reg-io-width = <4>;
			num-chipselect = <4>;
			bus-num = <0>;
			status = "disabled";
		};

		spi1: spi@ffda5000 {
			compatible = "intel,stratix10-spi",
				     "snps,dw-apb-ssi-4.00a", "snps,dw-apb-ssi";
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0xffda5000 0x1000>;
			interrupts = <0 100 4>;
			resets = <&rst SPIM1_RESET>;
			reg-io-width = <4>;
			num-chipselect = <4>;
			bus-num = <0>;
			status = "disabled";
		};

		sysmgr: sysmgr@ffd12000 {
			compatible = "altr,sys-mgr", "syscon";
			reg = <0xffd12000 0x1000>;
		};

		/* Local timer */
		timer {
			compatible = "arm,armv8-timer";
			interrupts = <1 13 0xf08>,
				     <1 14 0xf08>,
				     <1 11 0xf08>,
				     <1 10 0xf08>;
		};

		timer0: timer0@ffc03000 {
			compatible = "snps,dw-apb-timer";
			interrupts = <0 113 4>;
			reg = <0xffc03000 0x100>;
		};

		timer1: timer1@ffc03100 {
			compatible = "snps,dw-apb-timer";
			interrupts = <0 114 4>;
			reg = <0xffc03100 0x100>;
		};

		timer2: timer2@ffd00000 {
			compatible = "snps,dw-apb-timer";
			interrupts = <0 115 4>;
			reg = <0xffd00000 0x100>;
		};

		timer3: timer3@ffd00100 {
			compatible = "snps,dw-apb-timer";
			interrupts = <0 116 4>;
			reg = <0xffd00100 0x100>;
		};

		uart0: serial0@ffc02000 {
			compatible = "snps,dw-apb-uart";
			reg = <0xffc02000 0x100>;
			interrupts = <0 108 4>;
			reg-shift = <2>;
			reg-io-width = <4>;
			resets = <&rst UART0_RESET>;
			clock-frequency = <100000000>;
			bootph-all;
			status = "disabled";
		};

		uart1: serial1@ffc02100 {
			compatible = "snps,dw-apb-uart";
			reg = <0xffc02100 0x100>;
			interrupts = <0 109 4>;
			reg-shift = <2>;
			reg-io-width = <4>;
			resets = <&rst UART1_RESET>;
			status = "disabled";
		};

		usbphy0: usbphy@0 {
			#phy-cells = <0>;
			compatible = "usb-nop-xceiv";
			status = "okay";
		};

		usb0: usb@ffb00000 {
			compatible = "snps,dwc2";
			reg = <0xffb00000 0x40000>;
			interrupts = <0 93 4>;
			phys = <&usbphy0>;
			phy-names = "usb2-phy";
			resets = <&rst USB0_RESET>, <&rst USB0_OCP_RESET>;
			reset-names = "dwc2", "dwc2-ecc";
			status = "disabled";
		};

		usb1: usb@ffb40000 {
			compatible = "snps,dwc2";
			reg = <0xffb40000 0x40000>;
			interrupts = <0 94 4>;
			phys = <&usbphy0>;
			phy-names = "usb2-phy";
			resets = <&rst USB1_RESET>, <&rst USB1_OCP_RESET>;
			reset-names = "dwc2", "dwc2-ecc";
			status = "disabled";
		};

		watchdog0: watchdog@ffd00200 {
			compatible = "snps,dw-wdt";
			reg = <0xffd00200 0x100>;
			interrupts = <0 117 4>;
			resets = <&rst WATCHDOG0_RESET>;
			status = "disabled";
		};

		watchdog1: watchdog@ffd00300 {
			compatible = "snps,dw-wdt";
			reg = <0xffd00300 0x100>;
			interrupts = <0 118 4>;
			resets = <&rst WATCHDOG1_RESET>;
			status = "disabled";
		};

		watchdog2: watchdog@ffd00400 {
			compatible = "snps,dw-wdt";
			reg = <0xffd00400 0x100>;
			interrupts = <0 125 4>;
			resets = <&rst WATCHDOG2_RESET>;
			status = "disabled";
		};

		watchdog3: watchdog@ffd00500 {
			compatible = "snps,dw-wdt";
			reg = <0xffd00500 0x100>;
			interrupts = <0 126 4>;
			resets = <&rst WATCHDOG3_RESET>;
			status = "disabled";
		};
	};
};
