// SPDX-License-Identifier: GPL-2.0
/*
 * dts file for Hisilicon HiKey960 Development Board
 *
 * Copyright (C) 2016, Hisilicon Ltd.
 *
 */

/dts-v1/;

#include "hi3660.dtsi"
#include "hikey960-pinctrl.dtsi"
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/input/input.h>
#include <dt-bindings/interrupt-controller/irq.h>

/ {
	model = "HiKey960";
	compatible = "hisilicon,hi3660-hikey960", "hisilicon,hi3660";

	aliases {
		mshc1 = &dwmmc1;
		mshc2 = &dwmmc2;
		serial0 = &uart0;
		serial1 = &uart1;
		serial2 = &uart2;
		serial3 = &uart3;
		serial4 = &uart4;
		serial5 = &uart5;
		serial6 = &uart6;
	};

	chosen {
		stdout-path = "serial6:115200n8";
	};

	memory@0 {
		device_type = "memory";
		/* rewrite this at bootloader */
		reg = <0x0 0x0 0x0 0x0>;
	};

	reserved-memory {
		#address-cells = <2>;
		#size-cells = <2>;
		ranges;

		ramoops@32000000 {
			compatible = "ramoops";
			reg = <0x0 0x32000000 0x0 0x00100000>;
			record-size	= <0x00020000>;
			console-size	= <0x00020000>;
			ftrace-size	= <0x00020000>;
		};
	};

	reboot-mode-syscon@32100000 {
		compatible = "syscon", "simple-mfd";
		reg = <0x0 0x32100000 0x0 0x00001000>;

		reboot-mode {
			compatible = "syscon-reboot-mode";
			offset = <0x0>;

			mode-normal	= <0x77665501>;
			mode-bootloader	= <0x77665500>;
			mode-recovery	= <0x77665502>;
		};
	};

	keys {
		compatible = "gpio-keys";
		pinctrl-names = "default";
		pinctrl-0 = <&pwr_key_pmx_func &pwr_key_cfg_func>;

		power {
			wakeup-source;
			gpios = <&gpio4 2 GPIO_ACTIVE_LOW>;
			label = "GPIO Power";
			linux,code = <KEY_POWER>;
		};
	};

	leds {
		compatible = "gpio-leds";

		user_led1 {
			label = "green:user1";
			/* gpio_150_user_led1 */
			gpios = <&gpio18 6 0>;
			linux,default-trigger = "heartbeat";
		};

		user_led2 {
			label = "green:user2";
			/* gpio_151_user_led2 */
			gpios = <&gpio18 7 0>;
			linux,default-trigger = "none";
		};

		user_led3 {
			label = "green:user3";
			/* gpio_189_user_led3 */
			gpios = <&gpio23 5 0>;
			linux,default-trigger = "mmc0";
		};

		user_led4 {
			label = "green:user4";
			/* gpio_190_user_led4 */
			gpios = <&gpio23 6 0>;
			panic-indicator;
			linux,default-trigger = "none";
		};

		wlan_active_led {
			label = "yellow:wlan";
			/* gpio_205_wifi_active */
			gpios = <&gpio25 5 0>;
			linux,default-trigger = "phy0tx";
			default-state = "off";
		};

		bt_active_led {
			label = "blue:bt";
			gpios = <&gpio25 7 0>;
			/* gpio_207_user_led1 */
			linux,default-trigger = "hci0-power";
			default-state = "off";
		};
	};

	pmic: pmic@fff34000 {
		compatible = "hisilicon,hi6421v530-pmic";
		reg = <0x0 0xfff34000 0x0 0x1000>;
		interrupt-controller;
		#interrupt-cells = <2>;

		regulators {
			ldo3: LDO3 { /* HDMI */
				regulator-name = "VOUT3_1V85";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <2200000>;
				regulator-enable-ramp-delay = <120>;
			};

			ldo9: LDO9 { /* SDCARD I/O */
				regulator-name = "VOUT9_1V8_2V95";
				regulator-min-microvolt = <1750000>;
				regulator-max-microvolt = <3300000>;
				regulator-enable-ramp-delay = <240>;
			};

			ldo11: LDO11 { /* Low Speed Connector */
				regulator-name = "VOUT11_1V8_2V95";
				regulator-min-microvolt = <1750000>;
				regulator-max-microvolt = <3300000>;
				regulator-enable-ramp-delay = <240>;
			};

			ldo15: LDO15 { /* UFS VCC */
				regulator-name = "VOUT15_3V0";
				regulator-min-microvolt = <1750000>;
				regulator-max-microvolt = <3000000>;
				regulator-boot-on;
				regulator-always-on;
				regulator-enable-ramp-delay = <120>;
			};

			ldo16: LDO16 { /* SD VDD */
				regulator-name = "VOUT16_2V95";
				regulator-min-microvolt = <1750000>;
				regulator-max-microvolt = <3000000>;
				regulator-enable-ramp-delay = <360>;
			};
		};
	};

	wlan_en: wlan-en-1-8v {
		compatible = "regulator-fixed";
		regulator-name = "wlan-en-regulator";
		regulator-min-microvolt = <1800000>;
		regulator-max-microvolt = <1800000>;

		/* GPIO_051_WIFI_EN */
		gpio = <&gpio6 3 0>;

		/* WLAN card specific delay */
		startup-delay-us = <70000>;
		enable-active-high;
	};

	firmware {
		optee {
			compatible = "linaro,optee-tz";
			method = "smc";
		};
	};
};

/*
 * Legend: proper name = the GPIO line is used as GPIO
 *         NC = not connected (pin out but not routed from the chip to
 *              anything the board)
 *         "[PER]" = pin is muxed for [peripheral] (not GPIO)
 *         "" = no idea, schematic doesn't say, could be
 *              unrouted (not connected to any external pin)
 *         LSEC = Low Speed External Connector
 *         HSEC = High Speed External Connector
 *
 * Line names are taken from "HiKey 960 Board ver A" schematics
 * from Huawei. The 40 pin low speed expansion connector is named
 * J2002 63453-140LF.
 *
 * For the lines routed to the external connectors the
 * lines are named after the 96Boards CE Specification 1.0,
 * Appendix "Expansion Connector Signal Description".
 *
 * When the 96Board naming of a line and the schematic name of
 * the same line are in conflict, the 96Board specification
 * takes precedence, which means that the external UART on the
 * LSEC is named UART0 while the schematic and SoC names this
 * UART3. This is only for the informational lines i.e. "[FOO]",
 * the GPIO named lines "GPIO-A" thru "GPIO-L" are the only
 * ones actually used for GPIO.
 */
&gpio0 {
	/* GPIO_000-GPIO_007 */
	gpio-line-names =
		"",
		"TP901", /* TEST_MODE connected to TP901 */
		"[PMU0_SSI]",
		"[PMU1_SSI]",
		"[PMU2_SSI]",
		"[PMU0_CLKOUT]",
		"[JTAG_TCK]",
		"[JTAG_TMS]";
};

&gpio1 {
	/* GPIO_008-GPIO_015 */
	gpio-line-names =
		"[JTAG_TRST_N]",
		"[JTAG_TDI]",
		"[JTAG_TDO]",
		"NC", "NC",
		"[I2C3_SCL]",
		"[I2C3_SDA]",
		"NC";
};

&gpio2 {
	/* GPIO_016-GPIO_023 */
	gpio-line-names =
		"NC", "NC", "NC",
		"GPIO-J", /* LSEC pin 32: GPIO_019 */
		"GPIO_020_HDMI_SEL",
		"GPIO-L", /* LSEC pin 34: GPIO_021 */
		"GPIO_022_UFSBUCK_INT_N",
		"GPIO-G"; /* LSEC pin 29: LCD_TE0 */
};

&gpio3 {
	/* GPIO_024-GPIO_031 */
	/* The rail from pin BK36 is named LCD_TE0, we assume to be muxed as GPIO for GPIO-G */
	gpio-line-names =
		"[CSI0_MCLK]", /* HSEC pin 15: ISP_CCLK0_MCAM */
		"[CSI1_MCLK]", /* HSEC pin 17: ISP_CCLK1_SCAM */
		"NC",
		"[I2C2_SCL]", /* HSEC pin 32: ISP_SCL0 */
		"[I2C2_SDA]", /* HSEC pin 34: ISP_SDA0 */
		"[I2C3_SCL]", /* HSEC pin 36: ISP_SCL1 */
		"[I2C3_SDA]", /* HSEC pin 38: ISP_SDA1 */
		"NC";
};

&gpio4 {
	/* GPIO_032-GPIO_039 */
	gpio-line-names =
		"NC", "NC",
		"PWR_BTN_N", /* LSEC pin 4: GPIO_034_PWRON_DET */
		"GPIO_035_PMU2_EN",
		"GPIO_036_USB_HUB_RESET",
		"NC", "NC", "NC";
};

&gpio5 {
	/* GPIO_040-GPIO_047 */
	gpio-line-names =
		"GPIO-H", /* LSEC pin 30: GPIO_040_LCD_RST_N */
		"GPIO_041_HDMI_PD",
		"TP904", /* Test point */
		"TP905", /* Test point */
		"NC", "NC",
		"GPIO_046_HUB_VDD33_EN",
		"GPIO_047_PMU1_EN";
};

&gpio6 {
	/* GPIO_048-GPIO_055 */
	gpio-line-names =
		"NC", "NC", "NC",
		"GPIO_051_WIFI_EN",
		"GPIO-I", /* LSEC pin 31: GPIO_052_CAM0_RST_N */
		/*
		 * These two pins should be used for SD(IO) data according to the
		 * 96boards specification but seems to be repurposed for a IRDA UART.
		 * They are however named according to the spec.
		 */
		"[SD_DAT1]", /* HSEC pin 3: UART0_IRDA_RXD */
		"[SD_DAT2]", /* HSEC pin 5: UART0_IRDA_TXD */
		"[UART1_RXD]"; /* LSEC pin 13: DEBUG_UART6_RXD */
};

&gpio7 {
	/* GPIO_056-GPIO_063 */
	gpio-line-names =
		"[UART1_TXD]", /* LSEC pin 11: DEBUG_UART6_TXD */
		"[UART0_CTS]", /* LSEC pin 3: UART3_CTS_N */
		"[UART0_RTS]", /* LSEC pin 9: UART3_RTS_N */
		"[UART0_RXD]", /* LSEC pin 7: UART3_RXD */
		"[UART0_TXD]", /* LSEC pin 5: UART3_TXD */
		"[SOC_BT_UART4_CTS_N]",
		"[SOC_BT_UART4_RTS_N]",
		"[SOC_BT_UART4_RXD]";
};

&gpio8 {
	/* GPIO_064-GPIO_071 */
	gpio-line-names =
		"[SOC_BT_UART4_TXD]",
		"NC",
		"[PMU_HKADC_SSI]",
		"NC",
		"GPIO_068_SEL",
		"NC", "NC", "NC";

};

&gpio9 {
	/* GPIO_072-GPIO_079 */
	gpio-line-names =
		"NC", "NC", "NC",
		"GPIO-K", /* LSEC pin 33: GPIO_075_CAM1_RST_N */
		"NC", "NC", "NC", "NC";
};

&gpio10 {
	/* GPIO_080-GPIO_087 */
	gpio-line-names = "NC", "NC", "NC", "NC", "NC", "NC", "NC", "NC";
};

&gpio11 {
	/* GPIO_088-GPIO_095 */
	gpio-line-names =
		"NC",
		"[PCIE_PERST_N]",
		"NC", "NC", "NC", "NC", "NC", "NC";
};

&gpio12 {
	/* GPIO_096-GPIO_103 */
	gpio-line-names = "NC", "NC", "NC", "", "", "", "", "NC";
};

&gpio13 {
	/* GPIO_104-GPIO_111 */
	gpio-line-names = "NC", "NC", "NC", "NC", "NC", "NC", "NC", "NC";
};

&gpio14 {
	/* GPIO_112-GPIO_119 */
	gpio-line-names = "NC", "NC", "NC", "NC", "NC", "NC", "NC", "NC";
};

&gpio15 {
	/* GPIO_120-GPIO_127 */
	gpio-line-names =
		"NC", "NC", "NC", "NC", "NC", "NC",
		"GPIO_126_BT_EN",
		"TP902"; /* GPIO_127_JTAG_SEL0 */
};

&gpio16 {
	/* GPIO_128-GPIO_135 */
	gpio-line-names = "", "", "", "", "", "", "", "";
};

&gpio17 {
	/* GPIO_136-GPIO_143 */
	gpio-line-names = "", "", "", "", "", "", "", "";
};

&gpio18 {
	/* GPIO_144-GPIO_151 */
	gpio-line-names =
		"[UFS_REF_CLK]",
		"[UFS_RST_N]",
		"[SPI1_SCLK]", /* HSEC pin 9: GPIO_146_SPI3_CLK */
		"[SPI1_DIN]", /* HSEC pin 11: GPIO_147_SPI3_DI */
		"[SPI1_DOUT]", /* HSEC pin 1: GPIO_148_SPI3_DO */
		"[SPI1_CS]", /* HSEC pin 7: GPIO_149_SPI3_CS0_N */
		"GPIO_150_USER_LED1",
		"GPIO_151_USER_LED2";
};

&gpio19 {
	/* GPIO_152-GPIO_159 */
	gpio-line-names = "NC", "NC", "NC", "NC", "", "", "", "";
};

&gpio20 {
	/* GPIO_160-GPIO_167 */
	gpio-line-names =
		"[SD_CLK]",
		"[SD_CMD]",
		"[SD_DATA0]",
		"[SD_DATA1]",
		"[SD_DATA2]",
		"[SD_DATA3]",
		"", "";
};

&gpio21 {
	/* GPIO_168-GPIO_175 */
	gpio-line-names =
		"[WL_SDIO_CLK]",
		"[WL_SDIO_CMD]",
		"[WL_SDIO_DATA0]",
		"[WL_SDIO_DATA1]",
		"[WL_SDIO_DATA2]",
		"[WL_SDIO_DATA3]",
		"", "";
};

&gpio22 {
	/* GPIO_176-GPIO_183 */
	gpio-line-names =
		"[GPIO_176_PMU_PWR_HOLD]",
		"NA",
		"[SYSCLK_EN]",
		"GPIO_179_WL_WAKEUP_AP",
		"GPIO_180_HDMI_INT",
		"NA",
		"GPIO-F", /* LSEC pin 28: LCD_BL_PWM */
		"[I2C0_SCL]"; /* LSEC pin 15 */
};

&gpio23 {
	/* GPIO_184-GPIO_191 */
	gpio-line-names =
		"[I2C0_SDA]", /* LSEC pin 17 */
		"[I2C1_SCL]", /* Actual SoC I2C1 */
		"[I2C1_SDA]", /* Actual SoC I2C1 */
		"[I2C1_SCL]", /* LSEC pin 19: I2C7_SCL */
		"[I2C1_SDA]", /* LSEC pin 21: I2C7_SDA */
		"GPIO_189_USER_LED3",
		"GPIO_190_USER_LED4",
		"";
};

&gpio24 {
	/* GPIO_192-GPIO_199 */
	gpio-line-names =
		"[PCM_DI]", /* LSEC pin 22: GPIO_192_I2S0_DI */
		"[PCM_DO]", /* LSEC pin 20: GPIO_193_I2S0_DO */
		"[PCM_CLK]", /* LSEC pin 18: GPIO_194_I2S0_XCLK */
		"[PCM_FS]", /* LSEC pin 16: GPIO_195_I2S0_XFS */
		"[GPIO_196_I2S2_DI]",
		"[GPIO_197_I2S2_DO]",
		"[GPIO_198_I2S2_XCLK]",
		"[GPIO_199_I2S2_XFS]";
};

&gpio25 {
	/* GPIO_200-GPIO_207 */
	gpio-line-names =
		"NC",
		"NC",
		"GPIO_202_VBUS_TYPEC",
		"GPIO_203_SD_DET",
		"GPIO_204_PMU12_IRQ_N",
		"GPIO_205_WIFI_ACTIVE",
		"GPIO_206_USBSW_SEL",
		"GPIO_207_BT_ACTIVE";
};

&gpio26 {
	/* GPIO_208-GPIO_215 */
	gpio-line-names =
		"GPIO-A", /* LSEC pin 23: GPIO_208 */
		"GPIO-B", /* LSEC pin 24: GPIO_209 */
		"GPIO-C", /* LSEC pin 25: GPIO_210 */
		"GPIO-D", /* LSEC pin 26: GPIO_211 */
		"GPIO-E", /* LSEC pin 27: GPIO_212 */
		"[PCIE_CLKREQ_N]",
		"[PCIE_WAKE_N]",
		"[SPI0_CLK]"; /* LSEC pin 8: SPI2_CLK */
};

&gpio27 {
	/* GPIO_216-GPIO_223 */
	gpio-line-names =
		"[SPI0_DIN]", /* LSEC pin 10: SPI2_DI */
		"[SPI0_DOUT]", /* LSEC pin 14: SPI2_DO */
		"[SPI0_CS]", /* LSEC pin 12: SPI2_CS0_N */
		"GPIO_219_CC_INT",
		"NC",
		"NC",
		"[PMU_INT]",
		"";
};

&gpio28 {
	/* GPIO_224-GPIO_231 */
	gpio-line-names =
		"", "", "", "", "", "", "", "";
};

&i2c0 {
	/* On Low speed expansion */
	label = "LS-I2C0";
	status = "okay";
};

&i2c1 {
	status = "okay";

	adv7533: adv7533@39 {
		status = "ok";
		compatible = "adi,adv7533";
		reg = <0x39>;
	};
};

&uart3 {
	/* On Low speed expansion */
	label = "LS-UART0";
	status = "okay";
};

&uart4 {
	status = "okay";

	bluetooth {
		compatible = "ti,wl1837-st";
		enable-gpios = <&gpio15 6 GPIO_ACTIVE_HIGH>;
		max-speed = <3000000>;
	};
};

&i2c7 {
	/* On Low speed expansion */
	label = "LS-I2C1";
	status = "okay";
};

&uart6 {
	/* On Low speed expansion */
	label = "LS-UART1";
	status = "okay";
};

&spi2 {
	/* On Low speed expansion */
	label = "LS-SPI0";
	status = "okay";
};

&spi3 {
	/* On High speed expansion */
	label = "HS-SPI1";
	status = "okay";
};

&dwmmc1 {
	cd-gpios = <&gpio25 3 GPIO_ACTIVE_LOW>;
	pinctrl-names = "default";
	pinctrl-0 = <&sd_pmx_func
		     &sd_clk_cfg_func
		     &sd_cfg_func>;
	vmmc-supply = <&ldo16>;
	vqmmc-supply = <&ldo9>;
	status = "okay";
};

&dwmmc2 { /* WIFI */
	bus-width = <0x4>;
	non-removable;
	broken-cd;
	cap-power-off-card;
	pinctrl-names = "default";
	pinctrl-0 = <&sdio_pmx_func
		     &sdio_clk_cfg_func
		     &sdio_cfg_func>;
	/* WL_EN */
	vmmc-supply = <&wlan_en>;
	status = "ok";

	wlcore: wlcore@2 {
		compatible = "ti,wl1837";
		reg = <2>;      /* sdio func num */
		/* WL_IRQ, GPIO_179_WL_WAKEUP_AP */
		interrupt-parent = <&gpio22>;
		interrupts = <3 IRQ_TYPE_EDGE_RISING>;
	};
};
