// SPDX-License-Identifier: GPL-2.0+

#include "rk356x-u-boot.dtsi"

&gpio0 {
	bootph-pre-ram;
};

&sdhci {
	cap-mmc-highspeed;
	pinctrl-names = "default";
	pinctrl-0 = <&emmc_bus8 &emmc_clk &emmc_cmd &emmc_datastrobe>;
};

&sfc {
	flash@0 {
		bootph-pre-ram;
		bootph-some-ram;
	};
};

/*
 * U-Boot does not support multiple regulators using the same gpio,
 * use vcc5v0_usb20_host to fix use of USB 2.0 port
 */
&usb2phy0_otg {
	phy-supply = <&vcc5v0_usb20_host>;
};

&vcc3v3_sd {
	bootph-pre-ram;
};

&vcc_sd_h {
	bootph-pre-ram;
};
