// SPDX-License-Identifier: GPL-2.0
/*
 * dts file for Xilinx Versal a2197 RevA System Controller
 *
 * (C) Copyright 2019, Xilinx, Inc.
 *
 * Michal Simek <michal.simek@amd.com>
 */
/dts-v1/;

#include "zynqmp.dtsi"
#include "zynqmp-clk-ccf.dtsi"
#include <dt-bindings/gpio/gpio.h>
#include <dt-bindings/phy/phy.h>

/ {
	model = "Versal System Controller on a2197 Processor Char board RevA"; /* Tenzing */
	compatible = "xlnx,zynqmp-p-a2197-00-revA", "xlnx,zynqmp-a2197-revA",
		     "xlnx,zynqmp-a2197", "xlnx,zynqmp";

	aliases {
		ethernet0 = &gem0;
		i2c0 = &i2c0;
		i2c1 = &i2c1;
		mmc0 = &sdhci0;
		mmc1 = &sdhci1;
		nvmem0 = &eeprom;
		rtc0 = &rtc;
		serial0 = &uart0;
		serial1 = &uart1;
		serial2 = &dcc;
		usb0 = &usb0;
		usb1 = &usb1;
	};

	chosen {
		bootargs = "earlycon";
		stdout-path = "serial0:115200n8";
	};

	memory@0 {
		device_type = "memory";
		reg = <0x0 0x0 0x0 0x80000000>;
	};

	si5332_1: si5332-1 { /* clk0_sgmii - u142 */
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <125000000>;
	};

	si5332_2: si5332-2 { /* clk1_usb - u142 */
		compatible = "fixed-clock";
		#clock-cells = <0>;
		clock-frequency = <27000000>;
	};
};

&sdhci0 { /* emmc MIO 13-23 - with some settings  16GB */
	status = "okay";
	non-removable;
	disable-wp;
	no-sd;
	no-sdio;
	cap-mmc-hw-reset;
	bus-width = <8>;
	xlnx,mio-bank = <0>;
};

&uart0 { /* uart0 MIO38-39 */
	status = "okay";
};

&uart1 { /* uart1 MIO40-41 */
	status = "okay";
};

&sdhci1 { /* sd1 MIO45-51 cd in place */
	status = "okay";
	no-1-8-v;
	disable-wp;
	xlnx,mio-bank = <1>;
};

&psgtr {
	status = "okay";
	/* sgmii, usb3 */
	clocks = <&si5332_1>, <&si5332_2>;
	clock-names = "ref0", "ref1";
};

&gem0 {
	status = "okay";
	phy-handle = <&phy0>;
	phy-mode = "sgmii"; /* DTG generates this properly  1512 */
	mdio: mdio {
		#address-cells = <1>;
		#size-cells = <0>;
		/* reset-gpios = <&gpio 142 GPIO_ACTIVE_LOW>; */
		phy0: ethernet-phy@0 {
			reg = <0>;
		};
	};
};

&gpio {
	status = "okay";
	gpio-line-names = "", "", "", "", "", /* 0 - 4 */
		  "", "", "DC_SYS_CTRL0", "DC_SYS_CTRL1", "DC_SYS_CTRL2", /* 5 - 9 */
		  "DC_SYS_CTRL3", "DC_SYS_CTRL4", "DC_SYS_CTRL5", "EMMC_DAT0", "EMMC_DAT1", /* 10 - 14 */
		  "EMMC_DAT2", "EMMC_DAT3", "EMMC_DAT4", "EMMC_DAT5", "EMMC_DAT6", /* 15 - 19 */
		  "EMMC_DAT7", "EMMC_CMD", "EMMC_CLK", "EMMC_RST_B", "", /* 20 - 24 */
		  "", "", "", "", "", /* 25 - 29 */
		  "", "", "", "", "LP_I2C0_PMC_SCL", /* 30 - 34 */
		  "LP_I2C0_PMC_SDA", "LP_I2C1_SCL", "LP_I2C1_SDA", "UART0_RXD_IN", "UART0_TXD_OUT", /* 35 - 39 */
		  "UART1_TXD_OUT", "UART1_RXD_IN", "ETH_RESET_B", "", "", /* 40 - 44 */
		  "SD1_CD_B", "SD1_DATA0", "SD1_DATA1", "SD1_DATA2", "SD1_DATA3", /* 45 - 49 */
		  "SD1_CMD", "SD1_CLK", "USB0_CLK", "USB0_DIR", "USB0_DATA2", /* 50 - 54 */
		  "USB0_NXT", "USB0_DATA0", "USB0_DATA1", "USB0_STP", "USB0_DATA3", /* 55 - 59 */
		  "USB0_DATA4", "USB0_DATA5", "USB0_DATA6", "USB0_DATA7", "USB1_CLK", /* 60 - 64 */
		  "USB1_DIR", "USB1_DATA2", "USB1_NXT", "USB1_DATA0", "USB1_DATA1", /* 65 - 69 */
		  "USB1_STP", "USB1_DATA3", "USB1_DATA4", "USB1_DATA5", "USB1_DATA6", /* 70 - 74 */
		  "USB1_DATA7", "ETH_MDC", "ETH_MDIO", /* 75 - 77, MIO end and EMIO start */
		  "SYSCTLR_VERSAL_MODE0", "SYSCTLR_VERSAL_MODE1", /* 78 - 79 */
		  "SYSCTLR_VERSAL_MODE2", "SYSCTLR_VERSAL_MODE3", "SYSCTLR_POR_B_LS", "DC_PRSNT", "SYSCTLR_POWER_EN", /* 80 - 84 */
		  "SYSCTLR_JTAG_S0", "SYSCTLR_JTAG_S1", "SYSCTLR_IIC_MUX0_RESET_B", "SYSCTLR_IIC_MUX1_RESET_B", "SYSCTLR_LP_I2C_SM_ALERT", /* 85 - 89 */
		  "SYSCTLR_GPIO0", "SYSCTLR_GPIO1", "SYSCTLR_GPIO2", "SYSCTLR_GPIO3", "SYSCTLR_GPIO4", /* 90 - 94 */
		  "SYSCTLR_GPIO5", "VCCO_500_RBIAS", "VCCO_501_RBIAS", "VCCO_502_RBIAS", "VCCO_500_RBIAS_LED", /* 95 - 99 */
		  "VCCO_501_RBIAS_LED", "VCCO_502_RBIAS_LED", "SYSCTLR_VCCINT_EN", "SYSCTLR_VCC_IO_SOC_EN", "SYSCTLR_VCC_PMC_EN", /* 100 - 104 */
		  "SYSCTLR_VCC_RAM_EN", "SYSCTLR_VCC_PSLP_EN", "SYSCTLR_VCC_PSFP_EN", "SYSCTLR_VCCAUX_EN", "SYSCTLR_VCCAUX_PMC_EN", /* 105 - 109 */
		  "SYSCTLR_VCCO_500_EN", "SYSCTLR_VCCO_501_EN", "SYSCTLR_VCCO_502_EN", "SYSCTLR_VCCO_503_EN", "SYSCTLR_VCC1V8_EN", /* 110 - 114 */
		  "SYSCTLR_VCC3V3_EN", "SYSCTLR_VCC1V2_DDR4_EN", "SYSCTLR_VCC1V1_LP4_EN", "SYSCTLR_VDD1_1V8_LP4_EN", "SYSCTLR_VADJ_FMC_EN", /* 115 - 119 */
		  "SYSCTLR_MGTYAVCC_EN", "SYSCTLR_MGTYAVTT_EN", "SYSCTLR_MGTYVCCAUX_EN", "SYSCTLR_UTIL_1V13_EN", "SYSCTLR_UTIL_1V8_EN", /* 120 - 124 */
		  "SYSCTLR_UTIL_2V5_EN", "FMCP1_FMC_PRSNT_M2C_B", "FMCP2_FMC_PRSNT_M2C_B", "FMCP1_FMCP_PRSNT_M2C_B", "FMCP2_FMCP_PRSNT_M2C_B", /* 125 - 129 */
		  "PMBUS1_INA226_ALERT", "PMBUS2_INA226_ALERT", "SYSCTLR_USBC_SBU1", "SYSCTLR_USBC_SBU2", "TI_CABLE1", /* 130 - 134 */
		  "TI_CABLE2", "SYSCTLR_MIC2005_EN_B", "SYSCTLR_MIC2005_FAULT_B", "SYSCTLR_TUSB320_INT_B", "SYSCTLR_TUSB320_ID", /* 135 - 139 */
		  "PMBUS1_ALERT", "PMBUS2_ALERT", "SYSCTLR_ETH_RESET_B", "SYSCTLR_VCC0V85_TG", "MAX6643_OT_B", /* 140 - 144 */
		  "MAX6643_FANFINAL_B", "MAX6643_FULLSPD", "", "", "", /* 145 - 149 */
		  "", "", "", "", "", /* 150 - 154 */
		  "", "", "", "", "", /* 155 - 159 */
		  "", "", "", "", "", /* 160 - 164 */
		  "", "", "", "", "", /* 165 - 169 */
		  "", "", "", ""; /* 170 - 173 */
};

&i2c0 { /* MIO 34-35 - can't stay here */
	status = "okay";
	clock-frequency = <400000>;
	i2c-mux@74 { /* u33 */
		compatible = "nxp,pca9548";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x74>;
		/* reset-gpios = <&gpio SYSCTLR_IIC_MUX0_RESET_B GPIO_ACTIVE_HIGH>; */
		i2c@0 { /* PMBUS1 */
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0>;
			/* On connector J98 */
			reg_vcc_fmc: tps544@7 { /* u80 - FIXME name - don't know what it does */
				compatible = "ti,tps544b25"; /* Documentation/hwmon/pmbus.rst - wiring is missing */
				reg = <0x7>;
				regulator-name = "reg_vcc_fmc";
				regulator-min-microvolt = <1800000>;
				regulator-max-microvolt = <2600000>;
				/* enable-gpio = <&gpio0 23 0x4>; optional */
			};
			reg_vcc_ram: tps544@8 { /* u83 - FIXME name - don't know what it does */
				compatible = "ti,tps544b25"; /* Documentation/hwmon/pmbus.rst - wiring is missing */
				reg = <0x8>;
			};
			reg_vcc_pslp: tps544@9 { /* u85 - FIXME name - don't know what it does */
				compatible = "ti,tps544b25"; /* Documentation/hwmon/pmbus.rst - wiring is missing */
				reg = <0x9>;
			};
			reg_vcc_psfp: tps544@a { /* u86 - FIXME name - don't know what it does */
				compatible = "ti,tps544b25"; /* Documentation/hwmon/pmbus.rst - wiring is missing */
				reg = <0xa>;
			};
			reg_vccint: tps53681@60 { /* u70 - FIXME name - don't know what it does - also vcc_io_soc */
				compatible = "ti,tps53681";
				reg = <0x60>;
				/* vccint, vcc_io_soc */
			};
		};
		i2c@1 { /* PMBUS1_INA226 */
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <1>;
			/* FIXME check alerts coming to SC */
			vcc_fmc: ina226@42 { /* u81 */
				compatible = "ti,ina226";
				reg = <0x42>;
				shunt-resistor = <5000>;
			};
			vcc_ram: ina226@43 { /* u82 */
				compatible = "ti,ina226";
				reg = <0x43>;
				shunt-resistor = <5000>;
			};
			vcc_pslp: ina226@44 { /* u84 */
				compatible = "ti,ina226";
				reg = <0x44>;
				shunt-resistor = <5000>;
			};
			vcc_psfp: ina226@45 { /* u87 */
				compatible = "ti,ina226";
				reg = <0x45>;
				shunt-resistor = <5000>;
			};
		};
		i2c@2 { /* PMBUS2 */
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <2>;
			/* On connector J104 */
			reg_vccaus: tps544@d { /* u88 - FIXME name - don't know what it does */
				compatible = "ti,tps544b25"; /* Documentation/hwmon/pmbus.rst - wiring is missing */
				reg = <0xd>;
			};
			reg_vccaux_fmc: tps544@e { /* u90 - FIXME name - don't know what it does */
				compatible = "ti,tps544b25"; /* Documentation/hwmon/pmbus.rst - wiring is missing */
				reg = <0xe>;
			};
			reg_vcco_500: tps544@f { /* u93 - FIXME name - don't know what it does */
				compatible = "ti,tps544b25"; /* Documentation/hwmon/pmbus.rst - wiring is missing */
				reg = <0xf>;
			};
			reg_vcco_501: tps544@10 { /* u95 - FIXME name - don't know what it does */
				compatible = "ti,tps544b25"; /* Documentation/hwmon/pmbus.rst - wiring is missing */
				reg = <0x10>;
			};
			reg_vcco_502: tps544@11 { /* u97 - FIXME name - don't know what it does */
				compatible = "ti,tps544b25"; /* Documentation/hwmon/pmbus.rst - wiring is missing */
				reg = <0x11>;
			};
			reg_vcco_503: tps544@12 { /* u99 - FIXME name - don't know what it does */
				compatible = "ti,tps544b25"; /* Documentation/hwmon/pmbus.rst - wiring is missing */
				reg = <0x12>;
			};
			reg_vcc1v8: tps544@13 { /* u101 - FIXME name - don't know what it does */
				compatible = "ti,tps544b25"; /* Documentation/hwmon/pmbus.rst - wiring is missing */
				reg = <0x13>;
			};
			reg_vcc3v3: tps544@14 { /* u102 - FIXME name - don't know what it does */
				compatible = "ti,tps544b25"; /* Documentation/hwmon/pmbus.rst - wiring is missing */
				reg = <0x14>;
			};
			reg_vcc1v2_ddr4: tps544@15 { /* u104 - FIXME name - don't know what it does */
				compatible = "ti,tps544b25"; /* Documentation/hwmon/pmbus.rst - wiring is missing */
				reg = <0x15>;
			};
			reg_vcc1v1_lp4: tps544@16 { /* u106 - FIXME name - don't know what it does */
				compatible = "ti,tps544b25"; /* Documentation/hwmon/pmbus.rst - wiring is missing */
				reg = <0x16>;
			};
			reg_vcc1_1V8_lp4: tps544@17 { /* u108 - FIXME name - don't know what it does */
				compatible = "ti,tps544b25"; /* Documentation/hwmon/pmbus.rst - wiring is missing */
				reg = <0x17>;
			};
			reg_vadj_fmc: tps544@19 { /* u109 - FIXME name - don't know what it does */
				compatible = "ti,tps544b25"; /* Documentation/hwmon/pmbus.rst - wiring is missing */
				reg = <0x19>;
			};
			reg_mgtyavcc: tps544@1a { /* u111 - FIXME name - don't know what it does */
				compatible = "ti,tps544b25"; /* Documentation/hwmon/pmbus.rst - wiring is missing */
				reg = <0x1a>;
			};
			reg_mgtyavtt: tps544@1b { /* u114 - FIXME name - don't know what it does */
				compatible = "ti,tps544b25"; /* Documentation/hwmon/pmbus.rst - wiring is missing */
				reg = <0x1b>;
			};
			reg_mgtyvccaux: tps544@1c { /* u115 - FIXME name - don't know what it does */
				compatible = "ti,tps544b25"; /* Documentation/hwmon/pmbus.rst - wiring is missing */
				reg = <0x1c>;
			};
			reg_util_1v13: tps544@1d { /* u117 - FIXME name - don't know what it does */
				compatible = "ti,tps544b25"; /* Documentation/hwmon/pmbus.rst - wiring is missing */
				reg = <0x1d>;
			};
			reg_util_1v8: tps544@1e { /* u118 - FIXME name - don't know what it does */
				compatible = "ti,tps544b25"; /* Documentation/hwmon/pmbus.rst - wiring is missing */
				reg = <0x1e>;
			};
			reg_util_2v5: tps544@1f { /* u119 - FIXME name - don't know what it does */
				compatible = "ti,tps544b25"; /* Documentation/hwmon/pmbus.rst - wiring is missing */
				reg = <0x1f>;
			};
		};
		i2c@3 { /* PMBUS2_INA226 */
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <3>;
			/* FIXME check alerts coming to SC */
			vccaux: ina226@40 { /* u89 */
				compatible = "ti,ina226";
				reg = <0x40>;
				shunt-resistor = <5000>;
			};
			vccaux_fmc: ina226@41 { /* u91 */
				compatible = "ti,ina226";
				reg = <0x41>;
				shunt-resistor = <5000>;
			};
			vcco_500: ina226@42 { /* u92 */
				compatible = "ti,ina226";
				reg = <0x42>;
				shunt-resistor = <5000>;
			};
			vcco_501: ina226@43 { /* u94 */
				compatible = "ti,ina226";
				reg = <0x43>;
				shunt-resistor = <5000>;
			};
			vcco_502: ina226@44 { /* u96 */
				compatible = "ti,ina226";
				reg = <0x44>;
				shunt-resistor = <5000>;
			};
			vcco_503: ina226@45 { /* u98 */
				compatible = "ti,ina226";
				reg = <0x45>;
				shunt-resistor = <5000>;
			};
			vcc_1v8: ina226@46 { /* u100 */
				compatible = "ti,ina226";
				reg = <0x46>;
				shunt-resistor = <5000>;
			};
			vcc_3v3: ina226@47 { /* u103 */
				compatible = "ti,ina226";
				reg = <0x47>;
				shunt-resistor = <5000>;
			};
			vcc_1v2_ddr4: ina226@48 { /* u105 */
				compatible = "ti,ina226";
				reg = <0x48>;
				shunt-resistor = <1000>;
			};
			vcc1v1_lp4: ina226@49 { /* u107 */
				compatible = "ti,ina226";
				reg = <0x49>;
				shunt-resistor = <5000>;
			};
			vadj_fmc: ina226@4a { /* u110 */
				compatible = "ti,ina226";
				reg = <0x4a>;
				shunt-resistor = <5000>;
			};
			mgtyavcc: ina226@4b { /* u112 */
				compatible = "ti,ina226";
				reg = <0x4b>;
				shunt-resistor = <1000>;
			};
			mgtyavtt: ina226@4c { /* u113 */
				compatible = "ti,ina226";
				reg = <0x4c>;
				shunt-resistor = <1000>;
			};
			mgtyvccaux: ina226@4d { /* u116 */
				compatible = "ti,ina226";
				reg = <0x4d>;
				shunt-resistor = <5000>;
			};
			vcc_bat: ina226@4e { /* u12 */
				compatible = "ti,ina226";
				reg = <0x4e>;
				shunt-resistor = <10000000>; /* 10 ohm */
			};
		};
		i2c@4 { /* LP_I2C_SM */
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <4>;
			/* connected to J212G */
			/* zynqmp sm alert or samtec J212H */
		};
		/* 5-7 unused */
	};
};

&i2c1 { /* i2c1 MIO 36-37 */
	status = "okay";
	clock-frequency = <400000>;

	/* Must be enabled via J242 */
	eeprom_versal: eeprom@51 { /* x-prc-01-revA u116, x-prc-02-revA u12 */
		compatible = "atmel,24c02";
		reg = <0x51>;
	};

	i2c-mux@74 { /* u35 */
		compatible = "nxp,pca9548";
		#address-cells = <1>;
		#size-cells = <0>;
		reg = <0x74>;
		/* reset-gpios = <&gpio SYSCTLR_IIC_MUX1_RESET_B GPIO_ACTIVE_HIGH>; */
		dc_i2c: i2c@0 { /* DC_I2C */
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <0>;
			/* Use for storing information about SC board */
			eeprom: eeprom@54 { /* u34 - m24128 16kB */
				compatible = "st,24c128", "atmel,24c128";
				reg = <0x54>;
			};
			si570_ref_clk: clock-generator@5d { /* u32 */
				#clock-cells = <0>;
				compatible = "silabs,si570";
				reg = <0x5d>;	/* 570JAC000900DG */
				temperature-stability = <50>;
				factory-fout = <33333333>;
				clock-frequency = <33333333>;
				clock-output-names = "ref_clk";
				silabs,skip-recall;
			};
			/* Connection via Samtec J212D */
			/* Use for storing information about X-PRC card */
			x_prc_eeprom: eeprom@52 { /* x-prc-01-revA u120, x-prc-02-revA u16 */
				compatible = "atmel,24c02";
				reg = <0x52>;
			};

			/* Use for setting up certain features on X-PRC card */
			x_prc_tca9534: gpio@22 { /* x-prc-01-revA u121, x-prc-02-revA u17 */
				compatible = "nxp,pca9534";
				reg = <0x22>;
				gpio-controller; /* IRQ not connected */
				#gpio-cells = <2>;
				gpio-line-names = "sw4_1", "sw4_2", "sw4_3", "sw4_4",
						  "", "", "", "";
				gtr-sel0-hog {
					gpio-hog;
					gpios = <0 0>;
					input; /* FIXME add meaning */
					line-name = "sw4_1";
				};
				gtr-sel1-hog {
					gpio-hog;
					gpios = <1 0>;
					input; /* FIXME add meaning */
					line-name = "sw4_2";
				};
				gtr-sel2-hog {
					gpio-hog;
					gpios = <2 0>;
					input; /* FIXME add meaning */
					line-name = "sw4_3";
				};
				gtr-sel3-hog {
					gpio-hog;
					gpios = <3 0>;
					input; /* FIXME add meaning */
					line-name = "sw4_4";
				};
			};
		};
		i2c@1 { /* FMCP1_IIC */
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <1>;
			/* FIXME connection to Samtec J51C */
			/* expected eeprom 0x50 SE cards */
		};
		i2c@2 { /* FMCP2_IIC */
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <2>;
			/* FIXME connection to Samtec J53C */
			/* expected eeprom 0x50 SE cards */
		};
		i2c@3 { /* DDR4_DIMM1 */
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <3>;
			si570_ddr_dimm1: clock-generator@60 { /* u2 */
				#clock-cells = <0>;
				compatible = "silabs,si570";
				reg = <0x60>;	/* 570BAB000299DG */
				temperature-stability = <50>;
				factory-fout = <200000000>;
				clock-frequency = <200000000>;
				clock-output-names = "si570_ddrdimm1_clk";
			};
			/* 0x50 SPD? */
		};
		i2c@4 { /* DDR4_DIMM2 */
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <4>;
			si570_ddr_dimm2: clock-generator@60 { /* u3 */
				#clock-cells = <0>;
				compatible = "silabs,si570";
				reg = <0x60>;	/* 570BAB000299DG */
				temperature-stability = <50>;
				factory-fout = <200000000>;
				clock-frequency = <200000000>;
				clock-output-names = "si570_ddrdimm2_clk";
			};
			/* 0x50 SPD? */
		};
		i2c@5 { /* LPDDR4_SI570_CLK */
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <5>;
			si570_lpddr4: clock-generator@60 { /* u4 */
				#clock-cells = <0>;
				compatible = "silabs,si570";
				reg = <0x60>;	/* 570BAB000299DG */
				temperature-stability = <50>;
				factory-fout = <200000000>;
				clock-frequency = <200000000>;
				clock-output-names = "si570_lpddr4_clk";
			};
		};
		i2c@6 { /* HSDP_SI570 */
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <6>;
			si570_hsdp: clock-generator@60 { /* u5 */
				#clock-cells = <0>;
				compatible = "silabs,si570";
				reg = <0x60>;	/* 570JAC000900DG */
				temperature-stability = <50>;
				factory-fout = <156250000>;
				clock-frequency = <156250000>;
				clock-output-names = "si570_hsdp_clk";
			};
		};
		i2c@7 { /* PCIE_CLK */
			#address-cells = <1>;
			#size-cells = <0>;
			reg = <7>;
			/* u36 0xd8 or 0xde - pcie clk buf - 9ZML1241EKILF PCIe GEN 4 CLOCK BUFFER FIXME - no driver */
			/* u37 0xd0 DNP - pcie clocking 1 - 9FGV1006BQ505LTGI - PCIe GEN 4 CLOCK GENERATOR FIXME - no linux driver */
			/* u38 0xca - pcie clocking 2 - 9ZML1241EKILF PCIe GEN 4 CLOCK BUFFER FIXME - no driver */
			/* u39 8T49N240 - pcie clocking 3 */
		};
	};
};

&usb0 {
	status = "okay";
	phy-names = "usb3-phy";
	phys = <&psgtr 1 PHY_TYPE_USB3 0 1>;
};

&dwc3_0 {
	status = "okay";
	dr_mode = "peripheral";
	snps,dis_u2_susphy_quirk;
	snps,dis_u3_susphy_quirk;
	maximum-speed = "super-speed";
};

&usb1 {
	status = "okay";
};

&dwc3_1 {
	/delete-property/ phy-names ;
	/delete-property/ phys ;
	dr_mode = "host";
	maximum-speed = "high-speed";
	snps,dis_u2_susphy_quirk ;
	snps,dis_u3_susphy_quirk ;
	status = "okay";
};

&xilinx_ams {
	status = "okay";
};

&ams_ps {
	status = "okay";
};

&ams_pl {
	status = "okay";
};
