// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
// Copyright (C) 2017 Jagan Teki <jteki@openedev.com>

/dts-v1/;

#include "sun50i-a64.dtsi"
#include "sun50i-a64-cpu-opp.dtsi"

#include <dt-bindings/gpio/gpio.h>

/ {
	model = "Olimex A64-Olinuxino";
	compatible = "olimex,a64-olinuxino", "allwinner,sun50i-a64";

	aliases {
		ethernet0 = &emac;
		serial0 = &uart0;
	};

	chosen {
		stdout-path = "serial0:115200n8";
	};

	hdmi-connector {
		compatible = "hdmi-connector";
		type = "a";

		port {
			hdmi_con_in: endpoint {
				remote-endpoint = <&hdmi_out_con>;
			};
		};
	};

	leds {
		compatible = "gpio-leds";

		led-0 {
			label = "a64-olinuxino:red:user";
			gpios = <&pio 4 17 GPIO_ACTIVE_HIGH>; /* PE17 */
		};
	};

	reg_usb1_vbus: usb1-vbus {
		compatible = "regulator-fixed";
		regulator-name = "usb1-vbus";
		regulator-min-microvolt = <5000000>;
		regulator-max-microvolt = <5000000>;
		regulator-boot-on;
		enable-active-high;
		gpio = <&pio 6 9 GPIO_ACTIVE_HIGH>; /* PG9 */
		status = "okay";
	};

	wifi_pwrseq: pwrseq {
		compatible = "mmc-pwrseq-simple";
		reset-gpios = <&r_pio 0 2 GPIO_ACTIVE_LOW>; /* PL2 */
	};
};

&codec {
	status = "okay";
};

&codec_analog {
	cpvdd-supply = <&reg_eldo1>;
	status = "okay";
};

&cpu0 {
	cpu-supply = <&reg_dcdc2>;
};

&cpu1 {
	cpu-supply = <&reg_dcdc2>;
};

&cpu2 {
	cpu-supply = <&reg_dcdc2>;
};

&cpu3 {
	cpu-supply = <&reg_dcdc2>;
};

&dai {
	status = "okay";
};

&de {
	status = "okay";
};

&ehci0 {
	status = "okay";
};

&ehci1 {
	status = "okay";
};

&emac {
	pinctrl-names = "default";
	pinctrl-0 = <&rgmii_pins>;
	phy-mode = "rgmii";
	phy-handle = <&ext_rgmii_phy>;
	phy-supply = <&reg_dcdc1>;
	allwinner,tx-delay-ps = <600>;
	status = "okay";
};

&hdmi {
	hvcc-supply = <&reg_dldo1>;
	status = "okay";
};

&hdmi_out {
	hdmi_out_con: endpoint {
		remote-endpoint = <&hdmi_con_in>;
	};
};

&mdio {
	ext_rgmii_phy: ethernet-phy@1 {
		compatible = "ethernet-phy-ieee802.3-c22";
		reg = <1>;
	};
};

&mmc0 {
	pinctrl-names = "default";
	pinctrl-0 = <&mmc0_pins>;
	vmmc-supply = <&reg_dcdc1>;
	cd-gpios = <&pio 5 6 GPIO_ACTIVE_LOW>;
	disable-wp;
	bus-width = <4>;
	status = "okay";
};

&mmc1 {
	pinctrl-names = "default";
	pinctrl-0 = <&mmc1_pins>;
	vmmc-supply = <&reg_dcdc1>;
	vqmmc-supply = <&reg_dldo4>;
	mmc-pwrseq = <&wifi_pwrseq>;
	bus-width = <4>;
	non-removable;
	status = "okay";

	rtl8723bs: wifi@1 {
		reg = <1>;
		interrupt-parent = <&r_pio>;
		interrupts = <0 3 IRQ_TYPE_LEVEL_LOW>; /* PL3 */
		interrupt-names = "host-wake";
	};
};

&ohci0 {
	status = "okay";
};

&ohci1 {
	status = "okay";
};

&pio {
	vcc-pc-supply = <&reg_dcdc1>;
	vcc-pd-supply = <&reg_dcdc1>;
	vcc-pe-supply = <&reg_aldo1>;
	vcc-pg-supply = <&reg_dldo4>;
};

&r_pio {
	/*
	 * FIXME: We can't add that supply for now since it would
	 * create a circular dependency between pinctrl, the regulator
	 * and the RSB Bus.
	 *
	 * vcc-pl-supply = <&reg_aldo2>;
	 */
};

&pio {
	vcc-pa-supply = <&reg_dcdc1>;
	vcc-pb-supply = <&reg_dcdc1>;
	vcc-pc-supply = <&reg_dcdc1>;
	vcc-pd-supply = <&reg_dcdc1>;
	vcc-pe-supply = <&reg_aldo1>;
	vcc-pf-supply = <&reg_dcdc1>;
	vcc-pg-supply = <&reg_dldo4>;
	vcc-ph-supply = <&reg_dcdc1>;
};

&r_rsb {
	status = "okay";

	axp803: pmic@3a3 {
		compatible = "x-powers,axp803";
		reg = <0x3a3>;
		interrupt-parent = <&r_intc>;
		interrupts = <0 IRQ_TYPE_LEVEL_LOW>;
		x-powers,drive-vbus-en;	/* set N_VBUSEN as output pin */
	};
};

/* VCC-PL is powered by aldo2 but we cannot add it as the RSB */
/* interface used to talk to the PMIC in on the PL pins */
/* &r_pio { */
/*	vcc-pl-supply = <&reg_aldo2>; */
/* }; */

#include "axp803.dtsi"

&ac_power_supply {
	status = "okay";
};

&battery_power_supply {
	status = "okay";
};

&reg_aldo1 {
	regulator-always-on;
	regulator-min-microvolt = <2800000>;
	regulator-max-microvolt = <2800000>;
	regulator-name = "vcc-pe";
};

&reg_aldo2 {
	regulator-always-on;
	regulator-min-microvolt = <3300000>;
	regulator-max-microvolt = <3300000>;
	regulator-name = "vcc-pl";
};

&reg_aldo3 {
	regulator-always-on;
	regulator-min-microvolt = <3000000>;
	regulator-max-microvolt = <3000000>;
	regulator-name = "vcc-pll-avcc";
};

&reg_dcdc1 {
	regulator-always-on;
	regulator-min-microvolt = <3300000>;
	regulator-max-microvolt = <3300000>;
	regulator-name = "vcc-3v3";
};

&reg_dcdc2 {
	regulator-always-on;
	regulator-min-microvolt = <1040000>;
	regulator-max-microvolt = <1300000>;
	regulator-name = "vdd-cpux";
};

/* DCDC3 is polyphased with DCDC2 */

/*
 * The board uses DDR3L DRAM chips. 1.36V is the closest to the nominal
 * 1.35V that the PMIC can drive.
 */
&reg_dcdc5 {
	regulator-always-on;
	regulator-min-microvolt = <1360000>;
	regulator-max-microvolt = <1360000>;
	regulator-name = "vcc-ddr3";
};

&reg_dcdc6 {
	regulator-always-on;
	regulator-min-microvolt = <1100000>;
	regulator-max-microvolt = <1100000>;
	regulator-name = "vdd-sys";
};

&reg_dldo1 {
	regulator-min-microvolt = <3300000>;
	regulator-max-microvolt = <3300000>;
	regulator-name = "vcc-hdmi";
};

&reg_dldo2 {
	regulator-min-microvolt = <3300000>;
	regulator-max-microvolt = <3300000>;
	regulator-name = "vcc-mipi";
};

&reg_dldo3 {
	regulator-min-microvolt = <2800000>;
	regulator-max-microvolt = <2800000>;
	regulator-name = "vcc-avdd-csi";
};

&reg_dldo4 {
	regulator-min-microvolt = <3300000>;
	regulator-max-microvolt = <3300000>;
	regulator-name = "vcc-wifi-io";
};

&reg_drivevbus {
	regulator-name = "usb0-vbus";
	status = "okay";
};

&reg_eldo1 {
	regulator-min-microvolt = <1800000>;
	regulator-max-microvolt = <1800000>;
	regulator-name = "cpvdd";
};

&reg_eldo2 {
	regulator-min-microvolt = <1800000>;
	regulator-max-microvolt = <1800000>;
	regulator-name = "vcc-dvdd-csi";
};

&reg_fldo1 {
	regulator-min-microvolt = <1200000>;
	regulator-max-microvolt = <1200000>;
	regulator-name = "vcc-1v2-hsic";
};

/*
 * The A64 chip cannot work without this regulator off, although
 * it seems to be only driving the AR100 core.
 * Maybe we don't still know well about CPUs domain.
 */
&reg_fldo2 {
	regulator-always-on;
	regulator-min-microvolt = <1100000>;
	regulator-max-microvolt = <1100000>;
	regulator-name = "vdd-cpus";
};

&reg_rtc_ldo {
	regulator-name = "vcc-rtc";
};

&simplefb_hdmi {
	vcc-hdmi-supply = <&reg_dldo1>;
};

&sound {
	simple-audio-card,aux-devs = <&codec_analog>;
	simple-audio-card,widgets = "Microphone", "Microphone Jack Left",
		    "Microphone", "Microphone Jack Right",
		    "Headphone", "Headphone Jack";
	simple-audio-card,routing = "Left DAC", "DACL",
		    "Right DAC", "DACR",
		    "Headphone Jack", "HP",
		    "ADCL", "Left ADC",
		    "ADCR", "Right ADC",
		    "Microphone Jack Left", "MBIAS",
		    "MIC1", "Microphone Jack Left",
		    "Microphone Jack Right", "MBIAS",
		    "MIC2", "Microphone Jack Right";
	status = "okay";
};

&uart0 {
	pinctrl-names = "default";
	pinctrl-0 = <&uart0_pb_pins>;
	status = "okay";
};

&usb_otg {
	dr_mode = "otg";
	status = "okay";
};

&usbphy {
	status = "okay";
	usb0_id_det-gpios = <&pio 7 9 GPIO_ACTIVE_HIGH>; /* PH9 */
	usb0_vbus-supply = <&reg_drivevbus>;
	usb1_vbus-supply = <&reg_usb1_vbus>;
};
