# Configuration for building U-Boot to be flashed
# to the uefi partition of QCS9100 based dev boards with
# the "Linux Embedded" partition layout (which have
# a dedicated "uefi" partition for edk2/U-Boot)

#include "qcom_defconfig"

# Address where U-Boot will be loaded
CONFIG_TEXT_BASE=0xaf000000
CONFIG_REMAKE_ELF=y
CONFIG_DEFAULT_DEVICE_TREE="qcom/qcs9100-ride-r3"
CONFIG_ENV_IS_IN_SCSI=y
CONFIG_SCSI_ENV_PART_UUID="71cb9cd0-acf1-b6cb-ad91-be9572fe11a9"
# CONFIG_ENV_IS_DEFAULT is not set
# CONFIG_ENV_IS_NOWHERE is not set
