# Configuration for building U-Boot to be flashed
# to the uefi partition of QCS8300 dev boards with
# the "Linux Embedded" partition layout (which have
# a dedicated "uefi_a" partition for edk2/U-Boot)

#include "qcom_defconfig"

# Otherwise buildman thinks this isn't an ARM platform
CONFIG_ARM=y

CONFIG_DEBUG_UART=y
CONFIG_DEBUG_UART_ANNOUNCE=y
CONFIG_DEBUG_UART_BASE=0x99C000
CONFIG_DEBUG_UART_MSM_GENI=y
CONFIG_DEBUG_UART_CLOCK=14745600

# Address where U-Boot will be loaded
CONFIG_TEXT_BASE=0xaf000000
CONFIG_REMAKE_ELF=y

CONFIG_DEFAULT_DEVICE_TREE="qcom/qcs8300-ride"
