# Configuration for building U-Boot to be flashed
# to the uefi partition of QCM6490 dev boards with
# the "Linux Embedded" partition layout (which have
# a dedicated "uefi" partition for edk2/U-Boot)

#include "qcom_defconfig"

# Otherwise buildman thinks this isn't an ARM platform
CONFIG_ARM=y

# Address where U-Boot will be loaded
CONFIG_TEXT_BASE=0x9fc00000
CONFIG_REMAKE_ELF=y

CONFIG_DEFAULT_DEVICE_TREE="qcom/qcs6490-rb3gen2"
