// SPDX-License-Identifier: GPL-2.0+
/*
 * Topic Miami Plus board DTS
 *
 * Copyright (C) 2016 Topic Embedded Products
 */
#include "zynq-topic-miami.dts"

/ {
	model = "Topic Miami+ Zynq Board";
	compatible = "topic,miamiplus", "xlnx,zynq-7000";
};

/* The miamiplus contains a speedgrade-2 device and runs at 800MHz */
&cpu0 {
	operating-points = <
		/* kHz    uV */
		800000  1000000
		400000  1000000
	>;
};

&qspi {
};
