// SPDX-License-Identifier: GPL-2.0+
/*
 * SAMSUNG Arndale board device tree source
 *
 * Copyright (c) 2013 Samsung Electronics Co., Ltd.
 *		http://www.samsung.com
 */

/dts-v1/;
#include "exynos5250.dtsi"

/ {
	model = "SAMSUNG Arndale board based on EXYNOS5250";
	compatible = "samsung,arndale", "samsung,exynos5250";

	aliases {
		i2c0 = "/i2c@12C60000";
		i2c1 = "/i2c@12C70000";
		i2c2 = "/i2c@12C80000";
		i2c3 = "/i2c@12C90000";
		i2c4 = "/i2c@12CA0000";
		i2c5 = "/i2c@12CB0000";
		i2c6 = "/i2c@12CC0000";
		i2c7 = "/i2c@12CD0000";
		serial0 = "/serial@12C20000";
		console = "/serial@12C20000";
	};

	mmc@12200000 {
		bus-width = <8>;
		samsung,dw-mshc-ciu-div = <3>;
		samsung,dw-mshc-sdr-timing = <1 3>;
	};

	mmc@12210000 {
		status = "disabled";
	};

	mmc@12220000 {
		bus-width = <4>;
		samsung,dw-mshc-ciu-div = <3>;
		samsung,dw-mshc-sdr-timing = <1 2>;
	};

	mmc@12230000 {
		status = "disabled";
	};
};
