// SPDX-License-Identifier: (GPL-2.0+ OR MIT)
/*
 * (C) Copyright 2021 Rockchip Electronics Co., Ltd
 */

#include "rockchip-u-boot.dtsi"

/ {
	aliases {
		mmc0 = &sdhci;
		mmc1 = &sdmmc0;
		spi4 = &sfc;
	};

	chosen {
		u-boot,spl-boot-order = "same-as-spl", &sdmmc0, &sdhci;
	};

	dmc: dmc {
		compatible = "rockchip,rk3568-dmc";
		bootph-all;
	};

	otp: nvmem@fe38c000 {
		compatible = "rockchip,rk3568-otp";
		reg = <0x0 0xfe38c000 0x0 0x4000>;
		#address-cells = <1>;
		#size-cells = <1>;

		cpu_id: id@a {
			reg = <0x0a 0x10>;
		};
	};
};

#ifdef CONFIG_ROCKCHIP_SPI_IMAGE
&binman {
	simple-bin-spi {
		mkimage {
			args = "-n", CONFIG_SYS_SOC, "-T", "rksd";
			offset = <0x8000>;
		};
	};
};
#endif

&cru {
	bootph-all;
};

&emmc_bus8 {
	bootph-pre-ram;
	bootph-some-ram;
};

&emmc_clk {
	bootph-pre-ram;
	bootph-some-ram;
};

&emmc_cmd {
	bootph-pre-ram;
	bootph-some-ram;
};

&emmc_datastrobe {
	bootph-pre-ram;
	bootph-some-ram;
};

&emmc_rstnout {
	bootph-pre-ram;
	bootph-some-ram;
};

&fspi_pins {
	bootph-pre-ram;
	bootph-some-ram;
};

&grf {
	bootph-all;
};

&otp {
	bootph-some-ram;
};

&pcfg_pull_none {
	bootph-all;
};

&pcfg_pull_none_smt {
	bootph-pre-ram;
	bootph-some-ram;
};

&pcfg_pull_up {
	bootph-all;
};

&pcfg_pull_up_drv_level_2 {
	bootph-pre-ram;
	bootph-some-ram;
};

&pinctrl {
	bootph-all;
};

&pmucru {
	bootph-all;
};

&pmugrf {
	bootph-all;
};

&rng {
	status = "okay";
};

&sdhci {
	bootph-pre-ram;
	bootph-some-ram;
	max-frequency = <200000000>;
};

&sdmmc0 {
	bootph-pre-ram;
	bootph-some-ram;
};

&sdmmc0_bus4 {
	bootph-pre-ram;
	bootph-some-ram;
};

&sdmmc0_clk {
	bootph-pre-ram;
	bootph-some-ram;
};

&sdmmc0_cmd {
	bootph-pre-ram;
	bootph-some-ram;
};

&sdmmc0_det {
	bootph-pre-ram;
	bootph-some-ram;
};

&sdmmc0_pwren {
	bootph-pre-ram;
	bootph-some-ram;
};

&sfc {
	bootph-some-ram;
	u-boot,spl-sfc-no-dma;
};

&uart2 {
	bootph-all;
	clock-frequency = <24000000>;
};

&uart2m0_xfer {
	bootph-all;
};

&xin24m {
	bootph-all;
};
