CONFIG_ARM=y
CONFIG_SKIP_LOWLEVEL_INIT=y
CONFIG_COUNTER_FREQUENCY=24000000
CONFIG_ARCH_ROCKCHIP=y
CONFIG_SPL_GPIO=y
CONFIG_NR_DRAM_BANKS=1
CONFIG_SF_DEFAULT_SPEED=20000000
CONFIG_ENV_SIZE=0x3000
CONFIG_DEFAULT_DEVICE_TREE="rockchip/rk3399-puma-haikou"
CONFIG_DM_RESET=y
CONFIG_ROCKCHIP_RK3399=y
CONFIG_ROCKCHIP_BOOT_MODE_REG=0x0
CONFIG_ROCKCHIP_SPI_IMAGE=y
CONFIG_TARGET_PUMA_RK3399=y
CONFIG_SYS_LOAD_ADDR=0x800800
CONFIG_SF_DEFAULT_BUS=1
CONFIG_DEBUG_UART_BASE=0xFF180000
CONFIG_DEBUG_UART_CLOCK=24000000
CONFIG_SPL_SPI_FLASH_SUPPORT=y
CONFIG_SPL_SPI=y
CONFIG_DEBUG_UART=y
CONFIG_DEFAULT_FDT_FILE="rockchip/rk3399-puma-haikou.dtb"
CONFIG_CONSOLE_MUX=y
CONFIG_DISPLAY_BOARDINFO_LATE=y
CONFIG_SPL_MAX_SIZE=0x2e000
CONFIG_SPL_PAD_TO=0x38000
# CONFIG_SPL_RAW_IMAGE_SUPPORT is not set
CONFIG_SYS_MMCSD_RAW_MODE_U_BOOT_SECTOR=0x200
CONFIG_SPL_I2C=y
CONFIG_SPL_POWER=y
CONFIG_SPL_SPI_LOAD=y
CONFIG_TPL=y
CONFIG_TPL_GPIO=y
# CONFIG_BOOTM_NETBSD is not set
# CONFIG_BOOTM_PLAN9 is not set
# CONFIG_BOOTM_RTEMS is not set
# CONFIG_CMD_VBE is not set
# CONFIG_BOOTM_VXWORKS is not set
CONFIG_CMD_ERASEENV=y
CONFIG_CMD_GPIO=y
CONFIG_CMD_GPT=y
CONFIG_CMD_I2C=y
CONFIG_CMD_MMC=y
CONFIG_CMD_SPI=y
CONFIG_CMD_USB=y
# CONFIG_CMD_SETEXPR is not set
CONFIG_CMD_CACHE=y
CONFIG_CMD_TIME=y
CONFIG_CMD_PMIC=y
CONFIG_CMD_REGULATOR=y
CONFIG_CMD_EROFS=y
CONFIG_CMD_SQUASHFS=y
CONFIG_SPL_OF_CONTROL=y
CONFIG_OF_SPL_REMOVE_PROPS="interrupt-parent assigned-clocks assigned-clock-rates assigned-clock-parents"
CONFIG_ENV_OVERWRITE=y
CONFIG_ENV_IS_IN_MMC=y
CONFIG_ENV_IS_IN_SPI_FLASH=y
CONFIG_ENV_SPI_MAX_HZ=50000000
CONFIG_ENV_RELOC_GD_ENV_ADDR=y
CONFIG_ENV_MMC_DEVICE_INDEX=1
CONFIG_ENV_VARS_UBOOT_RUNTIME_CONFIG=y
CONFIG_BUTTON=y
CONFIG_BUTTON_GPIO=y
CONFIG_GPIO_HOG=y
CONFIG_SPL_GPIO_HOG=y
CONFIG_ROCKCHIP_GPIO=y
CONFIG_SYS_I2C_ROCKCHIP=y
CONFIG_MMC_DW=y
CONFIG_MMC_DW_ROCKCHIP=y
CONFIG_MMC_SDHCI=y
CONFIG_MMC_SDHCI_SDMA=y
CONFIG_MMC_SDHCI_ROCKCHIP=y
CONFIG_SPI_FLASH_GIGADEVICE=y
CONFIG_SPI_FLASH_WINBOND=y
CONFIG_PHY_ANEG_TIMEOUT=30000
CONFIG_PHY_MICREL=y
CONFIG_PHY_MICREL_KSZ90X1=y
CONFIG_ETH_DESIGNWARE=y
CONFIG_GMAC_ROCKCHIP=y
CONFIG_PHY_ROCKCHIP_INNO_USB2=y
CONFIG_PHY_ROCKCHIP_TYPEC=y
CONFIG_TPL_PINCTRL=y
CONFIG_TPL_PINCTRL_FULL=y
CONFIG_DM_PMIC_FAN53555=y
CONFIG_PMIC_RK8XX=y
CONFIG_SPL_PMIC_RK8XX=y
CONFIG_REGULATOR_PWM=y
CONFIG_REGULATOR_RK8XX=y
CONFIG_PWM_ROCKCHIP=y
CONFIG_DM_RTC=y
CONFIG_RTC_ISL1208=y
CONFIG_DEBUG_UART_SHIFT=2
CONFIG_SYS_NS16550_MEM32=y
CONFIG_ROCKCHIP_SPI=y
CONFIG_SYSRESET=y
CONFIG_USB=y
CONFIG_USB_XHCI_HCD=y
CONFIG_USB_EHCI_HCD=y
CONFIG_USB_EHCI_GENERIC=y
CONFIG_USB_DWC3=y
CONFIG_USB_DWC3_GENERIC=y
CONFIG_USB_ONBOARD_HUB=y
CONFIG_USB_HOST_ETHER=y
CONFIG_USB_ETHER_ASIX=y
CONFIG_USB_ETHER_ASIX88179=y
CONFIG_USB_ETHER_MCS7830=y
CONFIG_USB_ETHER_RTL8152=y
CONFIG_USB_ETHER_SMSC95XX=y
CONFIG_FS_EXFAT=y
CONFIG_ERRNO_STR=y
