CONFIG_ARM=y
CONFIG_SKIP_LOWLEVEL_INIT=y
CONFIG_SPL_SKIP_LOWLEVEL_INIT=y
CONFIG_TPL_SKIP_LOWLEVEL_INIT=y
CONFIG_SYS_ARCH_TIMER=y
CONFIG_ARCH_ROCKCHIP=y
CONFIG_TEXT_BASE=0x61000000
CONFIG_NR_DRAM_BANKS=2
CONFIG_HAS_CUSTOM_SYS_INIT_SP_ADDR=y
CONFIG_CUSTOM_SYS_INIT_SP_ADDR=0x61100000
CONFIG_ENV_OFFSET=0x3F8000
CONFIG_DEFAULT_DEVICE_TREE="rk3229-evb"
CONFIG_ROCKCHIP_RK322X=y
CONFIG_TARGET_EVB_RK3229=y
CONFIG_SPL_STACK_R_ADDR=0x60600000
CONFIG_SPL_TEXT_BASE=0x60000000
CONFIG_SPL_STACK_R=y
CONFIG_SYS_BOOTM_LEN=0x4000000
CONFIG_SYS_LOAD_ADDR=0x61800800
CONFIG_DEBUG_UART_BASE=0x11030000
CONFIG_DEBUG_UART_CLOCK=24000000
CONFIG_DEBUG_UART=y
CONFIG_FIT=y
CONFIG_FIT_VERBOSE=y
CONFIG_SPL_LOAD_FIT=y
CONFIG_USE_PREBOOT=y
CONFIG_DEFAULT_FDT_FILE="rk3229-evb.dtb"
# CONFIG_DISPLAY_CPUINFO is not set
CONFIG_DISPLAY_BOARDINFO_LATE=y
CONFIG_SPL_MAX_SIZE=0x100000
CONFIG_SPL_NO_BSS_LIMIT=y
# CONFIG_SPL_RAW_IMAGE_SUPPORT is not set
CONFIG_CMD_GPT=y
CONFIG_CMD_MMC=y
CONFIG_CMD_USB_MASS_STORAGE=y
# CONFIG_CMD_SETEXPR is not set
CONFIG_CMD_TIME=y
CONFIG_SPL_OF_CONTROL=y
CONFIG_TPL_OF_CONTROL=y
CONFIG_OF_SPL_REMOVE_PROPS="pinctrl-0 pinctrl-names clock-names interrupt-parent assigned-clocks assigned-clock-rates assigned-clock-parents"
CONFIG_ENV_IS_IN_MMC=y
CONFIG_ENV_RELOC_GD_ENV_ADDR=y
CONFIG_NET_RANDOM_ETHADDR=y
CONFIG_REGMAP=y
CONFIG_SPL_REGMAP=y
CONFIG_TPL_REGMAP=y
CONFIG_SYSCON=y
CONFIG_SPL_SYSCON=y
CONFIG_TPL_SYSCON=y
CONFIG_CLK=y
CONFIG_SPL_CLK=y
CONFIG_TPL_CLK=y
CONFIG_FASTBOOT_BUF_SIZE=0x04000000
CONFIG_FASTBOOT_CMD_OEM_FORMAT=y
CONFIG_ROCKCHIP_GPIO=y
CONFIG_SYS_I2C_ROCKCHIP=y
CONFIG_MMC_DW=y
CONFIG_MMC_DW_ROCKCHIP=y
CONFIG_ETH_DESIGNWARE=y
CONFIG_GMAC_ROCKCHIP=y
CONFIG_PHY=y
CONFIG_PINCTRL=y
CONFIG_RAM=y
CONFIG_SPL_RAM=y
CONFIG_TPL_RAM=y
CONFIG_BAUDRATE=1500000
CONFIG_DEBUG_UART_SHIFT=2
CONFIG_SYS_NS16550_MEM32=y
CONFIG_SYSRESET=y
CONFIG_USB=y
CONFIG_USB_GADGET=y
CONFIG_USB_GADGET_DWC2_OTG=y
CONFIG_TPL_TINY_MEMSET=y
CONFIG_ERRNO_STR=y
