#include <configs/socfpga_agilex_defconfig>

CONFIG_NR_DRAM_BANKS=1
CONFIG_SPL_LDSCRIPT="arch/arm/mach-socfpga/u-boot-spl-soc64.lds"
# CONFIG_TARGET_SOCFPGA_AGILEX_SOCDK is not set
# CONFIG_IDENT_STRING is not set
CONFIG_SPL_BSS_START_ADDR=0x1ff00000
CONFIG_TARGET_SOCFPGA_AGILEX7M_SOCDK=y
CONFIG_IDENT_STRING="socfpga_agilex7m"
# CONFIG_QSPI_BOOT is not set
CONFIG_SPL_CUSTOM_SYS_MALLOC_ADDR=0x1fa00000
CONFIG_SYS_PROMPT="SOCFPGA_AGILEX7M # "
CONFIG_MTDIDS_DEFAULT="nand0=ffb90000.nand.0"
CONFIG_MTDPARTS_DEFAULT="mtdparts=ffb90000.nand.0:2m(u-boot),-(root)"
# CONFIG_ENV_IS_IN_UBI is not set
# CONFIG_ENV_UBI_PART is not set
# CONFIG_ENV_UBI_VOLUME is not set
# CONFIG_USE_BOOTFILE is not set
# CONFIG_DESIGNWARE_SPI is not set
