CONFIG_ARM=y
CONFIG_ARCH_STM32MP=y
CONFIG_SYS_MALLOC_F_LEN=0x3000
CONFIG_HAS_CUSTOM_SYS_INIT_SP_ADDR=y
CONFIG_CUSTOM_SYS_INIT_SP_ADDR=0xc0100000
CONFIG_ENV_OFFSET=0x280000
CONFIG_DEFAULT_DEVICE_TREE="st/stm32mp157a-microgea-stm32mp1-microdev2.0-of7"
CONFIG_SPL_MMC=y
CONFIG_SPL_STACK=0x30000000
CONFIG_SPL_TEXT_BASE=0x2FFC2500
CONFIG_SYS_BOOTM_LEN=0x2000000
CONFIG_SYS_LOAD_ADDR=0xc2000000
CONFIG_SPL=y
CONFIG_ENV_OFFSET_REDUND=0x2C0000
CONFIG_TARGET_MICROGEA_STM32MP1=y
# CONFIG_ARMV7_VIRT is not set
CONFIG_SYS_MEMTEST_START=0xc0000000
CONFIG_SYS_MEMTEST_END=0xc4000000
CONFIG_FIT=y
CONFIG_DISTRO_DEFAULTS=y
CONFIG_BOOTCOMMAND="run bootcmd_stm32mp"
CONFIG_SYS_PBSIZE=1050
# CONFIG_BOARD_INIT is not set
CONFIG_SPL_FOOTPRINT_LIMIT=y
CONFIG_SPL_MAX_FOOTPRINT=0x3db00
# CONFIG_SPL_SHARES_INIT_SP_ADDR is not set
CONFIG_SPL_HAVE_INIT_STACK=y
CONFIG_SPL_SYS_MALLOC=y
CONFIG_SPL_HAS_CUSTOM_MALLOC_START=y
CONFIG_SPL_CUSTOM_SYS_MALLOC_ADDR=0xc0300000
CONFIG_SPL_SYS_MALLOC_SIZE=0x1d00000
CONFIG_SPL_SYS_MMCSD_RAW_MODE=y
CONFIG_SYS_MMCSD_RAW_MODE_U_BOOT_USE_PARTITION=y
CONFIG_SYS_MMCSD_RAW_MODE_U_BOOT_PARTITION=0x3
CONFIG_SPL_ENV_SUPPORT=y
CONFIG_SPL_I2C=y
CONFIG_SPL_POWER=y
CONFIG_SYS_PROMPT="STM32MP> "
CONFIG_CMD_ADTIMG=y
CONFIG_CMD_ERASEENV=y
CONFIG_CMD_MEMINFO=y
CONFIG_CMD_MEMTEST=y
CONFIG_CMD_ADC=y
CONFIG_CMD_CLK=y
CONFIG_CMD_FUSE=y
CONFIG_CMD_GPIO=y
CONFIG_CMD_I2C=y
CONFIG_CMD_MMC=y
CONFIG_CMD_REMOTEPROC=y
CONFIG_SYS_DISABLE_AUTOLOAD=y
CONFIG_CMD_CACHE=y
CONFIG_CMD_TIME=y
CONFIG_CMD_TIMER=y
CONFIG_CMD_PMIC=y
CONFIG_CMD_REGULATOR=y
CONFIG_CMD_EXT4_WRITE=y
# CONFIG_SPL_DOS_PARTITION is not set
CONFIG_OF_SPL_REMOVE_PROPS="interrupts interrupt-names interrupts-extended interrupt-controller \\\#interrupt-cells interrupt-parent dmas dma-names assigned-clocks assigned-clock-rates assigned-clock-parents hwlocks"
CONFIG_ENV_IS_NOWHERE=y
CONFIG_ENV_IS_IN_MMC=y
CONFIG_ENV_REDUNDANT=y
CONFIG_ENV_RELOC_GD_ENV_ADDR=y
# CONFIG_SPL_ENV_IS_NOWHERE is not set
CONFIG_USE_SERVERIP=y
CONFIG_SERVERIP="192.168.1.1"
CONFIG_DM_HWSPINLOCK=y
CONFIG_HWSPINLOCK_STM32=y
CONFIG_DM_I2C=y
CONFIG_SYS_I2C_STM32F7=y
CONFIG_LED=y
CONFIG_LED_GPIO=y
CONFIG_STM32_FMC2_EBI=y
CONFIG_SUPPORT_EMMC_BOOT=y
CONFIG_STM32_SDMMC2=y
CONFIG_PHY_REALTEK=y
CONFIG_DWC_ETH_QOS=y
CONFIG_PHY=y
CONFIG_PINCONF=y
# CONFIG_SPL_PINCTRL_FULL is not set
CONFIG_PINCTRL_STMFX=y
CONFIG_DM_PMIC=y
# CONFIG_SPL_PMIC_CHILDREN is not set
CONFIG_PMIC_STPMIC1=y
CONFIG_DM_REGULATOR=y
CONFIG_DM_REGULATOR_FIXED=y
CONFIG_DM_REGULATOR_GPIO=y
CONFIG_REMOTEPROC_STM32_COPRO=y
CONFIG_DM_RTC=y
CONFIG_RTC_STM32=y
CONFIG_SERIAL_RX_BUFFER=y
CONFIG_SYSRESET_SYSCON=y
CONFIG_WATCHDOG_AUTOSTART=y
CONFIG_WDT=y
CONFIG_WDT_STM32MP=y
# CONFIG_BINMAN_FDT is not set
CONFIG_LZO=y
CONFIG_ERRNO_STR=y
