CONFIG_ARM=y
CONFIG_COUNTER_FREQUENCY=25165824
CONFIG_TARGET_THUNDERX_88XX=y
CONFIG_TEXT_BASE=0x00500000
CONFIG_SYS_MALLOC_LEN=0x101000
CONFIG_SYS_MALLOC_F_LEN=0x400
CONFIG_NR_DRAM_BANKS=1
CONFIG_HAS_CUSTOM_SYS_INIT_SP_ADDR=y
CONFIG_CUSTOM_SYS_INIT_SP_ADDR=0x57fff0
CONFIG_ENV_SIZE=0x1000
CONFIG_DEFAULT_DEVICE_TREE="thunderx-88xx"
CONFIG_SYS_BOOTM_LEN=0x800000
CONFIG_SYS_LOAD_ADDR=0x500000
CONFIG_DEBUG_UART_BASE=0x87e024000000
CONFIG_DEBUG_UART_CLOCK=24000000
CONFIG_IDENT_STRING=" for Cavium Thunder CN88XX ARM v8 Multi-Core"
CONFIG_DEBUG_UART=y
CONFIG_REMAKE_ELF=y
CONFIG_BOOTDELAY=5
CONFIG_USE_BOOTARGS=y
CONFIG_BOOTARGS="console=ttyAMA0,115200n8 earlycon=pl011,0x87e024000000 debug maxcpus=48 rootwait rw root=/dev/sda2 coherent_pool=16M"
CONFIG_SYS_CBSIZE=512
CONFIG_SYS_PBSIZE=544
# CONFIG_DISPLAY_CPUINFO is not set
# CONFIG_DISPLAY_BOARDINFO is not set
# CONFIG_BOARD_INIT is not set
CONFIG_HUSH_PARSER=y
# CONFIG_AUTO_COMPLETE is not set
CONFIG_SYS_PROMPT="ThunderX_88XX> "
# CONFIG_CMD_EXPORTENV is not set
# CONFIG_CMD_IMPORTENV is not set
# CONFIG_CMD_EDITENV is not set
# CONFIG_CMD_SAVEENV is not set
# CONFIG_CMD_ENV_EXISTS is not set
CONFIG_ENV_RELOC_GD_ENV_ADDR=y
CONFIG_NO_NET=y
# CONFIG_MMC is not set
CONFIG_DM_SERIAL=y
CONFIG_DEBUG_UART_SKIP_INIT=y
